arXiv:0705.2386v1 [physics.ins-det] 16 May 2007

A large acceptance scintillator detector with wavelength shifting fibre read-out for search of eta-nucleus bound states

The GEM Collaboration: M.G.Betigeri^a, P.K.Biswas^b, A. Budzanowski^c, A. Chatterjee^a, R. Jahn^d, S.Guha^b, P.Hawranek^e, B.K.Jain^n, S.B.Jawale^b, V. Jha^{a,}∗ , K. Kilian^f, S. Kliczewski^c, Da. Kirillov^f, Di. Kirillov^g, D. Kolev^h, M. Kravcikova^i, T. Kutsarova^j, M. Lesiak^f , J. Lieb^k, H. Machner^{f,o}, A. Magiera^e, R. Maier^f, G. Martinska^ℓ, S. Nedev^m, N. Piskunov^g, D. Prasuhn^f, D. Protić^f, J. Ritman^f, P. von Rossen^f , B. J. Roy^a, P. Shukla^a, I. Sitnik^g, R. Siudak^{c,f}, R. Tsenov^h, M. Ulicny^ℓ, J. Urban^ℓ, G. Vankova^{f,h}

aNuclear Physics Division, BARC, Mumbai-400 085, India bCentre for Design and Manufacture, BARC, Mumbai-400 085, India cInstitute of Nuclear Physics, Polish Academy of Sciences, Krakow, Poland dHelmholtz-Institut für Strahlen- und Kernphysik der Universität Bonn, Bonn, Germany eInstitute of Physics, Jagellonian University, Krakow, Poland f Institut für Kernphysik, Forschungszentrum Jülich, Jülich, Germany gLaboratory for High Energies, JINR Dubna, Russia

Preprint submitted to Nucl. Instr. and Meth. in Phys. Res. A 5 May 2019 hPhysics Faculty, University of Sofia, Sofia, Bulgaria iTechnical University Kosice, Kosice, Slovakia jInstitute of Nuclear Physics and Nuclear Energy, Sofia, Bulgaria kPhysics Department, George Mason University, Fairfax, Virginia, USA ℓP. J. Safarik University, Kosice, Slovakia mUniversity of Chemical Technology and Metallurgy, Sofia, Bulgaria nPhysics Department, Mumbai University, Vidyanagari, Mumbai oFachbereich Physik, Universität Duisburg-Essen, Duisburg, Germany

Abstract

A large acceptance scintillator detector with wavelength shifting optical fibre readout has been designed and built to detect the decay particles of η-nucleus bound system (the so-called η-mesic nuclei), namely, protons and pions. The detector, named as ENSTAR detector, consists of 122 pieces of plastic scintillator of various shapes and sizes, which are arranged in a cylindrical geometry to provide particle identification, energy loss and coarse position information for these particles. A solid angle coverage of ∼95% of total 4π is obtained in the present design of the detector. Monte Carlo phase space calculations performed to simulate the formation and decay of η-mesic nuclei suggest that its decay particles, the protons and pions are emitted with an opening angle of 150^∘ ± 20^∘, and with energies in the range of 25 to 300 MeV and 225 to 450 MeV respectively. The detailed GEANT simulations show that ∼ 80 % of the decay particles (protons and pions) can be detected within ENSTAR. Several test measurements using alpha source, cosmic-ray muons etc. have been carried out to study the response of ENSTAR scintillator pieces. The inbeam tests of fully assembled detector with proton beam of momentum 870 MeV/c from the Cooler synchrotron COSY have been performed. The test results show that the scintillator fiber design chosen for the detector has performed satisfactorily well. The present article describes the detector design, simulation studies, construction details and test results.

Key words: Scintillator detector; WLS optical fibre read-out; Eta-nucleus bound states

1 Introduction 1

A large acceptance plastic scintillator detector ENSTAR has been designed 2 and built for studies of η-mesic nuclei - a bound system of η-meson and a 3 nucleus. The finding of strong and attractive nature of the η-nucleon(η-N) 4 scattering length and the presence of a resonance near the η-N threshold, pro- 5 vide an interesting possibility of the formation of η-nucleus bound states [1,2]. 6 The experimental confirmation of the existence of such bound systems would 7 open up new avenues for elucidation of the η-nucleus dynamics at intermediate 8 energies. Such experiments [3] are being performed at the intermediate energy 9 accelerator facility COSY Jülich, using GeV energy proton beam. The exper- 10 iments use recoil-free transfer reactions p+(^Z X_A) →^3He + (^{Z−1}X_{A−2})_η on 11 several target nuclei X = Li, C, Al, etc. The expected cross section for events 12 corresponding to formation of η-mesic nuclei is rather low, hence, a dedicated 13 detection system is needed to enhance the sensitivity of the measurement. 14 ENSTAR is the part of detection system which has been developed in order 15 to obtain an unambiguous signal for the formation and decay of the η-nucleus 16 ∗ Corresponding author. Nuclear Physics Division, BARC, Trombay, Mumbai- 400085, India. Tel:++91-22-25593457; Fax: ++91-22-25505151.

Email address: vjha@barc.gov.in (V. Jha).

bound state. The outgoing^3He particles are detected in the Big Karl detec- 17 tion system [4,5], which includes a magnetic spectrograph and its focal plane 18 detectors consisting of drift chambers and scintillator hodoscopes. The corre- 19 sponding proton and pion from the decay of η-mesic nucleus are registered in 20 ENSTAR. In addition to the η-bound states search, the ENSTAR detector can 21 also be used in many other experiments where the missing mass determination 22 of the reaction product needs to be done in coincidence with its decay prod- 23 ucts e.g., for the study of Δ interaction in nuclear matter, where the decay 24 products of Δ states, protons and pions can be detected by ENSTAR [6]. The 25 details of the Big Karl spectrometer have been reported elsewhere [4,5]. In this 26 paper, the description of the newly built ENSTAR detector is reported. The 27 geometric design, simulation studies and fabrication procedure are described. 28 Test measurements done at various stages during the construction of ENSTAR 29 as well as the in-beam tests performed at the COSY accelerator are presented. 30

2 Physics background and ENSTAR design considerations 31

Phase space calculations to simulate eta-mesic nucleus decay events were per- 32 formed using the N-body Monte-Carlo event generator program “Genbod” [7]. 33 The program generates multi-particle weighted events according to Lorentz in- 34 variant Fermi phase space. The reaction p+^{16}O →^3He+^{14}N_η was studied at 35 a momentum close to the magic momentum. The magic momentum is defined 36 as the beam momentum at which recoil-less η can be produced in the ele- 37 mentary process. For the reaction considered, the elementary reaction is pd 38 →^3Heη, for which the magic momentum was calculated to be 1.745 GeV/c, 39 corresponding to a proton kinetic energy of T_p=1.05 GeV. The η-nuclei for- 40

mation proceeds through the excitation of N^∗ (1535 MeV) resonance and one 41 of its decay channels is through proton and pion. The simulations were per- 42 formed in two steps. In the first step, Monte Carlo events were generated for 43 the p+^{16}O →^3He+^{14}N_{ex} reaction where an excitation energy of 547 MeV, 44 equal to the mass of eta meson, is given to^{14}N nucleus. Only those^{14}N events 45 were considered for which the corresponding^3He particle is within the Big 46 Karl acceptance (θ_{lab}(^3He) ≤ 6^∘). In the next step, the decay of N^∗ to p-π 47 pair was simulated. The mass of N^∗ was taken equal to the mass of a nucleon 48 plus the mass of an eta meson, while its velocity was assumed to be the same 49 as that of the recoil^{14}N modified by the Fermi momentum distribution. The 50 p-π opening angle distribution shows a peak at around ≈150^∘ with a width of 51 40^∘ (Fig. 1). The energy spectrum for the proton peaks at T_p ≈100 MeV with 52 a width (FWHM) of 120 MeV (Fig. 2), while the pion spectrum has a peak 53 at ≈320 MeV and a similar width(Fig. 3) as that of proton peak. The sim- 54 ulations were also carried out for other eta-mesic nuclei formation reactions 55 on different target nuclei. The energy spectra and opening angle distributions 56 were found to be similar as that in the previous case. 57

58

A detector employing plastic scintillators in the ΔE - E configuration, which 59 provides the particle identification and energy information of the measured 60 particles, has been chosen for the present design. The thickness of the detector 61 elements has been designed to stop the decay protons and obtain a good 62 signal for pions, keeping in mind the space constraints around the detector 63 in the experimental area. The detector has been segmented in both θ and ϕ 64 direction for obtaining position information with the desired granularity. Large 65 solid angle coverage has been achieved by minimising any unwanted material 66

Fig. 1. The p-π opening angle distribution for η-mesic nucleus decay particles obtained from Monte-Carlo phase space calculations as detailed in the text.

Fig. 2. Kinetic energy distribution of protons from η-mesic nucleus decay obtained from Monte-Carlo phase space calculations.

within the detector. 67

Fig. 3. Kinetic energy distribution of pions from η-mesic nucleus decay obtained from Monte-Carlo phase space calculations. 3 Design details and fabrication 68

3.1 Detector geometry 69

Based on the design and geometric criteria, ENSTAR is cylindrically shaped 70 with three layers of plastic scintillators. These layers are used to generate 71 ΔE − E spectrum for particle identification and to obtain total energy infor- 72 mation for the stopped particles. Each layer is divided into a number of pieces 73 to obtain θ and ϕ information. The detector, which is made up of two identi- 74 cal half cylinders, is assembled around a scattering chamber of 1.5 mm thick 75 carbon compound fibre material. The scattering chamber as shown in Fig. 4 is 76 designed in a ”T” shape with a thin target pipe projecting out from the middle 77 of beam pipe. The two half cylinders of the detector are placed on either side 78 of the target pipe. The target pipe has sufficient space from inside to enable 79 mounting of solid targets. A Liquid target chamber, similar to the one existing 80 at COSY laboratory can also be used after some modifications. The angular 81

Fig. 4. Photograph of the scattering chamber made from the carbon fibre material. It consists of a beam pipe and a thin target pipe for inserting a target ladder. coverage of the detector is θ_{lab} = 15^o − 165^o in the θ-direction, while its cylin- 82 drical geometry ensures an azimuthal angle coverage of ϕ = 0^o − 360^o. With 83 the present design, the detector provides a solid angle coverage of ∼95% of 84 4π. An assembly drawing of ENSTAR together with its sectional view through 85 the target is shown in Fig. 5. A total of 122 pieces of scintillators of different 86 shapes and dimensions are used to give three concentric cylindrical layers on 87 assembly. 88

89

The inner layer is used to provide the energy loss and ϕ information of the 90 particles passing through it and is designed as two hollow plastic scintillator 91 cylinders with the following dimensions; Inner diameter(ID) = 84 mm, Outer 92 diameter(OD)=96 mm and a length of 390 mm. Both the cylinders are split 93 into eight equal sectors with a sector angle equal to 45^o. Thus the inner layer 94 consists of a total of 16 segmented annuli each of which is read out separately. 95 A ϕ resolution of 45^o is satisfactory for the studies on η -mesic nuclei, as the 96 decay particles are emitted with a very large opening angle between them. 97

Signals from the middle layer are used to obtain energy and θ information. 98 This layer consists of seven identical scintillator bars in both the halves, each 99 in the form of an isosceles triangle with base = 243.1 mm and height = 152.4 100 mm arranged to form an annular cylinder of ID=100 mm, OD= 449.4 mm and 101 length = 390 mm in each half. Each of triangular bars (390 mm long) is further 102 split lengthwise into six pieces of length 13 mm, 16 mm, 21 mm, 37 mm, 213 103 mm, and 90 mm so that each piece covers an angle interval of Δθ_{lab} equal to 104 15^o. A total of 84 pieces of scintillators are used for the middle layer cylinder. 105 The geometrical granularity allows an angular resolution of Δθ_{lab} equal to 15^o. 106 In conjunction with signals from middle layer, signals from the outer layer are 107 expected to provide an unambiguous signal for pions. The outer layer consists 108 of a total of 22 identical bars, each 390 mm long and a cross section of an 109 isosceles triangle with base = 328.3 mm and height = 105.5 mm. These outer 110 layer pieces form an annular cylinder of ID = 453.5 mm, OD = 692.5 mm. 111 Thus, with two identical cylinders on either side of the target for all the three 112 layers, the detector provides an angular coverage of 15 ≤ θ_{lab} ≤ 165^o in the 113 θ-direction and almost full coverage in the ϕ-direction. 114

115

3.2 GEANT simulation 116

GEANT [8] calculations have been carried out by simulating the conditions 117 of the real experiment to simulate the ENSTAR detector’s response to eta- 118 nucleus decay particles, namely, protons and pions. The detector geometry has 119 all its 122 pieces arranged around the scattering chamber. The target has been 120 positioned at the centre of the detector, inside the scattering chamber which 121

Fig. 5. Left part : An assembly drawing of ENSTAR detector is shown. Some pieces of the middle and outer layers are moved out for an inside view. Detailed dimensions are given in the text. Right part : A Sectional view of the detector through the target is shown. Beam pipe along with the target pipe attached to it, is also drawn.

is in vacuum. The existing gap between the various layers of ENSTAR is filled 122 with air. The η-mesic nucleus decay events are produced in a collision of 1.05 123 GeV proton beam with a target. A Monte Carlo event generator as detailed 124 in section 2 is used to simulate such events. The protons are stopped in the 125 detector while pions, as expected, pass through it giving only partial energy 126 loss in the detector. Fig. 6 shows a two dimensional plot of energy loss in the 127 first layer versus total energy loss in the detector. The response of various 128 layers of ENSTAR for protons and pions from such events have been inves- 129 tigated. The present design does not plan to obtain full energy information 130 of pions, however, as desired a mass separation of pions from protons can be 131 achieved. From the particle selection in the ΔE-E two-dimensional spectrum 132 of Fig. 6, the decay events detected within the detector can be estimated. It 133 is found that the 80 % of total protons and pions generated can be identified 134 from the ΔE-E spectrum. It is further clear from the figure that the energy 135 loss for most of pions is in the 50-100 MeV range , where a clear separation 136

between protons and pions can be achieved. The separation of pions from the 137 protons could be difficult in the higher energy loss region of pions. However 138 the fraction of the pion events in the energy range of 100-250 MeV is less 139 compared to number of events in the low energy range. 140

Fig. 6. A two dimensional plot of ΔE (energy loss in the inner layer) vs E + ΔE (energy loss in all the layers) showing the particle separation in ENSTAR. The results are obtained from GEANT simulations for the events from the η-mesic nucleus decay. 141

3.3 Scintillator grooving and fibre coupling 142

Plastic scintillators, having the properties equivalent to Bicron BC-408 series, 143 were procured from Scionix Ltd, Netherlands [9], for the fabrication of detector 144 elements. The use of light guides for scintillator read out was not practicable 145 due to the complicated geometry of the detector. The idea of using wave- 146

length shifting (WLS) optical fibres for scintillator read out was invoked for 147 the present detector. Earlier studies[10,11] have shown that the double-clad fi- 148 bres give better light yield (70% more light) than comparable single clad ones, 149 due to an increase in the fraction of light that undergoes total internal re- 150 flection. The double-clad WLS optical fibres having 1mm diameter were used 151 for light transport. A number of grooves for fixing fibres to the scintillators 152 were made on the surface of scintillators . The middle and outer layer pieces 153 were machined for 19 grooves each having 4 mm width and 1.5 mm depth. 154 The grooves cover roughly 40 % of the area of one face of scintillator. For 155 the inner layer pieces, 15 grooves of 1.0 mm width and 1.5 mm depth were 156 machined with a spacing of 1.5 mm. The machining was done at the Central 157 Workshop, BARC using a computer controlled 4 mm (1mm for the grooves on 158 inner layer pieces) carbide cutter (End-Mill). A suitable cooling arrangement 159 with chilled air was used in order to avoid any local heating. Each piece of 160 middle and outer layer has 76 fibres placed in 19 grooves (4 fibres in each 161 groove), while each inner layer piece has 15 fibres (1 fibre in each groove. The 162 scheme of fibre scintillator coupling is illustrated in Fig. 7 for a typical middle 163 layer scintillator piece. 164

165

The total amount of fibre used was 7.8 km in length. The fibre length for 166 each scintillator pieces was decided on the basis of availability of space in the 167 experimental area. While the length of fibre should not be very long in order 168 to minimise attenuation losses, its bending radius should also be kept high. 169 The conventional minimum bending radius of these fibres is ten times the fi- 170 bre diameter. Bending fibres below this radius may result in significant light 171 loss due to damage in mechanical as well as optical properties. The length 172

Fig. 7. The sketch diagram of a typical middle layer scintillator piece showing the grooves and fibre alignment details. There are 19 grooves on one face of this triangular bar with four fibers placed inside each groove. The alignment of fibres with the scintillator is shown in (b) and (c). For illustration purposes fibres in only one groove are drawn.

of fibres for each scintillator piece was optimized accordingly. Since the light 173 readout is from one end of the fibres only, the light traversing to the other end 174 must be reflected back. Therefore, before fixing the fibres, a highly reflective 175 anodized aluminum sheet (known as EverBrite [12]) was placed on one face 176 of the scintillator and held in place with aluminized mylar tape. A good sur- 177 face finish and polished fibre ends are essential to prevent light losses at both 178 the reflecting as well as at the readout interface . This has been achieved by 179 different techniques. The cutting and polishing of fibres for the middle and 180 outer layer pieces were done before fixing them to the scintillators. For polish- 181 ing, many fibres were grouped together in bundles inside a perspex tube. The 182 fibre face was cut along with the perspex by a diamond tipped cutting tool 183

giving a surface finish of 0.7 μm. The final polishing of these fibres was done 184 with 0.3 μm size alumina powder on velvet cloth. The polished fibres were 185 fixed in the scintillator grooves with the Bicron 600 optical cement at few 186 locations along the grooves. However, to give an additional holding strength, 187 five-minute epoxy was used wherever necessary. It is preferable to use the 188 Bicron cement as it has the same refractive index as that of the scintillator 189 and its light transmission above 400 nm wavelength is more than 98 %. In 190 addition, aluminized mylar tape was also used at few places for holding the 191 fibres. For the inner layer pieces, a different method was followed. First, the 192 fibres were fixed in the grooves using Bicron cement with a small amount of 193 five-minute epoxy glue at the ends of the fibre-scintillator joint. This end of 194 the scintillator along with the fibres were then polished for all 16 inner-layer 195 pieces. This was done at the optics workshop of the Spectroscopy Division, 196 BARC by the lapping technique. Fine alumina powder of 20 μm, 12 μm and 197 6 μm were used in successive stages of lapping. The final finishing was then 198 achieved by polishing with diamond paste and alumina of 1 μm and 0.3 μm 199 sizes giving a surface finish of 0.3 μm. Fig. 8 (left part) shows the polished end 200 of one of the scintillator pieces. Finally the highly reflective EverBrite sheet 201 was placed at this polished end (not shown in the figure) for light reflection. 202 The other open end of all the fibres of individual scintillator pieces were bun- 203 dled together and then glued to the inside of a 2.54 mm diameter perspex tube 204 - known as “cookie” [11] (a cylindrical piece of acrylic, matching the photo 205 multiplier tube in diameter). This end of fibres were polished along with the 206 cookie. The fibres along with the cookies were diamond polished by diamond 207 paste and alumina powder. Fig. 8 (middle picture) shows some of the finished 208 (except for its covering by black foil) inner layer pieces with fibres and cookie 209 attached. One of the middle layer piece is also shown in Fig. 8(right picture). 210

The cookie end was coupled to the photo-multiplier tube for conversion of the 211 light signal into photo-electrons which were then processed electronically. In 212 order to reduce light losses from scintillators, the scintillator elements were 213 wrapped with tyvek, a paper-white reflecting foil made of polyethylene[13]. 214 The wrapping by tyvek, apart from light reflection, also helps in minimising 215 the cross-talk. All the detector pieces were finally covered by black tedlar foil 216 for light tightness and reducing the cross-talk among various detector elements. 217

218

Fig. 8. Photograph of some inner and middle layer pieces of ENSTAR while being fabricated. Left part shows inner layer pieces with fibres inside scintillator grooves while the middle part shows the some of the similar pieces after it has been covered with the Tyvek paper. At the other end fibres from each piece are bundled together and coupled to a“cookie”. In the right part of the figure one of the middle layer pieces with fibres placed inside the grooves is shown.

3.4 Scintillator readout details 219

The Bicron optical fibre BCF-91A, used in the present detector for collect- 220 ing light produced in the scintillator volume has an emission spectrum in the 221 visible green region. In order to have an efficient readout of this light, the 222 photomultiplier tubes (PMTs) that have a spectral response extending into 223

the green region and which match the light emission characteristic of the wave 224 length shifting fibres were selected. The PMTs are of the 9112B series manu- 225 factured by Electron Tubes Ltd (ETL), United Kingdom [14]. The PMTs are 226 of 25 mm diameter with Rubidium bialkali photocathode having an enhanced 227 green sensitivity. A total of 122 photomultiplier tubes are used for the readout 228 of ENSTAR. The PMTs have a current amplification of 10^6 and a dark cur- 229 rent of less than 10 nA. The tubes are fast and have a rise time of less than 3 230 ns. The PMTs, during the experiment, were covered by μ-metal sheets which 231 have also been procured from ETL, UK. The base of the PMTs i.e., voltage 232 dividers are also made by the same manufacturer. Special aluminum holders 233 were fabricated for holding the PMTs and cookies together. 234

3.5 Detector assembly 235

The pieces of the inner layer of the detector are the lightest ones and were 236 easy to mount. They were simply held around the beam pipe/target chamber 237 with tape. The other pieces of ENSTAR i.e., middle and outer layer pieces 238 are relatively heavier and special support structures were designed and built 239 for holding these pieces in place. The basic supporting structure, which is 240 mostly an exoskeleton, was made from hylam (low Z material) plates. Due to 241 the compact geometry of the detector no support structure was needed inside 242 the sensitive volume of the detector, except only at few places in the space 243 between the middle and the outer layer where three support strips made of 244 hylam have been put in each half of the detector. These support strips were 245 joined by aluminum rings on both ends for the middle layer. The simulations 246 were repeated with and without the hylam strips (acting as inactive material 247

inside the detector). An acceptance loss of less than ∼ 1% for the particles 248 to be detected is predicted. For the outer layer, the hylam plates were joined 249 by aluminum brackets at both ends. The detector after assembly was placed 250 on a stainless steel stand which was fixed on a movable trolley made from 251 angle-iron. A stand to hold PMTs was also constructed and integrated in the 252 same support structure. Fig. 9 shows a photograph of ENSTAR detector along 253 with its support structure mounted at the COSY beam line. 254

255

Fig. 9. A photograph of the ENSTAR detector mounted at the COSY beam line along with its support structure and the stand which has been used to transport the detector to the beam line.

4 Test Measurements 256

A number of test measurements were performed during the construction and 257 commissioning of the detector. A light-tight black box was constructed for the 258 preliminary tests of the phototubes and the scintillator pieces. The PMTs and 259 its bases were tested to check for their proper functioning and to determine 260 their optimum operating voltage. The variation of signal pulse height from a 261

scintillator tile was studied as a function of number of fibres. The pulse height, 262 which depends on the amount of light collected by the fibres, is observed to 263 increase with the increase in the number of fibres and saturates when fibre 264 covers about 30 - 40% of the scintillator tile surface. The number of fibres 265 for each scintillator tile has been optimized accordingly. The light output of 266 different pieces of ENSTAR was also tested with an alpha source for which a 267 simple test setup was constructed. 268

269

Fig. 10. A two dimensional spectrum of the energy losses in inner and middle layer pieces of ENSTAR mounted at the focal plane exit of Big Karl magnetic spectrograph in ΔE1 - ΔE2 configuration. The spectrum shows the pions, protons and deutrons of energies ∼430 MeV, ∼ 150 MeV and ∼ 80 MeV respectively, which are selected by a BigKarl momentum setting of 550 MeV/c.

The first in-beam test at COSY was performed by mounting a few pieces of 270 ENSTAR from the inner and middle layers arranged in a ΔE1 - ΔE2 configu- 271 ration at the exit of the focal plane of the magnetic spectrograph BigKarl. A 272 proton beam of momentum 1.54 GeV/c, corresponding to kinetic energy of 865 273 MeV, was bombarded on a thick Alumina target. The spectrograph BigKarl 274 was set for different momenta to select various energies of protons from 35 to 275 225 MeV and pions in the range of 150 to 560 MeV. Fig. 10 shows the ΔE1- 276 ΔE2 energy spectrum of various particles detected in scintillator pieces for a 277 typical BigKarl momentum setting of p/q=550 MeV/c. A Good separation 278 among all particle groups (e.g. pions, protons, deuterons etc.) was obtained. 279 The particle identification was confirmed from the time of flight information, 280 which was measured simultaneously between two hodoscopes layers placed at 281 a distance 4m apart at the focal plane of BigKarl. 282

283 The final test measurement of ENSTAR in fully assembled condition was per- 284 formed using a proton beam of momentum 0.870 GeV/c at COSY. In addition 285 to light-output test of all scintillator pieces, a study of the relative gain of vari- 286 ous elements and absolute calibration was performed. Several nuclear reactions 287 (pp elastic scattering, pp → dπ^+, proton impinging on a heavy target etc.) 288 were used for this purpose. Coincidence data i.e. a 2-fold coincidence between 289 different elements of ENSTAR were collected. In addition, cosmic-ray data 290 were also recorded with good statistics. 291

292 In the pp elastic scattering measurement scattered protons having energies 293 from 25 to 340 MeV are detected in the forward half of the detector. In this 294 case, the trigger was made from the events which have a double hit in the 295

Fig. 11. A two dimensional spectrum of one of the inner layer piece vs the corresponding middle layer piece of ENSTAR for protons in the energy range of 225-330 MeV obtained from pp elastic scattering data. Cosmic ray data from a different run are also shown in the same figure.

inner layer and at least a single hit in the middle layer. In addition, the condi- 296 tion of co-planarity of the elastically scattered proton pair was ensured. Light 297 output of one of the inner-layer scintillator piece versus the corresponding 298 middle-layer scintillator piece is plotted in Fig. 11. The proton band shown 299 in the figure corresponds to an energy range of 225 − 330 MeV. A band cor- 300 responding to cosmic muons is also shown in the figure which was obtained 301 from cosmic-ray data collected separately in a different run, as described later 302 in the text. 303

304

Fig. 12. ADC spectra of two adjacent middle layer scintillators uniformly illuminated in ϕ- direction by scattered particles from beam impinging on a thick target kept in front of detector. Peak positions are used to get the relative gains of various pieces in ϕ-direction.

The relative gain calibration among different scintillator pieces covering the 305 same θ- but different ϕ-ranges is achieved using reactions in which protons 306 are incident on a thick heavy target. In this case the target, instead of its 307 conventional location which is at the centre of ENSTAR, was placed at a po- 308 sition where the beam enters the detector, Scintillators of the same shape and 309 dimensions form an annular cylindrical ring and therefore, are uniformly illu- 310 minated by the scattered particles. The relative gain for the different elements 311 of the ring is obtained from the peak positions of the spectra shown in Fig. 12. 312 For measurements with the cosmic-rays, two additional scintillator hodoscope 313 paddles were placed just above and below the ENSTAR scintillator element 314 being tested. Signals from these paddles formed the cosmic-ray trigger. ADC 315 spectra from two adjacent scintillators of the middle layer for the cosmic data 316 are shown in Fig. 13 (left and middle part). The extreme right part of the 317

figure is a pedestal subtracted ADC spectrum generated from combination 318 of these two spectra using the relative gain between the corresponding two 319 pieces as determined above. The triangular shape of middle layer(as well as 320 outer layer) scintillators and the present detector geometry allow a selection of 321 an overlap portion between two adjacent scintillators such that muons travel 322 a constant thickness of 150 mm. The centre of the peak corresponds to an 323 average energy loss of ∼27 MeV since a minimum ionizing particle typically 324 loses ∼1.8 MeV per cm of plastic scintillator [15]. This method was used to 325 extract the absolute gain calibration of all the middle and outer layer scintil- 326 lator pieces. 327

328

Fig. 13. ADC spectra from two adjacent middle layer scintillators for cosmic ray data. The extreme right part of the figure is generated by demanding an overlapping geometry condition such that cosmic muons travel a constant thickness. See text for details.

5 Conclusions 329

We have presented a detailed description of a large acceptance scintillator 330 detector ENSTAR, which has been designed and constructed for studying 331 the production and decay of η-nucleus bound systems, the η-mesic nuclei at 332 the multi-GeV hadron facility COSY. Monte Carlo phase space calculations 333 to simulate the formation and decay of eta-mesic nucleus predict an energy 334 range of 25 to 250 MeV for the decay protons and energies from 250 to 500 335 MeV for the decay pions. The detector is cylindrically shaped in three layers 336 and is segmented into a number of pieces for the detection of η-mesic de- 337 cay events. GEANT simulations predict a clear mass separation between the 338 protons and pions based on the energy loss information in different layers. A 339 number of test measurements have been performed to test the performance of 340 the individual components of the detector. Some of the scintillator pieces have 341 been tested at COSY by placing them in ΔE1 − E2 configuration at the exit 342 of focal plane detection system of the magnetic spectrometer BigKarl. These 343 scintillator pieces have been tested with protons in the energy range of 35- 344 200 MeV and pions in 150-500 MeV energy range selected from the Big Karl. 345 The detector has been further tested in fully assembled condition, using 870 346 MeV/c proton beam from COSY, Jülich. In addition, the measurements using 347 the cosmic muons have been also performed. For the test measurement with 348 870 MeV/c proton beam, the elastically scattered protons having energy in 349 25-340 MeV range, were detected in ENSTAR. A satisfactorily good detector 350 response is obtained with the elastic protons as well as the cosmic muons. 351

352

Acknowledgements 353

This work has been part of the Indo-German bilateral agreement. We are 354 thankful to the International Studies Division, DAE, India. Our sincere thanks 355 goes to Dr.S.S.Kapoor and Dr.S.Kailas, BARC for their interest and sup- 356 port throughout this project. We are thankful to Prof. N. K. Mondal, TIFR, 357 Mumbai for many useful discussions and supply of EverBrite sheets. We 358 are indebted to the technical staff of the Centre for Design and Manufac- 359 ture, BARC, Spectroscopy Division, BARC and Institute of Nuclear Physics, 360 Forschungszentrum, Jülich for their assistance. We would like to acknowledge 361 the support from the European community research infrastructure activity 362 under the FP6 “Structuring the European Research Area” programme under 363 the contract no.RII3-CT-2004-506078. 364

References 365

[1] L. C. Liu and Q. Haider, Phys. Rev. C 34 (1986) 1845. 366 [2] R.S. Bhalerao and L.C. Liu, Phys. Rev. Lett. 54 (1985) 865. 367 [3] H Machner et al., GEM Collaboration, COSY-Proposal No 50, FZ Jülich, 2000. 368 [4] Siegfried A. Martin et al, Nucl. Instr. and Meth. 214 (1983) 281. 369 [5] Betigeri M. et al. GEM collaboration, Nucl. Instr. Meth. A 487 (2002) 314. 370 [6] A. Gillitzer et al., COSY-Proposal No 96, FZ Jülich, 2000. 371 [7] F.James , GENBOD - CERN Program Library write up no. W515. 372 [8] R. Brun et al, GEANT - CERN Program Library W5013. 373 [9] SCIONIX plastic scintillators, SCIONIX, http://www.scionix.nl 374 [10] M. Adams et. al., D0 collaboration, Nucl. Inst. and Meth. A 366, (1995) 263. 375

[11] B. S. Acharya et. al., D0 Collaboration, Nucl. Inst. and Meth. A 401, (1997) 376 45. 377 [12] EverBrite anodized aluminium, Alcoa Brite Products Inc., 3040, Northwood 378 Parkway, Norcross, GA 30071. 379 [13] Tyvek and Tedlar TCC 15BL3, DuPont de Nemours Int. SA, Switzerland. 380 [14] ETL Photo multiplier tubes, Electron Tubes Ltd., 381 http://www.electron-tubes.com. 382 [15] C.P.Achenbach et al., Nucl. Inst. Meth. A 539 (2005) 112 383