arXiv:0908.2938v2 [nucl-ex] 13 Jan 2010

TIARA: a large solid angle silicon array for direct reaction studies with radioactive beams

M. Labiche^{a,b,∗}, W.N. Catford^c, R.C. Lemmon^a, C.N. Timis^c, R. Chapman^b, N.A. Orr^d, B. Fernández-Domínguez^e, G. Moores^b, N.L. Achouri^d, N. Amzal^b, S. Appleton^a, N.I. Ashwood^f, T.D. Baldwin^c, M. Burns^b, L. Caballero^g, J. Cacitti^h, J.M. Casadjian^h, M. Chartier^e, N. Curtis^f, K. Faiz^a, G. de France^h, M. Freer^f, J.M. Gautier^d, W. Gelletly^c, G. Iltis^d, B. Lecornu^h, X. Liang^b, C. Marry^h, Y. Merrer^d, L. Olivier^h, S.D. Pain^c, V.F.E. Pucknell^a, B. Raine^h, M. Rejmund^h, B. Rubio^g, F. Saillant^h, H. Savajols^h, O. Sorlin^h, K. Spohr^b, Ch. Theisen^i, G. Voltolini^h, D.D. Warner^a

aNuclear Physics Group, STFC Daresbury Laboratory, Daresbury, Warrington, WA4 4AD, UK bDepartment of Engineering and Science, University of the West of Scotland, Paisley PA1 2BE, UK cDepartment of Physics, University of Surrey, Guildford GU2 5XH, UK dLaboratoire de Physique Corpusculaire, IN2P3-CNRS, ISMRA et Université de Caen, F-14050 Caen, France eOliver Lodge Laboratory, University of Liverpool, Liverpool L69 7ZE, UK fSchool of Physics and Astronomy, University of Birmingham, Birmingham B15 2TT, UK gInstituto de Fisica Corpuscular, CSIC-Universidad de Valencia, E-46071 Valencia, Spain hGrand Accélérateur d’Ions Lourds, BP 55027,14076 Caen Cedex 5, France iCommissariat d’Energie Atomique de Saclay, 91191 Gif-sur-Yvette, France

Abstract

A compact, quasi-4π position sensitive silicon array, TIARA, designed to study direct reactions induced by

radioactive beams in inverse kinematics is described here. The Transfer and Inelastic All-angle Reaction

Array (TIARA) consists of 8 resistive charge division detectors forming an octagonal barrel around the

target and a set of double-sided silicon-strip annular detectors positioned at each end of the barrel. The

detector was coupled to the γ-ray array EXOGAM and the spectrometer VAMOS at the GANIL Laboratory

to demonstrate the potential of such an apparatus with radioactive beams. The^{14}N(d,p)^{15}N reaction, well

known in direct kinematics, has been carried out in inverse kinematics for that purpose. The observation of

the^{15}N ground state and excited states at 7.16 and 7.86 MeV is presented here as well as the comparison of

the measured proton angular distributions with DWBA calculations. Transferred l-values are in very good

agreement with both theoretical calculations and previous experimental results obtained in direct kinematics.

Keywords: position sensitive silicon detectors, nucleon transfer reactions, radioactive beams, inverse

kinematics

∗Corresponding author. Address: Daresbury Laboratory, Daresbury, Warrington, WA4 4AD, UK. Email address: marc.labiche@stfc.ac.uk (M. Labiche)

Preprint submitted to Elsevier December 25, 2018

1. Introduction 1 A clear understanding of nuclear structure beyond the valley of β-stability requires detailed spectro- 2 scopic investigations. Direct reactions, such as single-nucleon transfer reactions are established probes of 3 the single-particle nuclear shell structure and have provided considerable insight into the properties of stable 4 nuclei in the past. With the on-going increase in radioactive nuclear beam intensities, such as those achieved 5 at the SPIRAL facility, this kind of reaction is now feasible. The inverse kinematics of such reactions leads, 6 however, to significant constraints on the experimental apparatus [1, 2]. One of the main obstacles to over- 7 come is to reach good energy resolution in the kinematically reconstructed excitation energy given that the 8 energy spread of the secondary beam may be relatively large, the target-like residue can be emitted over a 9 large angular range and that thick targets are often required to compensate for the relatively low intensities 10 of the beams [1]. Already, pioneer detectors such as MUST [3] and the active target MAYA [4] have been 11 build to tackle some of these obstacles and, the detector TIARA described here proposes a new alternative 12 to these other apparatus. The TIARA array is designed and built specifically to study direct reactions with 13 radioactive beams and addresses the challenge of the excitation energy resolution by employing the tech- 14 nique of γ-ray tagging. This has the advantage of providing, in principle, a final excitation energy resolution 15 limited only by Doppler broadening. 16 The TIARA array was commissioned at the GANIL laboratory through a study of the d(^{14}N,p)^{15}N reac- 17 tion [5, 6] with coincident γ-ray detection. The results are reported here together with a full description of 18 the array. 19 2. Detector Description 20 The TIARA array [7, 8] has been designed with the ultimate goal of performing nucleon transfer and 21 other direct reaction studies in inverse kinematics using radioactive ion beams [1, 9]. The array is used to 22 identify the binary reaction channels and to determine the excitation energies of the populated states. This 23 task is achieved by providing position and deposited energy measurements of the light charged target-like 24 residue, which can be emitted over a wide angular range. TIARA consists of a set of single-layer silicon 25 detectors manufactured by Micron Semiconductor [10] which covers 85% of 4π (Fig. 1). The set includes a 26 large annular double sided silicon strip detector (SiHyBall), eight resistive charge division silicon detectors 27 forming a “barrel” around the target, and two smaller “CD-type” silicon strip detectors (S1 and S2). 28

Figure 1: Position of the silicon TIARA array and the target changing mechanism in the reaction chamber. The beam goes from the right to the left. The angular range covered by each component of the array for the commisioning experiment (see text) is shown.

2.1. Resistive Charge Division Detectors 29 Eight resistive charge division detectors based on 6-inch silicon wafer technology form an octagonal 30 barrel around the beam axis and surrounding the target. Each of the detectors presents an active area 94.6 31 mm long and 22.5 mm wide with a thickness of 400 μm. The junction side facing the target is divided into 32 4 longitudinal resistive strips obtained by p^+ implantation on n-type silicon. Each 4kΩ-resistive strip has a 33 5.65 mm pitch while the inter-strip gap is 100 μm. The strips provide for measurement and pixellation of the 34 azimuthal angle in 32 bins of approximately 9.5^o. The PCB board around the silicon has been minimised 35 and bevelled so that the dead area between the detectors as well as between the barrel and annular detectors, 36 is minimised. At one end of the Ohmic side of the detector, the PCB board is extended by ∼15 mm in order 37 to gather all the output signal tracks: the 8 position signals (2 signals per strip) and the connection of the 38 Ohmic side to ground. Miniature Junkosha coaxial cables of 1 mm diameter and 30 cm length were chosen 39 for their favourable vacuum properties to transmit the signals from the detector to the vessel feed-throughs. 40 Once assembled (Fig. 2 right), the barrel presents an octagonal cross section of 27.6 mm side length and 41 33.3 mm inner radius. From the centre, the angular range spans 36^o to 144^o. For the commissioning 42 measurements described later, the centre of the barrel was mounted 1 mm forward of the target position 43 leading to an angular coverage of 35.5^o to 143.5^o. The measurement of the position along the strip is 44

Figure 2: The SiHyBall annular detector (left) and the octagonal barrel (right).

achieved by resistive charge division and, with alpha particles of 5.5 MeV, the position resolution along the 45 longitudinal axis is determined to better than 0.5 mm (FWHM). The resulting polar angle is thus deduced 46 with a precision better than 1^o. The energy of the particle is obtained simply by summing the signals from 47 the two strip ends. Figure 3 was obtained using a mixed source of^{239}Pu,^{241}Am and^{244}Cm with alpha 48 energies of 5156, 5484 and 5805 keV respectively. It illustrates the correlation between the signals from 49 the ends of the strips (Fig 3(a)). With a shaping time of 1μs the barrel suffers slightly from ballistic deficits 50 which result in a non-linear dependence of the energy sum, measured at each end of a strip, as a function of 51 the position. Nevertheless, this dependence is easily described with a second-order polynomial function and 52 a corresponding corrective factor can be applied to the energy sum. The resolution for one strip is ∼70 keV 53 (FWHM) for 5.5 MeV alphas (Fig 3(b)). 54 2.2. Annular Silicon Detectors 55 As noted earlier, in order to enhance the angular coverage of the TIARA array, double-sided DC annular 56 silicon-strip detectors are mounted at both ends of the barrel. For these detectors the annular rings on the 57 entrance face (junction side) were fabricated by p^+ implantation on n-type silicon. 58 The forward angles are covered by two 500 μm thick annular detectors based on 4-inch wafer technology. 59 The smallest of the two (S2-design) was positioned 150 mm downstream of the target position covering the 60 polar angular range [3.8^o,13.1^o]. The active area is delimited by a disk of 11 mm inner radius and 35 mm 61 outer radius. The detector is divided into 48 rings of 0.5 mm pitch at the front (target side) and 16 azimuthal 62

Figure 3: Typical response of the barrel and SiHyball strips with a 3-alpha source. (a): signals collected at both ends of a barrel strip. (b): total energy collected in a single strip of a barrel detector (thick dashed histogram) and in a single strip of the DSS SiHyBall detector (thin line histogram), obtained with a 1μs shaping time. (c): same as (b) for the 4 strips of a barrel detector.

sectors at the back. However, for the present measurements, the number of channels to instrument was 63 reduced by linking the rings in threes giving effectively 16 rings of 1.5 mm pitch. 64 The second forward annular detector (S1 design) was mounted 92 mm downstream of the target position 65 to cover the polar angular range [12.6^o,27.5^o]. Its active area is divided into 4 quadrants of 20.5 mm inner 66 and 48 mm outer radii. Although each quadrant has 16 front rings (1.65 mm pitch) and 4 azimuthal back 67 sectors, for the experiment reported here the four quadrants were combined to form two semi-circles to 68 reduce the total number of rings from 16×4 to 16×2. 69 The backward angles from 137.0^o to 169.4^o are covered by a 400 μm thick double-sided silicon-strip 70 detector (DSSSD) based on 6-inch wafer technology and positioned 150 mm upstream of the target position. 71 This detector is composed of six individual wedges (Fig. 2) originally developed at Oak Ridge for the SiHy- 72 Ball forward array [11]. Each wedge is divided into 16 strips facing the target and 8 azimuthal back sectors. 73 The active area of a wedge is delimited by inner and outer radii of 28.11 mm and 140 mm, respectively, 74 and spans approximately 55^o of the total azimuthal angle. The pitch of the rings is 5.3 mm and the polar 75 angular range is close to 2 degrees per strip. The energy resolution, illustrated in Fig. 3b, is typically ∼70 76 keV (FWHM) for 5.5 MeV alpha particles. 77

Figure 4: The target mechanism on a test bench. The rod has just picked up a target frame from the storage wheel.

2.3. Target Changing Mechanism 78 One of the critical features of the TIARA array is the target changing mechanism (Fig. 4). The design 79 of this mechanism has been chosen to maximise the solid angle coverage of the array. Positioned upstream, 80 just behind the SiHyBall, it offers the possibility to use four different targets during a run without breaking 81 vacuum. The mechanism consists of a target storage wheel with 4 positions and a rod parallel and slightly 82 offset to the beam axis. A set of clamps, four on the storage wheel and one at the extremity of the rod 83 (Fig. 4) are used to hold the target frames. The rod is driven along the beam axis via a ball screw. It first 84 picks up a target from the wheel and continues its motion along the beam axis through the inner hole of the 85 SiHyBall detector until the target position in the barrel is reached. The target frame is 3×3 cm^2 in area with a 86 central hole of 20 mm diameter. It can only be positioned perpendicular to the beam axis, introducing some 87 shadowing at 90^o in the barrel detector (Section 3.3). The whole mechanism is controlled remotely and the 88 position of both the wheel and the rod is monitored by optical readouts. Four feed-throughs on the vacuum 89 vessel are used for the target control system. 90 2.4. The Vacuum Vessel 91 The reaction chamber of TIARA is made of aluminium and is some 56 cm long (excluding the target 92 mechanism). Figure 5 shows the vessel in position in front of the VAMOS spectrometer and in the middle of 93 the EXOGAM support structure. The vessel presents a longitudinal diabolo shape with a central cylindrical 94 section of 85 mm outer diameter housing the barrel and two 500 mm diameter cylindrical sections at each 95

Figure 5: Left: Picture of TIARA in situ. The support structure holding 4 EXOGAM Ge clover detectors has been opened up, showing the TIARA reaction chamber at the entrance of the VAMOS spectrometer. Right: The TIARA array and chamber as defined in GEANT4 simulation.

end housing the annular detectors. Two aluminium end plates accommodating Fischer DBPE 105-series 96 feed-throughs (27 pins each) and supporting kinematics plates for detector alignment complete the chamber. 97 While one of the end-plates can accommodate up to 17 feed-throughs, the other one, which also includes two 98 pipes for additional pumping, can accommodate up to 15 of them. Given that 4 feed-throughs are already 99 used for the target mechanism, a total of 28 feed-throughs can be used for the transmission of the detector 100 signals. The TIARA reaction chamber has been designed to allow a gamma-ray array such as EXOGAM to 101 be placed as close as possible to the target. As such, the thickness of the walls of the central section has been 102 limited to 2 mm in order to reduce the γ-ray attenuation to a minimum. For a photon energy of 1 MeV, the 103 linear attenuation coefficient in Aluminium is 0.166 cm^{−1}. This leads to an attenuation of 3.3% in a 0.2 cm 104 layer compare to 8% in a 0.5 cm layer. 105

2.5. Electronics and Data Acquisition 106 There are 8×2×4 channels to be instrumented for the octagonal barrel, (16 rings + 8 sectors)×6 channels 107 for the SiHyBall detector, (16 rings + 8 sectors)×2 channels for the S1 detector and (16 rings + 16 sec- 108 tors) channels for the S2 detector, resulting in a total of 288 channels. A schematic diagram of the TIARA

Figure 6: Diagram of the TIARA electronics for one end of a barrel strip, one ring and one sector of the annular detectors (SiHyball, S1, S2). 109 electronics is shown in Fig. 6. Eighteen 16-channel charge-sensitive preamplifier modules manufactured at 110 the University of the West of Scotland^1, eighteen CAEN N568B 16-channel spectroscopy amplifiers con- 111 trolled remotely via a CAENET V288 controller module, eighteen CAEN V814 16-channel low threshold 112 discriminators and nine 32-channel ADC modules are employed to record the energy signals from the array. 113 A SY2527 CAEN universal multi-channel power supply system equipped with a A1737N 12 High Voltage 114 (HV) channel board provided the -50 Volts necessary for the full depletion of all the silicon detectors. Typ- 115

1Previously University of Paisley.

ically leakage currents of around 0.2, 0.3, 4.0 and 1.1 μA respectively are drawn by each element of the 116 barrel and each wedge of the SiHyBall, the S1 and the S2 detectors. 117 The 16 charge-sensitive preamplifiers are mounted in double width NIM modules and are designed 118 specifically for use with room temperature silicon-strip detectors and resistive-sheet detectors with capaci- 119 tances in the range of 0 to 1000pF. Each unit houses two 8 channel motherboards with easily dismountable 120 preamplifier chips. Both the motherboards and preamplifiers chips are housed in a rugged well shielded 121 metal housing. With a quiescent DC output approaching zero, this unit is well adapted for use with the 122 CAEN N568B spectroscopy amplifier, which has 50 Ω input impedance. For each of the six wedges of the 123 SiHyBall detector, one complete module was used for the 16 front rings (with all 16 HV inputs combined) 124 while half of another module was used for the eight back sectors. In this way, three preamplifier modules 125 instrumented two wedges of the SiHyBall. Similarly three and two modules instrumented the S1 and S2 126 detector, respectively. For the four resistive strips of each of the eight barrel detectors, only half a module 127 was required with all the corresponding eight preamplifier HV inputs combined and connected. 128 Among the eighteen discriminators, five had to be adapted by the manufacturer to run with positive 129 polarity inputs in order to instrument the eighty back sectors of the SiHyBall, S1 and S2 DSSSD annular 130 detectors. Both the CAEN amplifiers and discriminators are remotely programmable and, for TIARA, the 131 control of this hardware is ensured via the Multi Instance Data Acquisition System (MIDAS)[12] applica- 132 tion developed at the STFC Daresbury Laboratory. Also used for the present work, and programmable via 133 MIDAS, are the eight 32-channel GANIL XDC3214 ADCs [13] operating in common dead-time mode and 134 an additional 32-channel Silena S9418 ADC. 135 EXOGAM, VAMOS and the TIARA array have their own stand-alone electronics and data acquisition 136 systems (DAQs). For the TIARA commissioning measurements discussed below, the 3 DAQs were merged 137 together using 3 hardware VXI CENTRUM modules which provided time stamping of the events and the 138 MERGER software for building the events [14]. The principal trigger of this commissioning experiment 139 was defined by a hit in any element of TIARA. 140 Due to room constraint around the TIARA vacuum chamber, a ∼3 m cable length was necessary to 141 connect the TIARA detectors to the preamplifiers. As a direct consequence, the thresholds in energy had 142 to be set high. They were ∼1 MeV for the double sided annular detectors and ∼1.5 MeV for the resistive 143 charge division detector. 144

Figure 7: (a) Image of the TIARA and EXOGAM arrays reconstructed from the first interaction point of a simulated 1 MeV γ-ray. This is a projection in the plane perpendicular to the beam axis (z) and conditioned by -4 cm ≤ z ≤ 4 cm. (b) Simulation of EXOGAM efficiency as a function of the γ-ray energy. The 4 clovers, denuded of their BGO Compton shields, are only 5 cm away from the target/source position. The triangles and the stars represent the photopeak and total efficiencies, respectively. The dots and diamonds represent the photopeak efficiencies after incorporating the “addback” procedure with and without the Lorentz boost.

3. Commissioning 145 3.1. Experimental Details 146 For the commissioning of the array and in order to validate the technique of heavy-ion—particle— 147 γ coincidence measurements, the d(^{14}N,pγ)^{15}N reaction was investigated at an energy representative of 148 SPIRAL radioactive beams. The 10.6 MeV/nucleon^{14}N beam was delivered by the first cyclotron of the 149 GANIL facility. The target was a 1 mg/cm^2 deuterated polythene (CD^2)_n self-supporting foil. The choice 150 of the reaction was dictated by a number of considerations: (a) the ground state of^{15}N is isolated and easily 151 resolved from the excited states; (b) the excited states populated in the reaction cannot be easily resolved 152 in inverse kinematics and (c) the reaction has been studied before in direct kinematics with light-particle 153 detection at a similar centre-of-mass energy. 154 As shown in Fig. 5 the TIARA reaction chamber allows four clovers of the EXOGAM array [15] to 155 be mounted in a cube-like configuration. In this configuration the segmented Ge clover detectors are all 156 positioned at 90^o relative to the beam axis and from a distance between the target and the front face of 157

each detector of approximately 5 cm. The photopeak efficiency in this configuration (Figure 7) is 13.5% at 158 1.332 MeV when the 4 central contact signals of the 4 crystals in each clover detector are added together 159 (“addback”). 160 The TIARA and EXOGAM arrays were mounted at the entrance of the VAMOS spectrometer (Fig. 5) 161 operating in momentum-dispersive mode [16]. The forward focused beam-like fragments are then identified 162 in mass and charge from measurements of the time-of-flight, energy loss, residual energy and position in 163 VAMOS. A plastic finger was placed in front of the VAMOS focal plane detection system to intercept the 164 intense non-interacting direct beam, which could damage the focal plane detectors. The data presented here 165 were recorded over a total of approximately 4 hours of beam time with an average beam intensity of 2·10^6 166 pps. 167 3.2. Simulations and Data Analysis 168 Knowing the efficiency of the experimental setup is essential if reaction cross sections and, hence, spec- 169 troscopic factors, are to be extracted. In this context a complete and realistic simulation of the setup can 170 be extremely useful. A Monte-Carlo simulation based on the GEANT4 code [17] has been developed to 171 mimic the response of the TIARA and EXOGAM arrays. The geometry defined in this simulation includes, 172 in particular, the entire active area of the TIARA array and the 2 mm thick aluminium walls of the reaction 173 chamber, the four EXOGAM Ge clover detectors, and the target [18]. Figure 7(a) illustrates a reconstructed 174 image of the response of the setup to a 1MeV γ-ray. 175 For the simulation of nucleon-transfer reactions, the event generator takes into account the kinematics 176 of the 2-body reactions and the differential angular cross section is set to be isotropic. The position of 177 the proton source (or interaction) in the target is chosen randomly according to the beam spot size and the 178 target thickness. The γ-rays are simulated assuming isotropic emission in the rest frame of the beam-like 179 reaction product and then boosted by the Lorentz effect. The intrinsic resolutions of all the detectors are also 180 included. 181 Taking into account the inactive regions of the Si detectors, the simulated overall efficiency of the TIARA 182 array for proton detection with energies of a few MeV emitted isotropically was found to be 84%. The 183 efficiency of the various components of the array as a function of the polar angle is illustrated in Figure 8. 184 An isotropic γ-source at the target position and with variable energy was also simulated to estimate the 185 EXOGAM photopeak efficiency and the result is shown in Figure 7(b). The photopeak attenuation induced 186 by the presence of the TIARA detectors and the reaction chamber is about 5% at 1.332 MeV, with the silicon 187 layer accounting for about 1%. 188

The output of the simulation is recorded in a ROOT tree which includes as many leaves as channels for 189 the two arrays. The simulated data and the real calibrated data can then be analysed identically using the 190 same analysis code performing the “add-back” and Doppler corrections. 191 An “addback” correction between the clover detectors was not considered here and, as noted above, 192 was only applied to the 4 crystals of each clover. When more than one crystal was hit in a clover, the 193 energies collected by the central contacts were summed together. The crystal with the highest deposited 194 energy was taken to be, for the Doppler correction, the first crystal hit. Simulations (Figure 9) show that 195 this assumption is a valid approximation as long as the energy of the γ-rays is higher than 500 keV. Indeed, 196 below 500 keV, when two crystals are hit the energies deposited in each crystal tend to be similar (see 197 bottom-left panel of Fig. 9 ) and, as a consequence, the identification of the first crystal to be hit becomes 198 uncertain. For events of crystal multiplicity M_{crys} = 1, the average angles chosen for the Doppler correction 199 are 78^o for downstream crystals and 102^o for upstream crystals. For events of higher crystal multiplicity, the 200 angles become respectively 84^o and 96^o as the closer to an adjacent crystal a Compton interaction occurs 201 the higher is the probability for M_{crys} > 1. These angles have been determined empirically by matching 202 of the photopeaks in downstream and upstream crystals and are consistent with the angles returned by the 203 simulations. 204 3.3. Results 205 The energy of the charged particles deposited in TIARA resulting from the reaction of the^{14}N beam 206 with the (CD_2)_n target as a function of laboratory polar angle recorded in the TIARA array is displayed in 207 Figure 10. The shadowing introduced by the presence of the target frame at 90^o is noticeable. At backward 208 laboratory angles where the emission of protons is expected, two clear kinematic loci are observed. These 209 loci become even more pronounced when the^{15}N residue is identified in coincidence in the focal plane of the 210 VAMOS spectrometer (Fig. 10b). In the barrel detector, data associated with a low discriminator threshold 211 have been removed, resulting in a noticeable inverted V-shaped cut at low deposited energy in Figs 10a and 212 b. The additional requirement of the detection of any γ-ray in coincidence, shown in Figure 10c, leads to 213 the disappearance of the protons in region R1 and, consequently, allows one to definitively associate this 214 locus with the d(^{14}N,p)^{15}N_{gs} reaction. Indeed, when the kinematics of this reaction channel are used as 215 input to the simulation, a perfect match between the simulation and the data (Fig. 10d) is obtained. Both 216 the kinematics and the expected proton punch-through energies are well reproduced. Note that the results of 217 the simulations extend to very forward angles because the differential cross sections dσ/dΩ have, as noted 218 earlier, been assumed to be isotropic. Since the reaction cross-section decreases relatively sharply with 219

Figure 8: Efficiency of the TIARA array as a function of the laboratory angle according to a GEANT4 simulation in which 2-5 MeV protons were generated and emitted isotropically.

decreasing proton laboratory angle, the protons punching through the detectors are not so apparent in the 220 data. 221 Similarly, the simulation indicates that the protons observed in region R2 can be associated with the 222 population of the 5/2^+ (7.16 MeV), 3/2^+ (7.30 MeV) or 7/2^+ (7.57 MeV) states of the^{15}N. The energy 223 resolution of the excitation energy spectrum (Fig. 11) reconstructed from the proton energy and position 224 measured in the barrel detector is ∼1 MeV (FWHM) and is clearly insufficient to resolve the three states 225 that lie above 7.1 MeV within 500 keV of each other. Apart from a broad structure centred at 7.5 MeV, 226 Figure 11(a and b) only reveals a small structure above 5 MeV. This can easily be interpreted as the direct 227 population of the known 5/2^+ (5.27 MeV) and 1/2^+ (5.3 MeV) states. In addition, with a spectroscopic factor 228 only 6 times smaller than the spectroscopic factors of the 7.16 and 7.57 MeV states, and 15 times higher 229 than the 5.3 MeV state[6], the 5/2^+ state at 5.27 MeV is most probably the main contribution. 230 The spectrum shown in Figure 12 illustrates the crucial role played by the γ-ray array. All the spectra 231 of Figure 12 are conditioned by a clover multiplicity equal to one. The middle panel shows the energy 232 distribution of the γ-ray measured in coincidence with the protons of region R2, after “addback” and Doppler 233 correction. Two narrow peaks at 1885 and 2295 keV and a broader structure at 5270 keV which result from 234

the de-excitation of the 5/2^+ and 7/2^+ states of^{15}N at 7.16 and 7.57 MeV, are observed (Figs. 12). As 235 discussed earlier, the de-excitation of the 5/2^+ and 1/2^+ states at 5.27 and 5.30 MeV, populated directly in 236 the reaction (Fig. 11), also contributes to the broad structure at 5170 keV, to a small extent. It should be noted 237 that the 3/2^+ level at 7.30 MeV, also observed by [5], decays directly to the ground state (Fig.12d) and will, 238 therefore, not be seen in coincidence with γ-rays in EXOGAM (owing to the very low detection efficiency 239 at such high energies). The Compton edges of the 1885 and 5270 keV γ-rays are also evident at around 240 1650 and 5000 keV respectively. A simulation of the two decay cascades, taking into account the Lorentz 241 boost and assuming that the two states were equally populated, has been carried out. The result is displayed 242 by the histogram in Figure 12(a) which has been normalized to the data such that the integrals between 1 243 and 6 MeV are the same. Although the intensities of the photopeaks at 1885 and 2296 keV seem slightly 244 over-estimated, there is a good overall agreement between the simulation and the data. The discrepancy 245 below 1 MeV is believed to arise from γ-rays scattering in material surrounding the detectors that have not 246 been included in the simulation. Indeed, in both the data and the simulation, only the events for which a 247 single clover detector is hit, have been taken into account. When all multiplicities are required, the number 248 of counts at low energy increases in both the data and the simulated spectrum. Figure 12(b) also displays the 249 contribution of each cascade and, in particular, the contribution of the Compton background in the region 250 of the photopeaks. According to the simulation these Compton events represent 26% of the peak intensity 251 at 1885 keV and ∼3.5% at 5270 keV. Given that the γ-decay of the two states (assumed here to be equally 252 populated) proceeds via the 5.27 MeV state, half of the Compton contribution from the line at 5270 keV is 253 actually in coincidence with the unobserved 1885 keV γ-ray. Therefore the total background contribution 254 to the 1885 peak is 27.8%. The Compton background from the 5270 keV line to the 2296 keV peak has 255 similarly been estimated to be 2.5%. 256 While, with the proton detection only, the final resolution on the excitation energy is restricted to ∼1 257 MeV, the gamma tagging technique improves dramatically the resolution to ∼100 keV, allowing for the two 258 closely spaced^{15}N excited states to be resolved. During the experiment, the segmentation information of the 259 Ge crystals was only available for one of the four clover detectors. A comparison of the γ-ray energy spectra 260 recorded in this clover with and without segmentation information is shown in Figure 12(c). At 2.3 MeV, 261 the resolution (FWHM) is 80 and 120 keV with and without the segmentation information, respectively. 262 The proton angular distributions displayed in Figure 13 were extracted by selecting events in region R1 263 of Figure 10(b) corresponding to the^{15}N ground state, and in coincidence with the 1885 and 2296 keV γ-ray 264 lines (Fig. 12b) corresponding to the^{15}N levels at 7.16 and 7.57 MeV. 265

The DWBA calculations displayed in Figure 13 were performed using the TWOFNR code [19] with 266 the optical model parameters calculated according to the Johnson-Soper prescription [20]. Each of the 267 theoretical distributions have been multiplied by the corresponding spectroscopic factors derived from direct 268 kinematics measurements in order to obtain the absolute differential cross section [6]: C^2S(g.s.)=1.33 , 269 C^2S(7.16 MeV)=0.90 and C^2S(7.57 MeV)=0.88. Transferred angular momenta of l=1 for the ground state 270 and l=2 for the two excited states were considered in the DWBA calculations in agreement with the results 271 obtained in direct kinematics [5, 6]. The experimental proton angular distributions for the ground and excited 272 states were normalized to the theoretical distribution. The shape of the experimental distributions for the 273 ground state (Fig. 13a) is in good agreement with the theoretical distributions. Similarly, the shapes of the 274 experimental and theoretical distributions for the two excited states Figures 13(b), and (c), are also in good 275 agreement. 276 Unfortunately, in the present measurements, the absolute cross sections, and hence spectroscopic factors, 277 could not be derived from the data. As noted earlier, part of the focal plane of VAMOS was protected from 278 the transmitted beam by a “finger”. As a result, no direct measurement of the beam dose or of the elastic 279 scattering could be made. Using, however, as a global normalisation the spectroscopic factor of 1.33 for the 280 ground state [6], the relative spectroscopic factors for the two excited states may be estimated. Values some 281 0.7 that of those previously measured [6] were so deduced, which is within the statistical uncertainties of 282 the measured differential cross section. Future measurements with radioactive beams will employ an active 283 “finger” together with beam detectors also capable of counting the beam particles. 284 3.4. Discussion 285 In the present study, knowing the level scheme of^{15}N facilitates the identification of the populated states. 286 For a nucleus with unknown level scheme, provided that there is enough statistics, a γ-γ coincidence analysis 287 can be carried out, in addition of simulations, to restore or establish a consistent level scheme. Therefore, 288 when coupled to a high efficiency γ-ray detector array, the TIARA array proposes a new alternative to other 289 existing detectors for direct reaction with unstable beams. Other detectors like MUST offer a much higher 290 dynamic range, better particle identification and intrinsic resolution than the TIARA array but they have 291 a limited solid-angle coverage which can make (d,p) reactions studies difficult. On the other hand, active 292 target detectors like MAYA competes very much with the TIARA array in term of solid-angle coverage and 293 are known to have significant lower energy threshold than silicon detectors. However, the large volume 294 occupied by active target detectors prohibits a coupling with a γ-ray array and, consequently, the γ-tagging 295 technique can hardly be used. 296

4. Summary 297 A new compact, large solid-angle segmented silicon detector array, TIARA, designed for the study of 298 direct reactions in inverse kinematics with radioactive beams, has been described. Coupled with a high effi- 299 ciency γ-ray detector array, such as EXOGAM, TIARA employs the technique of light (target-like) particle-γ 300 coincidences to obtain the necessary resolution in excitation energy in the residual target-like recoil. Identi- 301 fication of the latter, if required, may be performed using a magnetic spectrometer such as VAMOS. These 302 techniques have been validated in a commissioning experiment in which the d(^{14}N,pγ)^{15}N reaction was mea- 303 sured. In the near future, it is planned to increase the dynamic range of the silicon detector by the installation 304 of a second 700 μm thick Si layer around the existing barrel detectors together with 15 mm thick CsI(Tl) 305 segmented detectors backing the forward angle annular detectors. 306 5. Acknowledgements 307 The collaboration wishes to thank the GANIL cyclotron operations crew for delivering the^{14}N beam. 308 Partial support from the European Union under contract N^o506065 and from the Spanish MEC Grant 309 FPA2005-03993 are also gratefully acknowledged. The development and construction of TIARA were fi- 310 nanced by an EPSRC(UK) grant. 311 References 312 [1] J.S. Winfield, W.N. Catford, N.A. Orr, Nucl. Instr. Meth. A 396 ¯ (1997) 147. 313 [2] H. Lenske and G. Schreider, Eur. Phys. J. A 2 (1998) 41. 314 [3] Y. Blumenfeld et al., Nucl. Inst. Meth. A 421 (1999) 471. 315 [4] C. E. Demonchy et al., Nucl. Inst. Meth. A 573 (2007) 145. 316 [5] G.W. Phillips and W.W. Jacobs, Phys. Rev. 184 (1969) 1052. 317 [6] W. Kretschmer, G. Pröbstle and W. Stach, Nucl. Phys. A 333 (1980) 13. 318 [7] W.N. Catford et al., Application of Accelerators in Research and Industry 2002, J.L. Duggan and I.L 319 Morgan (Eds.), AIP Conf. Proc. 680 (2002) 329. 320 [8] W.N. Catford et al., Tours Symposium V, edited by Arnould et al., AIP Conf. Proc. 704 (2004) 185. 321

[9] W.N. Catford, Nucl. Phys. A 701 (2002) 1c. 322 [10] Micron Semiconductor LTD, Lancing, Sussex, UK. 323 http://www.micronsemiconductor.co.uk/ 324 [11] A. Galindo-Uribarri et al., 325 http://www.phy.ornl.gov/hribf/research/equipment/hyball 326 [12] V.F.E Pucknell and S.C. Letts, 327 http://npg.dl.ac.uk/MIDAS 328 [13] L. Olivier, 329 http://www.ganil.fr/gip/electronique/ng63p26 gb.html 330 [14] G. Wittwer et al., Real Time Conference 2005, 14th IEEE-NPSS Volume (2005) 3. 331 [15] J. Simpson et al., Acta Physica Hungarica: Heavy Ion Physics 11 (2000) 159. 332 [16] H. Savajols et al., Nucl. Phys. A 654 (1999) 1027c. 333 [17] S. Agostinelli et al., Nucl. Inst. Meth. A 506 (2003) 250. 334 [18] M. Labiche et al., J. Phys. G 31 (2005) S1655. 335 [19] M. Toyama and M. Igarashi, Computer program TWOFNR, unpublished. 336 [20] R.C. Johnson and P.J.R. Soper PRC 1 (1970) 976. 337

Figure 9: Top panels: Simulation of the energy deposited in crystal A versus the energy deposited in crystal B for an incident γ-ray of E_γ=1332 keV, with no condition (left) and with the condition that crystal A is hit first (right). Middle Panels: E_γ=700 keV. Bottom panels: E_γ=500 keV.

Figure 10: (a) Proton energy-angle spectrum for events detected in TIARA in coincidence with VAMOS. (b) Same as (a) with a gate on^{15}N identified in VAMOS. (c) Same as (b) with a coincidence in EXOGAM. (d) Same as (b) with Monte-Carlo simulations superimposed.

Figure 11: Excitation energy spectra obtained from the charge particles detected in TIARA: (a) With^{15}N detected in coincidence in VAMOS; (b) As for (a) with a γ-ray in coincidence in EXOGAM; (c) As for (a) with a 1885 keV (solid) and 2295 keV (dash) γ-ray in coincidence.

Figure 12: The γ-ray energy spectra in coincidence with the protons in region R2 of Fig. 10. The data and the simulations (histograms) of the γ-cascades from 5/2^+ and 7/2^+ levels to the ground state are shown before (a) and after (b) Doppler correction. The contributions of the cascades from the 5/2^+ and 7/2^+ levels at 7.16 and 7.57 MeV excitation energy are shown separately in (b). The distributions are normalized to the data by the integral of the number of events between 1 and 6 MeV. (c) Displays the data collected by a single clover after Doppler correction based on the 4 central contact signals (black histogram) and on the 16 outer contact signals (grey histogram). (d) Low energy^{15}N level scheme including the strongest transitions.

Figure 13: Proton differential cross section from the population of the ground (a) and excited states at 7155 (b) and 7565 keV (c) of 15N in the reaction d(^{14}N,p). The filled circles show the DWBA calculations normalized by previously measured spectroscopic factors. The filled squares represent the data normalized to fit the DWBA calculations.