arXiv:1011.1352v1 [cs.IT] 5 Nov 2010

Average Sum-Rate of Distributed Alamouti Space–Time Scheme in Two-Way Amplify-and-Forward Relay Networks

Trung Q. Duong^†, Chau Yuen^‡, Hans-Jürgen Zepernick^†, and Xianfu Lei^§

†Blekinge Institute of Technology, SE-371 79, Karlskrona, Sweden ‡Singapore University of Technology and Design, Singapore §Southwest Jiaotong University, Chengdu 610031, China E-mail: dqt@bth.se, yuenchau@sutd.edu.sg, hjz@bth.se, xflei81@yahoo.com.cn

Abstract—In this paper, we propose a distributed Alamouti space-time code (DASTC) for two-way relay networks employing a single amplify-and-forward (AF) relay. We first derive closedform expressions for the approximated average sum-rate of the proposed DASTC scheme. Our analysis is validated by a comparison against the results of Monte-Carlo simulations. Numerical results verify the effectiveness of our proposed scheme over the conventional DASTC with one-way communication.

I. INTRODUCTION

Relay networking has been considered as an efficient approach to increase the communication range of wireless systems. However, dual-hop half-duplex relay networks lose half of the throughput compared to the direct communication due to the fact that the relay cannot transmit and receive simultaneously. To overcome this drawback, a two-way (or bi-directional) relay network has been presented in [1], where two nodes, namely S_1 and S_2, transmit simultaneously to the relay R in the first hop, and in the second hop the relay R forwards its received signals to both terminals S_1 and S_2. With this strategy, this loss can be remarkably compensated.

As a result, two-way relay networks have gained great attention in the research community (e.g., see [1]–[5]). In view of the related work of two-way relay networks, the upper and lower bounds for average sum-rate have been investigated in [1]. The performance of two-way amplify-and-forward (AF) relay with network coding has been investigated in [2]. By giving up the strict separation of downlink and uplink signals through either time or frequency division duplex, a two-hop relaying, namely space division duplex relaying, is proposed in [3]. The exact closed-form expressions of error probability, average sum-rate for two-way AF relays have been presented in [4], [5].

Distributed Alamouti space-time code (DASTC) with AF relays originally applied for one-way relay networks [6] has recently extended to two-way systems (see, e.g., [7]–[9]). In particular, a two-way relaying scheme where two sources equipped with two antennas transmit Alamouti code through the help of an AF relay has been proposed in [7], [8]. Upper and lower bounds of average sum-rate have also been derived for this particular bi-directional relaying system. Another system in which the burden of deploying multiple antennas on sources is transferred to the relay has been proposed in [9]. By assuming that the relay is equipped with two antennas and each source is equipped with a single antenna, an upper bound of symbol error probability has been obtained. As can be observed from all the above schemes, either relay or source requires multiple antennas which may be prohibited in practical implementations due to the high demand for low-cost and small-size portable devices.

To alleviate this requirement and make the system realistic, a DASTC scheme which all terminals having only one antenna has been presented for one-way AF relay networks [10], [11]. However, this system still faces loss in spectral efficiency. Hence, in this paper, we propose a DASTC scheme for two-way AF relay networks which significantly recovers this loss. More importantly, unlike the analysis work in [7], [8] where the bounds of average sum-rate have been shown, we have derived an asymptotically tight approximation for the average sum-rate of the proposed two-way scheme. The final expression is given in the form of Fox’s H-function which enables us to investigate the performance of the proposed scheme. In addition, we also provide the numerical results to verify the correctness of our analysis.

The rest of this paper is organized as follows. In Section II, we introduce the system model of the proposed DASTC for two-way AF relay networks. Then, in Section III, we derive the tight approximation for the average sum-rate of the proposed scheme. Numerical results are shown in Section IV to validate the analysis. Finally, we conclude the paper in Section V.

Notation: Throughout the paper, we shall use the following notation. Vector is written as bold lower case letter and matrix is written as bold upper case letter. The superscripts ∗ and † stand for the complex conjugate and transpose conjugate, respectively. I_n represents the n × n identity matrix. ‖A‖_F denotes Frobenius norm of the matrix A and |x| indicates the envelope of x. E_x {.} is the expectation operator over the random variable x. A complex Gaussian distribution with mean μ and variance σ^2 is denoted by CN (μ, σ^2). Let us denote Ñ_m (m, Σ) as a complex Gaussian random vector with mean vector m and covariance matrix Σ. Γ (a, x) is the incomplete gamma function defined as Γ (a, x) = ∫_∞ x t^{a−1}e^{−t}dt and K_n (.) is the nth-order modified Bessel function of the second

Fig. 1. System model.

kind.

II. SYSTEM MODEL OF DISTRIBUTED ALAMOUTI SPACE-TIME CODES WITH TWO-WAY AF RELAYING

In this section, we introduce the system model of the proposed DASTC scheme with two-way AF relaying. Consider a wireless AF relay network consisting of three terminals as shown in Fig. 1. Two sources, namely S_1 and S_2, exchange the information through the assistance of an AF relay R. Each terminal is equipped with a single antenna which operates in half-duplex mode. We also assume that the channel for all links induces quasi-static fading, i.e., the channel remains constant for a block spanning over at least six symbolsintervals and varies independently for every block. Due to the channel reciprocity, we note that channel gains of A −→ B and B −→ A links, with A, B ∈ {S_1, S_2, R}, are identical.

The communications of the proposed two-way AF DASTC scheme occur in three phases. In the first phase, both S_1 and S_2 transmit the first row of Alamouti code [12] to R with the same transmit power per symbol P_s. The received signal at the relay R is given by

y_R = h_1s_1 + h_2x_1 + n_R (1)

where s_1 = [ s_1 s_2 ] and x_1 = [ x_1 x_2 ] are the two first rows of the Alamouti codes generated by S_1 and S_2, respectively. The channel coefficients for the link from S_1 and S_2 to R, respectively denoted as h_1 and h_2, follow a Rayleigh distribution, i.e., h_1 ∼ CN (0, Ω_1) and h_2 ∼ CN (0, Ω_2). The vector n_R is the complex additive white Gaussian noise (AWGN) with zero mean and variance N_0.

In the second phase, R amplifies the received signal, i.e., y_R, with the same power constraint as in the first phase and forwards to S_2 while S_1 sends the second row of the Alamouti code to S_2. The received signal at the source S_2, y_2, is written as y_2 = h_2Gy_R + h_0s_2 + n_2 (2)

where G is the scalar amplifying gain at the relay, h_0 ∼ CN (0, Ω_0) is the channel gain for the link between S_1 and S_2, s_2 = [ −s^∗_2 s^∗_1 ] is the second row of the Alamouti code, and n_2 is the AWGN vector with zero mean and variance N_0.

Similarly, in the third phase, R transmit Gy_R whereas S_2 sends the second row of the Alamouti code to S_1. The received signal at the source S_1, y_1, is shown as

y_1 = h_1Gy_R + h_0x_2 + n_1 (3)

where x_2 = [ −x^∗_2 x^∗_1 ] is the second row of Alamouti code and n_1 is the AWGN vector with zero mean and variance N_0.

The amplifying gain G is determined to satisfy the average power constraint between the relay and source, i.e., R consumes the same amount of power as each source. In this paper, we assume channel state information (CSI)-assisted AF relay, i.e., the relay perfectly knows instantaneous values of the channel gains h_1 and h_2. Taking these information into account, we have E { ‖Gy_R‖^2_F } = E { ‖s_i‖^2_F } = E { ‖x_i‖^2_F } (4) yielding

G^2 = ( |h_1|^2 + |h_2|^2 + 1 γ̄ )_{−1} (5) where γ̄ = P_s/N_0 is the average signal-to-noise ratio (SNR). With sufficient large SNR, the amplifying gain can be tightly approximated as

G^2 ≈ ( |h_1|^2 + |h_2|^2 )_{−1} (6) It is assumed that the two sources have perfect knowledge of the corresponding channel coefficients to fully cancel selfinterference. Hence, the received signal at S_1 and S_2 given in (3) and (2) can readily be formed, respectively, as follows: y_1 = hX + z_1 (7) y_2 = hS + z_2 (8) where h = [ Gh_1h_2 h_0 ], z_1 = Gh_1n_R + n_1, z_2 = Gh_2n_R + n_2, S = [ s_1 s_2 −s^∗_2 s^∗_1 ] , and X = [ x_1 x_2 −x^∗_2 x^∗_1 ] . Here, the new noise vector z_i, with i ∈ {1, 2}, is the complex Gaussian vector, i.e., z_i ∼ Ñ_2 ( 0, N_0 ( 1 + |h_i|^2 G^2 ) I_2 ) . It is important to note that S and X are Alamouti space-time codes constructed at S_1 and S_2, respectively.

III. AVERAGE SUM-RATE OF DISTRIBUTED ALAMOUTI SPACE-TIME CODES WITH TWO-WAY AF RELAYING In this section, we investigate the information-theoretic performance of the proposed DASTC with two-way AF relaying presented in Section II. As mentioned above, since the channel model is assumed to be ergodic block fading, we can describe the average sum-rate as follows:

C_{sum} = E { 2 3 log_2 det ( I_2 + 1 N_0 (1 + G^2|h_2|^2) h^†R_sh )

+ 2 3 log_2 det ( I_2 + 1 N_0 (1 + G^2|h_1|^2) h^†R_xh )} (9) where R_s and R_x are the covariance matrices of Gaussian codewords and the pre-factor 2/3 accounts for the fact that each source received information consisting of two symbols over three time slots. Due to the orthogonality of Alamouti codeword, it is easy to see that R_s = E { SS^† } = 2P_sI_2 and R_x = E { XX^† } = 2P_sI_2. Then we can rewrite (9) as

C_{sum} = E { 2 3 log_2 [( 1 + 2γ̄

|h_1|^2|h_2|^2 + |h_0|^2 ( |h_1|^2 + |h_2|^2 ) |h_1|^2 + 2|h_2|^2 )

× ( 1 + 2γ̄

|h_1|^2|h_2|^2 + |h_0|^2 ( |h_1|^2 + |h_2|^2 ) |h_2|^2 + 2|h_1|^2 )]} (10)

where (10) is established by the fact that det (I + AB) = det (I + BA). For notational simplicity, let us denote γ_i = 2γ̄|h_i|^2 with i = 0, 1, 2. Moreover, in the high SNR regime, i.e., γ̄ is sufficient large, the average sum-rate C_{sum} given in (10), after some manipulations, can be tightly approximated as 3 ln 2 2 C_{sum} ≈ E { ln ( γ_1γ_2 γ_1 + 2γ_2 )}

I_1 + E { ln ( γ_1γ_2 γ_2 + 2γ_1 )}

I_2

+ 2 E { ln ( 1 + γ_0 (γ_1 + γ_2)

γ_1γ_2 )}

I_3

(11)

In order to calculate (11), we first start our derivation by considering the similarity between I_1 and I_2 in (11). To evaluate the integral I_1 we utilize the probability density function (PDF) of Z derived in Lemma 1 given in the Appendix. From (25), we have

I_1 = 2∑ u=1 1∑ v=0 ∞∫ 0 A_v ln z 1 + z z^u exp(−β_1z)K_v (αz) dz (12)

where

α = 2 √ 2 γ̄_1γ̄_2

, β_1 = 1 γ̄_2 + 2 γ̄_1 A_0 = α^2, A_1 = αβ_1

To further simplify (12), we will express ln z/(1 + z) and exp (−αz) K_v (αz) in terms of the Meijer’s G-function with the help of [13, eq. (8.4.6.13)] and [13, eq. (6.4.23.3)] as follows:

ln z 1 + z = −πG^{2,2}_{3,3} ( z | | | | 0, 0, 1/2 0, 0, 1/2 ) (13)

exp (−αz) K_v (αz) = √ πG^{2,0}_{1,2} ( 2αz | | | | | 1/2 v, −v ) (14)

where G^{m,n}_{p,q} (·) is the Meijer’s G-function [13, eq. (8.2.1.1)]. Moreover, the Meijer’s G-function is a special case of the Fox’s H-function [13, eq. (8.3.2.21)] G^{m,n}_{p,q} ( z | | | | (a_p)

(b_q ) ) = H^{m,n}_{p,q} ( z | | | | (a_p, 1)

(b_q , 1) ) (15)

By combining (13), (14), and (15) with (12), we obtain

I_1 = − 2∑ u=1 1∑ v=0 π^{3/2}A_v ∞∫ 0 z^u exp [− (β_1 − α) z]

× H^{2,2}_{3,3} [ z | | | | (0, 1), (0, 1), (1/2, 1)

(0, 1), (0, 1), (1/2, 1) ]

× H^{2,0}_{1,2} [ 2αz | | | | (1/2, 1) (v, 1), (−v, 1) ] dz (16)

Then, the integral I_1 can be calculated with the help of [14, eq. (2.6.2)] as follows:

I_1 = −π^{3/2} 2∑ u=1 1∑ v=0 A_v (β_1 − α)^{−u−1}

H^{1,2,0,2,2} 1,[3:1],0,[3:2]

1 α+β_1

2α α+β_1

| | | | | | |

(1 + u, 1) (1/1, 1); (0, 1), (0, 1), (1/2, 1)

(0, 1), (0, 1), (^1_2 , 1); (v, 1), (−v, 1) (17) where H^{K,N,N ′,M,M ′} E,[A:C],F,[B:D][·] is the generalized Fox’s H-function

[14, eq. (2.2.1)]. Similarly, we can obtain the closed-form expression for I_2.

We next evaluate the integral I_3 by utilizing the PDF of T derived in Lemma 2 given in the Appendix. From (32), we have

I_3 = 2∑ n=1 ξ_n ∞∫ 0 ln (1 + t) (t + ζ)^{−3−n}

×_2F_1 ( 3 + n, n +^1_2 ;^7_2 ;^{t+η}_{t+ζ} ) dt (18)

Then we exchange the variable^{t+η}_{t+ζ} =^x_{x+1} and assume that the relaying protocol is symmetric, i.e., γ̄_1 = γ̄_2, yielding η = 0. We next express ln(1 + ζx) and (1 + x)^{−a}_2F_1 ( a, b; c;^x_{x+1} ) in terms of the Meijer’s Gfunction with the help of [13, eq. (8.4.6.5)] and [13, eq. (8.4.49.26)] as follows:

ln(1 + ζx) = G^{1,2}_{2,2} ( ζx | | | | 1, 1

1, 0 ) (19)

(1 + x)^{−3−n}_2F_1 ( 3 + n, n +^1_2 ;^7_2 ;^x_{x+1} )

= G^{1,2}_{2,2} ( x | | | | −2 − n,^1_2 − n 0, −2n ) (20)

By combining (19) and (20) with (18), we have

I_3 = 2∑ n=1 ξ_n ∞∫ 0 G^{1,2}_{2,2} ( x | | | | −2 − n,^1_2 − n 0, −2n )

× G^{1,2}_{2,2} ( ζx | | | | 1, 1

1, 0 ) dx (21)

The integral given in (21) can be finalized in the form of Fox’s H-function by using [15, eq. (7.811.1)] and [13, eq. (8.3.2.21)] yielding I_3 as follows:

I_3 = 2∑ n=1 ξ_nH^{4,2}_{4,4} [ ζ | | | | (0, 1), (2n, 1), (1, 1), (1, 1)

(2 + n, 1), (n −^1_2 , 1), (1, 1), (0, 1) ]

(22)

By substituting (17) and (22) in (11) and considering the fact that I_2 can be obtained in a similar form of I_1, the sum-rate of DASTC with two-way AF relay can be shown as

C_{sum} ≈ −

2π^{3/2} 3 ln 2 2∑ k=1 2∑ u=1 1∑ v=0 A_v (β_k − α)^{−u−1}

H^{1,2,0,2,2} 1,[3:1],0,[3:2]

1 α+β_k

2α α+β_k

| | | | | |

(1 + u, 1) (1/1, 1); (0, 1), (0, 1), (1/2, 1)

(0, 1), (0, 1), (^1_2 , 1); (v, 1), (−v, 1) + 4 3 ln 2 2∑ n=1 ξ_nH^{4,2}_{4,4} [ ζ | | | | (0, 1), (2n, 1), (1, 1), (1, 1)

(2 + n, 1), (n −^1_2 , 1), (1, 1), (0, 1) ]

(23)

IV. NUMERICAL RESULTS In this section, we provide the numerical results to verify the proposed two-way DASTC and the correctness of our analysis in two specific examples. The path loss of each link follows an exponential-decay model: if the distance between the two sources is equal to d, then Ω_0 ∝ d^{−α} where an exponent of α = 4 corresponds to a typical non line-of-sight propagation [7]. Here we assume that the S_1 −→ S_2 link has unit channel mean power, i.e., Ω_0 = 1. In the first example, we consider the symmetric relaying protocol, i.e., Ω_0 = Ω_1 = Ω_2 = 1. In the second example, we assume that the geometry for locations of three communicating terminals is co-linear where the relay is placed half way between the two sources, i.e., Ω_1 = Ω_2 = 16 and Ω_0 = 1.

Fig. 2 and Fig. 3 illustrate the average sum-rate of DASTC in two-way AF relay networks versus average SNR for the two considered examples. As can be observed from these two figures, the analysis is very tight from the middle to high SNR regime. Specifically, from SNR=10 dB the analytical and simulation curves perfectly match with each other which verify the tightness of our approximation.

More importantly, the proposed two-way DASTC scheme outperforms the conventional one-way system in terms of the spectral efficiency in the whole considered range of SNR. In particular, at SNR=30 dB, the proposed scheme enhances the average sum-rate to 3.8 bps/Hz in both Example 1 and 2 compared to the conventional one. It is interesting to observe that with a fixed value of Ω_0 the gain is unchanged, irrespective of the relay’s location.

V. CONCLUSIONS We have proposed a DASTC scheme for two-way AF relay networks that circumvents the loss in spectral efficiency inherently occurred in conventional one-way DASTC system.

Fig. 2. Average sum-rate of DASTC with symmetric relaying protocol.

Fig. 3. Average sum-rate of DASTC with co-linear relaying protocol.

We also derive the tight approximation for the average sumrate of the proposed scheme. The closed-form expression for approximated sum-rate is given in the form of Fox’s H-function which readily allows us to analyze the spectral efficiency of the proposed scheme. The numerical results provided have validated our analysis.

APPENDIX The following lemmas will be helpful in the paper. Lemma 1: Let γ_i and γ_j be statistically independent and not necessarily identically distributed (i.n.i.d.) exponential random variables with hazard rate γ̄_i and γ̄_j , respectively. Suppose that the ratio of Z takes the form Z = γ_iγ_j γ_i + 2γ_j

(24)

Then, we obtain the PDF of random variable Z as

p_Z (z) = αz exp (−β_iz) [αK_0 (αz) + β_iK_1 (αz)] (25)

where α = 2

√_2

γ̄_iγ̄_j and βi = 1 γ̄_j + 2 γ̄_i .

Proof: Let us rewrite Z in a more tractable form as

Z = (X + Y )^{−1} (26)

where X = 1/γ_i and Y = 2/γ_j . Then, after some algebraic simplifications together with the help of [15, eq. (3.471.9)], the moment generating function (MGF) of X and Y can be expressed as, respectively

Φ_X (s) = E_X {exp (−sx)} = 2 √ s γ̄_i K_1 ( 2 √ s γ̄_i ) (27)

Φ_Y (s) = E_Y {exp (−sy)} = 2 √ 2s γ̄_j K_1 ( 2 √ 2s γ̄_j ) (28)

As can be seen from (26), since 1/Z is the sum of two statistically independent random variables, by using (27) and (28), the MGF of 1/Z can be expressed as

Φ_{1/Z} (s) = 4 √ 2 γ̄_iγ̄_j sK_1 ( 2 √ s γ̄_i ) K_1 ( 2 √ 2s γ̄_j ) (29)

Then, the cumulative distribution function (CDF) of 1/Z, F_{1/Z} (x), can be shown as

F_{1/Z} (x) = 1 − L^{−1}{Φ_{1/Z} (s) /s}|_{1/x} (30)

where L^{−1}{.} stands for the inverse Laplace transform. From (29) and (30) together with [16, eq. (13.2.20)], we have

F_Z (z) = 1 − αz exp (−β_iz) K_1 (αz) (31)

where α = 2

√_2

γ̄_iγ̄_j and βi = 1 γ̄_j + 2 γ̄_i . By differentiating (31)

with respect to z and using the fact that^{dKv (z)}_{dz} = −K_{v−1} (z)− v z K_v (z) [15, eq. (8.486.12)], we obtain (25) which completes the proof.

Lemma 2: Let γ_0, γ_1, and γ_2 be the three i.n.i.d. exponential random variables with hazard rates γ̄_0, γ̄_1, and γ̄_2, respectively, then the PDF of T = γ_0^{γ1 +γ2}_{γ1γ2} is given by

p_T (t) = 2∑ n=1 ξ_n^1_{(t+ζ)3+n 2}F_1 ( 3 + n, n +^1_2 ;^7_2 ;^{t+η}_{t+ζ} ) (32)

where

ξ_n = √ π ( 4 √ γ̄_1γ̄_2 )_n Γ (3 + n) Γ (3 − n)

Γ (7/2) ϖ_n ϖ_0 = 4 γ̄_0γ̄_1γ̄_2

, ϖ_1 =

2 (γ̄_1 + γ̄_2) γ̄_0 (γ̄_1γ̄_2)^{3/2}

ζ = γ̄_0 ( 1 γ̄_1 + 1 γ̄_2 + 2 γ̄_1γ̄_2 ) , η = γ̄_0 ( 1 γ̄_1 + 1 γ̄_2 − 2 γ̄_1γ̄_2 )

and_2F_1 (a, b; c; z) is the Gauss hypergeometric function [17, eq. (2.12.1)].

Proof: Since T = γ_0^{γ1+γ2}_{γ1γ2} , by defining W =^{γ1γ2}_{γ1 +γ2} , we have

F_T (t) = ∫_∞ 0 [ 1 − exp ( − wt γ̄_0 )] p_W (w) dw (33)

Following similar steps as in Lemma 1, we obtain p_W (w) as

p_W (w) = 2w γ̄_1γ̄_2 exp [ − ( 1 γ̄_1 + 1 γ̄_2 ) w ]

× [ 2K_0 ( 2w √ γ̄_1γ̄_2 ) + ( γ̄_1 + γ̄_2 γ̄_1γ̄_2 ) K_1 ( 2w √ γ̄_1γ̄_2 )] (34)

By substituting (34) in (33) and taking the derivative with respect to t, we obtain the PDF of T as

p_T (t) = 2∑ n=1 ϖ_n ∞∫ 0 w^2 exp [ − ( t γ̄_0 + 1 γ̄_1 + 1 γ̄_2 ) w ]

× K_n ( 2w √ γ̄_1γ̄_2 ) dw (35)

It is observed that the integral given in (35) can be simplified by using [13, eq. (6.621.3)] which results in (32). This completes the proof.

REFERENCES

[1] B. Rankov and A. Wittneben, “Spectral efficient protocols for halfduplex fading relay channels,” IEEE J. Sel. Areas Commun., vol. 25, no. 2, pp. 379–389, Feb. 2007.

[2] P. Popovski and H. Yomo, “Wireless network coding by amplify-and-forward for bi-directional traffic flows,” IEEE Commun. Lett., vol. 11, no. 1, pp. 16–18, Jan. 2007.

[3] T. Unger and A. Klein, “Duplex schemes in multiple antenna two-hop relaying,” EURASIP Journal on Advances in Signal Processing, vol. 2008, article ID 128592, 14 pages, 2008. doi:10.1155/2008/128592.

[4] T. Q. Duong, L.-N. Hoang, and V. N. Q. Bao, “On the performance of two-way amplify-and-forward relay networks,” IEICE Trans on Commun., vol. Vol.E92-B, no. 12, pp. 3957–3959, Dec. 2009.

[5] R. H. Y. Louie, Y. Li, and B. Vucetic, “Practical physical layer network coding for two-way relay channels: Performance analysis and comparison,” IEEE Trans. Wireless Commun., vol. 9, no. 2, pp. 764–777, Feb. 2010.

[6] T. Q. Duong, D.-B. Ha, H.-A. Tran, and N.-S. Vo, “Symbol error probability of distributed-Alamouti scheme in wireless relay networks,” in Proc. 67th IEEE Veh. Technol. Conf. Spring, Marina Bay, Singapore, May 2008, pp. 648–652.

[7] Y. Han, S. H. Ting, C. K. Ho, and W. H. Chin, “High rate two-way amplify-and-forward half-duplex relaying with OSTBC,” in Proc. 67th IEEE Veh. Technol. Conf. Spring, Singapore, Apr. 2008, pp. 2426–2430.

[8] ——, “Performance bounds for two-way amplify-and-forward relaying,” IEEE Trans. Wireless Commun., vol. 8, no. 1, pp. 432–439, Jan. 2009.

[9] M. Eslamifar, W. H. Chin, C. Yuen, and G. Y. Liang, “Performance analysis of two-way multiple-antenna relaying with network coding,” in Proc. 70th IEEE Veh. Technol. Conf. Fall, Alaska, U.S.A., Sep. 2009, pp. 1–5.

[10] R. U. Nabar, H. Bölcskei, and F. W. Kneubühler, “Fading relay channels:

Performance limits and space–time signal design,” IEEE J. Sel. Areas Commun., vol. 22, no. 8, pp. 1099–1109, Aug. 2004.

[11] T. Q. Duong, N.-T. Nguyen, T. Hoang, and V.-K. Nguyen, “Pairwise error probability of distributed space-time coding employing Alamouti scheme in wireless relays networks,” Wireless Personal Communications, vol. 51, no. 2, pp. 231–244, Oct. 2009.

[12] S. M. Alamouti, “A simple transmit diversity technique for wireless communications,” IEEE J. Sel. Areas Commun., vol. 16, no. 8, pp. 1451– 1458, Oct. 1998.

[13] A. P. Prudnikov, Y. A. Brychkov, and O. I. Marichev, Integrals and Series. New York: Gordon and Breach Science, 1990, vol. 3.

[14] A. M. Mathai and R. K. Saxena, The H-function with Applications in Statistics and Other Disciplines. New York: Wiley, 1978.

[15] I. S. Gradshteyn and I. M. Ryzhik, Table of Integrals, Series, and Products, 6th ed. San Diego, CA: Academic Press, 2000.

[16] G. E. Roberts and H. Kaufman, Table of Laplace Transforms. W. B.

Saunders, 1966.

[17] A. Erdelyi, Higher Transcendental Functions. New York: McGraw- Hill, 1953, vol. 1.