arXiv:1011.2246v1 [cs.NI] 10 Nov 2010

p-Norm Flow Optimization in a Network

Sina Z. Anaraki, Mehdi Kalantari

In this paper we study information flow paths in a data network, where traffic generated by servers ( or sources) takes a multi-hop path in order to reach its clients (destinations). Each node in the middle of this multi-hop path should route the incoming traffic and the traffic generated by itself to the next hop in such a way that the traffic reaches its destination while avoiding congestion in the links. For simplicity, we will assume the network only carries single commodity traffic, i.e., all of the traffic should be routed to a single destination.

Let us assume that the data network is modeled by a connected graph G(V, E) where the set of vertices, V (|V | = N) represents the nodes (or data servers) and the set of edges, E (|E| = M) represents the links. For our analysis, we assume that the destination for all of the traffic in the network is node N. Two nodes are called adjacent if they are connected by an edge. A cut-set is a set of edges that if they are removed from the graph it becomes disconnected. A minimum cut-set is a cut-set with minimum cardinality. The throughput of a network with arbitrary sources and destinations is limited by the capacity of the links in the minimum cut-set of the network. If traffic is not routed carefully, when the network is under heavy traffic, some of these links may become congested while other are under-utilized. It is desirable to route the traffic such that each link in the minimum cut-set achieves its maximum capacity. When the capacity of all of these links are the same, an optimal routing would route the traffic on the bottleneck links such that the traffic is distributed evenly among them.

We arbitrarily assign a direction to each edge e_m such that if it connects nodes r and s where r < s, then the the direction of e_m is from r to s. Let us denote the traffic load on edge e_m with I_m. Note that if traffic flows from node r to node s then I_m is positive and it is negative if traffic flows in opposite direction. For each node n, the sum of incoming traffic load (from adjacent nodes with lower index ) and the traffic generated by the node itself (T_n) is equal to the sum of outgoing traffic (to adjacent nodes with higher index). These conservation of traffic constraints are written for nodes 1 . . . N − 1 in matrix form as

C · I = T (1)

where C is a (N − 1) × M matrix with elements in {−1, 0, +1}, I is a M × 1 vector of traffic loads I_m and T is a N − 1 × 1 vector of traffic sources T_n. For

[C]_{ij} we have

[C]_{i,j} = −1 if e_j connects node i to a node with lower index 0 1if e_j does not start or end with node i +1 if e_j connects node i to a node with higher index (2)

We define a cost function J_p(I) = ‖I‖^p = M∑ m=1 I^p_m (3)

and write the following optimization problem:

minimize_I J_p(I)

subject to C · I = T (4) In order to solve this problem in a distributed fashion we employ Sequential Quadratic Programming (SQP) in conjunction Jacobi iterations.

Let i be a small perturbation in I such that C · (I + i) = T . Thus C · i = 0 . We also have

J_p(I + i) = M∑ m=1 (I_m + i_m)^p (5)

≃ J_p(I) + 1 2 i^T · Q · i + S^T · i (6)

where S = p(I^{p−1}_1 , . . . , I^{p−1}_M ) and Q = diag ( p(p − 1)(I^{p−2}_1 , . . . I^{p−2}_M ) ) . Thus, for a given initial value of I, problem (11) becomes

minimize_I J̃_p(i) = 1 2 i^T · Q · i + S^T · i subject to C · i = 0 (7)

We can write J̃_p(i) as

J̃_p(i) =^M ∑ m=1 = 1 2 p(p − 1)I^{p−2}_m i^2_m + pI^{p−1}_m i_m (8) = ∑ 1 2 p(p − 1)I^{p−2}_m ( i^2_m + 2I_m p − 1 ) (9) = ∑ 1 2 p(p − 1)I^{p−2}_m ( ( i_m + I_m p − 1 )_2 − I^2_m (p − 1)^2 ) (10)

defining a new variable î_m = i_m +^{Im}_{p−1} we have the following optimization problem minimize_I J̃_p(î) = M∑ m=1 r_mî^2_m

subject to C · î = 1 p − 1 CT (11)

where r_m =^1_2 p(p − 1)I^{p−2}_m . The problem in this canonical form is easy to solve distributedly using Jacobi iterations. For each node we define a potential u such that if nodes r and s with r < s are connected by edge m then we have

î_m = u^r − u^s r_m (12)

Each node calculates its potential only as a function of the potentials of its adjacent nodes. Let A_n be the set of nodes that are adjacent to node n. Let ξ_n(k) be the index of the link that connects node n to an adjacent node k. Then by Jacobi iterations we have

u_n = [CT ]_n p−1 + ∑ k∈A_n u_k r_{ξn(k)} ∑ k∈A_n 1 r_{ξn(k)} (13)

. Note that the potential for the destination (node N) is always zero. After calculating the potentials for all of the nodes it is i_m is

i_m = u_r − u_s r_m − I_m p − 1 (14) . To summarize, up to here we calculated distributedly a correction vector i so that changing the traffic loads from I to I +i reduces the cost function J_p(I). Since J_p is a convex function of I for p > 1, this SQP steps can be repeated several times in order to reach the global minimum of J_p. Note that as p → ∞ the optimization problem becomes a minimax problem trying to distribute the traffic load evenly in the minimum cut-set links.