arXiv:1206.0399v2 [cs.IT] 20 Aug 2012

On the Computation of the Higher-Order Statistics of the Channel Capacity for Amplify-and-Forward Multihop Transmission

Ferkan Yilmaz, Member, IEEE, Hina Tabassum, Student, IEEE, and Mohamed-Slim Alouini, Fellow, IEEE

Abstract Higher-order statistics (HOS) of the channel capacity provide useful information regarding the level of reliability of the signal transmission at a particular rate. We propose in this letter a novel and unified analysis, which is based on the moment-generating function (MGF) approach, to efficiently and accurately compute the HOS of the channel capacity for amplify-and-forward multihop transmission over generalized fading channels. More precisely, our mathematical formulism is easy-to-use and tractable specifically requiring only the reciprocal MGFs of the instantaneous signal-to-noise ratio distributions of the transmission hops. Numerical and simulation results, performed to exemplify the usefulness of the proposed MGF-based analysis, are shown to be in perfect agreement.

Index Terms

Higher-order statistics, ergodic capacity, multihop transmission, amplify-and-forward transmission, generalized fading channels.

I. INTRODUCTION Relay technology has emerged as one of the the key enablers, according to the latest and most recent technologies and standardizations [1], to achieve not only higher quality but also higher reliability in

Manuscript received August 13, 2012. The review of this paper was coordinated by Xxxxxxxx.

Ferkan Yilmaz, Hina Tabassum and Mohamed-Slim Alouini are with King Abdullah University of Science and Technology (KAUST), Al-Khawarizmi Applied Math. Building, Thuwal 23955-6900, Makkah Province, Saudi Arabia (e-mail: {ferkan.yilmaz, hina.tabassum, slim.alouini}@kaust.edu.sa).

This work was supported by KAUST.

Digital Object Identifier 10.1109/XXX.2012.xxxxxx.xxxxxx

throughput as well as larger coverage and lower latency in wireless signal transmission since the relay technology is an effective method to combat pathloss and fading [2]. Accordingly for wireless signal transmission, amplify-and-forward (AF) multihop transmission has incessantly attracted a great deal of attention of the researchers in the last decade [1], [2].

The ergodic capacity is one of the information-theoretic performance metrics to quantify the achievable maximum throughput in wireless signal transmission. Within this context, some recent analysis frameworks [3]–[5] have appeared in the literature to quantify the ergodic capacity of AF multihop transmission over generalized fading channels. In particular, Farhadi and Beaulieu elegantly proposed in [3] a characteristic function (CF)-based approach. Later, Waqar et al. proposed in [5] an approximation-based approach using deformed-Stieltjes transform applied on the truncated series expansion of the logarithm function. Finally, Yilmaz et al. introduced in [4] a moment-generating function (MGF)-based approach to efficiently and accurately compute the ergodic capacity of AF multihop transmission over generalized fading channels. Nonetheless, these analysis frameworks are not enough to fully explore the reliability of the signal transmission. More precisely, and referring to the fact that the reliability is the ability of an item to perform a required function under stated conditions for a stated period of time, the reliability of AF multihop transmission is mainly characterized by the degree of dispersion or scatter in the channel capacity, rather than by the average of the channel capacity.

In a reliable transmission, the maximum dispersion or the peak-and-trough in the channel capacity should be controlled in order to achieve a successful carrier aggregation [1]. It is hence very useful to obtain the higher-order statistics (HOS) of the channel capacity. Several papers have addressed the HOS of the channel capacity for different types of fading channels [6]–[8, and references there in]. In particular, while some of the references in [6] have dealt with multiple input multiple output (MIMO) transmission over Rayleigh or Rician fading channels, Laourine et al. considered in [6] the HOS of the channel capacity over log-normal fading channels. There has been indeed a lack of unified analysis in the literature on the HOS of the channel capacity. Within this fact, Di Renzo et al. have presented in [7] a numerical approach to evaluate the HOS of the channel capacity for maximal ratio combining (MRC) diversity receivers. However, as mentioned in [7, Section III-E], this numerical solution requires both higher-order differentiation and a limit operation. In order to circumvent these computational difficulties, [8] offered recently an MGF-based approach for the HOS of the channel capacity. While the approaches developed in [7], [8] are applicable to MRC diversity receivers, they are neither applicable nor extendible to the computation of the HOS of the channel capacity for the AF multihop transmission, and to the best of our knowledge, there is no unified analysis available in the literature investigating this subject. In this letter, we propose a unified MGF-based approach to efficiently and accurately compute the HOS of the channel capacity for AF multihop transmission over generalized fading channels.

II. HIGHER-ORDER STATISTICS OF THE CHANNEL CAPACITY FOR AF MULTIHOP TRANSMISSION The end-to-end instantaneous signal-to-noise ratio (SNR) γ_{end} of AF multihop transmission over generalized fading channels is simply characterized by the normalized harmonic mean of the transmission hops’ instantaneous SNRs, that is given by [2, Eq. (4)] γ_{end} = 1 1 γ_1 + 1 γ_2 + . . . + 1 γ_L , (1)

where L is the number of hops in the multihop transmission and γ_ℓ denotes the instantaneous SNR of the ℓth hop. Note that the reciprocal distribution of γ_{end} is defined by ~γ_{end} = 1/γ_{end} and can be readily re-written as ~γ_{end} = ∑_L ℓ=1 ~γ_ℓ where ~γ_ℓ is the reciprocal distribution of the ℓth hop’s instantaneous SNR γ_ℓ. Hence, the higher-order statistics of the channel capacity for AF multihop transmission, i.e., μ_n = E [log^n (1 + γ_{end})], where E [·] denotes the expectation operator, n ∈ N is the order of the statistics and log(·) represents the natural logarithm, can be obviously re-written as μ_n = E [log^n (1 + 1/~γ_{end})] = ∫_∞ 0 log^n (1 + 1/γ) p_{~γend} (γ) dγ, where p_{~γend} (γ) is the probability density function (PDF) of ~γ_{end} and typically not available in closed-form when L is greater than two. In general, μ_n is given by

μ_n = ∫_∞ 0 ∫_∞ 0 . . . ∫_∞ 0 L-fold

log^n ( 1 + (∑_L ℓ=1 γ_ℓ )_{−1}) p_{~γ1,~γ2,...,~γL} (γ_1, γ_2, . . . , γ_L) dγ_1dγ_2 . . . dγ_L, (2)

where p_{~γ1,~γ2,...,~γL} (γ_1, γ_2, . . . , γ_L) is the joint PDF of the reciprocal distributions ~γ_1, ~γ_2, . . . , ~γ_L. It should be mentioned that (2) is computationally cumbersome, especially as the number of hops L is greater than two. Further, it cannot be separated into a product of one dimensional integrals because of the non-linearity of the natural logarithm log(·). In order to circumvent these difficulties, a novel MGF-based approach is introduced in the following theorem requiring only the reciprocal MGFs of the hops.

TABLE I RECIPROCAL MGFS OF SOME WELL-KNOWN CHANNEL FADING MODELS AND THEIR FIRST-ORDER DERIVATIVES

Instantaneous SNR Model, i.e., p_{γℓ} (γ) Reciprocal MGF M_{~γℓ} (s) and its First-Order Derivative ∂ ∂s M_{~γℓ} (s) Gamma Fading Environment [2]

p_{γℓ} (γ) = 1 Γ(m_ℓ) ( m_ℓ γ̄_ℓ )_{mℓ} γ^{mℓ−1} exp ( − m_ℓ γ̄_ℓ γ ) , M_{~γℓ} (s) = 2 Γ(m_ℓ) ( m_ℓs γ̄_ℓ )^mℓ_2 K_{mℓ} ( 2 √ m_ℓs γ̄_ℓ ) , ∂ ∂s M_{~γℓ} (s) = − 2 Γ(m_ℓ) ( m_ℓs γ̄_ℓ )^mℓ^{+1}_2 s^{mℓ2} K_{mℓ−1} ( 2 √ m_ℓs γ̄_ℓ ) , where the fading parameters m_ℓ ≥ 1/2 and γ̄_ℓ > 0 are the fading figure and average power, respectively. Moreover, K_m (·) is the mth-order modified Bessel function of second kind [9, Eq.(18.16)].

Generalized Gamma Fading Environment [10]

p_{γℓ} (γ) = ξ_ℓ Γ(m_ℓ) ( β_ℓ γ̄_ℓ )_{mℓξℓ} γ^{mℓξℓ−1} exp ( − (β_ℓ/γ̄_ℓ)^{ξℓ} γ^{ξℓ} ) , M_{~γℓ} (s) = 1 Γ (m_ℓ) Γ ( m_ℓ, 0, β_ℓ γ̄_ℓ s, 1 ξ_ℓ ) , ∂ ∂s M_{~γℓ} (s) = − β_ℓ Γ (m_ℓ) γ̄_ℓ Γ ( m_ℓ − 1 ξ_ℓ , 0, β_ℓ γ̄_ℓ s, 1 ξ_ℓ ) , where the fading parameters m_ℓ (0.5 ≤ m_ℓ < ∞), ξ_ℓ (0 ≤ ξ_ℓ < ∞) and γ̄_ℓ > 0 are the fading figure, shaping factor and average power, respectively. Moreover, β_ℓ = Γ ( m_ℓ + 1/ξ_ℓ ) /Γ ( m_ℓ ) , and Γ (·, ·, ·, ·) is the extended incomplete Gamma function [11, Eq.(6.2)]. Note that the special or limiting cases of GNM fading are well-known in the literature including Rayleigh, half-normal (i.e., half-Gaussian), Nakagami-m, Weibull, lognormal, and AWGN.

A. General Result on the HOS of the Channel Capacity

Theorem 1. The HOS of the channel capacity for AF multihop transmission over generalized fading

channels is given by

μ_n = ∫_∞ 0 Z_n(s) { M_{~γend} (s) − ∂ ∂s M_{~γend} (s) } ds, (3) where n ∈ N denotes the order of the statistics, and where M_{~γend} (s) = E [exp(−s ~γ_{end})] is the reciprocal

MGF of the end-to-end instantaneous SNR γ_{end}. Furthermore, the auxiliary function Z_n(s) is given by^{1,2}

Z_n(s) = (−1)^n_1F^{(n,0,0)}_1 [1; 1; −s] , (4)

where for m, n, q ∈ N and a, b, x ∈ R,_1F^{(m,n,q)}_1 [a; b; x] denotes Kummer’s differentiated confluent hyperge-

ometric (DCH) function defined in [12, Eqs. (07.20.20.0010.02), (07.20.20.0011.02), and (07.20.20.0012.02)].

Proof: Note that using the relation between the differentiation and the nth power of logarithm [9,

Eq. (5.1.4/(i))], we can readily write ∂^n ∂a^n ~γ^a_{end} (1 + ~γ_{end})^a = (−1)^n ~γ^a_{end} (1 + ~γ_{end})^a log^n (1 + γ_{end}) . (5)

1Note that the auxiliary function Zn(s) is a closed-form expression and is implemented as a built-in function in MATHEMATICA^® , that is Z[n , s ] := (−1)^n Hypergeometric1F1^{(n,0,0)}[1, 1, −s];

It can be moreover efficiently computed using numerical differentiation in MAPLE^® and MATLAB^{TM} mathematical packages.

Then, μ_n = E [log^n (1 + γ_{end})] can be represented as

μ_n = (−1)^n ∂^n ∂a^n ∫_∞ 0 γ^a (1 + γ)^a p_{~γend} (γ) dγ | | | |_{a=0} . (6)

By means of using the integral equality [13, Eq. (3.35.1/3)], the integral representation of γ^a/(1 + γ)^{a+1}

can be given by γ^a (1 + γ)^{a+1} = ∫_∞ 0 exp (−γ u)_1F_1 [1 + a; 1; −u] du. (7)

Then, substituting (7) into (6) and utilizing the Kummer’s DCH function [12, Eq. (07.20.20.0010.02)]

results in

μ_n = (−1)^n ∫_∞ 0 1F^{(n,0,0)} 1 [1; 1; −u] {∫_∞ 0 (1 + γ) exp(−γ u) p_{~γend} (γ) dγ } du. (8) Substituting the definition of the reciprocal MGF, i.e., M_{~γend} (u) = ∫_∞ 0 exp(−γ u) p_{~γend} (γ) dγ into the

inner integral easily results in (11), which proves Theorem 1.

Under the well-justified assumption that there does not exist any correlation among all reciprocal

instantaneous SNRs ~γ_1, ~γ_2, . . . , ~γ_L, the HOS of the channel capacity can be easily computed by using the

following corollary.

Corollary 1. When there is no correlation among all hops, the HOS of the channel capacity is given by^2

μ_n = ∫_∞ 0 Z_n(s) { 1 − L∑ ℓ=1 (∂/∂s)M_{~γℓ} (s) M_{~γℓ} (s) }_L∏ ℓ=1 M_{~γℓ} (s) ds, (9) where M_{~γℓ} (s) and (∂/∂s)M_{~γℓ} (s) denote the reciprocal MGF of the ℓth hop’s instantaneous SNR and

its first-order derivative, respectively, and are available in closed-form for a variety of fading channel

models as exemplified in Table I.

Proof: When there is no correlation among hops, one can readily write the joint MGF M_{~γend} (s) = ∏_L ℓ=1 M_{~γℓ} (s). Then the proof is obvious using the derivative of M_{~γend} (s).

2It is worth emphasizing that the main goal in a MGF-based approach is to convert the multidimensional integration of interest into a product of single-dimensional integrations each of which can be obtained in a closed form using Laplace transform [14]. More specifically, after using an MGF-based approach, the obtained analytical result should have one single-integration, and the obtained analytical result should be then efficiently computed using only one single-quadrature rule. With these observations, the developed approach in Theorem 1 and Corollary 1 is evidently an MGF-based approach.

B. Special Cases of the Auxiliary Function Z_n(s) and Some Statistical Applications of the HOS of the

Channel Capacity

Note that substituting n = 1 into (4) and then performing some algebraic manipulations, one can reduce

Z_1(s) to Z_1(s) = −e^{−s} ( E − Ei (s) + log(s) ) , (10)

where the constant E = 0.5772156649015328606... is the Euler-Mascheroni constant [12] and Ei (·) is

the exponential integral function [12, Eq. (06.35.07.0001.01)]. The first-order statistics of the channel

capacity, i.e., the ergodic capacity μ_1 = E [log(1 + γ_{end})] is then efficiently computed by

μ_1 = − ∫_∞ 0 e^{−s} ( E − Ei (s) + log(s) ) { M_{~γend} (s) − ∂ ∂s M_{~γend} (s) } ds, (11) which is numerically equivalent to [4, Eq. (9)] but converging faster; within this respect, it may be useful

for the researchers working in this field.

The variance of the channel capacity is a measure of how far the channel capacity lies from the ergodic

capacity and related to the first and second-order statistics of the channel capacity by var = μ_2 − μ^2_1.

Furthermore, its normalization with respect to the ergodic capacity corresponds to the amount of dispersion

(AoD) in the channel capacity, specifically given by AoD = μ_2/μ_1 − μ_1 taking values between zero

and one^3. Within this context, the reliability of the throughput can be defined as R = 100 − 100 AoD.

Accordingly, substituting n = 2 into (4) results in

Z_2(s) = e^{−s} ( E^2 − π^2 6 − 2 E Ei (s) + 2 ( E + Ei (s) ) log(s) −

3 log^2(s) ) + 2∑ n=0 ( 2 n ) log^n(s) Q_∞(s; 2 − n), (12)

where Q_n(x; ν), x ∈ C and n, ν ∈ N is a computationally efficient and recurrent polynomial defined by

Q_n(x; ν) = Q_{n−1}(s; ν) + x^{(n−1)/2} Q_{n−1}(ν), (13a)

Q_n(ν) = 4 n^2

Γ^{(ν)}(1 + n/2) Γ^{(ν)}(n/2)

Q_{n−2}(ν), (13b)

with the initial conditions Q_0(x; ν) = 0, Q_0(ν) = Γ^{(ν)}(1) and Q_1(ν) = 0, where Γ^{(ν)}(·) is the ν-order

3Note that for generalized one-sided Gaussian, Weibull, generalized Gamma and extended generalized-K fading environments, there is no physical justification, to the best of our knowledge, in the literature that the shape parameter ξ (i.e., not fading figure / diversity order m) can be smaller than one.

derivative of the Gamma function [12]. Next, substituting (12) into (11), the second-order statistics of the channel capacity is efficiently computed. Accordingly, the variance and the AoD in the channel capacity can also be readily obtained.

The other two important statistical metrics of the channel capacity are the skewness S = (μ_3 −μ^3_1)/(μ_2 − μ^2_1)^{3/2} and the kurtosis K = (μ_4 −μ^4_1)/(μ_2 −μ^2_1)^2. More specifically, the skewness corresponds to a measure of the degree of asymmetry of the distribution of the channel capacity while the kurtosis to the degree of peakedness of the channel capacity around the ergodic capacity. It is apparent that in order to obtain the skewness and kurtosis, the third- and fourth-order statistics are strictly required; and for this purpose, (4) can be easily and efficiently computed. Within this context, it is worth mentioning that the higherorder statistics can also be efficiently and accurately computed by means of Theorem 1 utilized with the following theorem.

Theorem 2. A computationally efficient, numerically accurate and extremely tight approximation of the auxiliary function Z_n(s) is given by

Z_n(s) = n∑ k=0 (−1)^k 2Δ^n ( n k ){ L_{−1−kΔ} (−s) + (−1)^nL_{−1+kΔ} (−s) } , (14)

where L_n (·) is the Laguerre polynomial of order n [12, Eq. (07.02.02.0001.01)] and Δ is a small number (e.g., Δ ≈ 0.01).

Proof: Proof is obvious using the Grunwald-Letnikov differentiation [15] and the Laguerre polynomial representation of the hypergeometric function (i.e.,_1F_1 [1 + a; 1; z] = L_{−1−a} (z) where a, z ∈ R) [12, Eq. (07.20.03.0009.01)].

III. NUMERICAL AND SIMULATION RESULTS For multihop transmission in generalized Gamma fading environments, the HOS of the channel capacity can be easily and efficiently computed using Theorem 1 as well as Corollary 1, yielding the equation given at the top of the next page. In order to check its analytical simplicity and accuracy with the exact auxiliary function in (4) and its tight approximation in (14), the HOS of the channel capacity for the AF triple-hop transmission is depicted in Fig. 1, in which numerical and simulation results are shown to be in perfect agreement. Accordingly, the variance, skewness and kurtosis of the AF multihop transmission can be easily evaluated using (15). As further seen in Fig. 1, the HOS of the channel capacity are almost the same around 7 dB. For the average SNR lower than 7 dB, the multihop transmission significantly gets

PSfrag replacements

Fig. 1. HOS of the channel capacity for AF triple-hop transmission (L = 3) over generalized Gamma fading channels. The shape parameter and fading figure are chosen the same as ξ_ℓ = 1.23 and m_ℓ = 2.34 for all ℓ ∈ {1, 2, 3}.

PSfrag replacements

Fig. 2. AoD in the channel capacity for AF multihop transmission over generalized Gamma fading channels. The shape parameter and fading figure are chosen the same as ξ_ℓ = 1.23 and m_ℓ = 2.34 for all ℓ ∈ {1, 2, . . . , L}.

μ_n = ∫_∞ 0 Z_n(s) {_L ∏ ℓ=1 1 Γ (m_ℓ) Γ ( m_ℓ, 0, β_ℓ γ̄_ℓ s, 1 ξ_ℓ )}_L∑ ℓ=1 β_ℓ Γ (m_ℓ) γ̄_ℓ Γ ( m_ℓ − 1 ξ_ℓ , 0, β_ℓ γ̄_ℓ s, 1 ξ_ℓ )_L∏ k=1 k≠ℓ 1 Γ (m_ℓ) Γ ( m_ℓ, 0, β_ℓ γ̄_ℓ s, 1 ξ_ℓ ) ds, (15)

into the low-SNR regime, and the HOS of the channel capacity can be characterized in this regime with μ_n ≈ μ^n_1 . In particular, the variance of the channel capacity significantly goes to zero in low-SNR regime.

In addition, Fig. 2 depicts the behavior of the AoD in the channel capacity with respect to different number of hops and average SNR values. More precisely, as the average SNR increases, the AoD in the channel capacity for a specific number of hops sharply increases, reaches its peak value, and then slightly decreases. For low- and high-SNR values, the AoD distinctly diminishes, which means that the channel capacity does not change drastically and the throughput is reliable (i.e., stable around its mean value). Furthermore, the AoD decreases as the number of hops increases. The other important benefit of AF multihop transmission is therewith to prominently enhance the reliability of transmission. For a better communication configuration, the SNR should be consequently chosen greater than the SNR value for which the AoD peaks. As for example seen in Fig. 2, the AoD is 0.1024 for 13 dB in a single-hop transmission, and accordingly its reliability percentage is R = 89.76. In other words, either the average SNR should be chosen equal to or greater than 13 dB or the number of hops should chosen equal to or greater than 2 hops in order to reach at least R = 100 − 100 AoD = 89.76 percent reliable transmission throughput.

IV. CONCLUSION In this letter, a novel MGF-based approach is proposed for the higher-order statistics of the channel capacity for AF multihop transmission over generalized fading channels. Our approach leads to a generic new expression which is computationally efficient and accurate and which requires only the reciprocal MGFs of the transmission hops. In addition, numerical results are shown to be in perfect agreement with those obtained via Monte-Carlo simulations, thus verifying the accuracy of our theoretical analysis.

REFERENCES

[1] 3GPP, “Release 12,” 3rd Generation Partnership Project (3GPP), Tech. Rep., March 2012. [Online]. Available: http://www.3gpp.org/ [2] M. Hasna and M.-S. Alouini, “Outage probability of multihop transmission over Nakagami fading channels,” IEEE Communication Letters, pp. 216–218, May 2003.

[3] G. Farhadi and N. C. Beaulieu, “Capacity of amplify-and-forward multi-hop relaying systems under adaptive transmission,” IEEE Transactions on Communications, vol. 58, no. 3, pp. 758–763, March 2010.

[4] F. Yilmaz, O. Kucur, and M.-S. Alouini, “Exact capacity analysis of multihop transmission over amplify-and-forward relay fading channels,” in Proc. IEEE International Symp. on Personal Indoor and Mobile Radio Commun. (PIMRC 2010), Istanbul, Turkey, Sep. 2010, pp. 2293–2298.

[5] O. Waqar, M. Ghogho, and D. C. McLernon, “Exact evaluation of ergodic capacity for multihop variable gain relay networks: A unified framework for generalized fading channels,” IEEE Tran. on Vehic. Tech., vol. 59, no. 8, pp. 1165–1181, Oct. 2010.

[6] A. Laourine, A. Stephenne, and S. Affes, “On the capacity of log-normal fading channels,” IEEE Transactions on Communications, vol. 57, no. 6, pp. 1603–1607, June 2009.

[7] M. D. Renzo, F. Graziosi, and F. Santucci, “Channel capacity over generalized fading channels: A novel MGF-based approach for performance analysis and design of wireless communication systems,” IEEE Transactions on Vehicular Technology, vol. 57, no. 1, pp. 127–149, 2010.

[8] F. Yilmaz and M.-S. Alouini, “On the computation of the higher order statistics of the channel capacity over generalized fading channels,” To appear in IEEE Wireless Communications Letters, 2012, Available at http://arxiv.org/abs/1204.3719.

[9] D. Zwillinger, CRC Standard Mathematical Tables and Formulae, 31st ed. Boca Raton, FL: Chapman & Hall/CRC, 2003. [10] F. Yilmaz, O. Kucur, and M.-S. Alouini, “A novel framework on exact average symbol error probabilities of multihop transmission over amplify-and-forward relay fading channels,” in Proc. IEEE Inter. Symp. on Wireless Commun. System (ISWCS 2010), York, UK, Sep. 2010.

[11] M. A. Chaudhry and S. M. Zubair, On a Class of Incomplete Gamma Functions with Applications. Boca Raton-London-New York-Washington, D.C.: Chapman & Hall/CRC, 2002.

[12] Wolfram Research, Mathematica Edition: Version 8.0. Champaign, Illinois: Wolfram Research, Inc., 2010. [13] A. P. Prudnikov, Y. A. Brychkov, and O. I. Marichev, Integral and Series: Volume 4, Direct Laplace Transforms. CRC Press Inc., 1990.

[14] M. K. Simon and M.-S. Alouini, Digital Communication over Fading Channels, 2nd ed. New Jersey, USA: John Wiley & Sons, Inc., 2005.

[15] A. A. Kilbas, H. M. Srivastava, and J. J. Trujillo, Theory and Applications of Fractional Differential Equations. Elsevier, 2006.