arXiv:1207.1868v1 [cond-mat.soft] 8 Jul 2012

Anomalous Front Broadening During Spontaneous Imbibition in a Matrix with Elongated Pores

Simon Gruener,^∗ Zeinab Sadjadi,^† Helen E. Hermes,^‡ Andriy V. Kityk,^§ Klaus Knorr,^∗ Stefan U. Egelhaaf,^‡ Heiko Rieger † and Patrick Huber^{∗ ¶ ‖}

∗Experimental Physics, Saarland University, D-66041 Saarbruecken, Germany,^†Theoretical Physics, Saarland University, D-66041 Saarbruecken, Germany,^‡Condensed Matter Physics Laboratory, Heinrich-Heine University, D-40225 Duesseldorf, Germany,^§Faculty of Electrical Engineering, Czestochowa University of Technology, P-42200 Czestochowa, Poland,^¶ Department of Physics, Pontifical Catholic University, Santiago, Chile, and^‖Materials Physics and Technology, Hamburg University of Technology, Hamburg, Germany

Submitted to Proceedings of the National Academy of Sciences of the United States of America

During spontaneous imbibition a wetting liquid is drawn into a porous medium by capillary forces. In systems with comparable pore length and diameter, such as paper and sand, the front of the propagating liquid forms a continuous interface. Sections of this interface advance in a highly correlated manner due to an effective surface tension, which restricts front broadening. Here we investigate water imbibition in a nanoporous glass (Vycor) in which the pores are much longer than they are wide. In this case, no continuous liquid-vapor interface with coalesced menisci can form. Anomalously fast imbibition front roughening is experimentally observed by neutron imaging. We propose a theoretical pore network model, whose structural details are adapted to the microscopic pore structure of Vycor glass, and show that it displays the same large scale roughening characteristics as observed in the experiment. The model predicts that menisci movements are uncorrelated. This indicates that despite the connectivity of the network the smoothening effect of surface tension on the imbibition front roughening is negligible. These results suggest a new universality class of imbibition behavior which is expected to occur in any matrix with elongated, interconnected pores of random radii.

liquid imbibition | porous media | interface roughening | neutron imaging | pore network model | computer simulations

Abbreviations: NVG , nanoporous Vycor glass

M^{any everyday processes involve the flow of a liquid into}

a porous matrix, for instance when we dunk a biscuit into coffee, clean the floor with a cloth, or get drenched with rain. The same process is also important in nature, e.g. for water to reach the tips of the tallest trees or to flow through soil, and crucial for different industrial processes, ranging from oil recovery and chromatography to food processing, agriculture, heterogeneous catalysis, and impregnation (for reviews see [1, 2, 3, 4]).

The above processes are examples of imbibition (Fig. 1). Imbibition of a liquid into a porous matrix is governed by the interplay of capillary pressure, viscous drag, volume conservation and gravity. The porous matrix often has a complex topology. The inhomogeneities result in variations in the local bulk hydraulic permeability and in the capillary pressure at the moving interface. Nevertheless, the invasion front during solely capillarity-driven (i.e. spontaneous) imbibition advances in a simple square-root-of-time manner, according to the Lucas-Washburn law [5, 6]. This is a result of the time-independent mean capillary pressure and the increasing viscous drag in the liquid column behind the advancing front. It is valid down to nanoscopic pore sizes [7, 8, 9] and particularly robust with regard to the geometrical complexity of the porous matrix [1, 4, 10, 11]. The evolution of the invasion front displays universal scaling features on large length and time scales, which are independent of the microscopic details of the fluid and matrix [12, 13, 14, 15, 16, 17, 18]. This parallels the elegance of critical phenomena.

Typically imbibition is studied using paper [14, 15, 16] or Hele-Shaw cells [17, 18]. In these systems, pore space is laterally highly interconnected. This results in a continuous liquid-gas interface, whose advancement is spatially correlated due to an effective surface tension [19]. Consequently menisci advancement beyond the average front position is slowed down whilst menisci lagging behind are drawn forward. Hence, the roughening of the interface is slowed down. By contrast, in many real porous systems, e.g. rock and soil [20], the pore network consists of elongated pores with reduced connectivity [1].

Here we investigate the spontaneous imbibition of water into nanoporous Vycor glass (NVG), which is a silica substrate with an interconnected network of nanometer-sized, elongated pores [21]. The narrow pores lead to capillary pressures of several hundred times atmospheric pressure. This means that gravity would only halt capillary rise after several kilometers and several billion years [22]. Hence, with this system, we are able to observe pure spontaneous imbibition over large length (centimeter) and long time (hours) scales. The observation of the advancing front is difficult since it is deeply buried inside the matrix [23, 24]. Nevertheless, neutron radiography [25, 26, 27] allows us to image the liquid inside porous materials [28, 29]. Recent technical improvements in neutron imaging provide the spatial and temporal resolution (tens of μm and tens of s) to follow imbibition and to obtain quantitative information on the morphological evolution of the progressing interface.

Our experiments and simulations show that the interface roughness as measured by the interface width w(t) increases much faster than observed previously, namely w(t) ∝ t^β with β ≈ 0.45. This is close to the square-root-of-time progression of the invasion front H(t) ∼ t^{0.5}. The propagation front hence comprises an almost constant fraction, w(t)/H(t), of the occupied part of the matrix, including voids and overhangs. We find that lateral correlations of the invasion front are short-ranged and independent of time. This means that, in the present case, surface tension is irrelevant in a coarse grained description of interface broadening on macroscopic length scales. Similar broadening has been observed, but for

Reserved for Publication Footnotes

http://www.pnas.org/content/109/26/10245 PNAS June 26 109 26 10245–10250

different experimental conditions, namely drainage and forced imbibition of less-wetting fluids [30, 31].

Results and Discussion Quantitative Experimental Characterization of the Imbibition Front. We investigate imbibition in NVG which contains pores with a mean radius rav = 4 nm, a radius polydispersity of 20 %, a pore aspect ratio a = L/2rav between 5 and 7 (where L is the pore length), and a porosity of about 30 % [8, 21, 32, 33]. (For details see Methods.) The bottom face of an empty NVG is brought into contact with the surface of a water reservoir. Capillary forces draw the liquid into the porous matrix.

The invasion front appears as a bright region when imaged using reflected light (Fig. 2, top row). The pronounced (multiple) light scattering is caused by filled and empty regions randomly alternating on the length scale of the wavelength of visible light; several hundred nanometers [34]. These spatial scales are much larger than any intrinsic length of the porous matrix, such as the pore diameter or the pore-pore distance. Thus strong scattering of light at the advancing interface indicates structures of filled and empty parts (voids) of surprisingly large size. It prevents also a quantitative determination of the liquid profile in the propagating front and hence of the width of the interface. By contrast the spatial and temporal resolutions of neutron imaging [35] allow quantitative measurements in systems such as NVG (Fig. 2, bottom row).

From the neutron images we determine the spatial and temporal evolution of the local filling degree 0 ≤ f(x, z, t) ≤ 1. Due to the projection in the y-direction, this is the average amount of filled pore space at lateral position x, height z and time t. Its lateral average, that is the vertical concentration profile f̄(z, t) ≡ ⟨f(x, z, t)⟩x, is shown in Fig. 3a. The time-dependence of the front height, quantified by the mean median rise level H(t) ≡ ⟨z(f=0.5, x, t)⟩x, follows the Lucas- Washburn √ t-law (Figs. 3a,b, solid lines), consistent with previous studies [8]. Fits of Gauss error functions to the profiles yield the time-dependence of the width w(t) (Fig. 3c). The fit of w(t) ∝ t^β results in a growth exponent of the width or roughness, β = 0.46 ± 0.01 (Fig. 3c, solid line). The value β = 0.46 significantly exceeds previous theoretical predictions, in particular those from phase-field models which are based on quenched, random fields. Such models predict slower roughening dynamics with β ≈ 0.19 and a strong spatial correlation of the height fluctuations within the moving interface [13].

Instead of the median rise level averaged in x direction, H(t) = ⟨z(f=0.5, x, t)⟩x, we now consider the local xdependent median rise level h(x, t) ≡ z(f=0.5, x, t) (Fig. 3b) to investigate fluctuations in x-direction, i.e. within the front. We calculate the height-height correlation function: C(ℓ, t) = √ ⟨(h(x, t) − h(x+ℓ, t))^2⟩x . [1] The observed fluctuations in C(ℓ, t) (Fig. 3d) are due mainly to the limited data density and stray gamma radiation from the reactor and instrument hitting the camera. The data exhibit neither scaling of C(ℓ, t) with ℓ nor any indication of spatial correlations in the experimentally accessible range 75 μm ≤ ℓ ≤ 4000 μm. Although the correlations are reduced due to the projection in y-direction, the absence of any detectable correlation is in contrast to all previously reported experiments and theories on imbibition front roughening.

Pore-network Model.

No theoretical model is available that is consistent with our system and which predicts the spontaneous imbibition behavior observed. An ensemble of independent pores of random but constant radius exhibits a roughening exponent 1/2 since the meniscus heights evolve independently from one another as hi(t) = ai √ t with random pre-factors ai. However, this independent pore model is inappropriate for Vycor glass, since the pore radii vary strongly along individual pores (see Fig. 1). An ensemble of independent pores with radii which vary randomly along their length has a roughening exponent of 1/4 (see Appendix), which does not agree with the experimentally observed value. Thus independent pore models do not explain the observed exponent. A roughening exponent β ≈ 1/2 has recently been reported within the framework of a lattice gas model for spontaneous imbibition [41]. This model is appropriate for silica aerogels with an extremely large porosity of 87–95 % and gives rise to a continuous liquid-gas interface. Consequently one expects here an effective surface tension to be present, inducing height-height correlations in the advancing imbibition front. The model details are thus not appropriate for NVB. To our knowledge, all other existing theoretical models (for an overview see [4]) are also incompatible with our experimental observations which are i) fast broadening dynamics with a growth exponent close to 1/2, ii) absence of height-height correlations in the advancing imbibition front.

Hence we propose a pore-network model [36, 37] adapted to our experimental situation. This consists of individual, elongated capillaries arranged in a two-dimensional square lattice with laterally periodic boundary conditions. Capillaries are connected at nodes and inclined at 45^∘. All capillaries have the same length L, while the radius r of each capillary is randomly chosen from a uniform distribution with mean radius rav and width 2δr, i.e. disorder strength δr/rav . [21, 33]. (For details see Methods.) We investigated aspect ratios 2.5 ≤ a ≤ 10 and polydispersities 0.1 ≤ δr/rav ≤ 0.4.

The pressure at all nodes at the bottom of the lattice are set to zero while at the menisci the Laplace pressure prevails. This pressure difference drives the flow through the capillaries. This flow is opposed by viscous drag according to Hagen- Poiseuille’s law. During the whole process, volume conservation must be maintained. When a meniscus reaches an empty node it ‘jumps’ over the node, generating new menisci in a distance δ = L/100 from the node (Fig. 4a). This implementation of node crossing avoids a microscopic treatment of the filling process of the nodes and is valid as long as this is not the rate limiting step, which we will discuss below. If the Laplace pressure of a meniscus exceeds the node pressure the meniscus is arrested at the distance δ until the node pressure increases beyond the Laplace pressure (Fig. 4b). Then propagation of the meniscus resumes.

Computer Simulation Results of Imbibition. With our model, we observe a strong roughening of the imbibition front (Fig. 4d) with fast moving menisci advancing through sequences of thin capillaries and arrested menisci lagging behind. Quantitatively, the computer simulations yield a mean rise level H(t) = ⟨hi(t)⟩ (where ⟨. . .⟩ denotes an average over all menisci labelled by the index i), which obeys the Lucas-Washburn √ t-behavior (Fig. 5a). The width w(t) = (⟨h^2_i (t)⟩ − ⟨hi(t)⟩^2)^{1/2} increases rapidly as w(t) ∝ t^β with β = 0.42±0.01 or 0.45±0.01 for the smallest and largest polydispersities, respectively (Fig. 5b). We find a slight upward trend of w(t) at large times (Fig. 5b, inset), which is also suggested in the experimental data (Fig. 3c) and indicates that the asymptotic value of the growth exponent might be larger. This is consistent with the fact that a smaller β is observed when the asymptotic behavior is approached later (as in the case of the smaller polydispersity). This implies that

10246 http://www.pnas.org/content/109/26/10245 Footline Author

the asymptotic value is closer to that found for the larger polydispersity with an increased uncertainty, i.e. β = 0.45 ± 0.02. Variation of the aspect ratio in the range 2.5 ≤ a ≤ 10 gave identical results for the exponent β.

We systematically studied finite size effects, especially on w(t). Remarkably, we only find a dependence on the lateral system size Nx for the smallest system size Nx = 4 (Fig. 5c). This provides an upper bound for the characteristic length scale ξ(t) of height-height correlations. Within the framework of the scaling theory of roughening [38, 39], the interface width in a finite system of lateral size Nx is expected to behave as wN_x (t) ∼ { t^β for ξ(t)/L ≪ Nx const. for ξ(t)/L ≫ Nx [2]

The data (Fig. 5c) suggest ξ(t) < 4L, implying that the roughening dynamics are not or are only weakly spatially correlated. This is confirmed by the height-height correlation function C(ℓ, t) (eq. 1, Fig. 5d), which saturates quickly (around ℓ ≈ L). Scaling theory [38, 39] predicts saturation of C(ℓ, t) for ℓ ≫ ξ(t), which implies ξ(t)/L = O(1) independent of time t. This finding supports our experimental result (Fig. 3d) that any spatial roughness correlations are absent and extends its validity down to pore-pore distances and thus towards the nanometer-scale, i.e. far beyond our experimental resolution.

Experiments and Simulations Both Yield an Anomalous Roughness Growth Exponent. Experiments and simulations exhibit corresponding behavior, even on a quantitative level, i.e. progression of the imbibition front according to the Lucas-Washburn √ t-law, fast broadening of the front with a large growth exponent β ≈ 0.45 and short range height-height correlations over a maximum of 1–2 pore lengths only. The pore-network model with its elongated pores hence successfully mimics the characteristics of NVG. In such morphologies, all menisci are restricted to individual pores and thus cannot interact via an effective surface tension. In the absence of interactions between individual menisci local processes at the junction become important for the front roughening. The dynamics of junction filling, as analyzed in [40], describes a threshold mode in which meniscus propagation is halted whilst the junction is filled and the new menisci in the adjacent pores form. This takes only a few milliseconds in nanometer sized pores with filling heights up to 2 cm (as in the present case), for which gravity is negligible. Once the new menisci have formed, those in the thicker pores are arrested as long as their Laplace pressure is larger than the pressure within the junction. These arrests can last much longer than the filling process, up to times of the order of the age of the propagation front, which can be several hours in our experiments. Thus for the asymptotic (long time) behavior of the broadening dynamics, the filling process of individual junctions is negligible and front roughening is mainly influenced by the arrests after the filling of the junctions. As a consequence, the distribution of pore diameters and the frequencies of junctions is expected to be much more important than the topology, in particular the dimensionality, of the network. This contrasts with the role the latter usually plays in surface roughening and critical phenomena [38, 39].

It should be noted that it is crucial that the pores in NVG are connected [21, 33], since an ensemble of independent pores with randomly varying radii over their lengths would give a roughness exponent 1/4 (see Appendix). Perhaps counterintuitively, the introduction of junctions, i.e. branch points or crossings, enhances height fluctuations and hence the front width. This is because at each branch point one meniscus can split into two (or more) upwards moving menisci with one typically moving faster than the other, or even one moving and the other stopping until the node pressure exceeds its Laplace pressure.

Conclusions Pore Aspect Ratio Determines the Universality Class. Our results show that spontaneous imbibition crucially depends on the pore aspect ratio a. For short pores (small a), neighboring menisci coalesce and form a continuous imbibition front. Thus the smoothening effect of an effective surface tension within the interface leads to a slow broadening of the front. Various theoretical models describe the roughening of a vapor-liquid interface during spontaneous imbibition in the presence of an effective surface tension, e.g. phase field models [19]. These predict a roughening exponent β ≈ 0.19. The elongated pores in nanoporous Vycor glass (large aspect ratio a) inhibit the formation of a connected vapor-liquid interface. In this case the individual menisci cannot interact via an effective surface tension and the broadening of the imbibition front is anomalously fast with β ≈ 1/2 establishing another universality class. The regime of weak roughening (small a) must be separated from the regime of strong roughening (large a) by a critical value ac of the aspect ratio, but its precise value will depend on structural details of the pore network, in particular the pore junction geometry.

We want to stress that strong imbibition front broadening is not linked to the nanometer size of the pores. However, its experimental observation over large length and time scales significantly benefits from the dominance of capillary forces over gravitational forces, which results from the nanometer-sized pores. The theoretical model employs macroscopic hydrodynamic concepts only. Therefore, strong interfacial broadening is a consequence of any spontaneous imbibition process in porous structures with interconnected elongated capillaries independent of their macroscopic extension and mean pore diameter. It is not only important to nanofluidics, but for liquid transport in porous media in general.

Our observation of a new universality class of strong interfacial broadening is thus a very general finding, which has been made possible due to recent improvements in the resolution of neutron imaging [35]. The front roughness is crucial for many processes, such as water transport in geology, flux in oil recovery, glueing, dying and impregnation. Our results enable us to link the broadening dynamics during these processes to the properties of the porous materials. To what extent this behavior can be described with alternative models for transport in porous media, e.g. models which consider a saturation-dependent hydraulic permeability of the pores [4], warrants further investigation.

Materials and Methods

Neutron Imaging.

The nanoporous Vycor glass (NVG) consists of an interconnected network of elongated pores with a mean radius rav = 4 nm, a radius polydispersity

δr/rav = 0.2, a pore aspect ratio 5 ≲ a ≲ 7, and a porosity of about 30 %

[8, 21, 32, 33]. The macroscopic dimensions of the sample are 4.6×4.6×20 mm3 . Its faces, except the bottom face, are sealed to preclude liquid evaporation. To initiate imbibition, the bottom face of the sample is brought into contact with the surface of a water reservoir. During imbibition, the huge capillary pressure highly compresses entrapped air which is subsequently dissolved in water and hence does not affect our experiments. All experiments are performed at room temperature.

Footline Author PNAS June 26 109 26 10247

The neutron imaging experiments are performed at the ANTARES beamline of the research reactor FRM II of the Technical University Muenchen (Garching, Germany) [42]. A beam of cold neutrons passes through an aperture with size D and, after a distance L, ‘illuminates’ the sample, which is situated d = 30 mm in front of the scintillator. The geometrical resolution is d/(L/D) = 75 μm. The transmitted neutrons are detected using a very thin ‘Gadox’ scintillator, which does not limit the geometrical resolution, and a CCD camera with pixel size 15.97 μm. Series of images are recorded for total measurement times up to several hours. Individual measurement times are 30 s and data transfer times 10 s. In the first few kinetic images smearing occurs due to the front moving a significant distance during the individual measurement times. However, after about 1000 s, the smearing due to the limited time resolution is negligible compared to the spatial resolution (and only these data are used for fitting w(t)). Raw images were corrected for detection efficiency, background and noise, while corrections for scattered neutrons are not necessary [43].

The experimentally determined neutron transmission T (x, z, t), that is the ratio of transmitted intensity I(x, z, t) and incident intensity I0(x, z, t), is related to the absorption coefficient S(x, z, t) by T (x, z, t) = I(x, z, t) I0(x, z, t) = e^{−S(x,z,t) d} [ 3 ] where d = 4.6 mm is the sample thickness. The absorption coefficient S(x, z, t) = Sm(x, z, t) + f(x, z, t) Sw [ 4 ] depends on the absorption coefficient of the porous matrix Sm(x, z, t), experimentally determined from the dry matrix, and on that of the liquid Sw, determined from the completely filled matrix providing Sm(x, z, t)+Sw . The filling factor

f(x, z, t) can then be determined from the experimentally determined transmission T (x, z, t). While silica, and thus NVG, is almost transparent to neutrons, the neu-

tron beam is strongly attenuated by hydrogen in the water. The contrast is further enhanced by the characteristic wavelength distribution of the ANTARES beamline, which contains a large fraction of cold neutrons.

Computer Simulations. The pore-network model consists of capillaries arranged on a two-dimensional square lattice inclined at 45∘. The system consists of

Nx and Nz nodes in the horizontal and vertical directions, respectively, with peri-

odic boundary conditions in horizontal direction. At the nodes, four capillaries are connected to each other (Fig. 4). All capillaries have the same length L, while the radius of each capillary is chosen randomly from a uniform distribution with mean radius rav and distribution width δr, i.e. disorder strength δr/rav . We performed computer simulations for different lateral system sizes 4 ≤ Nx ≤ 32 and a vertical size up to Nz = 1000, which implies a maximum height H = √ 2 L Nz which

was not reached by the invasion front within the simulation time.

The water rises spontaneously from the bottom to the top of the lattice. The dynamics are controlled by capillary pressure, viscous drag and volume conservation. At each meniscus, i.e. for each capillary j connected to node i, we calculate the capillary pressure given by the Laplace pressure

P^j_{c,i} = 2σ r^j_i , [ 5 ]

where r j i is the radius of the capillary and σ the surface tension (σ = 72 mN/m for water). Flow through the capillary is driven by the pressure difference ΔP j i = Pi − P^j_{c,i}, where Pi is the pressure at node i.

According to Hagen-Poiseuille’s law, the volume flux Q j i from node i into capillary j is

Q^j_i = − π(r^j_i )^4 8η ΔP^j_i h^j_i , [ 6 ]

where h j i is the length of the liquid column in capillary j of node i and η the viscosity of the liquid (η = 0.88 mPa s for water). The volume flux Q j i determines the change of the liquid volume V j i and thus of the length of the liquid column

h^j_i according to Q^j_i = dV^j_i /dt = π(r^j_i )^2 dh^j_i /dt. Hence, once the node

pressures Pi are known, the time dependencies of the heights h j i (t) are given by

ordinary differential equations.

The node pressures Pi are determined by the boundary conditions and volume conservation. The boundary conditions are the Laplace pressure at the menisci, P j c,i, and zero pressure at all nodes at the bottom of the lattice which are connected to the water reservoir. The volume conservation at each node is given by ∑ j Q^j_i = 0 , [ 7 ]

which corresponds to Kirchhoff’s law. The sum runs over all capillaries j attached to node i. The resulting set of sparse linear equations is numerically solved to obtain the node pressures Pi for a given meniscus height configuration h j i . The differential equations for h j i are then numerically integrated using an implicit Euler scheme for time-stepping. Note that, due to the nanometer-sized capillaries, capillary pressure dominates gravity, which can thus be neglected.

The time step Δt in the numerical integration of the equations of motion of the menisci heights is chosen such that each meniscus moves at most a distance L/10 and no meniscus crosses a node. If this would occur for one meniscus, Δt is reduced such that this meniscus reaches the next node and then ‘jumps’ over the node, generating new menisci in a distance δ = L/100 from the node (Fig. 4a), and all other menisci are also processed with the reduced Δt. Similarly, if the meniscus retracts due to a negative pressure difference, ΔP j i < 0, the meniscus is arrested when it

has approached the node up to a distance δ. Thus a liquid column with a length of at least δ is kept in the capillary, i.e. h j i ≥ δ always holds. The meniscus is released

when ΔP j i > 0 (Fig. 4b). When two menisci meet, they merge and the capillary

thus is completely filled (Fig. 4c), which mimics the absence of entrapped air in our experimental system.

During a computer simulation of the time evolution of the model, the average rise level H(t) = ⟨hi(t)⟩i of the invading front and its width w(t) =

(⟨h^2_i (t)⟩i − ⟨hi(t)⟩^2_i )^{1/2} are calculated at different times t. Since the invasion

front contains overhangs and voids, the average ⟨. . .⟩i is taken over all menisci indexed by i. The presented data are averaged over 100 simulation runs using different disorder realizations. The statistical error of this average is represented by the error bars of the simulation results.

Appendix: Imbibition front broadening in an inhomogeneous porous medium of independent pores For comparison with the proposed model, we here consider spontaneous imbibition in an ensemble of independent, i.e. non-connected or isolated, pores. The radius of a single pore varies randomly with height h such that an appropriate model for the meniscus motion in such a pore is dh/dt = κ(h)/h, where κ(t) is uncorrelated white noise with mean c and variance σ, i.e. ⟨κ(h)⟩ = c, ⟨⟨κ(h)κ(h^′)⟩⟩ = σ δ(h − h^′). For the time T to reach some height H one thus gets T (H) = ∫_H 0 dh h ξ(h) where ξ(h) is white noise with mean 1/c and variance σ^′. Averaging the stochastic variable T yields ⟨T ⟩ ∝ H^2 (which is the Lucas-Washburn law) and for the variance ΔT^2 = ⟨(T − ⟨T ⟩)^2⟩ ∝ H^3, which means ΔT ∝ T^{3/4}. The time to reach height H therefore varies typically between H^2 +ΔT and H^2 −ΔT , vice versa at time T one then expects the height H(T ) to vary between (T − ΔT )^{1/2} and (T + ΔT )^{1/2} which means ΔH ≈ ΔT /T^{1/2} = T^{1/4}.

S.G. an Z.S. contributed equally to this work. S.G. and H.H. carried out the neutron radiography experiments, Z.S. performed the computer simulations for the pore network model. S.G., H.H., S.E. and P.H. designed, discussed and analyzed the experiments, Z.S. and H.R. designed and analyzed the theoretical model. All authors contributed to the writing of the manuscript.

ACKNOWLEDGMENTS. We acknowledge FRM II for providing beam time. We are grateful to our local contacts Michael Schulz, Elbio Calzada and Burkhard Schillinger. We thank Mikko Alava for helpful discussions. Part of this work was supported by the DFG priority program 1164, Nano- & Microfluidics (Grant. No. Hu 850/2) and the DFG graduate school 1276, ‘Structure formation and transport in complex systems’ (Saarbruecken).

10248 http://www.pnas.org/content/109/26/10245 Footline Author

1. Sahimi M (1993) Flow phenomena in rocks — from continuum models to fractals, percolation, cellular-automata, and simulated annealing. Rev Mod Phys 65: 1393.

2. Halpinhealy T and Zhang Y-C (1995) Kinetic roughening phenomena, stochastic growth directed polymers and all that. Phys Rep 254: 215.

3. Hinrichsen H (2000) Non-equilibrium critical phenomena and phase transitions into absorbing states. Adv Phys 49: 815.

4. Alava M, Dube M, and Rost M (2004) Imbibition in disordered media. Adv Phys 53: 83. 5. Lucas R (1918) Ueber das Zeitgesetz des kapillaren Aufstiegs von Fluessigkeiten.

Kolloid Zeitschrift23: 15.

6. Washburn E-W (1921) The dynamics of capillary flow. Phys Rev 17: 273. 7. Dimitrov D-I, Milchev A, and Binder K (2007) Capillary rise in nanopores: Molecular dynamics evidence for the Lucas-Washburn equation Phys Rev Lett 99: 054501.

8. Gruener S, Hofmann T, Wallacher D, Kityk A-V, and Huber P (2009). Capillary rise of water in hydrophilic nanopores. Phys Rev E 79: 067301.

9. Gruener S and Huber P (2009) Spontaneous imbibition dynamics of an n-alkane in nanopores: Evidence of meniscus freezing and monolayer sticking. Phys Rev Lett 103: 174501.

10. Courbin L, Denieul E, Dressaire E, Roper M. Ajdari A, Stone H-A (2007) Imbibition by polygonal spreading on microdecorated surfaces. Nature Materials 6: 661.

11. Reyssat M, Courbin L, Reyssat E, Stone H-A (2008) Imbibition in geometries with axial variations. J Fluid Mech 615: 335.

12. Planet R, Pradas M, Hernndes-Machado, and J. Ortin (2007) Pressure-dependent scaling scenarios in experiments of spontaneous imbibition. Phys Rev E 76: 056312.

13. Dube M, Daneault C, Vuorinen V, Alava M, and Rost M (2007) Front roughening in three-dimensional imbibition. Eur Phys J B 56: 15.

14. Buldyrev SV, Barabasi A-L, Caserta F, Havlin S, Stanley H-E, and Vicsek T (1992) Anomalous interface roughening in porous media — experiment and model. Phys Rev A 45: R8313.

15. Horvath V-K and Stanley H-E (1995) Temporal scaling of interfaces propagating in porous media. Phys Rev E 52: 5166.

16. Miranda A-M, Menezes-Sobrinho I-L, and Couto M-S (2010) Spontaneous imbibition in newspaper sheets. Phys Rev Lett 104: 086101.

17. Hernandez-Machado A et al. (2001) Interface roughening in Hele-Shaw flows with quenched disorder: Experimental and theoretical results. Europhys Lett 55: 194.

18. Geromichalos D, Mugele F, and Herminghaus S (2002) Nonlocal dynamics of spontaneous imbibition fronts. Phys Rev Lett 89: 104503.

19. Dube M, Rost M, and Alava M (2000) Conserved dynamics and interface roughening in spontaneous imbibition: A critical overview. Eur Phys J B 15: 691.

20. Song Y-Q, Ryu S, and Sen P-N (2000). Determining multiple length scales in rocks.

Nature 406: 178.

21. Gelb L-D and Gubbins K-E (1998) Characterization of porous glasses: Simulation models, adsorption isotherms, and the Brunauer-Emmett-Teller analysis method. Langmuir 14: 2097.

22. Caupin F, Cole M-W, Balibar S, and Treiner J (2008) Absolute limit for the capillary rise of a fluid. Europhys Lett 82: 56004.

23. Callaghan PT et al. (1991) Diffraction-like effects in NMR diffusion studies of fluids in porous solids. Nature 351: 467.

24. Howle L, Behringer R-P, Georgiadis J (1993) Visualization of convective fluid-flow in a porous-medium. Nature 362: 230.

25. Winkler B. Application of neutron radiography and neutron tomography (2006) Rev Mineralogy Geochem 63.

26. Kaestner A, Lehmann E, Stampanoni M. Imaging and image processing in porous media research (2008) Adv. Water Resources 31: 1174.

27. Strobl M, Manke I, Kardjilov N, Hilger A, Dawson M, Banhart J (2009) Advances in neutron radiography and tomography. J Phys D: Appl Phys 42: 243001.

28. Cnudde V, Dierick M, Vlassenbroeck J, Masschaele B, Lehmann E, Jacobs P, Van Hoorebeke L (2008) High-speed neutron radiography for monitoring the water absorption by capillarity in porous materials. Nucl. Instrum. Meth. Phys. Res. B 266: 155.

29. Hall SA, Hughes D, Rowe S (2010) Local charcaterization of fluid flow in sandstone with localized deformation deatures through fast neutron imaging. EPJ Web of Conferences 6: 22008.

30. Lenormand R (1990) Liquids in porous media. J Phys: Cond Matt 2: SA79. 31. Martys N, Cieplak M, Robbins MO (1991) Critical phenomena in fluid invasion of porous media. Physical Review Letters 66: 1058.

32. Gruener S. Rheology and Dynamics of Simple and Complex Liquids in Mesoporous Matrices. Ph.D. thesis, Saarland University, Saarbruecken, Germany (2010).

33. Levitz P, Ehret G, Sinha S-K, and Drake J-M (1991) Porous Vycor glass: The microstructure as probed by electron microscopy, direct energy transfer, small-angle scattering, and molecular adsorption. J Chem Phys 95: 6151.

34. Page J-H, Liu J, Abeles B, Deckman H-W, and Weitz D-A (1993) Pore-space correlations in capillary condensation in Vycor. Phys Rev Lett 71: 1216.

35. Lehmann E-H, Frei G, Kuehne G, Boillat P (2007) The micro-setup for neutron imaging: A major step forward to improve the spatial resolution. Nucl Instrum Meth Phys Res A 576: 389.

36. Aker E, Maloy K-J, Hansen A, and Batrouni G-G (1998) A two-dimensional network simulator for two-phase flow in porous media. Transp Porous Med 32: 163.

37. Lam C-H and Horvath V-K (2000). Pipe network model for scaling of dynamic interfaces in porous media. Phys Rev Lett 85: 1238.

38. Barabasi A-L and Stanley H-E. Fractal Concepts in Surface Growth (Cambridge University Press, New York, 1995).

39. Krug J. Origins of scale invariance in growth processes (1997) Adv Phys 46: 139. 40. Shikhmurzaev Y-D and Sprittles J-E. Wetting front dynamics in an isotropic porous medium (2012) J Fluid Mech 694: 399.

41. Leoni F, Kierlik E, Rosinberg M-L, and Tarjus G (2011) Spontaneous imbibition in disordered porous solids: A theoretical study of helium in silica aerogels. Langmuir 27: 8160.

42. Calzada E, Gruenauer F, Muehlbauer M, Schillinger B, Schulz M (2009). New design for the ANTARES-II facility for neutron imaging at FRM-II. Nucl. Instrum. Meth. Phys. Res. A 605:50).

43. Hassanein R, Lehmann E, Vontobel P. Methods of scattering corrections for quantitative neutron radiography (2005) Nucl Instrum Meth Phys Res A 542: 353.

Footline Author PNAS June 26 109 26 10249

Fig. 1. Schematic representation of spontaneous imbibition of a fluid into a porous matrix.

The arrows indicate the mean median rise level H(t) and the invasion front width w(t).

Fig. 2. Direct observation of spontaneous imbibition of water into nanoporous Vycor glass

using visible light (top row) and neutrons (lower row). The reflected light intensity and the local liquid concentration, i.e. the filling degree f(x, z, t), are shown in grayscale and pseudocolors, respectively. Snapshots are recorded for 0.1 s (light) and 30 s (neutrons) about every 15 min. The lateral direction x and the height z, i.e. the direction of capillary rise, are indicated. The width and height of the sample are 4.6 mm and 20 mm, respectively.

10250 http://www.pnas.org/content/109/26/10245 Footline Author

Fig. 3. Progression and broadening of the imbibition front of water in nanoporous Vy-

cor glass as quantified by neutron imaging. (a) Laterally-averaged filling degree f̄(z, t) ≡ ⟨f(x, z, t)⟩_x as a function of height z and time t. (b) Local median rise level h = z(f=0.5, x, t) as a function of lateral position x and time t. (c) Evolution of the front width w(t) along with a fit of w ∝ tβ (solid line). The first few data points show an apparently increased width due to smearing effects and are thus disregarded in the fit. (See text for details.) The inset shows the same data in a log-log representation. Axes units of the inset agree with the ones of the main plot. (d) Height-height correlation function C(ℓ, t) of the invasion front at three different times (as indicated). The data are shifted for clarity. In (a) and (b) the Lucas-Washburn law z∝ √ t is shown as solid lines. Parts (a) and (b) show only about the first half of the collected data, during which most of the front movement occurs.

Footline Author PNAS June 26 109 26 10251

Fig. 4. Computer simulation of spontaneous imbibition in a network of elongated capillaries.

Rules for the propagation of menisci are designed to mimic the experimental situation. (a) After reaching an empty node, the liquid immediately fills the connected capillaries for a distance δ. (b) After retracting up to δ toward a filled node, the meniscus is arrested until the pressure difference driving the liquid is again positive. (c) When two menisci meet, they merge. (d) Snapshots of configurations in a system with aspect ratio a = 5, radius polydispersity δ_r/r_{av} = 0.3 and lattice size 16 × 64 at different times (as indicated in units of ns).

10252 http://www.pnas.org/content/109/26/10245 Footline Author

Fig. 5. Progression and broadening of the imbibition front as observed in computer simu-

lations based on our pore-network model. Pore aspect ratio a = 5 and standard lattice size N_x × N_z = 16 × 1000. Lengths are measured in units of L, times in units of ns. All data are averaged over 100 simulations with different disorder realizations, the error bars reflect the standard deviation. (a) Mean median rise level H(t) = ⟨hi(t)⟩i for different polydispersities δ_r/r_{av} (as indicated). The lines represent fits of H ∝ √ t. The inset shows the same data in a log-log representation and H ∝ √ t as the dash-dotted line. (b) Evolution of the front width w(t) for different polydispersities (as indicated). The lines represent fits of w(t) ∝ tβ with growth exponents β = 0.42 ± 0.01, 0.42 ± 0.01 and 0.45 ± 0.01 for polydispersities of 0.1, 0.2 and 0.4, respectively. The inset shows the same data in a log-log representation and √ t as the dash-dotted line. (c) Evolution of the front width w(t) for a polydispersity δ_r/r_{av} = 0.1 and different lateral system sizes N_x (as indicated). The line represents a fit of w ∝ tβ with β = 0.42 ± 0.01 for Nx > 4. The inset shows the same data in a log-log representation, the dashed line represents an upper bound of the width, which is given by the difference between the front heights H(t) ∝ √ t in two homogeneous systems with constant minimal and maximal capillary radius r = rav −δr (slowest front propagation) and r = r_{av} +δ_r (fastest front propagation), respectively. (d) Height-height correlation C(ℓ, t) as a function of the distance ℓ at different times t (as indicated) for a sample with polydispersity δ_r/r_{av} = 0.1 and N_x × N_z = 128 × 32.

Footline Author PNAS June 26 109 26 10253