arXiv:1504.00956v1 [cond-mat.mtrl-sci] 3 Apr 2015

Hydrogenation of Nd-Fe-B magnet powder under a high pressure of hydrogen

Y. Kataoka^1 , Y. Kawamoto^1 , T. Ono^2 , M. Tsubota^2 , J. Kitagawa^1

1 Department of Electrical Engineering, Faculty of Engineering, Fukuoka Institute of Technology, 3-30-1 Wajiro-higashi, Higashi-ku, Fukuoka 811-0295, Japan 2 Physonit Inc., 6-10 Minami-Horikawa, Kaita Aki, Hiroshima 736-0044, Japan

Abstract The hydrogenation of Nd_2Fe_{14}B under a high pressure of hydrogen has been investigated for the first time. At the heat-treatment temperature of 600^∘C, the almost complete decomposition of Nd_2Fe_{14}B into NdH_{2+x} and α-Fe is observed, although a rather long heat-treatment time is necessary to achieve the sufficient hydrogenation. The desorption of hydrogen from NdH_{2+x} does not occur in the furnace-cooling process.

Keywords: hydrogenation, Nd-Fe-B magnet, HDDR process

Email address: j-kitagawa@fit.ac.jp (J. Kitagawa^1)

Preprint submitted to Results in Physics May 5, 2019

1. Introduction

Toward the improved magnetic-properties of the Nd-Fe-B permanent magnet, one of important technologies is the hydrogenation of Nd_2Fe_{14}B, which is employed in the so-called HDDR (hydrogenation, disproportionation, desorption, recombination) process[1]. The HDDR-processed magnet possesses a submicron grain-size, contributing a higher coercivity. H_2 atmosphere with rather low pressure (∼ 1 atm) is introduced in the hydrogenation process. After the heat-treatment at 750 ∼ 900^∘C for 30 min ∼ 3 h, the magnet disproportionates into Nd hydride (NdH_{2+x}), α-Fe and Fe_2B.

Several groups have reported the reactive milling of Nd-Fe-B powder under hydrogen at room temperature[2, 3, 4]. The mechanical activation of Nd-Fe-B powder leads to the decomposion into NdH_{2+x} and α-Fe, although we need high pressure of H_2 gas (∼ 1 MPa). These studies motivated us to investigate the conventional hydrogenation of Nd-Fe-B under a high pressure of H_2 gas, which has not been reported. In this study, we have studied the hydrogenation of Nd-Fe-B under a high pressure of hydrogen.

2. Experimental method

We used a commercial Nd-Fe-B magnet. The ground magnet powder, after demagnetization, weighting approximately 0.45 g were placed in a homemade cell with the volume of about 7.5 cc. After evacuating the cell, we introduced H_2 gas of 0.45 MPa. The cell was heated to the temperature ranging from 500^∘C to 600^∘C, taking 2 h, by an electric furnace, and kept at that temperature for 6 to 84 h, followed by a furnace-cooling. The heattreated samples were evaluated using the powder X-ray diffraction (XRD) pattern (Cu-Kα radiation). We also hydrogenated Nd-Fe-B powder in a continuous H_2 gas flow at 600^∘C for 12 h, in which the heating and cooling rates are the same as those in the above-mentioned hydrogenation process.

3. Results and discussion

Figure 1: XRD patterns of samples after heat-treatment at 500 or 550^∘C . The XRD pattern of Nd-Fe-B ingot is also shown.

The XRD patterns of samples heat-treated at 500^∘C for 12 and 24 h are shown in Fig. 1, where the pattern of Nd-Fe-B ingot is also exhibited. The pattern of Nd-Fe-B ingot is mainly composed of Nd_2Fe_{14}B in addition to the minor phase of NdFe_4B_4. The peaks of Nd_2Fe_{14}B in the samples heattreated at 500^∘C are shifted to lower 2θ values compared to those of the starting ingot. This implies the lattice expansion of Nd_2Fe_{14}B due to the insertion of hydrogen[5]. The decomposition of Nd_2Fe_{14}B does not occur because of no appearance of α-Fe, which is confirmed by further extending the heat-treatment time to 84 h. The NdH_{2+x} phase denoted by triangles would be generated from a Nd-rich phase[6].

Figure 2: XRD patterns of samples after heat-treatment at 575^∘C .

Fig. 1 also shows the XRD patterns of samples heat-treated at 550^∘C for 12 and 36 h. The shift of peaks of Nd_2Fe_{14}B does not occur in each sample, indicating no insertion of hydrogen in Nd_2Fe_{14}B. Although Nd_2Fe_{14}B is not completely decomposed, the simultaneous appearance of NdH_{2+x} and α-Fe means the partial hydrogenation of Nd_2Fe_{14}B.

As shown in Fig. 2, the hydrogenation of Nd_2Fe_{14}B proceeds by increasing the heat-treatment temperature to 575^∘C. The peaks of NdH_{2+x} and α-Fe phases dominate over those of unreacted Nd_2Fe_{14}B and NdFe_4B_4, which is observed throughout the heat-treatment time of interest.

Figure 3: XRD patterns of samples after heat-treatment at 600^∘C .

At the heat-treatment temperature of 600^∘C for longer than 12 h, the almost complete decomposition of Nd_2Fe_{14}B is observed (see Fig. 3). We cannot say whether the Fe_2B phase, which is detected after the disproportionation in the HDDR process, exists or not. To investigate the effect of high-pressure H_2 gas, we have carried out the hydrogenation of Nd-Fe-B in a continuous H_2 gas flow. The XRD pattern of the sample is shown at the top of Fig. 3. We have found that, even at the heat-treatment temperature lower than that in typical HDDR process, the complete decomposition of Nd_2Fe_{14}B into NdH_{2+x} and α-Fe can be achieved for the prolonged heattreatment time. However the peak intensity of NdH_{2+x} is very weak compared to that in samples hydrogenated under high H_2-pressure. In addition, Nd_2O_3 phase is detected (see arrows in Fig. 3). During the furnace-cooling, some hydrogen might desorb from NdH_{2+x} transforming into Nd_2O_3. On the other hand, the samples hydrogenated under high H_2-pressure do not show the desorption of hydrogen after the furnace-cooling.

4. Summary

We have investigated the hydrogenation of Nd-Fe-B powder under the high pressure of hydrogen. The hydrogenation of Nd_2Fe_{14}B proceeds almost completely at the heat-treatment temperature of 600^∘C, although the prolonged heat-treatment time is necessary for the sufficient decomposition of Nd_2Fe_{14}B.

References

[1] R. Nakayama, T. Takeshita, M. Itakura, N. Kuwano, and K. Oki: J.

Appl. Phys. 70 (1991) 3770.

[2] G. Khélifati, J. M. Le Breton, L. Aymard, and J. Teillet: J. Magn.

Magn. Mater 218 (2000) 42.

[3] S. Gang, Hu. Lianxi, and W. Erde: J. Magn. Magn. Mater 301 (2006) 319.

[4] H. Lianxi, L. Yuping, Y. Yuan, and S. Gang: J. Mater. Res. 23 (2008) 427.

[5] O. Isnard, W. B. Yelon, S. Miraglia, and D. Fruchart: J. Appl. Phys.

78 (1995) 1892.

[6] C. E. Rogríguez Torres, F. D. Saccone, and F. H. Sánchez: Materials Science and Engineering A292 (2000) 104.