arXiv:1507.00415v2 [cond-mat.mtrl-sci] 16 Feb 2016

Stabilization of highly polar BiFeO_3-like structure: a new interface design route for enhanced ferroelectricity in artificial perovskite superlattices

Hongwei Wang^1, Jianguo Wen^{2,∗}, Dean J. Miller^2, Qibin Zhou^4, Mohan Chen^5, Ho Nyung Lee^3, Karin M. Rabe^4, and Xifan Wu^{1,∗} 1Department of Physics, Temple University, Philadelphia, PA 19122, USA 2Center for Nanoscale Materials, Argonne National Laboratory, Argonne, IL 60439, USA 3 Materials Science and Technology Division, Oak Ridge National Laboratory, Oak Ridge, Tennessee 37831, USA 4Department of Physics and Astronomy, Rutgers University, Piscataway, NJ 08854-8019, USA and 5 Department of Mechanical and Aerospace Engineering, Princeton University, Princeton, New Jersey 08544, USA (Dated: May 5, 2019)

In ABO3 perovskites, oxygen octahedron rotations are common structural distortions that can promote large ferroelectricity in BiFeO3 with an R3c structure [1], but suppress ferroelectricity in CaTiO3 with a P bnm symmetry [2]. For many CaTiO3 -like perovskites, the BiFeO3 structure is a metastable phase. Here, we report the stabilization of the highly-polar BiFeO3-like phase of CaTiO3 in a BaTiO3 /CaTiO3 superlattice grown on a SrTiO3 substrate. The stabilization is realized by a reconstruction of oxygen octahedron rotations at the interface from the pattern of nonpolar bulk CaTiO3 to a different pattern that is characteristic of a BiFeO3 phase. The reconstruction is interpreted through a combination of amplitude-contrast sub 0.1nm high-resolution transmission electron microscopy and first-principles theories of the structure, energetics, and polarization of the superlattice and its constituents. We further predict a number of new artificial ferroelectric materials demonstrating that nonpolar perovskites can be turned into ferroelectrics via this interface mechanism. Therefore, a large number of perovskites with the CaTiO3 structure type, which include many magnetic representatives, are now good candidates as novel highly-polar multiferroic materials [3].

INTRODUCTION

New mechanisms to generate ferroelectricity (FE) have recently been the subject of active research, due to both fundamental interest and the technological importance of ferroelectrics and related materials [4]. Novel ferroelectrics have potentially higher performance for practical applications, as well as potential compatibility with other functional properties such as magnetism, yielding multiferroics and other multifunctional materials [3, 5, 6].

Artificially structured perovskite superlattices offer rich opportunities for novel ferroelectricity [7–11]. Nonbulk phases for the constituent layers can be stabilized by the mechanical and electrical boundary conditions characteristic of a superlattice [12, 13], potentially turning constituents that are nonpolar in bulk form into ferroelectrics [14, 15]. Competing low-energy metastable phases can be readily found in perovskites with low tolerance factors, promoting oxygen octahedron rotation (OOR) instabilities along the Brillouin-zone-boundary R- M line. The ground state structure in such cases is generally the nonpolar orthorhombic P bnm structure. As a typical example, the oxygen octahedron in a CaTiO_3 (CTO) can be described by its rotation around [110] axis and an in-phase rotation around [001] axis (a^−a^−c^+ in Glazer notation). Such a pattern of OOR favors antipolar behavior instead of FE [2]. On the other hand, OOR with a different pattern can also promote large FE. As one famous example, in BiFeO_3 (BFO) with R3c structure, the oxygen octahedron can be characterized by a rotation around [110] and an out-of-phase rotation around [001], yielding a fairly large polarization along [111] (a^−a^−a^− in Glazer notation). Compared to the widespread of CTOlike materials, BFO-like perovskites are relatively rarely seen. As a result, the OOR is generally thought to suppress FE in perovskites.

However, for many perovskites, the BFO-like structure serves as a low-energy metastable phase [2]. Therefore, it would be beneficial if an artificial perovskite superlattice could stabilize this metastable phase for the entire constituent layers or in a region near interface. To this end, a reliable design mechanism can be derived only from precisely determined atomic positions in experiments followed by theoretical interpretations based on first-principles calculations.

EXPERIMENTAL AND FIRST-PRINCIPLES RESULTS

Aberration-corrected high-resolution transmission electron microscopy (HRTEM) is a powerful method for accurate visualization of oxygen octahedron distortions [16, 17]. Recently, it was shown that amplitude contrast imaging in HRTEM could be used to discriminate heavy and light element columns based on channeling contrast [18], allowing one to locate the exact interface and to visualize OOR angles in different atomic layers (see Supplementary Materials S1). Fig. 1(a) shows an experimental HRTEM image of a 4BaTiO_3(BTO)/4CTO superlattice film along the [110] direction of the SrTiO_3 (STO) substrate. This

FIG. 1: Experimental and simulated HRTEM images showing oxygen octahedral tilts in the 4BTO/4CTO superlatice film grown on a STO substrate along [110]. (a). Experimental HRTEM image using an amplitude contrast imaging method (Cs = 3μm, Cc = 1μm, Δf = −1nm). BaO columns (dark dots) and CaO columns (bright dots) show different channeling contrast. Oxygen atomic columns displace differently, either upward or downward, with respect to the central Ti atoms in box 1, 2 and 3. 0.14nm indicates the spacing between Ti and O columns. Accumulated electron dose is 3 × 10^4 electrons/nm^2 . (b). Simulated HRTEM image using the atomic positions obtained from first-principles calculations. The simulated image matches well with the experimental image except a sharper column contrast in the simulated image compared to the experiment one because electron beam induced object excitations are omitted as pointed out by Kisielowski et al. (see Supplementary Materials S4) [19].

image was obtained by correcting both spherical and chromatic aberrations to achieve amplitude contrast imaging conditions (Cs = 3 μm, Cc = 1μm). In this image, channeling contrast between Ca and Ba columns is clearly observed: atomic columns of CaO and BaO appear as bright and dark dots, respectively; oxygen and Ti columns appear as bright dots. Due to the interdiffusion of Ba and Ca at the interface, the intensity at A site varies depending on the ratio of Ca and Ba as discussed in detail in the supplementary material (S2). It is seen that BTO and CTO grow coherently on the STO substrate, showing the same in-plane lattice constant as that of STO, and elongated c-axis in the BTO layer and shortened c-axis in the CTO layer (see Supplementary Materials S3). Within the CTO layer of the superlattice (box 1), a strongly corrugated TiO_2 plane is observed in which the oxygen atoms displace upward and downward with respect to the central Ti atoms, corresponding to an OOR around [110] by 9^∘, comparable to that of bulk CTO. For TiO_2 planes between two BaO planes (box 3), alternating displacement of the oxygen atoms, and thus the amplitude of the OOR, is negligible, consistent with the fact that bulk BTO strongly resists OORs. For TiO_2 planes between one BaO and one CaO plane (box 2), the OOR around [110] is 3^∘, smaller than that in the interior of the CTO layers.

For comparison, in Fig. 1(b) we present the simulated HRTEM image using the atomic positions of the 4BTO/4CTO superlattice obtained from first-principles calculations. The simulated HRTEM image for the computed structure shows the same pattern of OOR as in the experiment (compare boxes 1, 2, and 3 in Fig. 1(a) and (b)), with amplitudes of 12.5^∘ in the CTO layer and 5.5^∘ at the interface. The quantitative difference in OOR around [110] angles from the experimental observation can be partly attributed to the fact that the experiments were performed at T= 300 K, while the ground state structural relaxation by density functional theory was at T = 0 K. In addition, in this image it is possible to discern the small uniform displacement of the oxygens relative to the Ti atoms in the TiO_2 plane, which is associated with the spontaneous polarization of the superlattice. While this displacement is present in all the TiO_2 layers, it can be more easily identified in those belonging to the interior BTO layers, which do not have the corrugation associated with OOR.

We use the atomic-scale information from the firstprinciples results for a detailed layer-by-layer investigation of the properties of the superlattice. We focus our discussion on the 6BTO/6CTO superlattice, which allows a clearer distinction between the interface and interior layers; the corresponding results for the 4BTO/4CTO superlattice are similar (see Supplementary Materials S6). The computed spontaneous polarization is 29 μCcm^{−2} along [001] and 11 μCcm^{−2} along [110]. The resulting layer-by-layer decomposed structural distortions and polarizations are shown in Fig. 2.

TABLE I: Computed bulk properties of R^i_z(∘), R^o_z (∘), Rxy(∘), ADIS (Å), P001( μC/cm^2 ), P110 ( μC/cm^2), total polarization PT( μC/cm^2 ), c/a ratio, and the total energies (eV ) for strained BTO and CTO on STO substrate modeled in 20- atom supercells. Both fixed electric (E) field and displacement (D) field boundary conditions are considered, which are used to described the electric boundary conditions of a perovskite in its nature bulk or within an insulating superlattice.

Boundary Fixed E field Fixed D field Condition E = 0 V /m D = 29 μC/cm^2 Perovskite BaTiO3 CaTiO3 CaTiO3 CaTiO3 CaTiO3 Symmetry P4mm Pbnm e-R3c Pbnm e-R3c R^i_z 0 7.7 0 7.6 0 R^o_z 0 0 7.3 0 7.2 Rxy 0 12.7 11.5 12.8 11.7 ADIS 0 0.29 0 0.32 0 P001 41.93 0 20.01 27.81 28.96 P110 0 26.40 52.19 24.53 51.25 PT 41.93 26.40 55.89 37.08 58.87 c/a 1.067 0.964 0.968 0.965 0.967 Energy -162.645 -164.158 -164.066 -164.106 -164.040

According to the dielectric slab model [14], the structure of the constituent layers of the superlattice should

FIG. 2: Computed local properties associated with ferroelectric and non-polar modes in 6BTO/6CTO superlattice and schematic plots for the atomic displacements of the oxygen octahedron rotation and ferroelectric modes. First-principles calculations of 6BTO/6CTO superlattice showing layer-by-layer decompositions in-phase oxygen octahedron rotation around [001] R^i_z, out-of-phase oxygen octahedron rotation around [001] R^o_z , in-plane polarization P110 , outof-plane polarization P001, antipolar modes (AFE) represented by A-site cation displacements (ADIS), and oxygen octahedron rotation around [110] Rxy. The corresponding strained bulk values are also denoted by the open symbol in the plot, and in particular, the open strained bulk values in P001 are predicted by the dielectric slab model [14]. A highly polar BiFeO3-like interface phase in CTO is highlighted in blue.

be closely related to those of strained bulk materials under the electrical boundary condition of a fixed displacement (D) field, imposed by the superlattice as summarized in Table I. Indeed, as shown in Fig. 2, the interior BTO layers have negligible OOR with a polarization of 32 μC/cm^2 along the [001] direction. This is consistent with the structure and large polarization of strained BTO; the reduction from the strained bulk value of 42 μC/cm^2 can be attributed to the electrostatic cost of polarizing the nonpolar CTO layer. Both bulk CTO and strained bulk CTO are characterized by the strong OORs due to structural instabilities at the zone-boundary M and R points. Therefore, the interior CTO layers are dominated by R_{xy} and R^i_z, which are OOR around [110] and an in-phase OOR around [001] respectively as shown in Fig. 2. In addition, a large antipolar (AFE) mode develops in the CTO layers that can be clearly identified by the zig-zag movement of A-site displacement along [110] direction. It should be stressed that this antipolar distortion is a structural distortion at the X point favored by the trilinear coupling due to the pattern of OOR in CTO-like materials. The above distortion in the interior CTO layers can be clearly seen in Fig. 2, as well as in the TEM image in Fig. 1 (a) (see Supplementary Materials S5). This AFE mode was also recently pointed out to be the key to the suppressed FE in all CTO-like perovskites [2]. Due to the applied tensile epitaxial strain, the interior CTO layers are polar along [110] direction with a magnitude of 26.4 μc/cm^2 just like the strained CTO [20].

If the interface effect is negligible, the dielectric slab model can be used to predict the polarization, yielding a value of 22.4 μC/cm^2 along the [001] direction. The firstprinciples calculation gives P_{001} = 29.0 μC/cm^2. The discrepancy from the dielectric slab model suggests that the interface effect cannot be neglected. Such a large enhancement of the polarization (∼ 25%) is a strong indication of a highly polar interface reconstruction. Indeed, examination of Fig. 2 reveals that the structure at the interface of the CTO layers differs significantly from that of the strained bulk CTO, with the OOR being suppressed at the interface of the superlattice. The AFE type displacement, which is driven by the trilinear coupling [2] involving the OORs of CTO, is suppressed too. Furthermore, a new structural pattern of OOR emerges at the interface: an OOR around the [110] axis and an out-of-phase OOR around the [001] axis for a TiO_6 sandwiched between two interface CaO layers, with rotation angles comparable to those of the strained bulk in-phase OOR. This new structure pattern is exactly the same as one would observe for oxygen octahedron rotation in BiFeO_3 and similar perovskites with R3c symmetry.

MICROSCOPIC MECHANISM

Here, we propose that this change in structure at the interface can be interpreted as the local stabilization of a BFO-like structure different from that of the bulk CTO. As far as the topology of the oxygen octahedron rotation network is concerned, oxygen octahedra in both BFO and CTO rotate around [110]; however, BFO differentiates itself from CTO by its out-of-phase OOR around [001] instead of the in-phase counterpart in CTO. The outof-phase and in-phase OOR around [001] originate from symmetry-nonequivalent structural instabilities at the R and M points respectively. This stabilization of a BFOlike structure in CTO layers near the interface is derived from the metastable polar e-R3c phase and is compatible with a much larger polarization than that in bulk CTO as shown in Table I. It has been shown that this phase cannot be stabilized relative to the P bnm phase by epitaxial strain alone [21]. However, in the superlattice, the suppression of the tilt angles by proximity to BTO, assisted by the electrical and mechanical boundary conditions that favor a phase with a component of polarization along [001], is sufficient to stabilize the structure [22].

To explore the stabilization of this phase more quantitatively, we constructed first-principles based models for the strained P bnm phase (designated E_{“CTO}′′ (R^i_z, R_{xy}, AFE_{xy}, FE_{xy})) and for the metastable e-R3c phase (E_{“BFO}′′ (R^o_z , R_{xy}, FE_{xy}, FE_z)). Facilitated by space group symmetry analysis, the models of both E_{“CTO}′′ and E_{“BFO}′′ are built through polynomial expansions of the total energy from first-principles calculations with respect to the high-symmetry reference structure (P 4/mmm phase) in terms of the amplitudes of the relevant modes. In the above, R^i_z, R^o_z , R_{xy}, AFE_{xy}, FE_{xy}, FE_z represent the mode amplitude of in-phase OOR around [001], out-of-phase OOR around [001], OOR around [110], in-plane antipolar mode and in-plane and out-of-plane FE modes respectively. The resulting models are shown in the following for E_{“CTO}′′ and E_{“BFO}′′ respectively as (see Supplementary Materials S7 for fitted coefficients):

E_{“CTO}′′ = a_1R^i_z^2 + b_1R^i_z^4 + a_2R^2_{xy} + b_2R^4_{xy} + a_3AFE^2_{xy} +b_3AFE^4_{xy} + a_4FE^2_{xy} + b_4FE^4_{xy} + c_1R^i_z^2R^2_{xy} +c_2R^i_z^2AFE^2_{xy} + c_3R^i_z^2FE^2_{xy} + c_4R^2_{xy}AFE^2_{xy} +c_5R^2_{xy}FE^2_{xy} + c_6AFE^2_{xy}FE^2_{xy} + d_1R^i_zR_{xy}AFE_{xy}, (1)

FIG. 3: Appearances of both BiFeO3-like and CaTiO3- like phases and the transition from one to the other as functions of oxygen octahedral rotations in strained bulk CaTiO3. Phase stabilities studied by the relative energetics between BFO-like and CTO-like phase as plotted by ΔE as functions of magnitudes of oxygen octahedral rotation around [001] and [110] respectively. The FE mode amplitudes are represented by projected colors in the base as well.

E_{“BFO}′′ = α_1R^o_z^2 + β_1R^o_z^4 + α_2R^2_{xy} + β_2R^4_{xy} + α_3FE^2_z + β_3FE^4_z + α_4FE^2_{xy} + β_4FE^4_{xy} + γ_1R^o_z^2R^2_{xy} +γ_2R^o_z^2FE^2_z + γ_3R^o_z^2FE^2_{xy} + γ_4R^2_{xy}FE^2_z+ γ_5R^2_{xy}FE^2_{xy} + γ_6FE^2_z FE^2_{xy} + κ_1R^o_z R_{xy}FE_zFE_{xy}. (2) Assuming the angles of the oxygen octahedron rotations are tunable parameters under experimental conditions, we further define the functions F_{“CTO}′′ (R^i_z, R_{xy}) = min AFE_{xy},FE_{xy}

E_{“CTO}′′ (R^i_z, R_{xy}, AFE_{xy}, FE_{xy}),

and F_{“BFO}′′ (R^o_z , R_{xy}) = min FE_{xy},FE_z

E_{“BFO}′′ (R^o_z , R_{xy}, FE_{xy}, FE_z). In order to

understand how the BFO-like phase can be stabilized relative to the CTO-like phase, we then evaluate ΔE = F_{“BFO}′′ − F_{“CTO}′′ as functions of oxygen octahedron rotation magnitudes around [110] and [001]. The resulting ΔE is presented in Fig. 3. The total FE mode amplitudes are also presented by the color spectrum in the base plane in Fig. 3. It can be seen that when the angles are fixed to the values of bulk CTO regions in the superlattice, as shown in Fig. 2 (R^i_z = 8.3^∘ and R_{xy} = 12.6^∘), the CTO-like phase is strongly favored in energy. In the CTO-like phase, as shown in Fig. 2 and Table I, the antipolar distortion is favored over the FE distortion due to the large trilinear coupling term ∼ R^i_zR_{xy}AFE_{xy} in Eq. 1. Notably, when the amplitudes of OORs are reduced, the BFO-like phase becomes energetically more stable than the CTO-like phase as shown in Fig. 3. This indicates that the BFO-like phase can be stabilized over the CTO-like phase when the OOR is reduced. When the above transition takes place, the OOR around [001] will change abruptly from in-phase rotation to out-of-phase rotation signifying a more drastic change in the topology of the oxygen octahedron network, as guided by the yellow plane at ΔE = 0 in Fig. 3. In addition to the pattern change of OOR, the BFO-like phase is generally found to have much larger polarization than that in the CTO-like phase as shown by the color spectrum in Fig. 3. The much stronger FE polarization is expected, originating from the e-R3c phase; it can also be easily understood by the large four-linear coupling term ∼ R^o_z R_{xy}FE_zFE_{xy}, which promotes FE in both the in-plane and out-of-plane directions.

This mechanism leads to the BFO-like phase that exists at the interface of the BTO/CTO superlattice. Assuming the octahedra to be fairly rigid, the reduction of OOT is imposed by the adjoining BTO layer, which is strongly resistant to the OOR. A direct consequence of the stabilization of the BFO-like structure at the interface is that the polarization of the superlattice is greatly enhanced. For a particular choice of angles with R^o_z = 5.7^∘ and R_{xy} = 6.6^∘ similar to those at the interface of the BTO/CTO superlattice, the computed polarization of the BFO-like phase is over 54.0 μC/cm^2, which is comparable to the polarization in the bulk e- R3c CTO as shown in Table I. In the superlattice, the BFO-like phase is further favored by both the electric and mechanical boundary conditions imposed by the polarization of the BTO layer according to Eq. 2. Under the continuous displacement field along [001] direction, the electric boundary condition tends to polarize the CTO components with a larger FE_z. Under the tensile strain, the mechanical boundary condition effectively enhances FE_{xy}. The larger FE_z and FE_{xy} tend to further lower the energy through ∼ R^o_z R_{xy}FE_zFE_{xy} and stabilize the BFO-like phase.

INVERSE DESIGN OF NEW FERROELECTRIC MATERIALS

It has long been recognized that oxygen octahedron rotation can play different roles in perovskites promoting FE in BFO-like materials [1, 23] but suppressing FE in CTO-like materials [24]. However, the results presented here suggest that a transition between these two phases can be achieved through interface engineering in a superlattice. In addition to improving the fundamental understanding of these transitions, these results suggest a new pathway to induce FE in functional oxide materials.

The enhanced polarization observed in the BTO/CTO superlattice studied here demonstrates this mechanism. To explore the potential of this approach, we predict a few more superlattices A’BO_3/A”BO_3 as listed in Ta-

TABLE II: Predicted superlattices with enhanced polarizations. P^{sbulk}_A′_{BO3} (μc/cm^2) and P^{sbulk}_A′′_{BO3} (μc/cm^2) denote the computed polarizations for strained A’BO3 and A”BO3 respectively. PM(μc/cm^2) and P_{Cal.}(μc/cm^2) are the expected polarizations from the dielectric slab model [14] and the computed polarizations from first-principles in nA’BO3/nA”BO3 respectively. Polarization enhancement (Enh.) is calculated by (P_{Cal.}- PM)/PM. Sub. denotes the proposed substrate for the epitaxial growth of superlattice.

nA’BO_3/nA”BO_3 P^{sbulk}_{A′BO3} P^{sbulk}_{A′′BO3} P_M P_{Cal.} Enh. Sub.

2BaTiO_3 /2CaTiO_3 41.9 25.7 25.5 39.9 56% SrTiO_3 2BaTiO_3 /2CdTiO_3 50.8 37.8 34.2 50.4 47% NdGaO_3 2KNbO_3/2NaNbO_3 36.2 ∼ 0 19.8 37.5 89% DyScO_3 2KNbO_3/2AgNbO_3 36.2 ∼ 0 22.0 38.2 73% DyScO_3

ble II. Within this category of tailored materials, one of the parent bulk A’BO_3 is chosen to be a “CTO-like” perovskite with strong oxygen octahedron rotations, resulting in an antipolar type (CaTO_3 and CdTO_3) [25] or an antiferroelectric type (AgNbO_3 and NaNbO_3) [26, 27] ground state that is favored by the trilinear coupling term. The other parent bulk A”BO_3 is chosen to have a large tolerance factor resisting oxygen octahedron rotation and a strong FE polarization. Similar to what we have already shown for the BTO/CTO example, the out-of-phase OORs around [001] are induced around the interface layers of A’BO_3 (see Supplementary Materials S8 for examples of 2BaTiO_3/2CaTiO_3 and 2KNbO_3/2AgNbO_3). As a result, the overall polarizations of the superlattices are enhanced compared to the predictions from the dielectric slab model, which is equivalent to applying the charge continuity principle only and neglecting completely the possible interface reconstruction.

This approach to create new FE materials by interfacial control can also be used to create new materials even where the building blocks could come only from nonpolar perovskites. In Table III, we list a few predicted 1A’BO_3/1A”BO_3 superlattices within this category. These interface materials also provide us a good opportunity to perform rigorous mode decompositions based on space group theory followed by a careful comparison between the interface materials and the parent bulk compounds. The resulting mode decompositions and the local properties are also shown in Table III. The A’BO_3 is again a “CTO-like” perovskite with strong oxygen octahedron rotations. The above property is clearly represented by the large mode amplitudes of Q_{Rxy} and Q_Ri_z which correspond to an OOR around [110] and inphase OOR around [001] as shown in Table III. Under such a pattern of OORs, the antipolar mode Q_{AFExy} is favored, and FE is strongly suppressed resulting in zero polarization along all directions. On the other hand, A”BO_3 is a strong “cubic” perovskite [28–30] that does

TABLE III: Predicted new artificial ferroelectric materials based on non polar perovskites. (1)Mode decompositions (Å) of QRo_z as out-of-phase OOR around [001] , Q_Ri_z as in-phase OOR around [001], QR_{xy} as OOR around [110], QFE_z as polar distortion along [001], QFE_{xy} as polar distortion along [110], and QAFE_{xy} as in-plane antipolar distortion. Their symmetries are labeled as M^−_1 , M^+_3 , M^−_5 , Γ^−_3 , Γ^−_5 respectively; (2) OOR angles (degrees) R^o_z, R^i_z , Rxy for out-of-phase OOR around [001], in-phase OOR around [001], and OOR around [110] (octahedron tilt) respectively; (3) The polarizations (μc/cm^2) along [001] direction P001 , along [110] direction P110), and the total polarization PT; (4) The polarization enhancement (Enh.); (5) Substrate for the epitaxial growth of the superlattices, KTaO3(a=3.99Å), MgO(a=4.21Å). (6) Space group symmetry (Sym.) of both strained bulk and superlattice.

A’(A”)BO3 Mode Decompositions(Å) OOR Angles(∘) Polarization(μc/cm^2 ) Enh. Substrate Sym. nA’BO3/nA”BO3 QRo_z Q_Ri_z QR_{xy} QFE_z QFE_{xy} QAFE_{xy} R^o_z R^i_z Rxy P001 P110 PT CdSnO3 0 1.22 1.85 0 0 0.79 0 12.0 17.7 0 0 0 - KTaO3 Pnma BaSnO3 0 0 0 0 0 0 0 0 0 0 0 0 - KTaO3 P4/mmm 1CdSnO3/1BaSnO3 1.08 0 1.21 0.20 0.60 0 9.4 0 12.2 8.9 13.5 16.2 ∞ KTaO3 Pc CdHfO3 0 1.27 1.74 0 0 0.69 0 12.3 16.9 0 0 0 - KTaO3 Pbnm BaHfO3 0 0 0 0 0 0 0 0 0 0 0 0 - KTaO3 P4/mmm 1CdHfO3/1BaHfO3 1.07 0 1.17 0.18 0.64 0 9.3 0 12.2 7.8 10.8 13.3 ∞ KTaO3 Pc CaZrO3 0 1.02 1.82 0 0 0.72 0 9.2 16.2 0 0 0 - MgO Pcmn BaZrO3 0 0 0 0 0 0 0 0 0 0 0 0 - MgO P4/mmm 1CaZrO3/1BaZrO3 0.79 0 1.22 0.27 0.71 0 6.6 0 10.8 11.1 27.6 29.7 ∞ MgO Pc 1CaZrO3/1BaZrO3 0.90 0 1.16 0.30 0.67 0 8.1 0 10.6 13.5 22.5 26.2 ∞ Relaxed Pc

not display structural distortions associated with either OORs or polarization at its ground state as shown in Table III.

Strikingly, when A’BO_3 and A”BO_3 form a 1A’BO_3/1A”BO_3 superlattice, the resulting structural distortions are significantly different from their parent bulks. The differences come not only from the amplitudes of the modes but also from the symmetries associated with these modes. In Table III, the OORs around [110] Q_{Rxy} are preserved in all these superlattices but, with largely reduced mode amplitudes compared with those in bulk A’BO_3. In contrast, the in-phase OOR around [001] Q_Ri_z completely disappears and is replaced by a large mode amplitude Q_Ro_z associated with an out-of-phase OOR around the same axis in all the predicted new materials. As we have seen repeatedly in the previous discussions, such a new pattern of OOR signifies the stabilization of a “BFO-like” structure in all these artificial materials. Accordingly, large polarizations develop along both [001] and [110] directions with the generated total polarization vector roughly along the [111] direction due to the broken symmetry in the e-R3c phase. It can be noted that the polarization of BiFeO_3 is exactly along [111] direction in the R3c symmetry. At the same time, the antipolar mode Q_{AFExy} is completely eliminated. Here, we want to stress that none of the component perovskites in the predicted superlattices is polar either in its natural bulk or in its strained bulk formats!

OUTLOOK

Currently, there are two widely adopted interface approaches to induce FE in oxide superlattices, namely tricolor [10] and hybrid improper methods [31]. An artificially induced broken inversion symmetry lies at the heart of both the above two methods. In the former, the broken inversion symmetry along the out-of-plane direction is introduced by the number of species in the superlattice; while in the latter, the broken inversion symmetry along the in-plane direction is facilitated by the differences in the antipolar modes of the two perovskite materials across the interface. However, it should be noted that the interface approach discussed here is a new route that is conceptually different from the above. Instead of introducing artificial inversion symmetry breaking, the ferroelectric polarization is stabilized by favoring a “BFO-like” structure which is a metastable phase for many perovskite materials. Due to the nature of the energy term that stabilizes the “BFO-like” structure (∼ R^o_z R_{xy}FE_zFE_{xy}) , it is expected the switching of FE does not necessarily require switching the directions of oxygen octahedron rotations, which usually requires much larger energy as is implied in the hybrid improper mechanism. Indeed, the FE polarization switching has already been successfully demonstrated in 2BTO/2CTO by Lee’s group [32]. Based on nudged elastic band (transition state) theory [33, 34] and single domain assumption, the energy barrier in switching FE in 2BTO/2CTO (154 meV ) is found to be close to that of the predicted materials 1CdSnO_3/1BaSnO_3 (119 meV ) both of which are modeled in 40-atom supercells.

In conclusion, by combining HRTEM experimental and first-principles approaches, we introduced a comprehensive interface design method to stabilize a highly polar “BFO-like” metastable phase in perovskite materials. Both the electric and mechanical boundary conditions are taken into account as well. This scheme introduces a conceptually novel way to design artificial FE materials. By predicting some new materials, we demonstrate this approach of exploring novel functional materials. For example, if the FE could be recovered in orthogonal RFeO_3(R= Y,Gd, Tb Dy,Ho,Er,Tm,Yb, Lu) [35–37] by this approach, the synthesis of a new family of room temperature multiferroic materials could be achieved. Furthermore, the result of our current work indicates that, through an interface design mechanism, short-period superlattices can have stronger FE than longer ones. This is promising for modern device applications based on ultrathin films.

ACKNOWLEDGMENTS

X. W. was supported as part of the Center for the Computational Design of Functional Layered Materials, an Energy Frontier Research Center funded by the U.S. Department of Energy, Office of Science, Basic Energy Sciences under Award no. de-sc0012575. The work of K. M. R. was supported by NSF DMR-1334428. This research used resources of the National Energy Research Scientific Computing Center (NERSC), a DOE Office of Science User Facility supported by the Office of Science of the U.S. Department of Energy under Contract No. DE- AC02-05CH11231. The transmission electron microscopy was accomplished at the Electron Microscopy Center in the Center for Nanoscale Materials at Argonne National Laboratory, a DOE-BES Facility supported under Contract DE-AC02-06CH11357 by UChicago Argonne, LLC. The work at ORNL was supported by the U.S. Department of Energy, Office of Science, Basic Energy Sciences, Materials Sciences and Engineering Division. We thank Dr. Hua Zhou for useful discussions. X. W. is grateful for the useful discussions with Dr. Andrew J. Shanahan at University Medical Center of Princeton.

[1] J. B. Neaton, C. Ederer, U. V. Waghmare, N. A. Spaldin and K. M. Rabe, First-principles study of spontaneous polarization in multiferroic BiFeO3, Phys. Rev. B 71, 014113 (2005).

[2] N. A. Benedek and C. Fennie, Why are there so few perovskite ferroelectrics, J. Phys. Chem. C 117, 13339- 13349 (2013).

[3] N. A. Spaldin, S. W. Cheong and R. Ramesh, Multiferroics: Past, present, and future, Phys. Today 63, 38 (2010).

[4] M. Dawber, K. M. Rabe and J. F. Scott, Physics of thinfilm ferroelectric oxides, Rev. Mod. Phys. 77, 1083-1130 (2005).

[5] J. H. Lee, et al. A strong ferroelectric ferromagnet created by means of spin-lattice coupling, Nature 466, 954 (2010).

[6] N. A. Benedek and C. Fennie, Hybrid improper ferroelectricity: A mechanism for controllable polarizationmagnetization coupling, Phys. Rev. Lett. 106, 107204 (2011).

[7] C. H. Ahn, K. M. Rabe and J. M. Triscone, Ferroelectricity at the nanoscale: Local polarization in oxide thin films and heterostructures, Science 303, 488-491 (2004).

[8] H. N. Lee, H. M. Christen, M. F. Chisholm, C. M.

Rouleau and D. H. Lowndes, Strong polarization enhancement in asymmetric three-component ferroelectric superlattices, Nature 433, 395-399 (2005).

[9] M. P. Warusawithana, E. V. Colla, J. N. Eckstein and M. B. Weissman, Artificial dielectric superlattices with broken inversion symmetry, Phys. Rev. Lett. 90, 036802 (2003).

[10] N. Sai, B. Meyer and D. Vanderbilt, Compositional inversion symmetry breaking in ferroelectric perovskites, Phys. Rev. Lett. 84, 5636-5639 (2000).

[11] E. Bousquet, M. Dawber, N. Stucki, C. Lichtensteiger, P.

Hermet, S. Gariglio, J. Triscone and P. Ghosez, Improper ferroelectricity in perovskite oxide artificial superlattices, Nature 452, 732-737 (2008).

[12] D. G. Schlom, L. Q. Chen, C. B. Eom, et al. Strain tuning of ferroelectric thin films, Annu. Rev. Mater. Res. 37, 589-626 (2007).

[13] M. Stengel, N. A. Spaldin and D. Vanderbilt, Electric displacement as the fundamental variable in electronicstructure calculations, Nature Phys. 5, 304-308 (2009).

[14] J. B. Neaton and K. M. Rabe, Theory of polarization enhancement in epitaxial BaTiO3 /SrTiO3 superlattices, Appl. Phys. Lett. 82, 1586-1588 (2003).

[15] H. W. Jang, et al. Ferroelectricity in strain-free SrTiO3 thin films, Phys. Rev. Lett. 104, 197601 (2010).

[16] C. L. Jia, M. Lentzen and K. Urban, Atomic-resolution imaging of oxygen in perovskite ceramics, Science 299 870-873 (2003).

[17] C. L. Jia, S. B. Mi, K. Urban, I. Vrejoiu, M. Alexe and D.

Hesse, Atomic-scale study of electric dipoles near charged and uncharged domain walls in ferroelectric films, Nat. Mater. 7, 57-61 (2008).

[18] A. Wang, F. R. Chen, S. Van Aert, and D. Van Dyck, Direct structure inversion from exit waves: Part I: Theory and simulations, Ultramicroscopy 110, 527 (2010).

[19] Kisielowski et al., Real-time sub-Angstrom imaging of reversible and irreversible conformations in rhodium catalysts and graphene, Phys Rev. B 88, 024305, 2013.

[20] C. J. Eklund, C. J. Fennie and K. M. Rabe, Straininduced ferroelectricity in orthorhombic CaTiO3 from first principles, Phys. Rev. B 79, 220101 (2009).

[21] C. J. Eklund, Interplay of strain, polarization and magnetic ordering in complex oxides from first principles, Ph.D. thesis (Rutgers University, 2010).

[22] Q. Zhou, First-principles modeling of functional perovskite materials and superlattices, Ph.D. thesis (Rutgers University, 2014).

[23] R. J. Zeches, M. D Rossell, J. X Zhang, A. J. Hatt, et al. A Strain-Driven Morphotropic Phase Boundary in BiFeO3, Science 326, 13 (2009).

[24] N. A. Benedek, A. T. Mulder and C. J. Fennie, Polar octahedralrotations: Apathtonewmultifunctionalmaterials, Journal of Solid State Chemistry 195, 11C20 (2012).

[25] H. Moriwake, A. Kuwabara, C. A. J. Fisher, H.

Taniguchi, et al. First-principles calculations of lattice dynamics in CdTiO3 and CaTiO3: Phase stability and ferroelectricity, Phys. Rev. B 84, 104114 (2011).

[26] D. Fu, M. Endo, H. Taniguchi, T. Taniyama and M. Itoh, AgNbO3 : A lead-free material with large polarization and electromechanical response, Appl. Phys. Lett. 90, 252907 (2007).

[27] A. Kania and J. Kwapulinski, Ag1−xNaxNbO3 (ANN) solid solutions: from disordered antiferroelectric AgNbO3 to normal antiferroelectric NaNbO3, J. Phys.: Condens. Matter 11, 8933-8946 (1999).

[28] I. Ahmed, S. G. Eriksson, E. Ahlberg, C.S. Knee, M.

Karlsson, et al. Proton conductivity and low temperature structure of In-doped BaZrO3, Solid State Ionics 177, 2357C2362 (2006).

[29] A. Bouhemadou, F. Djabib and R. Khenata, First principles study of structural, elastic, electronic and optical properties of the cubic perovskite BaHfO3, Physics Letters A 372, 4527C4531 (2008).

[30] T. Maekawa, K. Kurosaki and S. Yamanaka, Thermal and mechanical properties of polycrystalline BaSnO3, Journal of Alloys and Compounds 416, 214C217 (2006).

[31] J. M. Rondinelli and C. J. Fennie, Octahedral Rotation-

Induced Ferroelectricity in Cation Ordered Perovskites, Adv. Mater. 24, 1961C1968 (2012).

[32] S. S. A. Seo, J. H. Lee, H. N. Lee, et al. Ferroelectricity in Artificial Bicolor Oxide Superlattices, Adv. Mater. 19, 2460C2464 (2007).

[33] D. Sheppard, R. Terrell and G. Henkelmana, Optimization methods for finding minimum energy paths, J. Chem. Phys. 128, 134106 (2008).

[34] G. Henkelmana and H. Jonssonb, Improved tangent estimate in the nudged elastic band method for finding minimum energy paths and saddle points, J. Chem. Phys. 113, 22 (2000).

[35] H. Shen, J. Xua, A. Wu, J. Zhao and M. Shi, Magnetic and thermal properties of perovskite YFeO3 single crystals, Materials Science and Engineering B 157, 77C80 (2009).

[36] X. Fu, X. Xi, K. Bi and J. Zhou, Temperature-dependent terahertz magnetic dipole radiation from antiferromagnetic GdFeO3 ceramics, Appl. Phys. Lett. 103, 211108 (2013).

[37] W. Zhu, L. Pi, S. Tan and Y. Zhang, Anisotropy and extremely high coercivity in weak ferromagnetic LuFeO3, Appl. Phys. Lett. 100, 052407 (2012).