arXiv:1507.06081v1 [cond-mat.mes-hall] 22 Jul 2015

Spin-current emission governed by nonlinear spin dynamics

Takaharu Tashiro,^1 Saki Matsuura,^1 Akiyo Nomura,^1 Shun Watanabe,^2 Keehoon Kang,^2 Henning Sirringhaus,^2 and Kazuya Ando^{∗1, 3} 1Department of Applied Physics and Physico-Informatics, Keio University, Yokohama 223-8522, Japan 2Cavendish Laboratory, University of Cambridge, J. J. Thomson Avenue, Cambridge CB3 0HE, United Kingdom 3PRESTO, Japan Science and Technology Agency, Kawaguchi, Saitama 332-0012, Japan

Coupling between conduction electrons and localized magnetization is responsible for a variety of phenomena in spintronic devices. This coupling enables to generate spin currents from dynamical magnetization. Due to the nonlinearity of magnetization dynamics, the spin-current emission through the dynamical spin-exchange coupling offers a route for nonlinear generation of spin currents. Here, we demonstrate spin-current emission governed by nonlinear magnetization dynamics in a metal/magnetic insulator bilayer. The spin-current emission from the magnetic insulator is probed by the inverse spin Hall effect, which demonstrates nontrivial temperature and excitation power dependences of the voltage generation. The experimental results reveal that nonlinear magnetization dynamics and enhanced spin-current emission due to magnon scatterings are triggered by decreasing temperature. This result illustrates the crucial role of the nonlinear magnon interactions in the spin-current emission driven by dynamical magnetization, or nonequilibrium magnons, from magnetic insulators.

Dynamical magnetization in a ferromagnet emits a spin current,^{1,2} enabling to explore the physics of spin transport in metals and semiconductors.^{3–22} The dynamical spin-current emission has been achieved utilizing ferromagnetic metals, semiconductors, and insulators.^{23–26} In particular, the discovery of the spin-current emission from a magnetic insulator yttrium iron garnet, Y_3Fe_5O_{12}, has drawn intense experimental and theoretical interests, opening new possibilities to spintronics based on metal/insulator hybrids, where angular momentum can be carried by both electrons and magnons.

A ferrimagnetic insulator yttrium iron garnet, Y_3Fe_5O_{12}, is characterized by the exceptionally small magnetic damping, making it a key material for the development of the physics of nonlinear magnetization dynamics.^{27–29} The nonlinear magnetization dynamics in Y_3Fe_5O_{12} has been extensively studied both experimentally and theoretically in the past half a century, benefited by the exceptional purity, high Curie temperature, and simplicity of the low-energy magnon spectrum.^{28–31} Recently, the nonlinear magnetization dynamics has been found to affect the spin-current emission from the magnetic insulator; the spin-current emission is enhanced by magnon scattering processes [see Fig. 1(a)], triggered by changing the excitation frequency or power of the magnetization dynamics.^{14,15,32} These findings shed new light on the long-standing research on nonlinear magnetization dynamics, promising further development of spintronics and magnetics based on the magnetic insulator.

In this work, we demonstrate that the spin-current emission from Y_3Fe_5O_{12} is strongly affected by nonlinear magnetization dynamics at low temperatures. The spin-

∗Correspondence and requests for materials should be addressed to ando@appi.keio.ac.jp

current emission is probed by the inverse spin Hall effect (ISHE) in a Pt film attached to the Y_3Fe_5O_{12} film,^{11,33,34} which enables to measure temperature dependence of the spin-current emission from the magnetic insulator under various conditions. In spite of the simple structure of the metal/insulator bilayer, we found nontrivial variation of the spin-current emission; the temperature dependence of the spin-current emission strongly depends on the microwave frequency and excitation power. This result reveals that nonlinear spin-current emission due to three and four magnon scatterings emerges by decreasing temperature, even at constant magnon excitation frequency and power. This finding provides a crucial piece of information for understanding the spin-current emission from ferromagnetic materials and investigating the magnon interactions in the metal/insulator hybrid.

A single-crystal Y_3Fe_5O_{12} (111) film (3 × 5 mm^2) with a thickness of 5 μm was grown on a Gd_3Ga_5O_{12} (111) substrate by liquid phase epitaxy (purchased from Innovent e.V., Jena). After the substrates were cleaned by sonication in deionized water, acetone and isopropanol, a piranha etching process, a mixture of H_2SO_4 and H_2O_2 (with the ratio of 7 : 3), was applied, then to be able to remove any residuals an oxygen plasma cleaning was performed outside a sputtering chamber. On the top of the film, a 10-nm-thick Pt layer was sputtered in an Ar atmosphere. Prior to sputtering 10-nm-thick Pt layer, an argon plasma cleaning was also performed in-situ. The Pt/Y_3Fe_5O_{12} bilayer film was placed on a coplanar waveguide, where a microwave was applied to the input of the signal line as show in Fig. 1(b). Two electrodes were attached to the edges of the Pt layer. The signal line is 500 μm wide and the gaps between the signal line and the ground lines are designed to match to the characteristic impedance of 50 Ω. An in-plane external magnetic field H was applied parallel to the signal line, or perpendicular to the direction across the elec-

FIG. 1: Detection of spin-current emission. (a) The magnon dispersion in Y3Fe5O12, where f and k are the frequency and wavenumber of magnons, respectively. The dispersion of the first 40 thickness modes propagating along and opposite to the magnetic field is shown. The blue and red arrows represent the four and three magnon scatterings. The magnon dispersion shows that both the three and four magnon scatterings create secondary magnons with small group velocity. The lowest frequency is f = fmin. (b) The experimental setup. The Pt/Y3Fe5O12 film placed on the coplanar waveguide was cooled using a Gifford-McMahon cooler. (c) Magnetic field (H) dependence of the microwave absorption P for the Pt/Y3Fe5O12 film at f0 = 7.6 GHz and Pin = 10 mW. μ0HR = 183 mT is the resonance field. P_{abs} is the definition of the magnitude of the microwave absorption intensity. The absorption peak structure comprises multiple signals due to spin-wave modes. (d) H dependence of the electric voltage V . VISHE is the magnitude of the electric voltage. The blue and red data were measured with the in-plane magnetic field H and −H, respectively. (e) H dependence of dV (H)/dH for the Pt/Y3Fe5O12 film. The damping constant of the Pt/Y3Fe5O12 film was roughly estimated to be 5 × 10^{−4} from f0 dependence of the linewidth at 5 mW.

trodes.^{11} Figure 1(c) shows the in-plane magnetic field H dependence of the microwave absorption P measured by applying a 10 mW microwave with the frequency of f_0 = 7.6 GHz at T = 300 K. Under the ferromagnetic resonance condition H = H_R, dynamical magnetization in the Y_3Fe_5O_{12} layer emit a spin current j_s into the Pt layer, resulting in the voltage generation through the ISHE as shown in Fig. 1(d).^{1,2} The sign of the voltage is changed by reversing H, consistent with the prediction of the spin-current emission from the magnetic insulator.^{35} Here, the absorption spectrum comprises multiple resonance signals due to spin-wave modes, including magnetostatic surface waves and backward-volume magnetostatic waves in addition to the ferromagnetic resonance. To extract the damping constant for the Pt/Y_3Fe_5O_{12} film, we have plotted dV/dH in Fig. 1(e), which allows rough estimation of the damping constant, α ∼ 5 × 10^{−4}.

Figure 2(a) shows temperature dependence of V_{ISHE}/P_{abs}, where V_{ISHE} and P_{abs} are the magnitude of the microwave absorption and electric voltage, respectively; V_{ISHE}/P_{abs} characterizes the angular-momentum conversion efficiency from the microwaves into spin currents. Notably, V_{ISHE}/P_{abs} increases drastically below T = 150 K by decreasing T at f_0 = 4.0 GHz. This drastic change is irrelevant to the temperature dependence of the spin pumping and spin-charge conversion efficiency in the Pt/Y_3Fe_5O_{12} bilayer, such as the spin Hall angle θ_{SHE}, the spin pumping conductance g_{eff}, the spin diffusion length λ, and the electrical conductivity σ. Figure 2(b) shows the temperature dependence of the electrical conductivity σ and the spin Hall conductivity σ_s. The spin Hall conductivity was obtained from the temperature dependence of V_{ISHE}/P_{abs} at 10 mW for f_0 = 7.6 GHz shown in Fig. 2(a); the value of V_{ISHE}/P_{abs} is insensitive to the excitation power from 5 to 15 mW, indicating that the spin-current emission is reproduced with a liner spin-pumping model:^{36}

V_{ISHE} P_{abs} = 2ew_Fσ_sf_0λg_{eff} tanh(d/2λ)

μ_0σ^2dv_FM_sΔH √ (γμ_0M_s)^2 + (4πf_0)^2

, (1)

where w_F = 3.0 mm and v_F = 7.5 × 10^{−11} m^3 are the width and volume of the Y_3Fe_5O_{12} film. d = 10 nm is the thickness of the Pt layer. μ_0ΔH is the half-maximum full-width of the ferromagnetic resonance linewidth. For the calculation of σ_s, we used the measured parameters of the electrical conductivity σ and saturation magnetization M_s. The spin-diffusion length^{37} λ = 7.7 nm and spin pumping conductance^{38} g_{eff} = 4.0 × 10^{18} m^{−2} were assumed to be independent of temperature, as demonstrated previously.^{39} The spin Hall conductivity of the Pt layer shown in Fig. 2(b) increases with decreasing temperature above 100 K. Below 100 K, the spin Hall conductivity decreases with decreasing temperature. This feature is qualitatively consistent with the previous report.^{39} Although the spin Hall conductivity varies with temperature, the variation of the spin Hall conductivity alone is not sufficient to explain the drastic increase of V_{ISHE}/P_{abs} for f_0 = 4 GHz shown in Fig. 2(a). Thus, the drastic change in V_{ISHE}/P_{abs} across 150 K at f_0 = 4.0 GHz can be attributed to the change in the magnetization dynamics in the Y_3Fe_5O_{12} layer. In fact, by decreasing T , the microwave absorption intensity P_{abs} decreased clearly across T = 150 K as shown in Fig. 2(c), suggesting the change of the magnetization dynamics in the Y_3Fe_5O_{12} layer across T = 150 K.

The origin of the temperature-induced drastic change of the spin-conversion efficiency V_{ISHE}/P_{abs} shown in Fig. 2(a) is enhanced spin-current emission triggered by the three magnon splitting. The three-magnon splitting

FIG. 2: Temperature evolution of spin-current emission. (a) Temperature (T ) dependence of VISHE/P_{abs} for the Pt/Y3Fe5O12 film at f0 = 7.6 (the black circles) and 4.0 GHz (the red circles). The data were measured with Pin = 10 mW microwave excitation. (b) T dependence of the electrical conductivity σ and the spin Hall conductivity σs for the Pt/Y3Fe5O12 film. (c) T dependence of P_{abs}/Pin, where P_{abs} is the microwave absorption intensity, for Pin = 10 mW and f0 = 4.0 GHz.

creates a pair of magnons with the opposite wavevectors and the frequency f_0/2 from the uniform magnon with f_0 [see also Fig. 1(a)]. The splitting process redistributes the magnons and changes the relaxation rate of the spin system, increasing the steady-state angular momentum stored in the spin system, or resulting in the stabilized enhancement of the spin-current emission.^{14,32} The splitting is allowed only when f_0/2 > f_{min}, where f_{min} is the minimum frequency of the magnon dispersion, because of the energy and momentum conservation laws. This condition can readily be found by finding f_{min} for the thin Y_3Fe_5O_{12} film from the lowest branch of the dipole-exchange magnon dispersion for the unpinned surface spin condition:^{40} f = √ Ω (Ω + ω_M − ω_M Q), (2)

where Ω = ω_H + ω_M (D/μ_0M_s)k^2, ω_H = γμ_0H, ω_M = γμ_0M_s, and Q = 1 − [1 − exp (−kL)] /(kL). D = 5.2 × 10^{−13} Tcm^2 is the exchange interaction constant, L = 5 μm is the thickness of the Y_3Fe_5O_{12} layer, and k is the wavenumber of the magnons. γ = 1.84×10^{11} Ts^{−1} is the gyromagnetic ratio. In Figs. 3(a) and 3(b), we show the lowest branch of the magnon dispersion at different temperatures for the Pt/Y_3Fe_5O_{12} film, calculated using Eq. (2). For the calculation, we used the saturation magnetization M_s at each temperature [see Fig. 3(c)], estimated from the resonance field data with Kittel’s formula. We assumed that D is independent of tempera-

FIG. 3: Magnon dispersion. (a) The lowest-energy branch of the magnon spectra for the Pt/Y3Fe5O12 film calculated for the resonance condition at f0 = 4.0 GHz. The dispersions were calculated using γ = 1.84 × 10^{11} Ts^{−1}. The dotted red line denotes f = f0/2 = 2.0 GHz. (b) The magnified view of the lowest-energy branch of the magnon spectra. (c) Temperature dependence of the saturation magnetization Ms estimated from the resonance field data.

ture, as demonstrated in literature.^{32,41,42} Although D can slightly depend on temperature,^{43} the shape of the magnon dispersion is not sensitive to the small variation of D. Figures 3(a) and 3(b) demonstrate that the minimum frequency f_{min} decreases with decreasing temperature and the splitting condition f_0/2 > f_{min} is satisfied below T = 150 K; the magnon redistribution is responsible for the enhancement of V_{ISHE}/P_{abs}. Thus, this result demonstrates that the enhanced spin-current emission can be induced not only by changing the excitation frequency or power of the magnetization dynamics, but also by changing temperature.

Figures 4(a) and 4(b) show temperature dependence of the spin-conversion efficiency V_{ISHE}/P_{abs} at different microwave excitation powers P_{in} for f_0 = 7.6 and 4.0 GHz, respectively. At f_0 = 4.0 GHz, the enhancement of V_{ISHE}/P_{abs} due to the three-magnon splitting below 150 K is observed for all the excitation powers as shown in Fig. 4(b). The drop in V_{ISHE}/P_{abs} at T = 50 K for f_0 = 4.0 GHz is induced by the decrease of the spin Hall conductivity shown in Fig. 2(b); below 100K, the spin Hall conductivity, or the spin Hall angle, decreases with decreasing temperature, whereas the spin-current enhancement through the magnon splitting increases by decreasing temperature. The competition gives rise to the peak structure in V_{ISHE}/P_{abs} around 70 K for 4.0

FIG. 4: Temperature evolution of spin-current emission for different microwave powers. (a) Temperature T dependence of VISHE/P_{abs} at f0 = 7.6 GHz for the in-plane magnetic field H (the upper panel) and reversed in-plane magnetic field −H (the lower panel). (b) T dependence of VISHE/P_{abs} at f0 = 4.0 GHz for the in-plane magnetic field H (the upper panel) and −H (the lower panel). (c) T dependence of [VISHE/P_{abs}]100 mW/[VISHE/P_{abs}]5 mW at f0 = 7.6 GHz. [VISHE/P_{abs}]100 mW and [VISHE/P_{abs}]5 mW are VISHE/P_{abs} measured at Pin = 100 mW and 5 mW, respectively.

GHz. This result also shows that the enhancement factor is almost independent of the excitation power. In contrast, notably, the variation of V_{ISHE}/P_{abs} depends on the excitation power, especially below 150 K, at f_0 = 7.6 GHz as shown in Fig. 4(a). These features for f_0 = 7.6 and 4.0 GHz were confirmed in V_{ISHE}/P_{abs} measured with the reversed external magnetic field [see the experimental data for −H in Figs. 4(a) and 4(b)], indicating that the change of the spin-current emission from the magnetic insulator is responsible for the nontrivial behavior of V_{ISHE}/P_{abs} at low temperatures.

To understand the temperature and power dependences of V_{ISHE}/P_{abs} at f_0 = 7.6 GHz in details, we plot [V_{ISHE}/P_{abs}]_{100 mW}/[V_{ISHE}/P_{abs}]_{5 mW} in Fig. 4(c). For the spin-current emission in the linear magnetization dynamics regime, V_{ISHE}/P_{abs} is constant with P_{in}, or [V_{ISHE}/P_{abs}]_{100 mW}/[V_{ISHE}/P_{abs}]_{5 mW} = 1 because the emitted spin current is proportional to P_{in}.^{35} Since the three-magnon splitting is prohibited at f_0 = 7.6 GHz, [V_{ISHE}/P_{abs}]_{100 mW}/[V_{ISHE}/P_{abs}]_{5 mW} ≈ 1.2, at T = 300 K, demonstrates enhanced spin-current emission without the splitting of a pumped magnon.

The observed enhancement of the spin-current emission at T = 300 K is induced by the four magnon scattering, where two magnons are created with the annihilation of two other magnons [see also Fig. 1(a)].^{44,45} The four-magnon scattering emerges at high microwave excitation powers P_{in} > P_{th}, known as the second order Suhl instability,^{46} where P_{th} is the threshold power of the scattering. Although this process conserves the number of magnons, the magnon redistribution can decrease the relaxation rate of the spin system through the annihilation of the uniform magnons with large damping η_0 and creation of dipole-exchange magnons with small damping η_q .

This results in the steady-state enhancement of the angular momentum stored in the spin system, or the enhanced spin-current emission.^{32} In the Pt/Y_3Fe_5O_{12} film, the damping η_0 of the uniform magnon at low excitation powers is mainly dominated by the two-magnon scattering; the temperature dependence of the ferromagnetic resonance linewidth is almost independent of temperature as shown in the inset to Fig. 5, indicating that the damping η_0 is not dominated by the temperature peak processes or the Kasuya-LeCraw mechanism.^{47} In contrast, the damping η_q of the secondary magnons created by the fourmagnon scattering is dominated by the Kasuya-LeCraw mechanism, since the two-magnon scattering events are suppressed due to the small group velocity; the group velocity of the secondary dipole-exchange magnons created at the same frequency as the uniform magnon can be close to zero because of the exchange-dominated standing spin-wave branches [see Fig. 1(a)].^{44,48–50} The exchangedominated branches, i.e. the thickness modes, show the energy minimum not only at the bottom of the dispersion but also at the excitation frequency. Therefore, in the present system, the damping η_0 of the uniform magnon is dominated by the temperature-independent two-magnon scattering, whereas the damping η_q of the secondary magnon is dominated by temperature-dependent threeparticle confluences, such as the Kasuya-LeCraw process.^{47} In the presence of the four magnon scattering, the total number of the nonequilibrium magnons N_t is expressed as^{32} N_t P_{abs} = 1 2πη_q ℏf_0 [ 1 − χ^{′′} 2γM_s (η_0 − η_q ) ] , (3)

where η_q is defined as the average decay rate to the thermodynamic equilibrium of the degenerate secondary

FIG. 5: Microwave power dependence of spin-current emission at different temperatures. Microwave excitation power Pin dependence of [VISHE/P_{abs}]/[VISHE/P_{abs}]5 mW at f0 = 7.6 GHz for different temperatures. The in-plane magnetic field is H for the upper panel and −H for the lower panel, respectively. The inset shows T dependence of the half-maximum full-width μ0ΔH of ferromagnetic resonance for the Pt/Y3Fe5O12 film.

magnons for simplicity. The imaginary part of the susceptibility is expressed as χ^{′′} = 2γM_s η_0 + η_{sp}f(P_{in})

, (4)

where

f(P_{in}) = 1 √ 1 − [χ^{′′}(η_0 + η_{sp})/(2γM_s)]^4(P_{in}/P_{th})^2

. (5)

Here, η_{sp} is the decay constant of the uniform precession to degenerate magnons at f_0 due to scattering on sample inhomogeneities. Under the assumption that the spinpumping efficiency is insensitive to the wavenumber k of the nonequilibrium magnons, that is V_{ISHE} ∝ j_s ∝ N_t, Eq. (3) is directly related to the spin-conversion efficiency: V_{ISHE}/P_{abs} ∝ N_t/P_{abs}.

The above model reveals that the spin-current enhancement due to the four-magnon scattering is responsible for the nontrivial behavior of the voltage generation shown in Fig. 4(a). As shown in Fig. 4(c), the nonlinearity of the spin-current emission is enhanced by decreasing temperature, from [V_{ISHE}/P_{abs}]_{100 mW}/[V_{ISHE}/P_{abs}]_{5 mW} ≈ 1.2 at T = 300 K to [V_{ISHE}/P_{abs}]_{100 mW}/[V_{ISHE}/P_{abs}]_{5 mW} ≈ 2.4 at 50 K. Figure 5 shows microwave excitation power P_{in} dependence of V_{ISHE}/P_{abs} for f_0 = 7.6 GHz at different temperatures. This result clearly shows that the threshold power

FIG. 6: Threshold power of spin-current enhancement. Microwave excitation power Pin dependence of [VISHE/P_{abs}]/[VISHE/P_{abs}]5 mW at f0 = 7.6 GHz for T = 300 K and T = 75 K.

P_{th} of the spin-current enhancement decreases with decreasing temperature, which is the origin of the nontrivial behavior of the temperature dependence of V_{ISHE}/P_{abs} shown in Figs. 4(a) and 4(c). The threshold power of the spin-current enhancement through the four-magnon process is very low at low temperatures, making it difficult to observe the threshold behavior. In fact, V_{ISHE}/P_{abs} deviates from the prediction of the linear model even at the lowest microwave excitation power that is necessary to detect the ISHE voltage in the Pt/Y_3Fe_5O_{12} film at T = 75 K [see the orange circles in Fig. 6]. At T = 300 K, a clear threshold is observed around P_{in} = 40 mW. The threshold power of the four-magnon scattering is given by^{47} P_{th} ∝ h^2_{th} = (η_0/γ)^2(2η_q /σ_q ), where h_{th} is the threshold microwave field and σ_q is the coupling strength between the uniform and secondary magnons. For simplicity, we neglect the surface dipolar interactions, or L → ∞. Under this approximation, the ferromagnetic resonance condition is given by f_0 = γμ_0H and the coupling strength can be approximated as σ_q = γμ_0M_s. Thus, the threshold power for the four-magnon scattering is proportional to

h^2_{th} = ( η_0 γ )_2 ( 2η_q γμ_0M_s ) . (6)

Equation (6) predicts that the threshold power of the spin-current enhancement decreases with decreasing temperature, since M_s increases by decreasing temperature as shown in Fig. 3(c). Although the damping η_0 of the uniform magnon is almost independent of temperature as shown in the inset to Fig. 5, the damping η_q of the dipole-exchange magnon tends to decrease the threshold power, since η_q , dominated by the Kasuya-LeCraw process is approximately proportional to temperature.^{47} At high power excitations, the competition between the increase of the spin-current enhancement due to the fourmagnon scattering and the decrease of the spin Hall effect by decreasing temperature gives rise to the peak structure in V_{ISHE}/P_{abs} around 100 K for f_0 = 7.6 GHz [see Fig. 4(a)].

In summary, we have demonstrated that the spincurrent emission from a Y_3Fe_5O_{12} film is strongly affected by nonlinear magnetization dynamics at low temperatures. The spin-current emission has been demonstrated to be enhanced even in the absence of the threemagnon splitting.^{15} The experimental results presented in this paper are consistent with this result and further extend the physics of the nonlinear spin-current emission from the magnetic insulator. Our study reveals that the spin-current enhancement arises from both the three and four magnon scatterings depending on the excitation frequency and temperature. We show that the enhanced spin-current emission can be triggered by decreasing temperature, which is evidenced by our systematic measurements for the Pt/Y_3Fe_5O_{12} film; the spin-current emission can be enhanced not only by changing the magnon excitation frequency or power, but also by changing temperature. This result demonstrates the generality of the crucial role of magnon interactions in the spin-current emission, combining the long-standing research on nonlinear spin physics with spintronics.

This work was supported by JSPS KAKENHI Grant Numbers 26220604, 26103004, 26600078, PRESTO-JST “Innovative nano-electronics through interdisciplinary collaboration among material, device and system layers,” the Mitsubishi Foundation, the Asahi Glass Foundation, the Noguchi Institute, the Casio Science Promotion Foundation, and the Murata Science Foundation.

1 Y. Tserkovnyak, A. Brataas, and G. E. W. Bauer, Phys.

Rev. Lett. 88, 117601 (2002).

2 A. Brataas, Y. Tserkovnyak, G. E. W. Bauer, and B. I.

Halperin, Phys. Rev. B 66, 060404(R) (2002). 3 Y. Sun et al., Phys. Rev. Lett. 111, 106601 (2013). 4 B. Heinrich et al., Phys. Rev. Lett. 107, 066604 (2011). 5 C. Hahn et al., Phys. Rev. B 87, 174417 (2013). 6 M. Weiler et al., Phys. Rev. Lett. 111, 176601 (2013). 7 S. M. Rezende, R. L. Rodriguez-Suarez, and A. Azevedo, Phys. Rev. B 88, 014404 (2013).

8 O. d’Allivy Kelly et al., Appl. Phys. Lett. 103, 082408 (2013).

9 C. W. Sandweg et al., Phys. Rev. Lett. 106, 216601 (2011). 10 H. Jiao and G. E. W. Bauer, Phys. Rev. Lett. 110, 217602 (2013).

11 E. Saitoh, M. Ueda, H. Miyajima, and G. Tatara, Appl.

Phys. Lett. 88, 182509 (2006).

12 E. Shikoh et al., Phys. Rev. Lett. 110, 127201 (2013). 13 K. Ando et al., Nature Mater. 10, 655 (2011). 14 H. Kurebayashi et al., Nature Mater. 10, 660 (2011). 15 V. Castel, N. Vlietstra, B. J. van Wees, and J. B. Youssef, Phys. Rev. B 86, 134419 (2012).

16 A. V. Chumak et al., Appl. Phys. Lett. 100, 082405 (2012). 17 M. B. Jungfleisch et al., Appl. Phys. Lett. 99, 182512 (2011).

18 K. Ando et al., Nature Mater. 12, 622 (2013). 19 M. B. Jungfleisch et al., Appl. Phys. Lett. 103, 022411 (2013).

20 C. Du, H. Wang, F. Yang, and P. C. Hammel, Phys. Rev.

Applied 1, 044004 (2014).

21 K. Ando and E. Saitoh, Phys. Rev. Lett. 109, 026602 (2012).

22 C. H. Du et al., Phys. Rev. Lett. 111, 247202 (2013). 23 S. Mizukami, Y. Ando, and T. Miyazaki, Phys. Rev. B 66, 104413 (2002).

24 F. D. Czeschka et al., Phys. Rev. Lett. 107, 046601 (2011). 25 L. Chen, F. Matsukura, and H. Ohno, Nature Commun.

4, 2055 (2013).

26 Y. Kajiwara et al., Nature 464, 262 (2010). 27 S. Demokritov, B. Hillebrands, and A. Slavin, Phys. Rep.

348, 441 (2001).

28 A. A. Serga, A. V. Chumak, and B. Hillebrands, J. Phys.

D 43, 264002 (2010).

29 B. Lenk, H. Ulrichs, F. Garbs, and M. Munzenberg, Phys.

Rep. 507, 107 (2011).

30 C. E. Patton, Phys. Rep. 103, 251 (1984).

31 V. S. L’vov, Wave Turbulence Under Parametric Excitation (Springer-Verlag, Berlin, 1994).

32 H. Sakimura, T. Tashiro, and K. Ando, Nature Commun.

5, 5730 (2014).

33 T. Kimura et al., Phys. Rev. Lett. 98, 156601 (2007). 34 S. O. Valenzuela and M. Tinkham, Nature 442, 176 (2006). 35 K. Ando et al., J. Appl. Phys. 109, 103913 (2011). 36 R. Iguchi et al., Jpn. J. Appl. Phys. 51, 103004 (2012). 37 H. Nakayama et al., Phys. Rev. B 85, 144408 (2012). 38 X. Jia, K. Liu, K. Xia, and G. E. W. Bauer, Europhys.

Lett. 96, 17005 (2011).

39 S. Meyer et al., Appl. Phys. Lett. 104, 242411 (2014). 40 B. Kalinikos, Microwaves, Optics and Antennas, IEE Proceedings H 127, 4 (1980).

41 R. C. LeCraw and L. R. Walker, J. Appl. Phys. 32, S167 (1961).

42 C. M. Srivastava and R. Aiyar, J. Phys. C: Solid State Phys. 20, 1119 (1987).

43 F. Heider and W. Williams, Geophys. Res. Lett. 15, 184 (1988).

44 G. de Loubens, V. V. Naletov, and O. Klein, Phys. Rev.

B 71, 180411 (2005).

45 H. Schultheiss, K. Vogt, and B. Hillebrands, Phys. Rev. B 86, 054414 (2012).

46 H. Suhl, J. Phys. Chem. Solids 1, 209 (1957). 47 M. Sparks, Ferromagnetic-Relaxation Theory (McGraw- Hill, New York, 1964).

48 G. A. Melkov, V. I. Vasyuchka, Y. V. Kobljanskyj, and A. N. Slavin, Phys. Rev. B 70, 224407 (2004).

49 M. B. Jungfleisch et al., Appl. Phys. Lett. 99, 182512 (2011).

50 A. V. Chumak, A. A. Serga, and B. Hillebrands, Nature Commun. 5, 4700 (2014).