arXiv:1604.00569v1 [math-ph] 2 Apr 2016

Implicit operators for networked mechanical and thermal systems with integer-order components

Mihir Sen,^1 John P. Hollkamp,^2 Fabio Semperlotti,^2 and Bill Goodwine^1 1)Department of Aerospace and Mechanical Engineering, University of Notre Dame, Notre Dame, IN 46556 2)Department of Mechanical Engineering, Purdue University, West Lafayette, IN 47907

(Dated: 13 October 2019)

Complex systems are composed of a large number of simple components connected to each other in the form of a network. It is shown that, for some network configurations, the equivalent dynamic behavior of the system is governed by an implicit integro-differential operator even though the individual components themselves satisfy equations that use explicit operators of integer order. The networks considered here are infinite trees and ladders, and each is composed only of two types of integer-order components with potential-driven flows that are repeated ad infinitum. In special cases the equivalent operator for the system is a fractional-order derivative, but in general it is implicit and can only be expressed as a solution of an operator equation. These implicit operators, which are a generalization of fractional-order derivatives, play an important role in the analysis and modeling of complex systems.

I. INTRODUCTION

Implicit functions and the conditions under which they exist are familiar^1. Fractional-order derivatives have also been around for some time, and have found applications in topics like viscoelasticity, mass diffusion, and fractal media, among others^{2,3}. In this work implicit integrodifferential operators are defined in a manner similar to implicit functions and used for the direct mathematical modeling of complex systems. In this context, fractional derivatives become a subset of implicit operators, and mathematical modeling of complex systems can go beyond the use of fractional calculus. It is shown that these implicit operators appear naturally in the modeling of networked mechanical and thermal systems. The components of these systems are bound by the laws of mechanics and thermodynamics which are usually integrodifferential of integer order. However, it has sometimes been mistakenly assumed that the larger system is also of integer order. Thus implicit operators, and their subset the fractional-order derivatives, are a basic tool for the modeling of complex systems.

There is an analogy between real numbers and operators that will be used. An equation such as f(x) = 0, where f : R → R is a known function, may have solutions for which x is real; furthermore, the integer, rational, irrational or transcendental nature of x is also determined by the form of f. A number x multiplied by itself n times, where n is an integer, is written as x^n, but on choosing f(x) suitably this can be extended to x^α for any real α; the law of indices, x^αx^β = x^{α+β} for any α and β, holds, but α in x^α no longer represents the number of times x is multiplied by itself. Finally, under appropriate conditions an equation such as g(y, x) = 0 with g : R × R → R defines an implicit function y = f(x).

Similarly, consider operators D and Ł which operate on a real function u(t), where t is a time-like independent variable (scalar variables will be written in Roman italic, real constants in Greek, matrices in Calligraphic, and integro-differential operators in Fraktur), and where D = d/dt is the usual first derivative operator. Both operators are assumed to return quantities to which they can be re-applied. Notation-wise Ł^m and D^n, where m and n are integers, denote the result of m and n repeated applications of Ł and D, respectively. As special cases, D^n is the identity operator if n = 0, is a derivative operator if n > 0, and is an integral operator if n < 0. In some respects the approach here will parallel that of operational calculus^4 in which D is manipulated as an algebraic variable.

The solution of an operator equation

g(Ł, D) = 0, (1)

where 0 is the zero operator, should give a similar variety of operators that g(y, x) = 0 did for numbers. If Ł − aD^n = 0, where n is an integer, then Ł = aD^n. Or take Ł^m − aD^n = 0, where m is another integer, for which symbolically Ł = p_iD^{n/m} (i = 1, 2, . . . , m), where p_1, p_2, . . . , p_m are the m^{th} roots of a. This defines D^α where α is rational. As examples, a semi-derivative operator Ł can be defined by Ł^2 − D = 0 and a semiintegral by Ł^2 − D^{−1} = 0; symbolically Ł = ±D^{1/2} and Ł = ±D^{−1/2}, respectively. A more general g(Ł, D) = 0 enables D^α to be defined where α is a real number. The linear operator D^α (α < 0) can be written in explicit closed form. An example is

D^αu(t) = 1 Γ (n − 1) ∫_t a (t − τ)^{n−α−1} d^nu dτ^n (τ)dτ (2) which is the Caputo definition of the fractional derivative. There are other definitions as well such as Riemann- Liouville, Grünwald-Letnikov, and others^{2,3}. D^α (α > 0) can be obtained by differentiating and using the law of indices D^αD^β = D^{α+β} . Since D^α can be explicitly defined, linear combinations ∑ i a_iD^{αi} are also explicit. Although

D^α can also be defined for complex α, for simplicity that will be excluded here.

Eq. 1 enables operators Ł to be defined that are not necessarily linear combinations of D^α, except in special cases. In general Eq. 1 cannot be “solved” for Ł nor can it be written in the form Ł = ∑ i a_iD^{αi} ; rather, Ł is defined by this equation, and is thus an implicit operator. This is in line with the adjective being used in mathematics with functions, differentiation, integration, differential equations, and so on (implicit methods in numerical algorithms are a slightly different but related use of the term). The equivalent order of an implicit integrodifferential operator can be taken to be the ratio between the highest powers of D and Ł, respectively, in g(Ł, D). Although Ł cannot be explicitly written, it is nonetheless appropriately though not uniquely defined by Eq. 1.

One example of an implicit operator Ł that will be used later is when it is defined by a quadratic equation

Ł^2 + B(D)Ł + C(D) = 0. (3)

The solution

Ł = 1 2 [ −B ± ( B^2 − 4C )_{1/2}] is symbolic since it cannot be used to write Ł explicitly; Ł is simply such that Eq. 3 is satisfied. Of course there are special cases for which an explicit Ł can indeed be found. For example, if B^2 = 4C then Ł = −B/2, or if B^2 − 4C = D^m then Ł = (−B ± D^{m/2})/2.

Sometimes a polynomial g(Ł, D) can be factorized, analytically or numerically, so that Eq. 1 can be written as (Ł − C_1D^{α1} )(Ł − C_2D^{α2} ) . . . (Ł − C_nD^{αn} ) = 0

for which the solutions are Ł = C_1D^{α1} , C_2D^{α2} , . . ., C_nD^{αn} . Each one of these operators is then explicitly definable. The multiplicity of operators Ł satisfying Eq. 1 is inherent in the equation, and whether all or only some are physically valid depends on the derivation of the equation from the underlying physics.

II. INFINITELY SELF-REPEATING CONFIGURATIONS

It is important to give examples where implicit operators appear in physical systems, because otherwise the subject would be somewhat sterile. It will be shown that some complex systems with self-repeating components can be modeled by implicit operators. In the following, network configurations or graphs will be considered that are made up of components (also called branches, edges, arcs or lines) that are joined at junctions (nodes, vertices, or points). Through each component there is a flow u(t) that is driven by a difference in potential between its terminals Δϕ(t). At each junction it will be assumed that the sum of all incoming flows is zero. These are generalized versions of Kirchhoff’s circuit laws that are common in network transport analysis.

In each component Ł is a linear operator that can be identified depending on the physics of the problem as illustrated in the following examples. The governing equation in each component then takes the form

Ł(u) = Δϕ. (4)

a. For passive electrical components like a resistor R, a capacitor C or an inductor L in series [ LD + RD^0 + 1 C D^{−1} ] (u) = Δϕ, (5a)

where u(t) is the current and Δϕ(t) the driving voltage difference.

b. Water flow in a pipe can be modeled by [ D + aD^0 ] (u) = b Δϕ, (5b)

where u(t) is the volume flow rate, aD^0u(t) is the laminar viscous force, and Δϕ(t) is the driving pressure difference.

c. If there is heat conduction along a rod, then [ D + aD^0 ] (u) = bΔϕ (5c)

where u(t) is the spatial average of the temperature, aD^0u is the convective loss of heat to the environment, and Δϕ(t) is the driving heat rate difference. Usually, the driving potential in heat transfer is the temperature and the flow is the heat rate, but here the roles are reversed.

d. For a spring-damper system [ cD + kD^0 ] (u) = Δϕ, (5d)

where u(t) is the displacement, c is the damping, k is the spring constant, and Δϕ(t) is the external driving force.

Component Eqs. 5 are all of the form of Eq. 4. The tree and ladder configurations below are basically onedimensional flows, and multi-dimensional configurations such as general networks will not be considered here. In the accompanying figures, the straight lines are components and the dots are junctions. The flows are from left to right and they are driven by an overall potential difference ϕ_{in} −ϕ_{out}. To simplify the analysis there are only two component operators, Ł_a and Ł_b, that are repeated infinitely. The flow can be written as Ł_{eq} (u) = ϕ_{in} −ϕ_{out}, where u(t) is the flow that results from an overall driving potential ϕ_{in} − ϕ_{out}, and the objective is to find the equivalent operator of the system Ł_{eq} .

A. Infinite bifurcating trees

This was investigated first for electrical components^5 and then for flows^{6,7} and controlled robots^8. In Fig. 1,

PSfrag replacements

FIG. 1. Infinite tree composed of operators Ła and Ł_b; components in boxed area identical to whole.

PSfrag replacements

FIG. 2. Components in boxed area in Fig. 1 replaced by equivalent.

Ł_a and Ł_b are known operators for the left and right components, respectively. The three equations below

(Ł_a + Ł_{eq} )(u_a) = ϕ_{in} − ϕ_{out}, (6a) (Ł_b + Ł_{eq} )(u_b) = ϕ_{in} − ϕ_{out}, (6b) Ł_{eq} (u_a + u_b) = ϕ_{in} − ϕ_{out}, (6c)

correspond to the left path, the right path, and the equivalent network, respectively, and u_a and u_b are the flows in the respective components.

Operating on Eq. 6a by Ł_{eq} (Ł_b + Ł_{eq} ), on Eq. 6b by Ł_{eq} (Ł_a + Ł_{eq} ), and adding

(Ł_a + Ł_{eq} ) (Ł_b + Ł_{eq} ) Ł_{eq} (u_a + u_b) =ϕ_{in}−ϕ_{out} = Ł_{eq} [Ł_a + Ł_b + 2Ł_{eq} )] (ϕ_{in} − ϕ_{out}).

Because this must be true for all (ϕ_{in} − ϕ_{out}), Ł_{eq} must satisfy

Ł^2_{eq} − Ł_a Ł_b = 0, (7)

where Eq. 6c has been used and some terms canceled. This is of the form of Eq. 3 where B(D) = 0 and C(D) = −Ł_a Ł_b and can be symbolically solved as Ł_{eq} = √ Ł_a Ł_b.

Only the positive root is considered since the negative was spuriously introduced when Eqs. 6a and 6b were multiplied by other terms in the derivation above.

It has been assumed in the derivation that the operators commute with each other^9. Alternative derivations of Eq. 7 can be through stronger assumptions on Ł^n such as the existence of an inverse operator Ł^{−n}, the Laplace transform (or its algebraic equivalents using operational calculus or by assuming harmonic solutions), and electrical impedance methods.

A simple example is: Ł_a = aD^n, Ł_b = bD^m, so that Ł_{eq} = √ ab D^{(n+m)/2} of order (n + m)/2. As mentioned before D^{(n+m)/2} can be explicitly defined. However, if Ł_a = a_1 + a_2D^n and Ł_b = b_1 + b_2D^m, then

Ł^2_{eq} − [ a_1b_1 + a_2b_1D^n + a_1b_2D^m + a_2b_2D^{n+m} ] = 0.

No general explicit representation exists for Ł_{eq} which can, however, be written symbolically as

Ł_{eq} = [ a_1b_1 + a_2b_1D^n + a_1b_2D^m + a_2b_2D^{n+m} ]_{1/2} , which is also of equivalent order (n + m)/2.

B. Infinitely multi-furcating trees

In an infinitely multi-furcating tree (called p-furcating in^7), like the one in Fig. 3, each junction has one connection from the lower generation and n + m going to the subsequent generation, with m of them with operators Ł_a and n with Ł_b. Following the same analysis as for the bifurcating tree except for m times for Ł_a and n times for Ł_b, Ł_{eq} must satisfy

(n + m − 1) Ł^2_{eq} + [(m − 1) Ł_a + (n − 1) Ł_b] Ł_{eq} − Ł_a Ł_b

= 0.

This is of the form of Eq. 3 with

B(D) =

(m − 1) Ł_a + (n − 1) Ł_b n + m − 1 C(D) = −

Ł_a Ł_b n + m − 1 . At least symbolically, the solution can be written as

Ł_{eq} = 1 2 (n + m − 1) [ − (m − 1) Ł_a − (n − 1) Ł_b + { [(m − 1) Ł_a + (n − 1) Ł_b]^2 + 4 (n + m − 1) Ł_a Ł_b

}_{1/2} ]

For a bifurcating tree, n = m = 1, which gives Eq. 7 as before.

C. Infinite ladders

Fig. 4 depicts an infinite ladder configuration^{10,11}. Equations for the two paths and the equivalent network give

Ł_a(u_a) + Ł_{eq} (u_a − u_b) = ϕ_{in} − ϕ_{out}, (8a) Ł_a(u_a) + Ł_b(u_b) = ϕ_{in} − ϕ_{out}, (8b) Ł_{eq} (u_a) = ϕ_{in} − ϕ_{out} (8c)

PSfrag replacements

FIG. 3. First generation of multi-furcating tree network. Each junction has m components with Ła and n components with Ł_b connecting to a junction of a subsequent generation.

PSfrag replacements

FIG. 4. Infinite ladder composed of operators Ła and Ł_b; components in boxed area identical to whole.

The difference between Eqs. 8a and 8b, and between Eqs. 8b and Eq. 8c give

(Ł_{eq} + Ł_b)(u_b) = Ł_{eq} (u_a), (9a) (Ł_{eq} − Ł_a)(u_a) = Ł_b(u_b), (9b)

respectively. Operating on Eq. 9b by (Ł_{eq} +Ł_b) and using Eq. 9a

(Ł_{eq} + Ł_b) (Ł_{eq} − Ł_a)(u_a) = (Ł_{eq} + Ł_b) Ł_b(u_b), = Ł_b (Ł_{eq} + Ł_b)(u_b) =Łeq (ua ) .

Canceling u_a and reshuffling

Ł^2_{eq} − Ł_a Ł_{eq} − Ł_a Ł_b = 0,

which is a quadratic in Ł_{eq} like Eq. 3.

Taking, for example, Ł_a = a_1 + a_2D^n and Ł_b = b_1 + b_2D^m

Ł^2_{eq} − (a_1 + a_2D^n)Ł_{eq} − (a_1 + a_2D^n) (b_1 + b_2D^m) = 0,

which is of equivalent order (m + n)/2.

III. CONCLUSIONS AND DISCUSSION

Implicit operators Ł are defined as solutions of Eq. 1. These operators are a generalization of commonly-used

PSfrag replacements

FIG. 5. Components in boxed area in Fig. 4 replaced by equivalent.

fractional-order derivatives D^α, where α is a real number. Implicit operators appear in the modeling and analysis of complex systems that are composed of two infinitely self-repeating integer-order components, Ł_a and Ł_b, of integer-order. It has been shown that the equivalent operator Ł_{eq} is implicit. The dynamic behavior of the system can be determined from Ł_{eq} alone. The derivation is very general and covers all potential-driven flows.

More generally, it is suggested that the response of complex systems can be studied by two equations, Ł(u) = h(t) and Eq. 1, where the first governs the response of the system to an excitation h(t), and the second defines the system operator Ł. In the present work linear integrodifferential operators appear at the component level, and a quadratic g(Ł, D) in Ł at a system level, but of course there are other possibilities depending on the application being considered. The independent variable has been taken to be time-like so, even though it has not been explicitly stated, the problems are initial value. Application to boundary value problems with a spatial independent variable is possible, as are extensions to partial differential equations. The future can be expected to bring both further analysis of the properties of implicit operators as well as diverse applications to physical problems.

Of course, for engineering applications, means to determine Ł_{eq} explicitly or to approximate it is important. One approach would be to consider low- and highfrequency cases^{12}, which can be used to make the operator explicit in the relevant frequency range. Other approaches could include Padé approximations using rational functions, other types of series approximation, continued fractions, eigen-function expansions, etc. What approximation is best is an open question, and the answer could, of course, be application-specific.

1S.G. Krantz and H.R. Parks. The Implicit Function Theorem: History, Theory, and Applications. Birkhauser, Boston, 2002. 2V.E. Tarasov. Fractional Dynamics: Applications of Fractional Calculus to Dynamics of Particles, Fields and Media. Springer, New York, 2010.

3B.J. West. Fractional Calculus View of Complexity: Tomorrow’s Science. CRC Press, Boca Raton, 2016.

4A. Erdélyi. Operational Calculus and Generalized Functions. Holt, Rinehart and Winston, New York, 1962.

5M. Nakagawa and K. Sorimachi. Basic characteristics of a fractance device. IEICE Transactions on Fundamentals of Electronics Communications and Computer Sciences, E75A:1814–1819, 1992.

6W. Franco, M. Sen, and K.T. Yang. Flows in large, selfsimilar tree networks and their control. Proceedings of the

Royal Society A–Mathematical Physical and Engineering Sciences, 462(2074):2907–2926, 2006.

7J.M. Mayes and M. Sen. Approximation of potential-driven flow dynamics in large-scale self-similar tree networks. Proceedings of the Royal Society A–Mathematical Physical and Engineering Sciences, 467(2134):2810–2824, 2011.

8B. Goodwine. Modeling a multi-robot system with fractionalorder differential equations. Proceedings of the IEEE International Conference on Robotics and Automation, pages 1763– 1768, 2014.

9M.D. Ortigueira and J.A. Tenreiro Machado. What is a fractional derivative? Journal of Computational Physics, 293(SI):4–13,

2015.

10H. Schiessel and A. Blumen. Hierarchical analogs to fractional relaxation equations. Journal of Physics A-Mathematical and General, 26(19):5057–5069, 1993.

11N. Heymans and J.C. Bauwens. Fractal rheological models and fractional differential-equations for viscoelastic behavior. Rheologica Acta, 33(3):210–219, 1994.

12J.F. Kelly and R.J. McGough. Fractal ladder models and power law wave equations. Journal of the Acoustical Society of America, 126(4):2072–2081, 2009.