arXiv:1903.12303v1 [cs.CE] 28 Mar 2019

Nonlinear Moment Matching for the Simulation-Free Reduction of Structural Systems

Maria Cruz Varona, Nico Schneucker, Boris Lohmann

Chair of Automatic Control, Technical University of Munich, Boltzmannstr. 15, D-85748 Garching, Germany (email: maria.cruz@tum.de).

Abstract: This paper transfers the concept of moment matching to nonlinear structural systems and further provides a simulation-free reduction scheme for such nonlinear second-order models. After first presenting the steady-state interpretation of linear moment matching, we then extend this reduction concept to the nonlinear second-order case based on Astolfi [2010]. Then, similar simplifications as in Cruz Varona et al. [2019] are proposed to achieve a simulation-free nonlinear moment matching algorithm. A discussion on the simplifications and their limitations is presented, as well as a numerical example which illustrates the efficiency of the algorithm.

Keywords: Model Order Reduction; Nonlinear Structural Dynamics; Steady-State Response

1. INTRODUCTION

Model order reduction (MOR) for nonlinear structural dynamics has gained an increased importance during the last years. This is due to the large number of engineering applications, where reduced order models are indispensable for the efficient analysis and computer-aided optimization of mechanical structures undergoing large deformations, and/or exhibiting nonlinear material behavior. In this regard, two different reduction streams can be distinguished.

Simulation-based dimensional reduction techniques such as Proper Orthogonal Decomposition (POD), often combined with hyper reduction methods for the efficient evaluation of the nonlinear terms via e.g. the Energy- Conserving Sampling and Weighting (ECSW), are established and successful nonlinear approaches (see e.g. Farhat et al. [2014]). Known in the context of nonlinear frequency response/modal analysis (Kerschen et al. [2009]), the Harmonic Balance Method (HBM) and the Nonlinear Normal Modes (NNMs) have lately become very popular also in the model reduction field (Weeger et al. [2014], Sombroek et al. [2018]). These procedures, however, rely on either numerical continuation methods or shooting techniques, making them also fairly computational expensive in comparison to a numerical integration needed e.g. for POD. Simulation-free reduction procedures have been also studied in the last years. In particular, the concept of basis augmentation with so-called modal derivatives (MDs) has been successfully applied as reduction technique in various structural applications (see e.g. Rutzmoser [2018] and references therein). The key idea is to first compute some dominant vibration modes of the linearized, second-order system, and then to augment the reduction basis with perturbation derivatives capturing the nonlinear behavior.

A few years ago, the concept of moment matching and Krylov subspaces known from linear MOR has been carried over to nonlinear first-order systems by Astolfi [2010].

The extension is based on the steady-state interpretation of linear moment matching, as well as on the steadystate response of nonlinear systems, the center manifold theory and the techniques of nonlinear output regulation [Isidori 1995, Ch. 8], Huang [2004]. Although the method is system-theoretically attractive, it involves the difficult solution of a nonlinear partial differential equation (PDE). Thus, some simplifications have been proposed recently towards a practicable, simulation-free nonlinear moment matching algorithm (Cruz Varona et al. [2019]). The proposed reduction approach is related to the datadriven, low-order nonlinear system identification technique from Scarciotti and Astolfi [2017], in the sense that both methods approximately match nonlinear moments.

The goal of this paper is to transfer the concept of moment matching for linear structural systems to the nonlinear second-order case. In Section 2 we first present the time domain (aka. steady-state) interpretation of moment matching for linear second-order systems. Based on Astolfi [2010], we then transfer this reduction method to the nonlinear second-order case and provide the corresponding nonlinear, Sylvester-like PDE. In Section 4, simplifications are proposed to avoid the PDE, and achieve a simulationfree second-order nonlinear moment matching algorithm, which relies on the solution of nonlinear systems of equations. Finally, numerical results for a geometrically nonlinear structural model are provided.

2. MOMENT MATCHING FOR LINEAR STRUCTURAL SYSTEMS

Consider a large-scale, linear time-invariant (LTI), asymptotically stable, multiple-input multiple-output (MIMO) second-order model of the form Mq̈(t) + Dq̇(t) + Kq(t) = BF (t), q(0)=q_0, q̇(0)=q̇_0 y(t) = Cq(t), (1) where M, D, K ∈R^{n×n} are the mass, damping and stiffness matrices, and q(t) ∈ R^n , F (t) ∈ R^m , y(t) ∈ R^p denote the displacements, forces (inputs) and outputs of the system. The goal of model reduction is to approximate the full order model (FOM) (1) by a reduced order model (ROM) M_rq̈_r(t) + D_rq̇_r(t) + K_rq_r(t) = B_rF (t), y_r(t) = C_rq_r(t), (2) of much smaller dimension r ≪ n with reduced matrices {M_r, D_r, K_r} = W^T {M , D, K} V , B_r = W^TB, C_r = C V and initial conditions q_r(0) = W^T q_0, q̇_r(0) = W^T q̇_0, such that y(t) ≈ y_r(t). In this projection-based framework, the main task consists in finding suitable (orthogonal) projection matrices V , W ∈ R^{n×r} that span appropriate subspaces.

Remark 1. Note that, for second-order systems, the reduction is usually performed by a Galerkin projection with W = V rather than by a two-sided (oblique) Petrov- Galerkin projection. This choice preserves the symmetry and definiteness of the original matrices, which implies the preservation of the stability and passivity of the FOM.

2.1 Notion of Moments and Krylov subspaces

The transfer function of the system (1) is

G(s) = C(s^2M + sD + K)^{−1}B. (3) Definition 1. The moments m_i(σ) of G(s) at the complex expansion point σ ∈C are given by

m_i(σ) = (−1)^i [C 0] [ K^{−1}_σ D_σ K^{−1}_σ M −I 0 ]_i [ K^{−1}_σ B 0 ] , where K_σ =K + σD + σ^2M and D_σ =D + 2σM.

Depending on the considered damping, two different Krylov subspaces for second-order systems can be distinguished to achieve implicit moment matching:

• For general damping (D ≠ 0), so-called second-order Krylov subspaces

K^{2nd}_r ( K^{−1}_σ D_σ, K^{−1}_σ M, K^{−1}_σ B ) ⊆ ran(V ), (4a)

K^{2nd}_r ( K^{−T}_μ D^T_μ, K^{−T}_μ M^T, K^{−T}_μ C^T ) ⊆ ran(W ), (4b)

are employed. These Krylov subspaces yield a twostage Arnoldi-like recurrence, aka. second-order Arnoldi (SOAR). Further details concerning this case are available in Bai and Su [2005], Salimbahrami [2005].

• For proportional (D = αM + βK) or zero (D = 0) damping, the classical first-order Krylov subspaces K^{1st}_r ( K^{−1}_σ M , K^{−1}_σ B ) ⊆ ran(V ), (5a)

K^{1st}_r ( K^{−T}_μ M^T, K^{−T}_μ C^T ) ⊆ ran(W ), (5b)

can be employed instead, yielding – exemplarily for V = [V_0, . . . , V_{r−1}] – the one-stage Arnoldi-like recurrence

(K + σD + σ^2M) V_0 = B, (K + σD + σ^2M) V_i = M V_{i−1}, i ≥ 1. (6) For further details, see Beattie and Gugercin [2005], Salimbahrami [2005].

Note that, in addition to the multimoment matching strategy, it is also possible to match (high-order) moments at a set of different shifts {σ_i}^q_{i=1} and {μ_i}^q_{i=1} with associated multiplicities {r_i}^q_{i=1} (aka. multipoint moment matching). Also note that, besides the block Krylov subspaces, in the

MIMO case we alternatively may use so-called tangential Krylov subspaces (e.g. for (5) and r_1 = . . . = r_q = 1):

span { K^{−1}_{σ1} B r_1, . . . , K^{−1}_{σr} B r_r } ⊆ ran(V ), (7a)

span { K^{−T}_{μ1} C^Tl_1, . . . , K^{−T}_{μr} C^Tl_r } ⊆ ran(W ), (7b)

yielding the following tangential multipoint moment matching conditions:

G(σ_i) r_i = G_r(σ_i) r_i, i = 1, . . . , r,

l^T_i G(μ_i) = l^T_i G_r(σ_i), i = 1, . . . , r. (8) Here, convenient right and left tangential directions r_i ∈ C^m and l_i ∈ C^p should be chosen. Besides, the shifts σ_i, μ_i ∈ C cannot be quadratic eigenvalues of (M , D, K).

2.2 Equivalence of Krylov subspaces and Sylvester equations

Any basis of an input and output Krylov subspace (7) can be interpreted as the solution V and W of the following second-order Sylvester equations:

M V S^2_v + D V S_v + K V = B R , (9a)

M^T W S^{2 T}_w + D^T W S^T_w + K^T W = C^T L. (9b) Hereby, the input interpolation data {σ_i, r_i} is specified by the matrices S_v = diag(σ_1, . . . , σ_r) ∈ C^{r×r} and R = [r_1, . . . , r_r] ∈ C^{m×r} , where the pair (R, S_v ) is observable. Similarly, the output interpolation data {μ_i, l_i} is denoted by the matrices S_w = diag(μ_1, . . . , μ_r) ∈ C^{r×r} and L = [l_1, . . . , l_r] ∈ C^{p×r} , where the pair (S_w, L^T) is controllable.

2.3 Time domain interpretation of Moment Matching

In addition to the frequency domain perception of moment matching (cf. (8)), one can also interpret this concept in the time domain.

Theorem 1. Consider the interconnection of system (1) with the linear signal generator

q̇^v_r (t) = S_v q^v_r (t), q^v_r (0) = q^v_{r,0} ≠ 0, q̈^v_r (t) = S_v q̇^v_r (t), q̇^v_r (0) = q̇^v_{r,0} ≠ 0, F (t) = R q^v_r (t),

(10)

where the triple (S_v , R, q^v_{r,0}) is such that (R, S_v) is observable, λ(S_v) ∩ λ^2(M, D, K) = ∅ and (S_v, q^v_{r,0}) is excitable. Let V be the solution of (9a) and W such that det(W^TEV ) ≠ 0. Furthermore, let q_0 = V q^v_{r,0}, q̇_0 = V q̇^v_{r,0} with q^v_{r,0} ≠ 0, q̇^v_{r,0} ≠ 0 arbitrary. Then, the (asymptotically stable) ROM (2) exactly matches the steady-state response of the output of the FOM, i.e. e(t)= y(t) − y_r(t)=Cq(t) − CV q_r(t)=0 ∀ t (see Fig. 1).

Corollary 1. Interconnecting system (1) with the signal generator (10) is equivalent to exciting the FOM with exponential input signals F (t)=R q^v_r (t)=R e^{Sv t} q^v_{r,0} with exponents given by the shift matrix S_v. Consequently, moment matching for linear structural systems can be interpreted as the exact matching of the steady-state response of the FOM

y_{SS}(t) = C r∑ i=1 (σ^2_i M + σ_iD + K)^{−1}Br_i v_i e^{σi t}q^v_{r,0,i} q^v_{r,i} (t) ≡ y_r(t) = CV q^v_r (t), m_0(σ_i, r_i)=C v_i,

(11)

when both FOM and ROM are excited with exponential input signals F (t) = R q^v_r (t) = R e^{Sv t} q^v_{r,0} (see Fig. 1). For

q̇^v_r (t) = S_v q^v_r (t) q̈^v_r (t) = S_v q̇^v_r (t)

F (t) = R q^v_r (t) M q̈(t) + Dq̇(t) + Kq(t) = BF (t) y(t) = Cq(t) M_rq̈_r(t) + D_rq̇_r(t) + K_rq_r(t) = B_rF (t) y_r(t) = C_rq_r(t) F (t)=R e^{Sv t}q^v_{r,0} y(t) y_r(t) e(t) = 0 q^v_{r,0} ≠ 0 q̇^v_{r,0} ≠ 0 q_0 = V q^v_{r,0} q̇_0 = V q̇^v_{r,0} q_{r,0} = W^T q_0

q̇_{r,0} = W^T q̇_0 linear signal generator FOM ROM −

Fig. 1. Interconnection between the linear FOM/ROM and the lin-

ear signal generator to illustrate the time domain interpretation of moment matching for linear structural systems.

other input signals, the steady-state response is interpolated. Note that the transient response of the FOM is also matched, if the initial conditions are chosen like above.

The Sylvester equation (9a) can be derived using the notion of signal generators. To this end, first insert the linear approximation ansatz q(t) = V q_r(t) with q_r(t)^!= q^v_r (t) in the state equation of (1). Then, the linear signal generator (10) is plugged in, yielding ( M V S^2_v + D V S_v + K V − B R ) · q^v_r (t) = 0. (12)

Since (12) holds for q^v_r (t)=e^{Sv t}q^v_{r,0}, the state vector q^v_r (t) can be factored out and the constant (state-independent) linear Sylvester equation (9a) of dimension n×r is obtained.

3. MOMENT MATCHING FOR NONLINEAR STRUCTURAL SYSTEMS

Consider now a large-scale, nonlinear time-invariant, exponentially stable, MIMO second-order model of the form Mq̈(t) + Dq̇(t) + f ( q(t) ) = BF (t), q(0)=q_0, q̇(0)=q̇_0, y(t) = Cq(t), (13) with q(t) ∈ R^n , F (t) ∈ R^m , y(t) ∈ R^p and the smooth mapping f (q) : R^n → R^n . Note that the modeling of damping in nonlinear dynamic analysis is not a trivial task. Thus, zero damping (D=0) or a linear Rayleigh damping D =αM +βK(q_0), K(q_0)=^{∂f(q)}_{∂q} | | |_{q=q0} are often assumed.

3.1 Nonlinear vs. Linear (Petrov-)Galerkin projection

The goal is to find a nonlinear ROM of dimension r ≪ n using again a projection framework.

One possibility consists in applying a nonlinear projection, where the approximation ansatz is given by q(t)=ν ( q_r(t) ) with the smooth nonlinear mapping ν(q_r) : R^r → R^n . Then,

q̇ =

∂ν(q_r) ∂q_r q̇_r, q̈ =

∂ν(q_r) ∂q_r q̈_r +

∂^2ν(q_r) ∂q^2_r q̇_r ⊗ q̇_r,

with the Jacobian ~V (q_r) = ∂ν(q_r)/∂q_r ∈ R^{n×r} and the second derivative (Hessian) ∂^2ν(q_r)/∂q^2_r ∈ R^{n×r2} . Inserting the ansatz and its derivatives in (13) yields an overdetermined systems of equations with the residual ε. To obtain a quadratic system, we define q_r(t) = ω ( q(t) ) with smooth mapping ω(q) : R^n → R^r and premultiply the equations with the Jacobian ~W (q)^T =^{∂ω(q)}_{∂q} | |_{q=ν(qr )}, thus enforcing the Petrov-Galerkin condition ~W (q)^Tε=0. This yields the ROM ~M_rq̈_r + ~g + ~D_rq̇_r + ~W (q)^Tf(ν(q_r)) = ~B_rF ,

y_r = C ν ( q_r ) , (14)

with { ~M_r, ~D_r } = ~W (q)^T{M, D} ~V (q_r), ~B_r = ~W (q)^TB,

the convective term ~g = ~W (q)^TM^{∂2ν(qr)}_{∂q2r} q̇_r ⊗ q̇_r and the

initial conditions q_r(0)= ~W (q)^T q_0, q̇_r(0)= ~W (q)^T q̇_0.

Another possibility to reduce the nonlinear system (13) is to apply the common and well-known linear Petrov- Galerkin projection, where linear mappings given by the matrices V , W are used instead. This yields the ROM M_rq̈_r(t) + D_rq̇_r(t) + W^Tf ( V q_r(t) ) = B_rF (t), y_r(t) = C_rq_r(t),

(15)

with reduced matrices and initial conditions given as in the linear case.

Remark 2. Please note that the use of a linear projection q ≈ V q_r constitutes a special case of the most general nonlinear projection q ≈ν(q_r) or the power series ansatz q = N∑ k=1 V^{(k)} q^{(k)}_r = V^{(1)}q^{(1)}_r + V^{(2)}q^{(2)}_r + · · · (16)

with V^{(k)} ∈ R^{n×rk} and q^{(k)}_r =

k times

q_r ⊗ · · · ⊗ q_r ∈ R^{rk} .

3.2 Steady-State-Based Nonlinear Moment Matching

The steady-state-based interpretation of moment matching can be carried over to nonlinear structural systems. Theorem 2. Consider the interconnection of system (13) with the nonlinear signal generator

q̇^v_r (t) = s_v ( q^v_r (t) ) , q^v_r (0) = q^v_{r,0} ≠ 0,

q̈^v_r (t) = ∂s_v ( q^v_r (t) ) ∂q^v_r (t) · s_v ( q^v_r (t) ) , q̇^v_r (0) = q̇^v_{r,0} ≠ 0, F (t) = r ( q^v_r (t) ) , (17) where s_v (q^v_r ) : R^r → R^r , r(q^v_r ) : R^r → R^m are smooth mappings. Let ν(q^v_r ) be the unique solution of the following Sylvester-like partial differential equation (PDE) M ∂ν(q^v_r ) ∂q^v_r ∂s_v ( q^v_r ) ∂q^v_r s_v(q^v_r ) + M

∂^2ν(q^v_r ) ∂q^{v2}_r s_v (q^v_r ) ⊗ s_v(q^v_r ) + D ∂ν(q^v_r ) ∂q^v_r s_v(q^v_r ) + f ( ν(q^v_r ) ) = B r ( q^v_r ) . (18)

and ω(q) such that ω(ν(q^v_r )) = q^v_r . Furthermore, let q_0 = ν(q^v_{r,0}), q̇_0 =ν(q̇^v_{r,0}) with q^v_{r,0} ≠0, q̇^v_{r,0} ≠0 arbitrary. Then, the (exponentially stable) ROM (14) exactly matches the steady-state response of the output of the FOM, i.e. e(t)= y(t) − y_r(t)=Cq(t) − Cν ( q_r(t) ) =0 ∀ t.

Corollary 2. The 0-th moment of system (13) at (s_v(q^v_r ), r(q^v_r ), q^v_{r,0}) is related to the (locally well-defined) steadystate response of the FOM y_{SS}(t) = Cν ( q^v_r (t) ) . Thus, nonlinear moment matching can be interpreted as the exact matching of the steady-state response of the FOM y_{SS}(t) = C q_{SS}(t) ≡ y_r(t) = Cν ( q^v_r (t) ) := m_0 ( s_v (q^v_r (t)), r(q^v_r (t)), q^v_{r,0} ) , (19)

when both FOM and ROM are excited with the signal generator (17). For other input signals, the steady-state response is interpolated. Please note here again that the transient response of the FOM is also matched, if the initial conditions are chosen like above. In such case, the matching conditions hold for all t (transient+steadystate). Otherwise, they hold only for t → ∞ (steady-state).

The Sylvester-like PDE (18) represents the nonlinear counterpart of the linear equation (12). Thus, the PDE (18) has been derived similarly as follows. First, the nonlinear approximation ansatz q(t) = ν(q_r(t)) with q_r(t)^!= q^v_r (t) is inserted in the state equation of (13). Afterwards, the nonlinear signal generator (17) is plugged in, yielding (18). Note that – as opposed to the linear, state-independent Sylvester equation (9a) of dimension n×r – the PDE (18) is a nonlinear, state-dependent equation of dimension n×1.

4. SIMULATION-FREE REDUCTION OF NONLINEAR STRUCTURAL SYSTEMS

4.1 Simplifications

The approach for nonlinear moment matching described in Section 3 requires the solution ν(q^v_r (t)) of the nonlinear, state-dependent PDE (18) to reduce the FOM (13). We propose similar step-by-step simplifications as in Cruz Varona et al. [2019] to achieve a practicable, simulation-free reduction method for nonlinear structural systems, which relies on solving nonlinear systems of equations rather than on the difficult solution of the nonlinear PDE (18). The proposed simplifications are (i) the use of a linear projection, (ii) the column-wise consideration of the equation and (iii) a time discretization with timesnapshots. In the following, we explain the simplifications for three different signal generator cases:

1.) Nonlinear signal generator

(i) Linear projection Motivated by the fact that nonlinear projections are complicated, whereas linear ones are often successfully employed even in nonlinear MOR, we propose to apply a linear projection q(t)=ν(q^v_r (t))=V q^v_r (t) instead of the nonlinear projection mapping ν(q^v_r (t)).

By doing so, the PDE (18) becomes the following algebraic nonlinear system of equations MV ∂s_v ( q^v_r (t) ) ∂q^v_r (t) s_v ( q^v_r (t) ) + D V s_v ( q^v_r (t) ) + f ( V q^v_r (t) ) − B r ( q^v_r (t) ) = 0,

(20)

where the triple ( s_v (q^v_r (t)), r(q^v_r (t)), q^v_r (t) ) is user-defined.

(ii) Column-wise consideration System (20) consists of n equations for n · r unknowns in V ∈ R^{n×r} , i.e. it is underdetermined. To overcome this problem, we propose to consider the equation column-wise for each v_i ∈ R^n , i = 1, . . . , r M v_i ∂s_{vi} ( q^v_{r,i}(t) ) ∂q^v_{r,i}(t) s_{vi} ( q^v_{r,i}(t) ) + D v_i s_{vi} ( q^v_{r,i}(t) ) + f ( v_i q^v_{r,i}(t) ) − B r_i ( q^v_{r,i}(t) ) = 0,

(21)

with q^v_{r,i}(t) ∈ R and V = [v_1, . . . , v_r]. Please be aware that, in contrast to the linear setting, a column-wise construction of V using columns v_i satisfying (21) does generally not fulfill the “true” equation (20).

(iii) Time discretization Different from the linear case (see (12)), in the nonlinear setting q^v_r (t) can generally not be factored out in (18) anymore. Consequently, the nonlinear equation (21) is still state-dependent. Thus, inspired by POD, we propose to discretize the state-dependent equation with time-snapshots {t^∗_k}, k = 1, . . . , K.

With user-defined s_{vi} (q^v_{r,i}(t^∗_k )), r_i (q^v_{r,i}(t^∗_k)) and q^v_{r,0,i}, the following time-independent equation results M v_{ik} ∂s_{vi} ( q^v_{r,i}(t^∗_k) ) ∂q^v_{r,i}(t^∗_k) s_{vi} ( q^v_{r,i}(t^∗_k) ) + D v_{ik} s_{vi} ( q^v_{r,i}(t^∗_k) ) + f ( v_{ik} q^v_{r,i}(t^∗_k) ) − B r_i ( q^v_{r,i}(t^∗_k) ) = 0, (22)

which can be solved for each v_{ik} ∈ R^n , with i = 1, . . . , r and k = 1, . . . , K. The discrete solution q^v_{r,i}(t^∗_k) of the nonlinear signal generator equation (17) must be given or computed via simulation before solving equation (22).

2.) Linear signal generator

One may also come to the idea of interconnecting the nonlinear system (13) with the linear signal generator (10), where s_v(q^v_r (t))=S_v q^v_r (t) and r(q^v_r (t))=R q^v_r (t).

(i) Linear projection By doing so, equation (20) becomes

MV S^2_vq^v_r (t) + DV S_v q^v_r (t) + f ( V q^v_r (t) ) − BRq^v_r (t) = 0. (23) where the triple (S_v, R, q^v_{r,0}) is user-defined. Note that a linear signal generator corresponds to exciting the nonlinear system with exponential input signals F (t)= R q^v_r (t) = R e^{Sv t} q^v_{r,0}. Although exponential functions are the characterizing eigenfunctions for linear systems, the question raises whether complex (growing) exponentials are sufficiently valid for characterizing nonlinear systems. Nevertheless, one might hope that such exponential input signals can be sufficient in certain cases to describe the underlying nonlinear dynamics adequately as well.

(ii) Column-wise consideration Considering the underdetermined equation (23) again column-wise delivers Mv_iσ^2_i q^v_{r,i}(t)+Dv_iσ_iq^v_{r,i}(t)+f ( v_iq^v_{r,i}(t) ) −Br_iq^v_{r,i}(t) = 0, (24) where the signal generator (10) becomes q̇^v_{r,i}(t)=σ_i q^v_{r,i}(t), F_i(t)=r_i q^v_{r,i}(t) with q^v_{r,i}(t)=e^{σi t}q^v_{r,0,i} for i = 1, . . . , r.

(iii) Time discretization Using the time-discretized signal generator q̇^v_{r,i}(t^∗_k) = σ_i q^v_{r,i}(t^∗_k), F_i(t^∗_k) = r_i q^v_{r,i}(t^∗_k) and q^v_{r,0,i}, equation (24) becomes time-independent

M v_{ik} σ^2_i q^v_{r,i}(t^∗_k) + D v_{ik} σ_i q^v_{r,i}(t^∗_k) + f ( v_{ik} q^v_{r,i}(t^∗_k) ) − B r_i q^v_{r,i}(t^∗_k) = 0,

(25)

with q^v_{r,i}(t^∗_k) = e^{σit∗k} q^v_{r,0,i} for i = 1, . . . , r. Note that in this case, the discrete solution q^v_{r,i}(t^∗_k) of the linear signal generator equation (10) is analytically given by exponential functions with exponents σ_i, so that no simulation of the linear signal generator is required.

3.) Zero signal generator

This special (linear) signal generator is defined as q̇^v_r (t) = s_v(q^v_r (t)) = 0, yielding q^v_r (t) = q^v_{r,0} = const and F (t) = Rq^v_r (t) = R q^v_{r,0} = const. Thus, this generator corresponds to exciting the nonlinear system with a constant input.

(i) Linear projection In this particular case, equation (20) becomes f ( V q^v_{r,0} ) − B R q^v_{r,0} = 0, (26) i.e. a nonlinear, time-independent system of equations.

(ii) Column-wise consideration A column-wise consideration of the above underdetermined equation yields f ( v_i q^v_{r,0,i} ) − B r_i q^v_{r,0,i} = 0, (27)

where q̇^v_{r,i}(t) = 0 with σ_i = 0, F_i(t) = r_i q^v_{r,0,i} = const and q^v_{r,i}(t) = q^v_{r,0,i} = const hold for i = 1, . . . , r. In other words, the employment of a zero signal generator is equivalent to moment matching at shifts σ_i =0.

(iii) Time discretization For this special case, no time discretization is needed, since (27) already represents a time-independent equation. Please note that solving (27) is strong related to computing the steady-state q_∞ (aka. equilibrium or static displacement) of the nonlinear mechanical system (13) by means of f ( q_∞ ) −BF_{const} =0.

4.2 Simulation-free nonlinear moment matching algorithm

Based on the simplifications discussed before, we now state our proposed simulation-free nonlinear moment matching algorithm for nonlinear structural systems:

Algorithm 1 Second-order NLMM (SO-NLMM)

Input: M, D, f(q), B, J_f (q), q^v_{r,i}(t^∗_k), q̇^v_{r,i}(t^∗_k), q̈^v_{r,i}(t^∗_k) r_i (q^v_{r,i}(t^∗_k)), initial guesses v_{0,ik}, deflated order r_{defl} Output: orthogonal basis V 1: for i = 1 : r do ▷ e.g. r different shifts σ_i 2: for k = 1 : K do ▷ e.g. K samples in each shift

3: fun=@(v)M v q̈^v_{r,i}(t^∗_k )+D v q̇^v_{r,i}(t^∗_k )+f (v q^v_{r,ik})−B r_i (q^v_{r,ik})

4: Jfun=@(v) M q̈^v_{r,i}(t^∗_k ) + D q̇^v_{r,i}(t^∗_k ) + J_f (v q^v_{r,ik}) q^v_{r,ik}

5: V(:,(i-1)*K+k)= Newton(fun, v_{0,ik} ,Jfun)

6: V = gramSchmidt((i-1)*K+k, V) ▷ optional

7: end for 8: end for 9: V = svd(V, r_{defl}) ▷ deflation is optional

Since the different strategies, the computational effort and further aspects of the algorithm have been already discussed in detail for nonlinear first-order systems in Cruz Varona et al. [2019], here we briefly summarize these aspects for the second-order case, and rather provide some new clarifying insights that also hold true for the firstorder case.

a) Different strategies, degrees of freedom and special cases

• Besides the depicted most general approach using different signal generators and time-snapshots (i=1, . . . , r, k =1, . . . , K), one could also consider a single signal generator at several collocation points (i = 1, k = 1, . . . , K) or different signal generators at only one time-snapshot (i=1, . . . , r, K =1). • In addition to a nonlinear signal generator, one could also apply a linear or a zero signal generator. To this end, line 3 (and correspondingly line 4 also) in Algorithm 1 should be replaced by the equations (25) and (27).

• If the NLMM algorithm is applied to a linear secondorder system (2) with f (q) = Kq using a linear signal generator, the algorithm boils down to the classical rational Krylov subspace method, since line 3 becomes (Mv_{ik} σ^2_i + Dv_{ik} σ_i + Kv_{ik})e^{σi t∗k} q^v_{r,0,i} = Br_i e^{σi t∗k} q^v_{r,0,i} ⇔ (K + σ_iD + σ^2_i M ) v_i = B r_i. (28)

In this special case, the reduction parameters condensate to (s_{vi} , r_i , q^v_{r,0,i}, t^∗_k). b) Computational effort The presented reduction technique is simulation-free or simulation-lean, since it “only” involves the solution of (at most r·K) nonlinear systems of equations (NLSE) of full order dimension n. These NLSEs can be solved using a Newton-Raphson scheme (cf. line 5).

Reduction techniques like POD require a forward numerical simulation (one/multistep, explicit/implicit, adaptive/fixed step-size) of the FOM to gather the snapshots. In case of an implicit scheme, the computational effort of POD compared to NLMM is supposed to be higher, since – within an implicit simulation – a NLSE must be solved in each time-step with the Newton-Raphson method.

c) Other aspects Initial guesses for a NLSE can be taken (depending on the case) from the solution for a zero signal generator v_{0,i} ← (27), from linearized models v_{0,i} = K^{−1}_{σi} Br_i, K = ∂f(q)/∂q|_{qeq} , or from the solutions at neighbouring shifts v_{0,i+1} ← v_{iK} or time-snapshots v_{0,i,k+1} ←v_{ik} . A deflation of the basis V (cf. line 9) is highly recommended, to truncate redundant column vectors and obtain a full rank, orthogonal matrix. Alternatively, an orthogonalization process via Gram-Schmidt or QRdecomposition can optionally be employed.

4.3 Analysis, Discussion and Limitations

This section serves as a complementary discussion to the one already presented in Cruz Varona et al. [2019].

∗ As mentioned in Remark 2, a linear projection represents a special case of the most general nonlinear projection or the polynomial expansion-based ansatz (16) proposed in [Huang 2004, Ch. 4]. Applying e.g. a quadratic/cubic projection (see e.g. Rutzmoser [2018]) or a series expansion ansatz with basis functions customized for the nonlinear system at hand (Scarciotti and Astolfi [2017]) could be superior and even indispensable in certain cases. However, from a numerical perspective, nonlinear projections are much more difficult to handle than linear ones. Moreover, the latter are often used and might be sufficient for many types of nonlinearities.

∗ The choice of the signal generator determines (1) the ansatz for the dynamics q^v_r (t), q̇^v_r (t), q̈^v_r (t) and (2) the exciting input of the system. Thus, the signal generator should be chosen such that (1) q^v_r (t) constitutes representative eigen-/ansatz functions of the underlying nonlinear system and (2) F (t) represents a typical operating input which excites the important dynamics. Although the validity of a linear signal generator for characterizing nonlinear systems is questionable, this type of signal generator (where complex exponentials serve as ansatz functions) is being implicitly used for the reduction of bilinear and quadratic bilinear systems. Complex exponentials are also being employed in the Fourier approximation ansatz of the Harmonic Balance.

Please note that the linear signal generator (10) constitutes a special case of the expansion-based ansatz

q̇^v_r = N∑ k=1 S^{(k)}_v q^v_r^{(k)} = S^{(1)}_v q^v_r + S^{(2)}_v (q^v_r ⊗ q^v_r ) + · · · ,

F = N∑ k=1 R^{(v)}q^v_r^{(k)} = R^{(1)}q^v_r + R^{(2)}(q^v_r ⊗ q^v_r ) + · · · , (29)

with S^{(k)}_v ∈ C^{r×rk} , R^{(k)} ∈ C^{m×rk} and q^v_r^{(k)} ∈ R^{rk} . ∗ In the Sylvester-like PDE (18) the state vector q^v_r (t) cannot be factored out so easily than in (12). In fact, the key to obtain a constant/state-independent matrix equation of dimension n × r from (18) lies on both the choice of an adequate projection ansatz (e.g. (16)) and an appropriate signal generator (e.g. (29)), tailored for the nonlinear system at hand. Interestingly, the state-independent matrix Sylvester equations used in bilinear/quadratic bilinear MOR can indeed be derived from (18) by using the Volterra series representation, with a linear projection and a linear signal generator (Cruz Varona and Gebhart [2018]).

∗ If a linear projection is applied and the factorization of q^v_r (t) does not succeed, then, lamentably, the underdetermined system (20) is obtained. The proposed column-wise consideration has the limitation that (20) is generally not fulfilled, since the couplings in V q^v_r (t), V s_v(q^v_r (t)) and r(q^v_r (t)) are not being considered. We are currently working on possible ways to numerically solve the underdetermined systems (20), (23) and (26).

∗ In Astolfi [2010], the signal generator is assumed to be Poisson stable^1 , so that the steady-state of the nonlinear system is well-defined. In linear MOR, however, shifts σ_i ∈ C \ λ^2(M, D, K) can be used. Indeed, due to the Meier-Luenberger conditions, the shifts are often chosen on the right half-plane (σ_i ∈ C^{>0} ), meaning that the system is being excited by growing exponentials. We believe that, within the NLMM algorithm, the nonlinear system can be excited by a stable, Poisson stable or even an unstable generator, as long as the considered time interval for t^∗_k is (naturally) well chosen, but limited.

5. NUMERICAL EXAMPLE

The SO-NLMM algorithm is illustrated by means of a cantilever beam. The 2D model is discretized using 246 triangular elements with quadratic shape functions, yielding (after Dirichlet boundary conditions) n=1224 degrees of freedom in x- and y-direction. The beam is made of steel, which is modeled as linear Kirchhoff material with E = 210 GPa, ν = 0.3 and ρ = 1 · 10^{4 kg}/m^3. However, the model exhibits geometric nonlinear behavior due to the used Green-Lagrange strain tensor, which is a quadratic function of the nodal displacements. The model equation is given by (13), where zero damping (D = 0) is assumed. The input force F (t) is applied at the tip in negative ydirection. The output y(t) is the y-displacement of the tip. We use the open-source research code AMfe (Rutzmoser [2018]) for the setup and numerical simulation of the finite element model. Gmsh and ParaView serve hereby as mesh generation and post-processing tools, respectively. The

1 Corresponds to λ(S_v ) ∈ C^0 in the linear setting, i.e. exciting the system with a permanent oscillation ([Isidori 1995, Ch. 8]).

SO-NLMM algorithm 1 has been implemented in Python using a self-programmed Newton-Raphson scheme.

We apply Algorithm 1 using a single signal generator with K =10 or K =20 equidistant time-snapshots in the interval [0, 1]. For the training phase of SO-NLMM and POD, we use the signal generator q^v_r (t) = sin(10t) with corresponding q̇^v_r (t), q̈^v_r (t) and the training input F (t)=r(q^v_r (t))=10^8· q^v_r (t). For the test phase of FOM and ROMs, we apply the different input F (t) = 10^8 sin(31t). We compare both approaches with ROMs obtained via V_ϕ containing only linear vibration modes ϕ_i, and an augmented basis V_{aug} containing vibration modes and static modal derivatives to capture the nonlinear behavior. The numerical integration of FOM and ROMs is accomplished by an implicit generalized-α scheme with fixed step-size h = 1 ms. In terms of approximation quality, some numerical results are given in Fig. 2, 3 and 4. The pure linear basis V_ϕ cannot capture the nonlinear behavior at all. Both SO- NLMM and POD yield satisfactory results, being POD superior. In terms of computational effort, POD required ≈ 92 s, whereas SO-NLMM needed only ≈ 13 s (r = 10) or ≈19 s (r =20) to compute the reduction basis.

Fig. 2. Displacement snapshot of the cantilever beam (r_ϕ = 3,

r_{aug} = 9, r = 10).

0.00.20.40.60.81.0 −20 2 time (s) y-displacement (m)

FOM V_ϕ V_{aug} POD SO-NLMM

Fig. 3. y-displacement of beam’s tip for FOM and different ROMs

(r_ϕ = 3, r_{aug} = 9, r = 10).

SOURCE CODE

The Python implementation of SO-NLMM and further numerical results including some videos are available at

https://zenodo.org/record/2611120.

0.00.20.40.60.81.0 10^{−9} 10^{−7} 10^{−5} 10^{−3} 10^{−1} time (s) rel. L_2 output-error

V_ϕ V_{aug} POD SO-NLMM

Fig. 4.^{|y(t)−yr,{∗}(t)|} ||y(t)||L2 -error for different ROMs {∗} (rϕ = 5, r = 20).

REFERENCES

Astolfi, A. (2010). Model reduction by moment matching for linear and nonlinear systems. IEEE TAC, 55(10), 2321–2336.

Bai, Z. and Su, Y. (2005). Dimension reduction of largescale second-order dynamical systems via a second-order Arnoldi method. SISC, 26(5), 1692–1709, SIAM.

Beattie, C.A. and Gugercin, S. (2005). Krylov-based model reduction of second-order systems with proportional damping. In 44th IEEE CDC, 2278–2283.

Cruz Varona, M. and Gebhart, R. (2018). Nonlinear model order reduction: A system-theoretic viewpoint. MoRePaS IV, ScienceOpen Posters.

Cruz Varona, M. et al. (2019). Practicable Simulation- Free Model Order Reduction by Nonlinear Moment Matching. Submitted to ECC 2019, https://arxiv.

org/abs/1901.10750.

Farhat, C. et al. (2014). Dimensional reduction of nonlinear finite element dynamic models with finite rotations and energy-based mesh sampling and weighting for computational efficiency. IJNME, 98(9), 625–662.

Huang, J. (2004). Nonlinear Output Regulation: Theory and Applications. SIAM Advances in Design & Control.

Isidori, A. (1995). Nonlinear Control Systems. Springer, 3rd edition.

Kerschen, G. et al. (2009). Nonlinear Normal Modes, Part I: A Useful Framework for the Structural Dynamicist. MSSP, 23(1), 170–194.

Rutzmoser, J.B. (2018). Model Order Reduction for Nonlinear Structural Dynamics: Simulation-free Approaches. Ph.D. thesis.

Salimbahrami, S.B. (2005). Structure preserving order reduction of large scale second order models. Ph.D. thesis.

Scarciotti, G. and Astolfi, A. (2017). Data-driven model reduction by moment matching for linear and nonlinear systems. Automatica, 79, 340–351.

Sombroek, C.S.M., Tiso, P., Renson, L., and Kerschen, G. (2018). Numerical computation of nonlinear normal modes in a modal derivative subspace. Computers & Structures, 195, 34–46.

Weeger, O., Wever, U., and Simeon, B. (2014). Nonlinear frequency response analysis of structural vibrations. Computational Mechanics, 54(6), 1477–1495.