arXiv:1907.10560v1 [eess.SP] 24 Jul 2019

Accurate Angular Inference for 802.11ad Devices Using Beam-Specific Measurements

Haichuan Ding and Kang G. Shin University of Michigan, Ann Arbor Email:dhcbit@gmail.com, kgshin@umich.edu

Abstract—Due to their sparsity, 60GHz channels are characterized by a few dominant paths. Knowing the angular information of their dominant paths, we can develop various applications, such as the prediction of link performance and the tracking of an 802.11ad device. Although they are equipped with phased arrays, the angular inference for 802.11ad devices is still challenging due to their limited number of RF chains and limited phase control capabilities. Considering the beam sweeping operation and the high communication bandwidth of 802.11ad devices, we propose variation-based angle estimation (VAE), called VAE-CIR, by utilizing beam-specific channel impulse responses (CIRs) measured under different beams and the directional gains of the corresponding beams to infer the angular information of dominant paths. Unlike state-of-the-arts, VAE-CIR exploits the variations between different beam-specific CIRs, instead of their absolute values, for angular inference. To evaluate the performance of VAE-CIR, we generate the beam-specific CIRs by simulating the beam sweeping of 802.11ad devices with the beam patterns measured on off-the-shelf 802.11ad devices. The 60GHz channel is generated via a ray-tracing simulator and the CIRs are extracted via channel estimation based on Golay sequences. Through experiments in various scenarios, we demonstrate the effectiveness of VAE-CIR and its superiority to existing angular inference schemes for 802.11ad devices.

I. INTRODUCTION The completion of the 802.11ad standard and its device commercialization have led to various research efforts to either improve the communication performance of 60GHz devices, such as link performance prediction, access point (AP) deployment, and seamless indoor multi-Gbps wireless connectivity, or develop novel applications with these devices, such as single AP decimeter-level localization [1]–[5]. All these applications usually rely on the length and angular information of strong signal (or dominant) paths in the sparse 60GHz channel. Since this path information is often unavailable, we must be able to effectively infer such information for which angular information serves as the starting point.

As demonstrated in various studies, the starting point for inferring path information is the collection of angular information — such as angles of departure (AODs) and angles of arrival (AOAs) — of dominant paths [1]–[5]. Unfortunately, inferring angular information is not easy for 802.11ad devices. On the one hand, for cost reasons, phased arrays on offthe-shelf 802.11ad devices only support 2 to 4-bit phase control [6]. Due to this limited phase control capability, the generated beams can have multiple strong side lobes, thus making it difficult for 802.11ad devices to directly learn angular information from the adopted beams. On the other hand, due to the limited number of RF chains, existing direction estimation schemes are not applicable to off-the-shelf 802.11ad devices. As reported in [1], 802.11ad devices adopt analog phased arrays and the signals received at different antenna elements are mixed at the output of the RF chain. Since most existing direction estimation schemes require the signal received at each antenna element to be known, they are not applicable to millimeter wave (mmWave) devices with analog phased arrays. Although there have been a few direction estimation schemes proposed for antenna arrays with a hybrid beamforming architecture, they cannot be directly integrated into 802.11ad devices which are equipped with a single RF chain.

Considering this fact, several direction estimation schemes have recently been proposed for 802.11ad devices based on a single RF chain and analog arrays. Wei et al. [1] exploited the orthogonality within the codebook to map the output of the RF chain to the signals received at different antenna elements and used the MUSIC algorithm to estimate the AOAs of different paths. In their scheme, the device receives the incoming signal using different weight vectors (i.e., beam patterns) and isolates the signal received at each antenna element through a matrix inversion. As pointed out in [5], to make this scheme effective, we should ensure that exactly the same signal is sampled by all of the adopted beam patterns, thus limiting its applicability. Furthermore, the placement and enclosures of the phased array antenna might affect its radiation pattern, making the relationship between weight vectors and directional gains invalid, and thus adversely impacting the performance of the AOA estimation schemes based on weight vectors [7]. So, most existing direction estimation schemes for 802.11ad devices exploit the correlation between wireless measurements made under different beams and the directional gains of the corresponding beams for angular inference [4], [5], [8]. Steinmetzer et al. [8] proposed a direction estimation scheme based on received signal strength (RSS) to infer the AOA of a dominant path. In that scheme, multiple RSS measurements are made using different beams, and the estimated AOA is the direction that provides the best match between the directional gains and the RSS measurements. Although its effectiveness has been demonstrated in a specific environment, the experimental results in [5] show this RSS-based scheme to be highly inaccurate in a different environment due to irregular beam patterns and multipath propagation. In this case, the RSS not only depends on the path of interest but also is affected by the signals received from other paths.

This observation motivates two recent direction estimation schemes which exploit the measured channel impulse response (CIR), instead of the RSS, for angular inference [4], [5]. According to [9], each 802.11ad frame begins with a short training field (STF) and a channel estimation (CE) field, which allow 802.11ad devices to acquire the corresponding CIR. Additionally, since the 802.11ad frames are delivered over a spectrum of ≥ 1760MHz bandwidth, two path components are resolvable for 802.11ad devices as long as their arrival times have a 0.57ns difference. In other words, two paths are resolvable as long as their lengths have a 0.17m difference. Given the sparsity of mmWave channels, it is very likely that each dominant component in the CIR corresponds to one of the dominant propagation paths between the transmitter and the receiver. Thus, each dominant CIR component is very likely to be completely determined by a dominant path. In view of this, Ghasempour et al. [4] and Pefkianakis et al. [5] propose two direction estimation schemes for 802.11ad devices, which exploits beam-specific CIRs measured under different beam patterns during, for example, beam sweeping to gradually narrow down the potential AOAs/AODs. In both of these two schemes, CIR components are first mapped to dominant paths through their time of arrival. Then, the corresponding CIR components measured under different beams are used to gradually refine the AOA/AOD estimates of the paths of interest. For each dominant path, the scheme in [4] maintains a score for each direction with initial value 0. Once a new CIR measurement comes in, the score of each direction is updated depending on whether the desired CIR component is received or not, as well as the directional gain of the adopted beam pattern. When the measurement process completes, the direction with the highest score will be considered as the AOA of the corresponding path. The authors of [5] adopted a similar procedure to estimate the AOD of the line-of-sight (LOS) path by utilizing the CIR feedback from the receiver. To improve the accuracy of AOD estimation further, they selected a few CIR measurements with the strongest LOS components for AOD estimation and weighted the contribution of each CIR measurement with the amplitude of its LOS component. They then chose the estimated AOA to be the center of the direction interval spanned by a few directions with the highest scores. Despite the differences, both of these schemes rely on a hidden assumption that, if a CIR component is received under a beam, the angle of the corresponding path is more likely to be along the direction with a higher directional gain. As a result, once the desired CIR component is measured under a beam, they always assign the highest score increase to the direction with the highest directional gain. However, the reception of a CIR component only implies that the directional gain along the AOA/AOD of the corresponding path is higher than a certain threshold, rather than that the AOA/AOD of this path is along the direction with the highest gain. Blindly assigning higher score increments to the directions with higher directional gains might lead to large estimation errors.

As seen from the above discussions, despite the various angle estimation schemes proposed thus far, accurate AOA/AOD estimation for 802.11ad devices is still lacking. The goal of this paper is to address this need by developing a variationbased angle estimation (VAE), called VAE-CIR. Like [4], [5], for each path of interest, VAE-CIR maintains the score for each direction and utilizes the beam-specific CIR measurements under different beam patterns to update the score. Unlike existing schemes where the CIR measured under each beam is used independently to update the score, VAE-CIR updates the score based on the variations in the corresponding CIR component under different beams. Specifically, for the considered path, VAE-CIR updates the score for each direction based on the variations between every two CIRs measured using different beams, and the direction where the variation in directional gain better matches that in the CIR will be assigned a higher score increase. In other words, VAE-CIR picks the direction in which the variations of directional gain best match the variations in the CIR component as the estimated angle for the path of interest. The rationale behind VAE-CIR is that, during measurement processes like beam sweeping, different beams encounter the same set of signal paths and the variations in CIR measurements are the results of the variations in directional gain along the AOA/AOD of each path. This paper makes the following contributions.

• Study of the angular inference for 802.11ad devices based on wireless measurements. Unlike prior work, we propose to not directly utilize each CIR component but employ its variations under different beams to infer the angle of each path.

• Design of VAE-CIR which exploits the variations in every two CIR measurements to infer the AOA/AOD of dominant paths. For a specific path, VAE-CIR exploits the variations in its corresponding CIR component between every two measurements to update the score assigned to different directions and the inferred AOA/AOD is the direction with the highest final score. VAE-CIR allows us to flexibly weight the contribution of every two CIR measurements to the score. For example, a lower weight can be assigned when the amplitude of the interested CIR component is below a certain threshold in at least one of the two CIR measurements since the accuracy of the CIR measurements is more prone to noise in this case.

• Extensive simulation to evaluate effectiveness of VAE-CIR. We generate the transmit signals and implement the channel estimation based on Golay sequences for CIR extraction by following the IEEE 802.11ad standard. Using the beam pattern measured on the off-the-shelf 802.11ad devices and the channel model approved by IEEE 802.11 Task Group ad, we demonstrate the superiority of VAE-CIR to state-of-the-arts.

Fig. 1. The structure of a typical 802.11ad PPDU.

II. BEAM-SPECIFIC CIR AND CHANNEL ESTIMATION

A. Beam-Specific CIR

To compensate high path loss and facilitate high speed transmissions, mmWave communication devices exploit phased arrays and beamforming to concentrate energy in the desired directions. Due to the constraints on hardware implementation, 802.11ad devices adopt an analog beamforming architecture where each antenna is connected with a phase shifter and beamforming is performed in the analog domain with these phase shifters. This analog beamforming architecture cannot simultaneously support more than one beam, and can steer the beam to different directions by controlling the amount of phase shift of each phase shifter [10]. Due to the use of beamforming, the CIR observed at the receiver depends on both the underlying signal paths and the radiation pattern of the adopted beam. Denoting the equivalent lowpass representation of the continuous-time CIR as h(t) [11], we have

h (t) = K∑ k=1 α_kG_m (ϑ_k) G_l (θ_k) δ (t − τ_k), (1)

where K is the total number of underlying signal paths, α_k and and τ_k are the complex path gain and the delay of the k-th path, respectively. ϑ_k is the AOD of the k-th path at the transmitter and G_m (ϑ_k) is the beamforming gain along the spatial direction ϑ_k when the transmitter uses its m-th beam for transmissions. θ_k is the AOA of the k-th path at the receiver and G_l (θ_k) is the beamforming gain along direction θ_k when the receiver employs its l-th beam for reception. Each summand in Eq. (1) corresponds to a CIR component. Let h_k be the k-th CIR component and h_k (l) be the k-th CIR component measured using the l-th receiving beam. When the underlying signal path remains the same, the amplitude of each CIR component, |h_k|, will track the changes of directional gains. For example, if the receiver switches to the (l + 1)-th beam, we have |h_k| = |h_k (l + 1)| = |α_kG_m (ϑ_k) G_{l+1} (θ_k)| and |h_k (l + 1)|/|h_k (l)| = |G_{l+1} (θ_k)|/|G_l (θ_k)|. In other words, the variations in the directional gain along the AOA θ_k of a path matches the variations in the amplitude of its corresponding CIR component h_k. This observation motivates VAE-CIR which we introduce in the next section.

B. Channel Estimation in 802.11ad

According to the IEEE 802.11ad standard, each physical layer convergence procedure protocol data unit (PPDU) contains a CE field right next to the STF. 802.11ad physical layer (PHY) supports three modulation methods — control modulation, single carrier (SC) modulation and OFDM modulation — which share a common preamble structure [9]. The structure of a typical 802.11ad PPDU is shown in Fig. 1, where Gau_{256}[n], Gbu_{256}[n], Gav_{256}[n], Gbv_{256}[n] are Golay sequences of length 256. Ga_{128}(n) and Gb_{128}(n) are two Golay sequences of length 128 defined in subclause 21.11 of the 802.11ad standard. Gau_{256}(n) and Gbu_{256}(n) are complementary sequences with the following property:

R_a [i] + R_b [i] = { 512 i = 0 0 −255 ≤ i ≤ 255, i ≠ 0 , (2)

where R_a [i] and R_b [i] are autocorrelation of Gau_{256} [n] and Gbu_{256} [n], defined as

R_a [i] = (Gau_{256} ⋆ Gau_{256}) [i] = min{255+i,255} ∑ n=max{0,i} Gau_{256} [n] Gau_{256} [n − i],

− 255 ≤ i ≤ 255, R_b [i] = (Gbu_{256} ⋆ Gbu_{256}) [i] = min{255+i,255} ∑ n=max{0,i} Gbu_{256} [n] Gbu_{256} [n − i],

− 255 ≤ i ≤ 255, (3)

where ⋆ is the correlation operator. Similarly, Gav_{256}(n) and Gbv_{256}(n) are complementary sequences. Ga_{128}(n) and Gb_{128}(n) are complementary sequences. These two pairs of complementary sequences also have the autocorrelation property in Eq. (2), and this property of Golay sequences is exploited in 802.11ad for channel estimation [12], [13]. Clearly from Fig. 1, both the STF and CE field are built up from Golay sequences. Each STF ends with −Ga_{128}(n), and each CE field ends with −Gb_{128}(n), which facilitates the creation of a length-127 zero-correlation zones as discussed below [14]. It should be noted that the CE field shown in Fig. 1 is the CE field for control PHY and SC PHY. OFDM PHY adopts a similar CE field where Gv_{512}[n] is transmitted before Gu_{512}[n]. The STF and CE fields are modulated prior to transmission using π/2-BPSK. We use ~Gau_{256} [n] and ~Gbu_{256} [n] to denote Gau_{256} [n] and Gbu_{256} [n] after constellation mapping. It can be easily shown that ~Gau_{256} [n] and ~Gbu_{256} [n] also have the autocorrelation property shown in Eq. (2).

Let s(t) be the transmitted preamble before upconversion. Then, we have

s (t) =

1279∑

n=0 s [n] (g ∗ h_T ) (t − nT_c), (4) where s [n] is a sequence obtained by sequentially concatenating − ~Ga_{128}, ~Gu_{512}, ~Gv_{512}, and −~Gb_{128}, h_T (t) represents the transmit shaping filter, and T_c is the chip time. T_c = 0.57ns for control and SC PHY. g (t) = u (t) − u (t − T_c), where u (t) is the unit step function defined in [15]. ∗ in Eq. (4) represents the operation of convolution. It should be noted that, for ease of presentation, we only consider the part of the preamble related to channel estimation in Eq. (4). Then, the received signal after going through the wireless channel, downcoversion, and the anti-aliasing filter is

r (t) = K∑ k=1 h_k (s ∗ h_R) (t − τ_k) + z (t) , (5)

where h_k is the kth CIR component defined in the last subsection, h_R (t) is the impulse response of the anti-aliasing filter at the receiver, and z (t) is the additive noise. Suppose (h_T ∗ h_R) (t) has a flat frequency response with magnitude 1 in the band of interest, the received signal sampled at a rate of 1/T_c is

r (nT_c) = K∑ k=1 h_k 1279∑

j=0 s [j] g (nT_c − τ_k − jT_c) + z (nT_c) . (6) Let r [n] = r (nT_c) and z [n] = z (nT_c), we have

r [n] = K∑ k=1 h_ks [n − ⌈τ_k/T_c⌉] + z [n] , (7)

where ⌈.⌉ is the ceiling function. To obtain the estimated CIR, r [n] is first correlated with ~Gau_{256}, ~Gbu_{256}, ~Gav_{256}, and ~Gbv_{256}. Specifically, we have ( r ⋆ ~Gau_{256} ) [i] = K∑ k=1 h_k ( s ⋆ ~Gau_{256} ) [i − ⌈τ_k/T_c⌉] + ( z ⋆ ~Gau_{256} ) [i] , (8)

where ( s ⋆ ~Gau_{256} ) [i]

= min{ℓ_s−i,255} ∑ n=max{−i,0} s [n] ~Gau_{256} [n − i] −255 ≤ i ≤ ℓ_s 0 o.w. . (9) Similar results can be obtained for ~Gbu_{256}, ~Gav_{256}, and ~Gbv_{256}. As shown in Fig. 2, ( r ⋆ ~Gau_{256} ) [i] is then combined

with ( r ⋆ ~Gbu_{256} ) [i], ( r ⋆ ~Gav_{256} ) [i], and ( r ⋆ ~Gbv_{256} ) [i] to obtain the estimated CIR. By adding ( r ⋆ ~Gau_{256} ) [i] and ( r ⋆ ~Gbu_{256} ) [i + 256], we have

R_{ru} [i] = K∑ k=1 h_kR_{su} [i − ⌈τ_k/T_c⌉] + ~z [i] , (10)

Fig. 2. Golay sequence based estimation for the k-th CIR component. z^{256} is the delay operator.

Fig. 3. The value of |R_{su} [i]|. We have i_p = 128 since ~Gau_{256} starts at the 128th element of s. A length-127 zero correlation zone can be clearly seen before and after the index of 128.

where ~z [i] is the noise after correlation operation and

R_{ru} [i] = ( r ⋆ ~Gau_{256} ) [i] + ( r ⋆ ~Gbu_{256} ) [i + 256] ,

R_{su} [i] = ( s ⋆ ~Gau_{256} ) [i] + ( s ⋆ ~Gbu_{256} ) [i + 256] . (11)

Clearly from Eq. (10), the value of R_{ru} [i] is closely related to that of R_{su} [i]. Let R_{sau} [i] = ( s ⋆ ~Gau_{256} ) [i], and R_{sbu} [i] = ( s ⋆ ~Gbu_{256} ) [i]. By exploiting the property of Golay sequences shown in Eq. (2), we have |R_{su} [i]| = |R_{sau} [i] + R_{sbu} [i + 256]| = { 512 i = 128 0 0 ≤ i ≤ 255, i ≠ 128 , (12)

From Eq. (12), |R_{su} [i]| has a peak at the index i_p = 128 where ~Gau_{256} aligns with ~Gau_{256} in s, and there is a length-127 zero-correlation zone before and after the peak. This matches the result in Fig. 3 well.

Noting that R_{su} [i − ⌈τ_k/T_c⌉] is a shifted version of R_{su} [i], |R_{su} [i − ⌈τ_k/T_c⌉]| has a peak at location i_p (k) = i_p + ⌈τ_k/T_c⌉. Without of loss generality, let us assume ⌈τ_k′ /T_c⌉ ≠ ⌈τ_k/T_c⌉ if k^′ ≠ k and |τ_K − τ_1| ≤ 128T_c. Then, if the noise is neglected, we get |R_{ru} [i_p + ⌈τ_k/T_c⌉]| = 512 |h_k|. In other words, we can recover the k-th CIR component by extracting the i_p + ⌈τ_k/T_c⌉th element in R_{ru} [i] through ^h^u_k =

R_{ru} [i_p + ⌈τ_k/T_c⌉]/512, where ^h^u_k represents the estimate of the k-th CIR component. Following the same procedure, we can obtain another estimate of the k-th CIR component, denoted as ^h^v_k, by correlating r [n] with ~Gav_{256} and ~Gbv_{256}. To reduce the impact of noise, we average ^h^u_k and ^h^v_k to obtain the final estimate for the k-th CIR component as ^h_k = ( ^hu_k + ^hv_k )/ 2. For ease of presentation, we assume the signal is transmitted with unit power in the above discussion. The effect of actual transmit power P_t can be easily incorporated by scaling h_k with a factor of √ P_t. In practice, the quality of the estimated CIR component ^h_k is affected by noise and other non-resolvable CIR components with respect to the k-th CIR component, which could, in turn, affect the performance of VAE-CIR. As mentioned in [16], the channel at 60GHz is inherently sparse with a few dominant paths. Thanks to the high transmission bandwidth, two CIR components can be resolved as long as the difference in their time of arrival is larger than 0.57ns. Thus, the impact of non-resovlable CIR components on ^h_k is expected to be limited if it corresponds to a dominant path. In Section IV, we will discuss how noise affects the performance of VAE-CIR and show that non-resolvable CIR components have only limited effect on VAE-CIR.

III. DESIGN OF VAE-CIR VAE-CIR addresses the problem of estimating the AOA/AOD of a specific dominant path, given a set of beamspecific CIR measurements. How to identify the dominant paths of a channel is out of the scope of VAE-CIR. As mentioned in [4], [5], the dominant paths of a channel can be identified by detecting and aggregating the peaks in the given set of beam-specific CIR measurements. Without loss of generality, we assume K dominant paths, indexed as {1, · · · , K}, are identified from the given set of beam-specific CIR measurements, and we are interested in the angular information of the κ-th (κ ∈ {1, · · · , K}) dominant path. For simplicity, we call the CIR component corresponding to the κ-th dominant path as the κ-th dominant CIR component.

As mentioned before, VAE-CIR exploits the CIR measured under different beams to infer the AOAs/AODs of dominant paths. These CIR measurements can be collected using, for example, sector sweep (SSW) frames during the sector-level sweep phase or a specific beam-sweeping process [3]–[5]. In general, the beam-sweeping is carried out in one or multiple stages. During each stage, one party fixes its beam pattern and the other party sweeps through different beams. For ease of presentation, we focus on AOA estimation in the following development and thus are interested in the case where the transmitter fixes its beam and the receiver receives the beam training frames, such as the SSW frames, with different beams. By following the procedure in [5], VAE-CIR presented in this section can also be applied in AOD inference using the transmitter-side beam sweeping. Suppose the receiver can sweep through a maximum of L beams, and thus we have the CIRs measured under L different beams. Let h_κ (l) be the value of the κ-th dominant CIR component when the l-th beam is used for reception. As shown in [4], [5], the estimate of h_κ (l), denoted as ^h_κ (l), can be extracted from the estimated CIR under the l-th receiving beam based on the time of arrival of the κ-th dominant path.

Let θ_κ be the AOA of the κ-th dominant path. To infer θ_κ from ^h_κ (l)’s, we need to draw a quantity from ^h_κ (l)’s so that it is determined solely by θ_κ. Clearly from Eq. (1), it is difficult to directly infer θ_κ from the amplitudes of h_κ (l)’s since they are also affected by many other factors, such as the path gain and the directional gain of the transmit beam. Notice that, when the transmit power and transmit beam pattern are fixed, h_κ (l)’s satisfy:

|h_κ (l_1)|/|h_κ (l_2)| = |G_{l1} (θ_κ)|/|G_{l2} (θ_κ)|. (13)

In other words, when the l_1-th and the l_2-th beams are used for reception, the ratio of |h_κ (l_1)| to |h_κ (l_2)| is completely determined by θ_κ. This observation leads us to use the ratio between | | |^hκ (l) | | |’s, instead of their absolute values, for AOA estimation.

Due to the very irregular beam pattern of 802.11ad devices, it is challenging to analytically derive the inverse function of |G_{l1} (θ_κ)|/|G_{l2} (θ_κ)| for AOA estimation. In view of Eq. (13), we address this challenge by searching for the direction which minimizes the difference between the left-hand and right-hand sides of Eq. (13). Specifically, given ^h_κ (l_1) and ^h_κ (l_2), we have

^θ_κ = arg min θ∈Θ | | | | | | |^hκ (l1) | | | | |^hκ (l2) | | | − |G_{l1} (θ)| |G_{l2} (θ)| | | | | | , (14)

where ^θ_κ is the estimated AOA of the κth dominant path, and Θ represents the search space. When new CIR measurements are available, we can combine them with ^h_κ (l_1) and ^h_κ (l_2) to refine our estimation, which leads to VAE-CIR.

To infer the AOA of the κ-th path, VAE-CIR maintains a score for each direction. VAE-CIR does not assume the order in which ^h_κ (1), · · · , ^h_κ (L) are used for updating the score, but, in this section, we assume they are sequentially used for score updating for ease of presentation. Let s^ℓ_κ (θ) be the score assigned to each direction based on ^h_κ (1), · · · , ^h_κ (ℓ). Observing that the score is updated based on the variation between different CIR measurements, we have s^1_κ (θ) = 0, ∀θ ∈ Θ. For ℓ ≥ 2, s^ℓ_κ (θ) can be obtained from s^{ℓ−1}_κ (θ) using ^h_κ (ℓ) as

s^ℓ_κ (θ)

= s^{ℓ−1}_κ (θ) + ∑ l∈L α (ℓ, l, κ, θ) × | | ||^{^hκ (ℓ)}| |^^hκ(l)| − |G_ℓ(θ_κ)| |G_l(θ_κ)| | | | L ≠ ∅, ℓ /∈ L s_κ (θ) otherwise , (15)

where L is the set of receiving beams used in the previous CIR measurement, and ∅ is an empty set. Initially, we have L = {1}. α (ℓ, l, κ, θ)’s are weight factors which allows us to

Algorithm 1 : VAE-CIR Input: ^h_κ (l), l ∈ {1, · · · , L}, G_l (θ), l ∈ {1, · · · , L}, θ ∈ Θ, Θ, ℏ Output: ^θ_κ 1: s^1_κ (θ) = 0, ∀θ ∈ Θ, L = {1} 2: for ℓ=2 to L do 3: for l ∈ L do 4: Determine α (ℓ, l, κ, θ) based on ^h_κ (ℓ), ^h_κ (l), and other information (e.g., ℏ in this paper) 5: end for 6: ∀θ ∈ Θ, update s^{ℓ−1}_κ (θ) to s^ℓ_κ (θ) according to Eq. (15) 7: L = L ∪ {ℓ} 8: end for 9: ^θ_κ = arg min θ∈Θ s^L_κ (θ)

weight the contribution of every two CIR measurements based on the corresponding beams, the considered direction, and the dominant path of interest. In this paper, we set α (ℓ, l, κ, θ) as 1 (| |^hκ (ℓ) | | | ≥ ℏ ) 1 (| |^hκ (l) | | | ≥ ℏ ) , where 1 (.) is the indicator function. ℏ is a threshold and can be set to, for example, ν | | |^h | | |^{max}_κ , where ν ∈ [0, 1], and | | |^h | | |^{max}_κ = max l∈{1,··· ,L} | | |^hκ (l) | | |. We adopt such weight factors since the value of | | |^hκ (l) | | | cannot be fully trusted when it is too small. On the one hand, the small | | |^hκ (l) | | | could be caused by either a low beamforming gain along θ_κ or an abrupt blockage of the κ-th dominant path. On the other hand, a small | | |^hκ (l) | | | is more susceptible to noise and might not be able to accurately track the variations in |h_κ (l)|. In other words, when either | |^h_κ (ℓ) | | or | |^h_κ (l) | | is small, the

variation in the beamforming gain along θ_κ might not be the major reason for the variation in | |ĥ_κ (ℓ) | |/ | |ĥ_κ (l) | |, and applying these | | |^hκ (l) | | |’s in AOA estimation could adversely affect the accuracy. Besides limiting the impact of small | | |^hκ (l) | | |’s, α (ℓ, l, κ, θ) also allows VAE-CIR to incorporate prior information. For example, if θ_κ is known to be within a direction range ~Θ, we can exploit such information for AOA estimation by assigning 1 to α (ℓ, l, κ, θ), ∀θ ∈ ~Θ, and 0 otherwise.

Once the updated score s^ℓ_κ (θ) is obtained, we update L as L = L ∪ {ℓ} . (16) After going through all L CIR measurements, VAE-CIR outputs the estimated AOA of the κ-th dominant path as

^θ_κ = arg min θ∈Θ s^L_κ (θ) . (17)

VAE-CIR is summarized in Algorithm 1.

Given ^θ_κ, we are interested in whether it is an accurate estimate of θ_κ. This information is helpful since it enables us to determine, for example, whether we should collect more beam-specific measurements to refine ^θ_κ. Without noise and non-resolvable multipath components, θ_κ should satisfies Eq. (13). Considering the potential impacts of noise and nonresolvable multipath components, we propose to determine if ^θ_κ is an accurate estimate of θ_κ through the following inequality: | | | | | | | |^hκ (l) | | | | |^hκ ( l )| | − | |G_l (θ) | | | G_l (θ) | | | | | | ≤ ε, (18)

where l = arg max l∈{L−1,L} ^h_κ (l), l = arg min l∈{L−1,L} ^h_κ (l), and ε ∈ [0, 1]

is a threshold. We use l and l, instead of L − 1 and L, in Eq. (18) so that we can employ the same ε no matter | | |^hκ (L − 1) | | | ≥ | | |^hκ (L) | | | or | | |^hκ (L) | | | ≥ | | |^hκ (L − 1) | | |. The effectiveness of this criterion will be evaluated in the next section using simulations.

IV. PERFORMANCE EVALUATION

A. Simulation Setup and Evaluation Methodology We now evaluate the performance of VAE-CIR based on beam patterns measured on the Dell D5000 docking station and the TP-Link Talon AD7200 router, which are off-the-shelf 60GHz devices with phased array antenna and beam sweeping implementation. The 32-beam patterns swept by D5000 docking stations for device discovery and the 35 default beams used by Talon routers are provided in [17] and [8]. In this evaluation, we process the measurement data in [17] and [8] so that the highest directional power gain among all beams of each device is 15dB. Our evaluation is conducted in a 4 × 3m room. The signal propagation in this environment follows the model suggested by the IEEE Task Group ad, which is validated by experimental results [18]. In this model, signal paths are generated by exploiting the clustering phenomenon in a 60GHz channel. Specifically, the first- and second-order reflections are first generated using ray-tracing techniques [19], and these paths are then blurred to generate path clusters. For each path identified via raytracing, a path cluster is generated by following the procedure (Section 3.7) and the parameter settings (Table 10) presented in [18]. Besides multipath propagation, the received signal is also affected by an additive Gaussian noise. We assume the CIRs are extracted from the SSW frames, and thus the preamble is generated according to the control PHY. Following [9], the signal is transmitted over a band with center frequency 60.48GHz and bandwidth 1760MHz. We are interested in the AOAs of dominant paths and thus consider a receive sector sweep where the transmitter transmits SSW frames using the same beam pattern while the receiver sweeps over a set of beams to receive these SSW frames. The STF and CE field of these SSW frames are generated through Golay sequences and modulated using π/2-BPSK according to the 802.11ad standard. Once the signal is received at the receiver, we implement the channel estimation presented in Section II to extract the beam-specific CIR measurements, which will

(a) Scenario A. (b) Scenario B. (c) CIR of Scenario A. (d) CIR of Scenario B.

Fig. 4. The considered scenarios and the CIR measured in these scenarios. Black blocks in the figure represent objects which could block and reflect the mmWave signals. (a) The transmitter locates at [−2, 0]. The receiver locates at [2, 0]. The three objects are characterized by (0.1, 1, 0.4, 0.2, 0^∘, 3.24), (−0.4, −1, 0.6, 0.2, 180^∘, 3.24), (0, 1.45, 0.6, 0.1, 0^∘, 3.24). (b) The transmitter locates at [−0.6, 1.4]. The receiver locates at [0.6, −1.4]. The three objects are characterized by (1.8, −0.2, 0.2, 0.6, 0^∘, 3.24), (−2, −0.5, 0.2, 0.5, 180^∘, 3.24), (−1.2, 0.8, 0.4, 0.4, 45^∘, 3.24). (c-d) The CIR measured in scenario A and B.

be used in VAE-CIR for AOA inference. It should be noted that the antenna arrays of the transmitter and the receiver are facing each other in our simulation.

In what follows, we will evaluate the performance of VAE-CIR based on the two scenarios shown in Figs. 4(a) and (b) where the transmitter and the receiver are characterized by their locations. We consider a coordinate system with the origin at the center of the room. The objects in the environment are characterized by six-element tuples where the first two elements record their locations, the next two elements present their length and width, the fifth element is their orientation, and the last one is their dielectric constant. The examples of beam-specific CIRs extracted from these two scenarios are shown in Figs. 4(c) and (d) where the receiver uses the 2nd beam measured on the D5000 docking station for reception and the transmitter adopts a quasi-omni pattern with a transmit power of 25dBm. The dielectric constant of the wall is set to 2 [20]. Form Figs. 4(c) and (d), we can observe 3 peaks in Scenario A and 2 peaks in Scenario B, which correspond to dominant paths in the environment. We will take the paths/peaks identified in Figs. 4(c) and (d) as examples to evaluate the performance of VAE-CIR.

B. Result and Analysis

Fig. 5 compares the probability of correct AOA estimation of VAE-CIR with those of existing schemes. For effective comparison, we consider the angular inference schemes in [4] and [5], which are referred to as “Rice” and “HP” in Fig. 5. Similar to VAE-CIR, both of these schemes assign scores to different directions by correlating beam-specific CIR measurements with the corresponding beams in use and infer angular information based on the final scores of different directions. However, unlike VAE-CIR, they exploit absolute beam-specific CIR measurements, instead of their variations under different beams, for score updating. Besides, these two schemes always assign larger score increments to the directions with higher directional power gain, instead of the directions offering better match between the variations in CIRs and the variations in directional gains. For VAE-CIR, the threshold ℏ in α (ℓ, l, κ, θ) is set to ν | |^h | |^{max}_κ , where ν = 0.1 and | | |^h | | |^{max}_κ = max l∈{1,··· ,L} | | |^hκ (l) | | |. In other words, | | |^hκ (l) | | | will

be used to infer θ_κ only if | | |^hκ (l) | | | ≥ 0.1 | | |^h | | |^{max}_κ . For the “Rice” scheme, the κ-th dominant CIR component is considered to be detected under the l-th beam if | | |^hκ (l) | | | ≥ μ | | |^h | | |^{max}_κ

[4]. For the “HP” scheme, the five | |^h_κ (l) | |’s with the highest

amplitudes are used for AOA inference and the estimated AOA is the center of the direction interval spanned by the five directions with highest final scores [5]. In Fig. 5, the estimated AOA ^θ_κ is considered to be accurate as long as | |^θ_κ − θ_κ | | ≤ ξ, where θ_κ is the true AOA of the κ-th path.

In our experiment, the signal is transmitted at a power of 25dBm using the quasi-omni pattern and propagates through a multipath channel illustrated in Section IV.A. We evaluate the performance of VAE-CIR by using the beam patterns measured on different off-the-shelf 802.11ad devices (Dell D5000 docking station and TP-Link Talon AD7200 router) as the receiving beam patterns swept by the receiver^1. Our following evaluations are based on those paths identified in Fig. 4. First, we investigate the performance of VAE-CIR in Scenario A and B with the beam patterns measured from the Dell D5000 docking station. In Fig. 5(a) and 5(b), we present the AOA estimation results for the first dominant paths in Scenario A and B with −30dBm noise in the channel. In Fig. 5(c) and 5(d), we are interested in the AOA of the third path in Scenario A and the AOA of the second path in Scenario B, where the channel noise is set to −40dBm and −45dBm, respectively. Then, we redo the experiment for the first paths in Scenario A and B, but, using the beam patterns measured from the Talon router. The obtained results are shown in Fig. 5(e) and 5(f) where the noise power is set to −40dBm. From Fig. 5, although the “Rice” and “HP” schemes achieve reasonable performance in a few cases, they do not performance well in other cases. In contrast, VAE-CIR can achieve good AOA estimation results in all these cases, which demonstrates its effectiveness and the limited impact of nonresovable CIR

1By viewing this receiver-side beam sweeping as the transmitter-side sweeping, our experiment can also be regarded as an evaluation of the AOD estimation performance of VAE-CIR [5].

(a) Scenario A, D5000, 1st path. (b) Scenario B, D5000, 1st path. (c) Scenario A, D5000, 3rd path.

(d) Scenario B, D5000, 2nd path. (e) Scenario A, Talon, 1st path. (f) Scenario B, Talon, 1st path.

Fig. 5. The probability of correct AOA estimation in different scenarios.

components on VAE-CIR. As shown in Fig. 5, the accuracy of the “Rice” scheme highly depends on the value of μ, and both the “Rice” and “HP” schemes do not perform well for the 3rd path in Scenario A and the 2nd path in Scenario B. All of these are resulted from their score updating mechanism. Based on the values of | |^hκ (l) | |’s, these schemes determine whether the corresponding beam patterns should be used for score increment. For each selected beam pattern, they assign higher score increment to the direction with higher directional power gain and thus are likely to output an accurate AOA estimation if the beams used for score updating have strong side lobes around the angle of interest. Clearly, if | | |^hκ (l) | | | is small, the l-th beam is unlikely to have strong side lobes along θ_κ. In this case, exploiting | | |^hκ (l) | | | and the l-th beam for score increment would lead to erroneous score increase along the direction around the strong side lobes of the lth beam. This explains why the performance of the “Rice” scheme degrades with a smaller μ. By examining the beam patterns of the D5000 docking station, we notice that most of its beams do not have strong side lobes around the AOAs of the 3rd path in Scenario A and the 2nd path in Scenario B, and thus the “Rice” and the “HP” schemes do not assign high enough score increments to the directions of interest, which eventually leads to inaccurate AOA estimation. In other words, since the “Rice” and the “HP” schemes select beam patterns for score increments based on the absolute values of | |^hκ (l) | |’s, which are not closely related to the direction of interest, their accuracy highly depends on the match between selected beam patterns and path directions. This observation further validates VAE-CIR which uses the variations in | | |^hκ (l) | | |’s, the quantities closely related to the direction of interest, for AOA estimation.

Then, we investigate how the performance of VAE-CIR is affected by the additive noise and the number of beams used for measurement. Similar to Fig. 5, we assume the signal is transmitted at 25dBm using the quasi-omni pattern, and ^θ_κ is considered to be accurate as long as | | |^θκ − θκ | | | ≤ 2. The noise power is set to the value shown in the legend of Fig. 6. The results shown in Fig. 6 are obtained based on the 32 beams of the Dell D5000 docking station. From Fig. 6, the accuracy of AOA estimation generally improves when more beams are available for beam-specific CIR collection. With more beam-specific measurements, we could make more informative decisions and thus improve the accuracy of the AOA estimation. It can be observed from Fig. 6 that more accurate angular inference can be achieved when there is less noise in the channel. Clearly from Section III, the accuracy of VAE-CIR depends on how accurately | |^h_κ (l) | | approximates |h_κ (l)|. The derivation in

Section II.B shows that | | |^hκ (l) | | | more accurately approximates |h_κ (l)| when there is less noise in the channel. This explains why the performance of VAE-CIR improves with noise power decreasing. The impact of noise also can be shown through the observation that VAE-CIR achieves different accuracy for different paths. For example, for the two paths identified in Fig. 4(d), we can achieve a higher probability of correct AOA estimation for the 1st path (shown in Fig. 6(b)). From 4(d), the dominant CIR component corresponding to the 1st path is

(a) Scenario A.

(b) Scenario B.

Fig. 6. The probability of correct AOA estimation v.s. additive noise and the number of beams used for CIR measurement.

much stronger than that corresponding to the 2nd path and thus is less susceptible to noise, which eventually leads to a higher probability of correct AOA estimation. This can be further corroborated by the results in Fig. 7 where we change ν from 0.1 to 0.5 and ^h_κ (l) will be used in score updating only when | | |^hκ (l) | | | ≥ 0.5 | | |^h | | |^{max}_κ . In so doing, weak | | |^hκ (l) | | |’s significantly distorted by noise are more likely to be excluded from AOA estimation, which reduces accumulation of noise effect and improves the probability of correct AOA estimation as shown in Fig. 7, particularly when a large number of beam-specific CIRs are used for angular inference. These observations also demonstrate the importance of introducing the weight factors α (ℓ, l, κ, θ)’s to VAE-CIR. It should be noted that a large ν will not always lead to a better performance since it might limit the number of CIR measurements exploited for AOA estimation. As shown in Fig. 6, in this case, we might not be able to accurately estimate the AOAs due to limited information. In practice, the value of ν should be carefully selected. How to choose the optimal ν is out of the scope this paper and will be left for future work.

Finally, we evaluate if the criterion introduced at the end of Section III can correctly determine if ^θ_κ is an accurate estimate of θ_κ. Specifically, we redo the simulation in Fig. 6 with ν = 0.1 and the 32 beams of the D5000 docking station. Similar to Fig. 6, ^θ_κ is considered to be an accurate

Fig. 7. The probability of correct AOA estimation v.s. weight factors.

TABLE I THE PERFORMANCE OF THE CRITERION IN EQ. (18)

Path

Metric −45dBm −50dBm P_F P_D P_F P_D Scenario A, 1st 0% 100% 0% 100% Scenario A, 2nd 0% 99% 0% 99% Scenario A, 3rd 2% 100% 1% 100% Scenario B, 1st 0% 100% 0% 100% Scenario B, 2nd 8.43% 91.57% 1.06% 98.94%

estimate of θ_κ if | |^θκ − θκ | | ≤ 2. Each time VAE-CIR outputs an estimated AOA, ^θ_κ, we check if Eq. (18) is valid, with ε set to 0.3 to account for the potential impact of noise. If the inequality is valid, the criterion determines ^θ_κ to be an accurate estimate of θ_κ. The decisions being made is then compared to the ground truth. The results are shown in Table I where P_F is the percentage that the proposed criterion misclassifies ^θ_κ as an accurate estimate of θ_κ and P_D is the percentage that the proposed criterion correctly identify ^θ_κ as an accurate estimate of θ_κ. From Table I, the criterion in Eq. (18) can accurately determine if ^θ_κ is an accurate estimate of θ_κ. As demonstrated in Fig. 4(d), the 2nd path in Scenario B is weaker than the 1st path. Hence, for the two paths in Scenario B, the criterion in Eq. (18) is more susceptible to noise and thus less accurate when applied to the 2nd path.

V. CONCLUSION

In this paper, we propose an angle estimation scheme, called VAE-CIR, for 802.11ad devices by exploiting beamspecific CIR measurements. Unlike existing work, we exploit the variations between the CIRs measured under different beams, instead of their absolute values, for angle estimation. To evaluate the performance of VAE-CIR, we simulate the beam sweeping operation of 802.11ad devices with beam patterns measured on off-the-shelf 802.11ad devices and the ray-tracing based channel generation. Our experimental results show that VAE-CIR can enable accurate angular inference for 802.11ad devices and demonstrate its superiority to existing schemes. We expect VAE-CIR to enable various applications, such as link performance prediction and device tracking, on

802.11ad devices when combined with other proposals for 60GHz networking.

REFERENCES

[1] T. Wei, A. Zhou, and X. Zhang, “Facilitating robust 60 ghz network deployment by sensing ambient reflectors,” in Proceedings of the 14th USENIX Symposium on Networked Systems Design and Implementation (NSDI 17), Mar. 2017, pp. 213–226.

[2] S. Sur, I. Pefkianakis, X. Zhang, and K.-H. Kim, “Towards scalable and ubiquitous millimeter-wave wireless networks,” in Proceedings of the 24th Annual International Conference on Mobile Computing and Networking (MobiCom 2018). ACM, Oct. 2018, pp. 257–271.

[3] A. Zhou, X. Zhang, and H. Ma, “Beam-forecast: Facilitating mobile 60 ghz networks via model-driven beam steering,” in Proceedings of the 2017 IEEE Conference on Computer Communications (INFOCOM 2017). IEEE, May 2017, pp. 1–9.

[4] Y. Ghasempour, M. K. Haider, C. Cordeiro, D. Koutsonikolas, and E. Knightly, “Multi-stream beam-training for mmwave mimo networks,” in Proceedings of the 24th Annual International Conference on Mobile Computing and Networking (MobiCom 2018). ACM, Oct. 2018, pp. 225–239.

[5] I. Pefkianakis and K.-H. Kim, “Accurate 3d localization for 60 ghz networks,” in Proceedings of the 16th ACM Conference on Embedded Networked Sensor Systems (SenSys 18). ACM, Nov. 2018, pp. 120–131.

[6] S. Sur, I. Pefkianakis, X. Zhang, and K.-H. Kim, “Wifi-assisted 60 ghz wireless networks,” in Proceedings of the 23rd Annual International Conference on Mobile Computing and Networking (MobiCom 2017). ACM, Oct. 2017, pp. 28–41.

[7] K. Hosoya, N. Prasad, K. Ramachandran, N. Orihashi, S. Kishimoto, S. Rangarajan, and K. Maruhashi, “Multiple sector id capture (midc): A novel beamforming technique for 60-ghz band multi-gbps wlan/pan systems,” IEEE Trans. Antennas Propag., vol. 63, no. 1, pp. 81–96, Jan. 2015.

[8] D. Steinmetzer, D. Wegemer, M. Schulz, J. Widmer, and M. Hollick, “Compressive millimeter-wave sector selection in off-the-shelf ieee 802.1 lad devices,” in Proceedings of the 13th International Conference on emerging Networking EXperiments and Technologies (CoNEXT 2017). ACM, Dec. 2017, pp. 414–425.

[9] IEEE 802.11 Working Group, IEEE Standards 802.11ad-2012, Amendment 3: Enhancements for Very High Throughput in the 60 GHz Band, Std., Oct. 2012.

[10] I. Ahmed, H. Khammari, A. Shahid, A. Musa, K. S. Kim, E. De Poorter, and I. Moerman, “A survey on hybrid beamforming techniques in 5g: Architecture and system model perspectives,” IEEE Commun. Surveys Tuts., vol. 20, no. 4, pp. 3060–3097, Fourthquarter 2018.

[11] A. Goldsmith, Wireless communications. Cambridge university press, 2005.

[12] K. V. Mishra and Y. C. Eldar, “Sub-nyquist channel estimation over ieee 802.11 ad link,” in Proceedings of 2017 International Conference on Sampling Theory and Applications (SampTA). IEEE, 2017, pp. 355–359.

[13] W.-C. Liu, F.-C. Yeh, T.-C. Wei, C.-D. Chan, and S.-J. Jou, “A digital golay-mpic time domain equalizer for sc/ofdm dual-modes at 60 ghz band,” IEEE Trans. Circuits Syst. I, Reg. Papers, vol. 60, no. 10, pp. 2730–2739, Oct. 2013.

[14] S.-K. Yong, P. Xia, and A. Valdes-Garcia, 60GHz Technology for Gbps WLAN and WPAN: from Theory to Practice. John Wiley & Sons, 2011.

[15] A. V. Oppenheim, A. S. Willsky, and S. H. Nawab, Signals and Systems (2nd Edition). Prentice-Hall, 1997.

[16] S. Sur, V. Venkateswaran, X. Zhang, and P. Ramanathan, “60 ghz indoor networking through flexible beams: A link-level profiling,” in Proceedings of the 2015 ACM SIGMETRICS International Conference on Measurement and Modeling of Computer Systems (SIGMETRICS 2015). ACM, Jun. 2015, pp. 71–84.

[17] G. Bielsa, A. Loch, I. Tejado, T. Nitsche, and J. Widmer, “60 ghz networking: Mobility, beamforming, and frame level operation from theory to practice,” IEEE Trans. Mobile Comput., to be published 2018.

[18] IEEE P802.11 – TASK GROUP AD, “Channel models for 60 ghz wlan systems,” Tech. Rep., May 2010.

[19] D. Steinmetzer, J. Classen, and M. Hollick, “mmtrace: Modeling millimeter-wave indoor propagation with image-based ray-tracing,” in Proceedings of 2016 IEEE Conference on Computer Communications Workshops (INFOCOM WKSHPS). IEEE, Apr. 2016, pp. 429–434.

[20] E. De Groot, T. Bose, C. Cooper, and M. Kruse, “Remote transmitter tracking with raytraced fingerprint database,” in Proceedings of 2014 IEEE Military Communications Conference (MILCOM 2014). IEEE, Oct. 2014, pp. 325–328.