arXiv:2009.12320v1 [eess.SP] 25 Sep 2020

Novel Visible Light Communication Assisted Perspective-Four-Line Algorithm for Indoor Localization

Lin Bai

Abstract

In this paper, we propose a novel visible light communication (VLC) assisted Perspective-four- Line algorithm (V-P4L) for practical indoor localization. The basic idea of V-P4L is to joint VLC and computer vision to achieve high accuracy regardless of LED height differences. In particular, we first exploit the space-domain information to estimate the orientation and coordinate of a single rectangular LED luminaire in the camera coordinate system based on the plane and solid geometry. Then, based on the time-domain information transmitted by VLC and the estimated luminaire information, V-P4L can estimate the position and pose of the camera by the single-view geometry theory and the linear least square (LLS) method. To further mitigate the effect of height differences among LEDs on localization accuracy, we then propose a correction algorithm of V-P4L based on the LLS method and a simple optimization method. Due to the combination of time- and space-domain information, V-P4L only requires a single luminaire for localization without limitation on the correspondences between the features and their projections. Simulation results show that for V-P4L the position error is always less than 15 cm and the orientation error is always less than 3^∘ using popular indoor luminaires.

Index Terms

Camera, computer vision based localization, Perspective-n-Line (PnL), visible light positioning.

L. Bai is with the Beijing Key Laboratory of Network System Architecture and Convergence, School of Information and Communication Engineering, Beijing University of Posts and Telecommunications, Beijing 100876, China (e-mail: bailin2126@bupt.edu.cn).

I. INTRODUCTION Accurate indoor localization is increasingly important due to the surging position based services such as position tracking, navigation and robot movement control. In this research field, visible light positioning (VLP) technologies and computer vision based localization have the advantage of high accuracy and low cost. Visible light positioning technologies exploit visible light signals for determining the position of the receiver. Visible light possesses strong directionality and low multipath interference, and thus VLP can achieve high accuracy localization performance [1]–[3]. Additionally, VLP utilizes light-emitting diodes (LEDs) as transmitter. Benefited from the increasing market share of LEDs, VLP has relatively low cost on infrastructure [1], [4]. On the other hand, computer vision based localization relies on the images of the reference features captured by cameras to estimate the position and pose of cameras with high accuracy [5], [6]. Cameras can provide an extensive amount of information at limited power consumption, small size and reasonable cost [6]. Additionally, nowadays cameras are essential parts of smartphones, which further corroborates the feasibility of vision based localization technologies [7]. Therefore, VLP and computer vision based localization have been gained increasing attentions in recent years [7], [8].

Typical VLP algorithms include proximity [9], fingerprinting [10], time of arrival (TOA) [11], angle of arrival (AOA) [12], received signal strength (RSS) [13]–[16] and image sensing [17]. Proximity and fingerprinting cannot estimate the receiver pose even though only a single luminaire is required. Additionally, the accuracy of proximity is insufficient [13] while fingerprinting requires at least three luminaires to reduce the effect of ambiguity issues [18]. Among these VLP algorithms, RSS algorithms are most widely-used due to their high accuracy and low cost [13]. However, RSS algorithms require multiple luminaires for localization, like image sensing, TOA and AOA algorithms [7]. Moreover, RSS algorithms rely on accurate channel model, which is challenging to be achieved in practice. A popular assumption in RSS algorithms is that the radiation pattern of LEDs is the Lambertian model which may not be true for many luminaires especially when a lampshade is used [19]. Meanwhile, the estimated channel gain is affected by sunlight, dust and shadowing in practice [20], [21]. Therefore, the feasibility of RSS algorithms is limited.

On the other hand, typical computer vision based localization methods include Perspective-n- Line (PnL) and Perspective-n-Point (PnP). The methods are usually performed by analyzing n correspondences between three dimensional (3D) reference features and their two dimensional (2D) projections on the image (i.e., 3D-2D correspondences), where the features are either points or lines [22]. In particular, PnP methods employ the point features, while PnL methods employ the line features. Compared with the point features, line features can carry richer information [22]. Therefore, compared with PnP methods, PnL methods can achieve higher detection accuracy and are more robust to occlusions [23], [24]. However, PnL methods need 3D-2D correspondences which are difficult to obtain. In existing PnL studies, the 3D-2D correspondences assumed to be perfectly known in advance [22], [25], which is impractical in practice [8]. To circumvent this challenge, the work in [8] proposed a method to find the 3D-2D correspondences for the scenario where the number of the vertical lines are more than that of horizontal lines. However, this method cannot be applied to the scenario where there is no significant difference between the numbers of horizontal and vertical lines, such as the scenario where the rectangular beacons are deployed on the ceiling. Therefore, the feasibility of the method is constrained.

The main contribution of this paper is a novel visible light communication (VLC) assisted Perspective-four-Line algorithm (V-P4L), which can achieve feasible and accurate indoor localization. To the authors’ best knowledge, this is the first localization algorithm that only requires a single luminaire^1 for position and pose estimation without given 3D-2D correspondence. The key contributions of this paper include:

• We propose an indoor localization algorithm termed as V-P4L, which uses camera to simultaneously capture the information in time and space domains of LEDs to achieve high feasibility and high accuracy. Based on the plane and solid geometry theory, V-P4L estimates the luminaire’s information in the camera coordinate system first using the space-

1All the LEDs in the luminaire transmit the same information for ease of implementation. Note that the proposed algorithm can also be implemented when LEDs in the luminaire transmit different information. In this case, the 3D-2D correspondence can be obtained directly from the different information. However, this requires higher implementation complexity and the robustness of the link may be affected by inter-channel-interference. Therefore, in this work, we adopt the former strategy for higher robustness and lower complexity.

domain information of LEDs. Then, based on the single-view geometry theory and the time-domain information of LEDs, V-P4L can estimate the pose and position of the camera exploiting the luminaire’s information in different coordinate systems. In this way, V-P4L can estimate the position and pose of the receiver only using a single luminaire.

• To avoid the requirement of the 3D-2D correspondences, the time-domain information transmitted by VLC and the linear least square (LLS) method are exploited in V-P4L to properly match 3D-2D correspondences. Based on the time-domain information, V-P4L can obtain the information of LEDs in the world coordinate. Then, based on the LLS method and the LEDs’ information in different coordinate systems, the 3D-2D correspondences can be properly matched. In this way, V-P4L can achieve high feasibility.

• To further improve the feasibility of V-P4L, we then propose a correction algorithm for V-P4L to correct for the scenarios with LED height differences based on the information in both time and space domains. When LEDs have different heights, based on the single-view geometry theory and the LLS method, the correction algorithm can first estimate the pose and 2D position of the camera, and then based on the single-view geometry theory and a simple optimization method, the correction algorithm can estimate the 3D position of the camera. In this way, V-P4L can be used regardless of the height differences among LEDs.

Simulation results show that for V-P4L the position error is always less than 15 cm and the orientation error is always less than 3^∘ using popular indoor luminaires.

The rest of the paper is organized as follows. Section II introduces the system model. Section III calculates the luminaire information in the camera coordinate system. The proposed basic algorithm of V-P4L is detailed in Section IV, and the proposed correction algorithm is detailed in Section V. Simulation results are presented in Section VI. Finally, the paper is concluded in Section VII.

The following notations are used throughout the paper: A and a with or without subscript denote scalars; v denotes a column vector and A stands for a matrix; |A| denotes the absolute value of A; A^T, A^{−1}, det (A) and ‖A‖_2 indicate the transpose, inverse, determinant and Eculidean norm of A, respectively; v × u denotes the cross product of v and u; v · u, A · v and AB denotes the dot products of v and u, A and v, and A and B, respectively; Â, Â and v̂ represent the estimate of A, A and v, respectively. In addition, there are some special or important symbols used throughout in this paper, which are listed in Table I with their meaning. In particular, P with subscript denotes the 3D vertex of the LED luminaire; p with subscript denotes the 2D point on the image plane; L with subscript represents the 3D line; l with subscript represents the 2D line on the image plane. We use subscript to represent the indices or objects that the scalars, points, vectors and matrices corresponding to. For example, P_i denotes the ith vertex of the luminaire, and ρ_{lij} denotes a parameter in the equation of l_{ij}. Furthermore, we use the superscript to represent the coordinates of points and vectors in different coordinate systems. For example, the coordinates of the 2D point p_i in the world, camera, image and pixel coordinates are denoted as p^w_i , p^c_i , p^i and p^p_i , respectively.

II. SYSTEM MODEL The system diagram is illustrated in Fig. 1. Four coordinate systems are utilized for localization, which are the pixel coordinate system (PCS) o^p − u^pv^p on the image plane^2, the image coordinate system (ICS) o^i − x^iy^i on the image plane, the camera coordinate system (CCS) o^c − x^cy^cz^c and the world coordinate system (WCS) o^w − x^wy^wz^w. In PCS, ICS and CCS, the axes u^p, x^i and x^c are parallel to each other and, similarly, v^p, y^i and y^c are also parallel to each other. Additionally, o^p is at the upper left corner of the image plane and o^i is at the center of the image plane. Moreover, o^i is termed as the principal point, whose pixel coordinate is (u_0, v_0)^T. In contrast, o^c is termed as the camera optical center. Furthermore, o^i and o^c are on the optical axis. The distance between o^c and o^i is the focal length f, and thus the z-coordinate of the image plane in CCS is z^c = f.

A VLC-enabled rectangular LED luminaire is constructed by four vertices P_i (i ∈ {1, 2, 3, 4}) mounted on the ceiling. The four 3D reference lines L_{ij} (i, j ∈ {1, 2, 3, 4} , i ≠ j) are the edges of the luminaire. In addition, P^w_i = (x^w_i , y^w_i , z^w_i )^T is the world coordinate of the ith vertex of

2As shown in Fig. 1, the image plane is a virtual plane. In this paper, the camera is a standard pinhole camera. The actual image plane is behind the camera optical center (i.e., the pinhole), o^c. To show the geometric relations more clearly, the virtual image plane is set up in front of o^c as done in many papers [26], [27]. In particular, the virtual image plane and the actual image plane are centrally symmetric, and o^c is the center of symmetry.

TABLE I SYMBOLS AND THEIR MEANING.

Symbol Meaning (u_0, v_0)^T Pixel coordinate of o^i f Focal length f_u, f_v Focal ratios d_x, d_y Physical size of each pixel

P_i The ith vertex of the luminaire p_i Projection of P_i on the image plane p^p_i /p^i Pixel/Image coordinate of p_i P^c_i /P^w_i Camera/World coordinate of P_i

L_{ij} 3D reference line connecting P_i and P_j l_{ij} 2D projection of L_{ij} on the image plane n^c_{Lij} Direction vector of L_{ij} in CCS ϕ_{lij} Rotate angle from y^i-axis to l_{ij} in anticlockwise direction ρ_{lij} Distance from o^i to l_{ij} n^w_{LED}/n^c_{LED} Normal vector of the luminaire in WCS/CCS Π_{ij} Lateral face determined by the vertices P_i, P_j and o^c n^c_{Πij} Normal vector of Π_{ij} in CCS

S Area of the luminaire H Distance from o^c to the luminaire V Volume of rectangular pyramid o^c − P_1P_2P_3P_4 V_i Volume of triangular pyramid o^c − P_iP_jP_k φ, θ, ψ Euler angles corresponding to the x^c−axis, y^c−axis and z^c−axis R^w_c /t^w_c Pose/Position of the camera in WCS

the luminaire, which is assumed to be known at the transmitter and can be transmitted by VLC

as the time-domain information [3], [4]. Moreover, the unit normal vector of the luminaire in

WCS, n^w_{LED}, can be calculated by the world coordinates of the luminaire’s vertices.

On the other hand, the receiver is a standard pinhole camera which is not coplanar with

the luminaire. Therefore, the transmitter and the receiver produced a rectangular pyramid o^c −

P_1P_2P_3P_4 which contains many space-domain information. In the rectangular pyramid o^c −

P_1P_2P_3P_4, the rectangle P_1P_2P_3P_4 is called the base face. Meanwhile, we define Π_{ij} as the

lateral face determined by the vertices P_i, P_j (i, j ∈ {1, 2, 3, 4} , i ≠ j) and o^c. In addition, P_i is

the ith vertex and o^c is called the apex. In the camera, p_i is the projection of P_i on the image plane. Moreover, l_{ij} is the 2D projection on the image plane of L_{ij} . Note that many existing PnL algorithms assume that the 3D-2D correspondences (L_{ij} ⇐⇒ l_{ij} ) are known in advance, which is too ideal in practice [8]. In contrast, in this work, the 3D-2D correspondences are unknown. To estimate the pose and position of the receiver without the 3D-2D correspondences, the camera is used to simultaneously capture the time- and space-domain information.

The pixel coordinate of p_i is denoted by p^p_i = (u^p_i , v^p_i )^T, and this coordinate can be obtained by the camera through image processing [17]. Based on the single-view geometry theory, the image coordinate of p_i, p^i = ( x^i, y^i

)_T

, can be obtained as follows:

p^i = d_x d_y p^p_i − u_0d_x v_0d_y , (1)

where d_x and d_y are the physical size of each pixel in the x and y directions on the image plane, respectively. The camera’s intrinsic parameters, including (u_0, v_0)^T and the focal ratio f_u =^f_{dx} and f_v =^f_{dy} , can be calibrated in advance [13]. The transformation from CCS to WCS can be expressed as follows [22]:

P^w = R^w_c · P^c + t^w_c , (2)

where P^w and P^c are the world and camera coordinates of the same object, respectively. In addition, R^w_c and t^w_c ∈ R^3 denote the pose and the position of the camera in WCS, respectively. The task of the localization is to find out R^w_c and t^w_c . III. CALCULATING THE LUMINAIRE INFORMATION IN CCS In this section, the information of the luminaire in CCS, including its normal vector n^c_{LED} and its vertices’ coordinates P^c_i , i ∈ {1, 2, 3, 4}, is calculated based on the space-domain information in two steps. In the first step, n^c_{LED} is estimated based on the plane and solid geometry theory. Then, based on n^c_{LED}, P^c_i , i ∈ {1, 2, 3, 4} are estimated by the solid geometry theory. A. The Normal Vector Of The Luminaire In CCS

In ICS, the point-normal form equation of a given l_{ij} can be expressed as [25]:

x^i cos ϕ_{lij} + y^i sin ϕ_{lij} = ρ_{lij} , (3)

Fig. 1. The system diagram of the proposed algorithm.

where ( x^i, y^i

)_T is the image coordinate of a point on l_{ij} which can be obtained by the single-view geometry theory , ϕ_{lij} is the rotate angle from y^i-axis to l_{ij} in anticlockwise direction, and ρ_{lij} is the distance from o^i to l_{ij} . Since p_i and p_j are on l_{ij} , ϕ_{lij} and ρ_{lij} can be obtained based on the image coordinates of p_i and p_j. From (2), there are two points whose image coordinates are p^i_{lij ,1} = (_{ρlij} cos ϕ_{lij} , 0

)_T and p^i_{lij ,2} = ( 0,^{ρlij}_{sin ϕlij} )_T are on l_{ij}. Since the two points are also on the image plane, their camera coordinates are p^c_{lij ,1} = (_{ρlij} cos ϕ_{lij} , 0, f )_T and p^c_{lij ,2} = ( 0,^{ρlij}_{sin ϕlij} , f )_T . Since the two points and o^c = (0, 0, 0)^T are on Π_{ij} , we can represent Π_{ij} in CCS in the general form as:

A_{Πij} x^c + B_{Πij} y^c + C_{Πij} z^c = 0, (4)

where A_{Πij} = f cos ϕ_{lij} , B_{Πij} = f sin ϕ_{lij} and C_{Πij} = −ρ_{lij} .

In CCS, the general form equation of the rectangle P_1P_2P_3P_4 can be expressed as:

A_{LED}x^c + B_{LED}y^c + C_{LED}z^c = 1, (5)

where A_{LED}, B_{LED} and C_{LED} are unknown constants. From (5), the normal vector of the rectangle P_1P_2P_3P_4 can be expressed by (A_{LED}, B_{LED}, C_{LED})^T. In CCS, let n^c_{Πij} = ( A_{Πij} , B_{Πij} , C_{Πij} )_T

(i, j ∈ {1, 2, 3, 4} , i ≠ j) denotes the normal vector of Π_{ij} and v^c_{Lij} ∈ R^3 (i, j ∈ {1, 2, 3, 4} , i ≠ j) denotes the direction vector of L_{ij}. Since L_{ij} is the intersection line of the rectangle P_1P_2P_3P_4 and Π_{ij} , v^c_{Lij} can be calculated as v^c_{Lij} = (A_{LED}, B_{LED}, C_{LED})^T × n^c_{Πij} . Based on the solid geometry, we have: v^c_{L34} · n^c_{Π12} = 0 v^c_{L41} · n^c_{Π23} = 0. (6)

Define m =^{ALED}_{CLED} and n =^{BLED}_{CLED} , and we can obtain m and n as the functions of A_{Πij} , B_{Πij} and C_{Πij} by solving (6). Therefore, the normalized normal vector of the rectangle P_1P_2P_3P_4 (i.e., the orientation of the luminaire) in CCS can be expressed as:

n^c_{LED} = (cos α, cos β, cos γ)^T , (7)

where: cos α =^{m√}_{m2+n2+1} cos β =^{n√}_{m2+n2+1} cos γ =^{1√}_{m2+n2+1} . (8)

B. Camera Coordinates Of The Luminaire’s Vertices

Since P_1 is the intersection point of the rectangle P_1P_2P_3P_4, Π_{12} and Π_{41}, its camera coordinate can be calculated as P^c_1 =^{MP1}_{CLED} , where:

M_{P1} = m n 1 A_{Π12} B_{Π12} C_{Π12} A_{Π41} B_{Π41} C_{Π41}

−1 · 1 0 0 . (9)

The other three M_{Pi} (i ∈ {2, 3, 4}) can be calculated in the similar method of (9). In general, the camera coordinate P^c_i (i ∈ {1, 2, 3, 4}) can be calculated as follows:

P^c_i = M_{Pi} C_{LED}

. (10)

From (10), we can observe that P^c_i can be represented according to C_{LED}. Next, we will calculate C_{LED} based on the solid geometry.

The volume of the rectangular pyramid o^c − P_1P_2P_3P_4 can be calculates as V =^1_3 SH, where S is the area of the luminaire and is known in advance. Additionally, H =^1_{CLED}^√_{m2+n2+1} is the distance from o^c to the rectangle P_1P_2P_3P_4. For the triangular pyramid o^c − P_1P_2P_3, its volume can be calculated as follows: V_1 = 1 6 |det(M_{V1} )| , (11)

where M_{V1} = [P^c_1 , P^c_2 , P^c_3 ]^T. Substituting (10) into (11), we have V_1 =^{q1}_{C3LED} , where q_1 = 1 6 |det(M_{q1} )|, where M_{q1} = [M_{P1} , M_{P2} , M_{P3} ]^T. The volumes of the other three triangular pyramid o^c − P_2P_3P_4, o^c − P_3P_4P_1 and o^c − P_4P_1P_2, denoted by V_2, V_3 and V_4, respectively, can be obtained in the same way. Since V =^1_2

∑_4 i=1 V_i, C_{LED} can be calculated as follows:

C_{LED} = √ 3 ∑_4 i=1 q_i · √ m^2 + n^2 + 1 2S . (12)

Substituting (12) into (10), P^c_i (i ∈ {1, 2, 3, 4}) can be obtained. IV. THE BASIC ALGORITHM OF V-P4L In this section, the basic algorithm of V-P4L is proposed for scenarios where LEDs have the same height. The basic algorithm of V-P4L contains three steps. In the first step, based on the orientation information of the luminaire estimated in Section III, the rotation angles corresponding to the x^c−axis and y^c−axis can be obtained by the single-view geometry theory. Then, based on the LLS method and the single-view geometry theory, the basic algorithm of V- P4L can properly match the 3D-2D correspondences, and obtain the rotation angles corresponding to the z^c−axis and the 2D coordinate of the camera. Finally, based on the single-view geometry theory, V-P4L can estimate the z-coordinate of the camera.

A. Calculate the rotation angles corresponding to the x^c−axis and y^c−axis

Let R_X , R_Y and R_Z denote the rotation matrices of WCS along the x^c−axis, y^c−axis and z^c−axis, respectively. Given R_X , R_Y and R_Z as follows [28]:

R_X =

1 0 0 0 cos φ − sin φ 0 sin φ cos φ

, (13)

R_Y = cos θ 0 sin θ 0 1 0 − sin θ 0 cos θ

, (14)

and

R_Z = cos ψ − sin ψ 0 sin ψ cos ψ 0 0 0 1

, (15)

where φ ∈ ( −^π_2 ,^π_2 ] , θ ∈ ( −^π_2 ,^π_2 ] and ψ ∈ (−π, π] are the unknown Euler angles corresponding to the x^c−axis, y^c−axis and z^c−axis, respectively, the rotation matrix R^w_c from CCS to WCS can be given as [28]:

R^w_c = R_Z R_Y R_X . (16)

In this section, the basic algorithm of V-P4L is proposed for scenarios where LEDs have the same height. Therefore, the normal vector of the luminaire can be denoted by n^w_{LED} = (0, 0, 1)^T. Based on the single-view geometry theory, the relationship between n^w_{LED} = (0, 0, 1)^T and n^c_{LED} = (cos α, cos β, cos γ)^T can be given as [22]:

n^w_{LED} = R^w_c · n^c_{LED}. (17)

Therefore, we have: cos α = − sin θ cos β = cos θ · sin φ cos γ = cos θ · cos φ.

(18)

The estimated rotation angles φ̂ and θ̂ can be obtained by solving (18).

B. Calculate the rotation angles corresponding to the z^c−axis and the 2D coordinate of the camera

Based on the single-view geometry theory, the relationship between P^c_i (i ∈ {1, 2, 3, 4}) and P^w_i = (x^w_i , y^w_i , z^w_i )^T can be given as [22]:

P^w_i = R^w_c · P^c_i + t^w_c , (19)

where P^w_i is known in advance and can be obtained by the camera as the time-domain information. In addition, P^c_i is the space-domain information that is estimated in Subsection III-B. Moreover, t^w_c = (t_x, t_y, t_z)^T is the 3D world coordinate of the camera. In (19), there are four unknown parameters ψ, t_x, t_y and t_z. If the 3D-2D correspondences are known in advance, we can easily obtain the four unknown parameters with the four vertices’ world and camera coordinates. However, as analyzed in Section I, the 3D-2D correspondences are unknown for practical considerations. In this paper, we can calculate these parameters based on the LEDs’ information in both time and space domains. For mathematical analysis, we define:

R_Y R_X = cos θ sin θ · sin φ sin θ · cos φ 0 cos φ − sin φ − sin θ cos θ · sin φ cos θ · cos φ = a_1 a_2 a_3 b_1 b_2 b_3 c_1 c_2 c_3

, (20) and thus we can rewrite (19) as follows:

P^w_i = cos ψ − sin ψ 0 sin ψ cos ψ 0 0 0 1 · a_1 a_2 a_3 b_1 b_2 b_3 c_1 c_2 c_3

· P^c_i + t^w_c . (21)

The three unknown parameters ψ, t_x and t_y in (21) can be calculated by the LLS estimator, which can be expressed in a matrix form as follows:

A_{rs} · x = b_{ij} , (22)

where A_{rs} = [A_r; A_s] and b_{ij} = [b_i; b_j] (r, s, i, j ∈ {1, 2, 3, 4} , i ≠ j, r ≠ s), where:

A_r =

[a_1, a_2, a_3]^T · P^c_r − [b_1, b_2, b_3]^T · P^c_r 1 0 [b_1, b_2, b_3]^T · P^c_r [a_1, a_2, a_3]^T · P^c_r 0 1 (r ∈ {1, 2, 3, 4}), (23)

x = [cos ψ, sin ψ, t_x, t_y]^T , (24) and b_i = [x^w_i , y^w_i ]^T (i ∈ {1, 2, 3, 4}). (25)

Therefore, the unknown parameters can be given by:

x̂ = (A^T_{rs} A_{rs} )^{−1}A^T_{rs} b_{ij} , (26)

where x̂ = [ ĉos ψ, ŝin ψ, t̂_x, t̂_y ]_T

is the estimate of x.

Since the 3D-2D correspondences are not known in advance, given a certain A_{rs} and b_{ij} (r, s, i, j ∈ {1, 2, 3, 4} , r ≠ s, i ≠ j), we cannot obtain their exact correspondence relationship. Fortunately, there are four A_r (r ∈ {1, 2, 3, 4}) and b_i (i ∈ {1, 2, 3, 4}), and that means there are only C^2_4 = 6 different A_{rs} and b_{ij} (r, s, i, j ∈ {1, 2, 3, 4} , r ≠ s, i ≠ j). Therefore, for each b_{ij} = [b_i, b_j]^T (i, j ∈ {1, 2, 3, 4}, i ≠ j), we can obtain 6 candidate solutions corresponding to 6 A_{rs} (r, s ∈ {1, 2, 3, 4} , r ≠ s), and one of which is x̂_{ij} , where x̂_{ij} represents the exact x̂ corresponding to b_{ij} . Therefore, we can obtain total 36 solutions which can further be separated into 6 groups according to 6 different b_{ij} . To obtain a reasonable solution, here we propose a strategy that estimates x̂ by averaging the 6 closest solutions (i.e., 6 x̂_{ij} ) in the 6 groups of solutions, which can be expressed as follows:

x̂ = 1 6 4∑ i=1 4∑ j=1,j>i x̂_{ij}. (27)

This strategy will be verified in simulations. In this way, based on the information in both time and space domains, the basic algorithm of V-P4L can properly match the 3D-2D correspondences, and obtain the rotation angles corresponding to the z^c−axis ψ and the 2D coordinate of the camera (t_x, t_y)^T.

C. Calculate the z-coordinate of the camera

In Subsection IV-B, we have obtained ψ and (t_x, t_y)^T. In (21), there is still one unknown parameter t_z. In this section, the basic algorithm of V-P4L is proposed for scenarios where LEDs have the same height, i.e., z^w_1 = z^w_2 = z^w_3 = z^w_4 . Based on the single-view geometry theory, we can obtain the relationship between z^w_i and t_z from (21) as:

z^w_i = [c_1, c_2, c_3]^T · P^c_i + t_z. (28)

The estimated z-coordinate of the camera in WCS t̂_z can be calculated as follows:

t̂_z = 1 4 (_4 ∑ i=1 z^w_i − 4∑ i=1 [ĉ_1, ĉ_2, ĉ_3]^T · P^c_i ) , (29)

where ĉ_k (k ∈ {1, 2, 3}) is the estimate of c_k.

In this way, the estimated pose R̂^w_c and position of the camera t̂^w_c can be obtained without the ideal 2D-3D correspondence assumption.

V. THE CORRECTION ALGORITHM OF V-P4L Most of existing studies including the basic algorithm of V-P4L proposed in Subsection IV assume that LEDs have the same height [14], [15]. However, this may not always be true in practice. For instance, ceilings may be tilted due to the imperfect decoration or deliberate design. In these scenarios, the localization accuracy can be significantly degraded. Therefore, in this subsection, based on the basic algorithm of V-P4L, we propose a correction algorithm of V- P4L for the scenarios where LEDs have different heights, V-P4L-DH. Based on the single-view geometry theory and the LLS method, V-P4L-DH can properly match the 3D-2D correspondences and obtain the 2D position of the camera. Based on the 2D localization, V-P4L-DH can achieve 3D localization by a simple optimization method.

A. 2D Localization

For 2D-localization case where the z-coordinate of the camera t_z is known in advance, based on the single-view geometry theory, (28) can be rewritten as follows:

[c_1, c_2, c_3]^T · P^c_i = z^w_j − t_z, (30)

where i, j ∈ {1, 2, 3, 4}. Since the 3D-2D correspondence are not known in advance, given a certain P^c_i and z^w_j , we do not know their correspondence relationship. Fortunately, there are four P^c_i and z^w_j , and thus we can estimate c_k (k ∈ {1, 2, 3}) using the same LLS method of solving (26). Then, from (20), we have:

ĉ_1 = − sin θ ĉ_2 = cos θ · sin φ ĉ_3 = cos θ · cos φ,

(31)

where ĉ_k (k ∈ {1, 2, 3}) is the estimate of c_k. The estimated rotation angles corresponding to the x^c−axis φ̂ and y^c−axis θ̂ can be obtained by solving (31). Then, the pose of the camera R̂^w_c and 2D position of the camera t̂^w_{c,2D} = ( t̂_x, t̂_y )_T can be obtained according to (20)−(27), where t̂_x and t̂_y are the estimated x and y-coordinates of the camera, respectively.

B. 3D Localization

For 3D-localization case, the z-coordinate of the camera t_z is not known in advance. For indoor scenario, the range of t_z must be [0, H_m), where H_m is the maximum height of the room.

Based on the above 2D-localizatoin algorithm, for different t_z ∈ [0, H_m), we can obtain different R̂^w_c (t_z) and t̂^w_{c,2D} (t_z). Based on the estimated normal vector of the luminaire in CCS n^c_{LED}, we have [22]:

n̂^w_{LED} (t_z) = R̂^w_c (t_z) · n^c_{LED}, (32)

where n̂^w_{LED} (t_z) denotes the estimated normal vector of the luminaire in WCS when the zcoordinate of the camera is t_z. Since the world coordinates of the luminaire’s vertices s^w_i (i ∈ {1, 2, 3, 4}) are known in advance, the actual normal vector of the luminaire in WCS n^w_{LED} can be calculated as follows: n^w_{LED} = ( P^w_i − P^w_j ) × (P^w_i − P^w_k ) , (33)

where i, j, k ∈ {1, 2, 3, 4} , i ≠ j ≠ k. Therefore, the difference between the estimated and actual normal vectors of the luminaire in WCS can be given as:

ΔG (t_z) = ‖n^w_{LED} − n̂^w_{LED} (t_z)‖_2 . (34)

The estimated z-coordinate of the camera t̂_z can be obtained by the minimum ΔG (t_z), i.e.:

t̂_z = arg min_{tz} ΔG (t_z) . (35)

To reduce the complexity of V-P4L-DH, we propose a n-step segmentation optimization strategy for V-P4L-DH. In the first step, we divide the range of t_z into N segments evenly, and set: t_z ∈ { 0, H_m N , 2 H_m N , 3 H_m N , . . . , H_m } , (36)

i.e., we set the interval between adjacent t_z as ε_1 ≜^{Hm}_N . Substituting all the t_z into (34), we have ΔG (t_z) = {ΔG (t_{z,0}) , ΔG (t_{z,1}) , . . . , ΔG (t_{z,N} )}. According to (35), we can find the minimal ΔG (t_z). We denote the minimal ΔG (t_z) by ΔG (t_{z,i}) where i ∈ {0, 1, . . . , N} is the index of the t_z that corresponding to ΔG (t_{z,i}). In the second step, we reduce the range of t_z to

Fig. 2. A occlusion scenario where the projection of P2, p2, is blocked by barriers and not on the image plane.

(_{Hm} N (i − 1) ,^{Hm}_N (i + 1) ) . We set: t_z ∈ { H_m N (i − 1) + ε_2,

H_m N (i − 1) + 2ε_2, . . . ,

H_m N (i + 1) − ε_2 } , (37)

i.e., the interval between adjacent t_z is ε_2, where ε_2 < ε_1. We repeat the process of the first step for the second step to the nth step until we can obtain the precise t̂_z according to (35), and obtain the optimal R̂^w_c and t̂^w_{c,2D}. Therefore, based on the simple optimization method, we can obtain the pose and 3D position of the receiver when LEDs have different heights.

In this way, when LEDs have the same height, the basic algorithm of V-P4L can be implemented for high accuracy at low complexity. When LEDs have different heights, V-P4L-DH can be implemented for high accuracy. In summary, V-P4L algorithm is elaborated in Algorithm 1. Although V-P4L requires the LED luminaire to be a rectangle, it is robust to partial occlusion, which is meaningful due to the limitation on the camera’s field of view. For instance, if the projection of P_2, p_2, is blocked by barriers and not on the image plane as shown in Fig. 2, the pixel coordinate of p_2 can be determined by the intersection of l_{12} and l_{23}, and thus V-P4L can be still successively implemented.

Algorithm 1 V-P4L Algorithm. Input:

P^w_i = (x^w_i , y^w_i , z^w_i )^T (i ∈ {1, 2, 3, 4}); p^p_j = ( u^p_j , v^p_j

)_T (j ∈ {1, 2, 3, 4}); u_0, v_0, f, f_u, f_v and ε_1.

1: Calculate p^i = ( x^i, y^i

)_T (i ∈ {1, 2, 3, 4}) according to (1).

2: for i = 1 → 4, j = 1 → 4 and j ≠ i do 3: Calculate ϕ_{lij} and ρ_{lij} by p^i and p^i_j.

4: A_{Πij} ← f cos ϕ_{lij} , B_{Πij} ← f sin ϕ_{lij} and C_{Πij} ← −ρ_{lij} , and then n^c_{Πij} ← ( A_{Πij} , B_{Πij} , C_{Πij} )_T . 5: v^c_{Lij} ← (A_{LED}, B_{LED}, C_{LED})^T × n^c_{Πij} , where (A_{LED}, B_{LED}, C_{LED})^T denotes the normal vector of the luminaire in CCS.

6: end for 7: Define m =^{ALED}_{CLED} and n =^{BLED}_{CLED} . Calculate m and n according to v^c_{L34} · n^c_{Π12} = 0 and v^c_{L41} · n^c_{Π23} = 0.

8: cos α ←^{m√}_{m2+n2+1} , cos β ←^{n√}_{m2+n2+1} and cos γ ←^{1√}_{m2+n2+1} , and then n^c_{LED} ← (cos α, cos β, cos γ)^T.

9: Calculate M_{P1} according to (9), and M_{Pi} (i ∈ {2, 3, 4}) can be calculated in the same way as M_{P1} .

10: q_1 ←^1_6 |det(M_{q1} )|, where M_{q1} = [M_{P1} , M_{P2} , M_{P3} ]^T, and q_i (i ∈ {2, 3, 4}) can be calculated in the same way as q_1.

11: C_{LED} ← √_{3 ∑4i=1 qi·√m2+n2+1} 2S .

12: P^c_i ←^{MPi}_{CLED} (i ∈ {1, 2, 3, 4}). 13: if z^w_1 = z^w_2 = z^w_3 = z^w_4 then 14: n^w_{LED} ← (0, 0, 1)^T.

15: Calculate φ̂ and θ̂ according to (18). 16: Calculate ψ̂, t̂_x and t̂_y according to (22) - (26). 17: Calculate t̂_z according to (29) if t_z is not known in advance. 18: else 19: if t_z is known in advance then 20: Calculate ĉ_i (i ∈ {1, 2, 3}) following the same method of solving (26). 21: Calculate φ̂ and θ̂ according to (31).

22: Calculate ψ̂, t̂_x and t̂_y according to (20) - (27). Therefore, R̂^w_c and t̂^w_{c,2D} = ( t̂_x, t̂_y )_T

can be obtained. 23: else 24: n^w_{LED} ← ( P^w_i − P^w_j ) × (P^w_i − P^w_k ), where i, j, k ∈ {1, 2, 3, 4} , i ≠ j ≠ k.

25: for i = 0 →^{Hm}_{ε1} do 26: t̂_{z,i} ← iε_1.

27: Calculate R̂^w_c (t_{z,i}) and t̂^w_{c,2D} (t_{z,i}). 28: n̂^w_{LED} (t_{z,i}) ← R̂^w_c (t_{z,i}) · n^c_{LED}. 29: ΔG (t_{z,i}) ← ‖n^w_{LED} − n̂^w_{LED} (t_{z,i})‖_2. 30: end for 31: t̂_z ← min_{tz} ΔG (t_z). Meanwhile, R̂^w_c ← R̂^w_c ( t̂_z ) and t̂^w_{c,2D} = ( t̂_x, t̂_y )_T ← t̂^w_{c,2D} ( t̂_z ) . 32: end if 33: end if Output: R̂^w_{c,est} and t̂^w_{c,est} = ( t̂_x, t̂_y, t̂_z )_T .

TABLE II SYSTEM PARAMETERS.

Parameter Value Room size (length × width × height) 5 m × 5 m × 3 m Length and width of LED luminaire

Length Width 120 cm 20 cm − 100 cm LED semi-angle, Φ1_{/2} 60^∘ Principal point of camera (u_0, v_0) = (320, 240) Focal ratio of camera f_u = f_v = 800 The distance between the PD and the camera in eCA-RSSR, dpc

1 cm

VI. SIMULATION RESULTS AND ANALYSES Since V-P4L combines VLC and computer vision based localization, a VLP algorithm named enhanced camera assisted received signal strength ratio algorithm (eCA-RSSR) [14], and a typical computer vision algorithm termed P4L algorithm [25] are conducted as the baselines schemes in this section.

A. Simulation Setup

The system parameters are listed in Table II. The LED luminaire is deployed in the center of the ceiling. The length of the luminaire which is along the x^w-axis is set to 120 cm [10], [29], and the widths of luminaire which is along the y^w-axis are varied according to configurations. We set the rectangular luminaire tilt with various angles along the y^w-axis to represent that LEDs have different heights. All statistical results are averaged over 1000 independent runs. For each simulation run, the receiver positions are selected in the room randomly. The pinhole camera is calibrated. The image noise is modeled as a white Gaussian noise having an expectation of zero and a standard deviation of 2 pixels [30]. Since the image noise affects the pixel coordinate of the luminaire’s projection on the image plane, the pixel coordinate is obtained by processing 20 images for the same position. Moreover, we use two-step segmentation optimization strategy, and we set ε_1 = 10 cm and ε_2 = 1 cm.

Note that since eCA-RSSR requires three LEDs for localization, we assume that the four LEDs at the vertices of the luminaire are used for eCA-RSSR and we choose the three LEDs with the highest RSSs to achieve best performance for eCA-RSSR. Additionally, all the LEDs transmit different information in eCA-RSSR, which is not required in V-P4L and the P4L algorithm. Therefore, compared with V-P4L, the VLC link of eCA-RSSR is more complex. Furthermore, eCA-RSSR relies on the perfect Lambertian pattern model. However, the VLC channel model can be quiet different from the Lambertian pattern model even using the LED having nearlyideal Lambertian pattern, as shown in [19], and the difference can be over 100% in certain cases. Therefore, we set a random deviation δ_1 ≤ 10% for the Lambertian pattern model for eCA-RSSR, conservatively. On the other hand, the P4L algorithm exploits a rectangle to estimate the position and pose of the camera. The P4L algorithm assumes that the camera knows the 3D-2D correspondences. However, the beacon in the P4L algorithm cannot convey time-domain information to the camera, which make the assumption impractical. In addition, the method to find the 3D-2D line correspondences given by [8] is also not practical when the camera captures the beacons on the ceiling as stated in Section I. Therefore, we set a random error rate δ_2 ≤ 10% for the 3D-2D correspondences, conservatively. Moreover, the P4L algorithm can only obtain the relative position. For comparison with V-P4L, we transform the relative position into the absolute position for the P4L algorithm in this section.

We evaluate the performance of V-P4L in terms of its accuracy of position and pose estimation. We define position error as:

P E = ‖r^w_{true} − r^w_{est}‖ , (38)

where r^w_{true} = ( x^w_{r,true}, y^w_{r,true}, z^w_{r,true} ) and r^w_{est} = ( x^w_{r,est}, y^w_{r,est}, z^w_{r,est} ) are the actual and estimated world coordinates of the receiver, respectively. Additionally, the accuracy of pose estimation can be measured by the orientation error which is defined as:

OE = |Θ_{true} − Θ_{est}| , (39)

where Θ_{true} and Θ_{est} are the actual and estimated rotation angles, respectively.

In this section, we will evaluate the performance of V-P4L under various tilted angles of the luminaire, various widths of the luminaire and various image noise. We compare for both scenarios where LEDs have the same height and have different heights, which are denoted by

(a) Without occlusion. (b) With occlusion.

Fig. 3. The comparison of position errors (PEs) with varying tilted angles of the luminaire between the basic algorithm of V-P4L and V-P4L-DH. (a) There is no occlusion. (b) The projection of P2, p2, is blocked by barriers and not on the image plane as shown in Fig. 2.

(a) OEs along the x-axis. (b) OEs along the y-axis. (c) OEs along the z-axis. Fig. 4. The comparison of orientation errors (OEs) along the x-axis, y-axis and z-axis between V-P4L-SH and V-P4L-DH.

SH and DH, respectively in the figures. Since the basic algorithm of V-P4L is used when LEDs have the same height, we denote the basic algorithm of V-P4L by V-P4L-SH in figures. B. Effect Of Luminaire’s Tilted Angle On Accuracy Performance

We first evaluate the effect of the tilted angles of the luminaire on localization accuracy of V-P4L for both 2D and 3D localization. This performance is represented by the means of PEs with the tilted angles of the luminaire varying from 0^∘ to 40^∘. The width of the luminaire is 40 cm. As shown in Fig. 3(a), for 2D localization, when the tilted angle of the luminaire is 0^∘, i.e., LEDs have the same height, the basic algorithm of V-P4L can obtain a slight better performance than V-P4L-DH. However, as the tilted angle of the luminaire varying from 0^∘ to 40^∘, the means of PEs of the basic algorithm of V-P4L increase from about 5 cm to about 98 cm. For 3D localization, the means of PE of the basic algorithm of V-P4L increase from about

10 cm to about 135 cm. In contrast, for all the tilted angles of the luminaire, the means of PEs of V-P4L-DH are less than 18 cm for both 2D and 3D localization. Since in 3D localization the estimated 2D position and pose is optimized meanwhile when search for the optimal t̂_z, V-P4L can achieve better performance for 3D localization than 2D localization.

Since the accuracy of pose estimation is also affected by the tilted angle of the luminaire, we then evaluated the effect of the tilted angles on OEs of V-P4L for both 2D and 3D localization. As shown in Fig. 4, the OEs along the x-axis, y-axis and z-axis are shown seperately. When the tilted angle of the luminaire is 0^∘, the basic algorithm of V-P4L can obtain slight better performance than V-P4L-DH. However, as the tilted angle of the luminaire varying from 0^∘ to 40^∘, the means of OEs of the basic algorithm of V-P4L increase from about 2^∘ to about 20^∘. In contrast, for all the tilted angles of the luminaire, V-P4L-DH can achieve consistent well performance, and the means of OEs are always less than 6^∘.

We also evaluate the effect of partial occlusion as shown in Fig. 2 on localization accuracy of V-P4L. Figure 3(a) shows the accuracy performance of position estimation when there is no occlusion in the scenario. In contrast, Fig. 3(b) shows the accuracy performance of position estimation when p_2 is blocked and is not on the image plane. As shown in Fig. 3(b), when the luminaire is partially blocked, V-P4L can still achieve high accuracy. In particular, the accuracy performance of the basic algorithm of V-P4L is almost the same in Fig. 3(a) and Fig. 3(b). In addition, for V-P4L-DH, the 2D-localization accuracy reduces about 2 cm, while the 3Dlocalization accuracy improves about 4 cm. Therefore, V-P4L is robust to partial occlusion as introduced in Section V.

In this subsection, we have verified V-P4L can achieve high accuracy for both 2D and 3D localization. Since 2D localization is the special case of 3D localization where the height of the receiver is known in advance, in the following subsections, we will only show the simulation results for 3D localization.

C. Effect Of Luminaire’s Widths On Accuracy Performance

We then evaluate the effect of the luminaire’s width on localization accuracy of V-P4L. This performance is represented by the means of PEs with the width varying from 20 cm to 100 cm.

Fig. 5. The comparison of position errors (PEs) with varying widths of the luminaire among eCA-RSSR, the P4L algorithm and V-P4L for both the scenarios where LEDs have the same height and have different heights.

For the scenarios where LEDs have different heights, the tilted angle of the luminaire is 20^∘. As shown in Fig. 5, for both the scenarios where LEDs have the same height and have different heights, V-P4L is able to obtain the best performance among the three algorithms. When LEDs have the same height, the means of PEs of the basic algorithm of V-P4L are below 15 cm. In contrast, for eCA-RSSR, the means of PEs are around 70 cm as the width of the luminaire increases from 20 cm to 100 cm. Additionally, for the P4L algorithm, the means of PEs decrease from over 100 cm to about 40 cm. On the other hand, when LEDs have different heights, the means of PEs of V-P4L-DH decrease from about 10 cm to 5 cm. In contrast, the means of PEs of both eCA-RSSR and the P4L algorithm are higher than 50 cm for all the widths of the luminaire. As shown in Fig. 5, the localization accuracy increases with the increase of the width for V-P4L. However, the PEs of V-P4L are always less than 15 cm regardless of the height differences among LEDs using a single LED luminaire whose width is longer than 20 cm, and thus V-P4L can be applied to popular indoor luminaires.

Since the accuracy of pose estimation is also affected by the width of the LED luminaire, we then compare the OEs between V-P4L and the P4L algorithm with varying widths of the luminaire. As shown in Fig. 6, for V-P4L, all the means of OEs along the x-axis, y-axis and z-axis are less than 3.5^∘ regardless of the height differences among the LEDs. When LEDs have the same height, the means of OEs along the x-axis and y-axis decrease from about 2^∘ to about 0.5^∘ and from 1^∘ to about 0.3^∘, respectively for both the basic algorithm of V-P4L and the P4L

(a) OEs along the x-axis. (b) OEs along the y-axis. (c) OEs along the z-axis. Fig. 6. The comparison of orientation errors (OEs) along the x-axis, y-axis and z-axis between the P4L algorithm and V-P4L with varying widths of the luminaire.

algorithm. Additionally, the means of OEs of the basic algorithm of V-P4L along the z-axis decrease from about 3^∘ to about 0.5^∘, which is over 5^∘ better than that of the P4L algorithm. On the other hand, when LEDs have different heights, for V-P4L-DH, the means of OEs along the x-axis, y-axis and z-axis decrease from 2.5^∘ to 1.5^∘, from 1.5^∘ to 0.5^∘ and from 2.2^∘ to 1.5^∘, respectively. In contrast, for the P4L algorithm, the means of OEs along the x-axis, y-axis and z-axis are about 9^∘, 6^∘, 13^∘, respectively. Therefore, compared with the P4L algorithm, V-P4L can obtain higher accuracy for pose estimation using popular indoor luminaire.

D. Effect Of Image Noise On Accuracy Performance

In this subsection, we evaluate the effect of the image noise on the localization performance of V-P4L when the width of the luminaire is 40 cm. When LEDs have different heights, the tilted angle of the luminaire is 20^∘. The image noise is modeled as a white Gaussian noise having an expectation of zero and a standard deviation, σ_n, ranging from 0 to 4 pixels [30]. Figure 7 shows the means of PEs versus image noises. As shown in Fig. 7, when LEDs have the same height, the means of PEs of the basic algorithm of V-P4L increase from 0 cm to 20 cm as the image noise increases from 0 to 4 pixels. In contrast, for the P4L algorithm, the means of PEs increase from 30 cm to 40 cm. Additionally, for eCA-RSSR, the means of PEs are around 75 cm. When LEDs have different heights, the means of PEs of V-P4L-DH increase from 0 cm to 11 cm. In contrast, for the P4L algorithm, the means of PEs are about 85 cm. Additionally, for eCA-RSSR, the means of PEs are about 135 cm. Therefore, compared with the P4L algorithm and eCA-RSSR, V-P4L can obtain higher accuracy for position estimation.

Fig. 7. The comparison of position errors (PEs) with varying image noise among eCA-RSSR, the P4L algorithm, V-P4L for both the scenarios where LEDs are at the same height and at different heights.

Finally, we compare the accuracy of pose estimation between V-P4L and the P4L algorithm under different image noises. Figure 8 show the means of orientation errors along x-axis, y-axis and z-axis with the image noise ranging from 0 to 4 pixels. When LEDs have the same height, the means of OEs of the basic algorithm of V-P4L along x-axis, y-axis and z-axis increase from 0^∘ to 2.5^∘, from 0^∘ to 1.2^∘ and from 0^∘ to 3.8^∘, respectively. In contrast, for the P4L algorithm, the means of OEs along the x-axis and y-axis increase from 0^∘ to 1.2^∘ and from 0^∘ to 0.5^∘, respectively, which is slight better than the basic algorithm of V-P4L. However, the means of OEs of the P4L algorithm along the z-axis increase from about 6^∘ to about 8^∘ which is over 4^∘ worse than that of the basic algorithm of V-P4L. On the other hand, when LEDs have different heights, for V-P4L-DH, the means of OEs along x-axis, y-axis and z-axis increase from about 1^∘ to less than 3.5^∘. In contrast, for the P4L algorithm, the means of OEs along x-axis, y-axis and z-axis are about 9^∘, 6^∘, 13^∘, respectively. Therefore, compared with the P4L algorithm, V-P4L can obtain more stable and accurate pose estimation regardless of the image noise. VII. CONCLUSION We have proposed a novel indoor localization algorithm named V-P4L that estimates the position and pose of the camera using a single, VLC-enabled LED luminaire. The camera is used to simultaneously capture the information in both time and space domains. Based on the

(a) OEs along the x-axis. (b) OEs along the y-axis. (c) OEs along the z-axis. Fig. 8. The comparison of orientation errors (OEs) along the x-axis, y-axis and z-axis between the P4L algorithm and V-P4L with varying image noise.

information captured by the camera, V-P4L does not require the 3D-2D correspondences. Moreover, V-P4L can be implemented regardless of the height differences among LEDs. Therefore, V-P4L can achieve higher feasibility and higher accuracy than eCA-RSSR and the conventional PnL algorithms. Simulation results have shown that for V-P4L the position error is always less than 15 cm and the orientation error is always less than 3^∘ using popular indoor luminaires. In the future, we will experimentally implement V-P4L based on a dedicated test bed. REFERENCES

[1] P. Pathak, X. Feng, P. Hu, and P. Mohapatra, “Visible light communication, networking and sensing: Potential and challenges,” IEEE Commun. Surveys Tuts., vol. 17, no. 4, pp. 2047–2077, 4th Quart. 2015.

[2] J. Lim, “Ubiquitous 3D positioning systems by LED-based visible light communications,” IEEE Wireless Commun., vol.

22, no. 2, pp. 80–85, Apr. 2015.

[3] Y. Yang, Z. Zeng, J. Cheng, C. Guo, and C. Feng, “A relay-assisted OFDM system for VLC uplink transmission,” IEEE Trans. Commun., vol. 67, no. 9, pp. 6268–6281, Sept. 2019.

[4] Y. Yang, Z. Zeng, J. Cheng, and C. Guo, “An enhanced DCO-OFDM scheme for dimming control in visible light communication systems,” IEEE Photon. J., vol. 8, no. 3, pp. 1–13, Jun. 2016.

[5] N. Piasco, D. Sidibé, C. Demonceaux, and V. Gouet-Brunet, “A survey on visual-based localization: On the benefit of heterogeneous data,” Pattern Recognition, vol. 74, pp. 90–109, Sep. 2018.

[6] A. Ben-Afia, L. Deambrogio, D. Salós, A.-C. Escher, C. Macabiau, L. Soulier, and V. Gay-Bellile, “Review and classification of vision-based localisation techniques in unknown environments,” IET Radar, Sonar &amp; Navigation, vol. 8, no. 9, pp. 1059–1072, Aug. 2014.

[7] T.-H. Do and M. Yoo, “An in-depth survey of visible light communication based positioning systems,” Sensors, vol. 16, no. 5, pp. 678, May 2016.

[8] T. Goto, S. Pathak, Y. Ji, H. Fujii, A. Yamashita, and H. Asama, “Line-based global localization of a spherical camera in manhattan worlds,” in 2018 IEEE Int. Conf. Robotics Automation (ICRA), 2018, pp. 2296–2303.

[9] C. Sertthin, T. Ohtsuki, and M. Nakagawa, “6-axis sensor assisted low complexity high accuracy-visible light communication based indoor positioning system,” IEICE Trans. Commun., vol. 93, no. 11, pp. 2879–2891, Nov. 2010.

[10] K. Qiu, F. Zhang, and L. Ming, “Let the light guide us: VLC-based localization,” IEEE Robot. Autom. Mag., vol. 23, no.

4, pp. 174–183, Dec. 2016.

[11] T. Q. Wang, Y. A. Sekercioglu, A. Neild, and J. Armstrong, “Position accuracy of time-of-arrival based ranging using visible light with application in indoor localization systems,” J. Lightw. Technol., vol. 31, no. 20, pp. 3302–3308, Oct. 2013.

[12] B. Zhu, J. Cheng, Y. Wang, J. Yan, and J. Wang, “Three-dimensional VLC positioning based on angle difference of arrival with arbitrary tilting angle of receiver,” IEEE J. Sel. Areas Commun., vol. 36, no. 1, pp. 8–22, Jan. 2018.

[13] L. Bai, Y. Yang, C. Guo, C. Feng, and X. Xu, “Camera assisted received signal strength ratio algorithm for indoor visible light positioning,” IEEE Commun. Lett., vol. 23, no. 11, pp. 2022–2025, Nov. 2019.

[14] L. Bai, Y. Yang, C. Feng, and C. Guo, “An enhanced camera assisted received signal strength ratio algorithm for indoor visible light positioning,” in Proc. IEEE Int. Conf. Commun. Workshops (ICC Wkshps), 2020, pp. 1–6.

[15] L. Li, P. Hu, C. Peng, G. Shen, and F. Zhao, “Epsilon: A visible light based positioning system,” in Proc. 11th USENIX Symp. Netw. Syst. Design Implement (NSDI’14), 2014, vol. 14, pp. 331–343.

[16] M. Yasir, S.-W. Ho, and B. N. Vellambi, “Indoor position tracking using multiple optical receivers,” J. Lightw. Technol., vol. 34, no. 4, pp. 1166–1176, Feb. 2015.

[17] Y. Li, Z. Ghassemlooy, X. Tang, B. Lin, and Y. Zhang, “A VLC smartphone camera based indoor positioning system,” IEEE Photon. Technol. Lett., vol. 30, no. 13, pp. 1171–1174, Jul. 2018.

[18] A.M. Vegni and M. Biagi, “An indoor localization algorithm in a small-cell led-based lighting system,” in Proc. IEEE Int. Conf. Indoor Position. Indoor Navig. (IPIN), 2012, pp. 1–7.

[19] F. Miramirkhani and M. Uysal, “Channel modeling and characterization for visible light communications,” IEEE Photonics J., vol. 7, no. 6, pp. 1–16, Dec. 2015.

[20] Z. Dong, T. Shang, Y. Gao, and Q. Li, “Study on VLC channel modeling under random shadowing,” IEEE Photonics J., vol. 9, no. 6, pp. 1–16, Dec. 2017.

[21] A. Cailean and M. Dimian, “Current challenges for visible light communications usage in vehicle applications: A survey,” IEEE Commun. Surveys Tuts., vol. 19, no. 4, pp. 2681–2703, 4th Quart. 2017.

[22] C. Xu, L. Zhang, L. Cheng, and R. Koch, “Pose estimation from line correspondences: A complete analysis and a series of solutions,” IEEE Trans. Pattern Anal. Mach. Intell., vol. 39, no. 6, pp. 1209–1222, Jun. 2017.

[23] B. Přibyl, P. Zemčík, and M. Čadík, “Absolute pose estimation from line correspondences using direct linear transformation,” Comput. Vis. Image Und., vol. 161, pp. 130–144, Aug. 2017.

[24] Alexander V., Jan F., and Francesc M.-N., “Accurate and linear time pose estimation from points and lines,” in Europ.

Conf. Comp. Visi. (ECCV), 2016, pp. 583–599.

[25] Wang X., Pan S., Qiu L., S L., and Song Z., “Analytic algorithm of pose estimation based on two pairs of parallel lines,” Chin. J. Sci. Instrum., vol. 29, no. 3, pp. 600, Oct. 2008.

[26] A. Masselli and A. Zell, “A new geometric approach for faster solving the perspective-three-point problem,” in Proc.

22nd Int. Conf. Pattern Recognit. (ICPR), 2014, pp. 2119–2124.

[27] L. Kneip, D. Scaramuzza, and R. Siegwart, “A novel parametrization of the perspective-three-point problem for a direct computation of absolute camera position and orientation,” in Proc. 24th IEEE Conf. Comput. Vis. and Pattern Recognit. (CVPR), 2011, pp. 2969–2976.

[28] Arthur M. L., “On the calculation of Euler angles from a rotation matrix,” IEEE Trans. on Commun., vol. 17, no. 3, pp.

335–337, Aug. 1986.

[29] Philips, “LED-tubes,” http://www.lighting.philips.com.cn/prof/led-lamps-and-systems/led-tubes#pfpath=0-LED GR, 2020, [Online, accessed 8-Apr.-2020].

[30] L. Zhou, Y. Yang, M. Abello, and M. Kaess, “A robust and efficient algorithm for the pnl problem using algebraic distance to approximate the reprojection distance,” in Proc. AAAI Conf. Artif. Intell., 2019, vol. 33, pp. 9307–9315.