arXiv:2107.09187v1 [cond-mat.supr-con] 19 Jul 2021

Noname manuscript No. (will be inserted by the editor)

Superconductivity in Al-Nb-Ti-V-Zr multicomponent alloy

Yuta Harayama · Jiro Kitagawa

Received: date / Accepted: date

Abstract The superconducting high-entropy alloys (HEAs) recently attract considerable attention due to their exciting properties, such as the robustness of superconductivity against atomic disorder and extremely high-pressure. The wellstudied crystal structure of superconducting HEAs is body-centered-cubic (bcc) containing Nb, Ti, and Zr atoms. The same elements are contained in Al5Nb24Ti40V5Zr26, which is a recently discovered bcc HEA and shows a gum-metal-like behavior after cold rolling. The gum metal is also an interesting system, exhibiting superelasticity and low Young’s modulus. If gum metals show superconductivity and can be used as a superconducting wire, the gum-metal HEA superconductors might be the next-generation superconducting wire materials. Aiming at a fundamental assessment of as-cast Al-Nb-Ti-V-Zr multicomponent alloys including Al5Nb24Ti40V5Zr26, we have investigated the structural and superconducting properties of the alloys. All alloys investigated show the superconductivity, and the

Yuta Harayama Department of Electrical Engineering, Faculty of Engineering, Fukuoka Institute of Technology, 3-30-1 Wajiro-higashi, Higashi-ku, Fukuoka 811-0295, Japan

Jiro Kitagawa Department of Electrical Engineering, Faculty of Engineering, Fukuoka Institute of Technology, 3-30-1 Wajiro-higashi, Higashi-ku, Fukuoka 811-0295, Japan E-mail: j-kitagawa@fit.ac.jp

valence electron concentration dependence of the superconducting critical temperature is very close to those of typical superconducting bcc HEAs.

Keywords multicomponent alloy · high-entropy alloy · superconductivity · gum metal

1 Introduction

High-entropy alloy (HEA) is a new class of materials and was initially proposed for simple crystal structures such as face-centered-cubic, body-centered-cubic (bcc), and hexagonal-closed packing in which more than five elements, each having the atomic fraction between 5% and 35%, randomly occupy one crystallographic site[1, 2]. Nowadays, the HEA concept is adopted in many alloys with multiple Wyckoff positions, oxides, chalcogenides, etc.[3,4,5]. The definition of HEA other than by the atomic concentration relies on the order of mixing entropy ΔS_{mix}: low-entropy alloys as having ΔS_{mix} less than 0.69R (R is the gas constant), medium-entropy alloys with ΔS_{mix} between 0.69R and 1.60R, and HEAs with ΔS_{mix} of 1.60R or larger[6]. The high atomic-disorder leads to the severe lattice distortion effect, and especially bcc HEAs show the enhancement of mechanical properties, which attract researchers all over the world. The enhancement of property beyond the simple mixture of those of constituent elements is also observed as, for example, outstanding thermal stability or enhanced magnetic frustration[7,8].

The HEA superconductivity is one of the hot topics of the HEA research field due to its exotic properties[3,9]. For example, the superconductivity is robust against atomic disorder and highly insensitive to the application of extremely highpressure[10,11]. Although the bcc HEA superconductors have been well studied[10, 11,12,13,14,15,16,17,18], several HEAs with multisite crystal structures such as the CsCl-type, A15, NaCl-type, σ-phase, and layered structures also show the interesting superconductivities[19,20,21,22,23,24,25]. While the relation between the superconductivity and the high-entropy state is unclear in many systems, in high-entropy (La0.2Ce0.2Pr0.2Nd0.2Sm0.2)O0.5F0.5BiS2 with the BiS2-based superconducting layer and the REO (RE: rare earth) blocking layer, the bulk nature of superconductivity is improved compared to PrO0.5F0.5BiS2 with the lowentropy state, which suggests that the mixing entropy at the blocking layer severely affects the superconducting state[24,25].

The gum metals, which have received considerable attention due to their unusual mechanical behaviors such as superelasticity and low Young’s modulus[26], possess chemical compositions similar to those of bcc HEA superconductors. The unusual properties are obtained after the cold rolling of as-cast materials. The valence electron concentration per atom (VEC) of the gum metals is 4.24, which is appropriate for the appearance of the superconductivity of d-electron alloy superconductors. Recently Al5Nb24Ti40V5Zr26 is reported as a gum-metal-like HEA[27]. If gum metals show superconductivity, they are highly advantageous for making superconducting wires, and this kind of material may be a good candidate for the next-generation superconducting wire.

In this paper, we have started from Al5Nb24Ti40V5Zr26, and characterized the structural and superconducting properties of Al5NbxTi35V5Zr55−x and Al5NbxTi59−xV5Zr31 alloys in the as-cast form. The superconducting properties were investigated by measuring the ac magnetic susceptibility and the electrical resistivity. This study will contribute to the basic understanding of superconductivity in gum metals in the future.

2 Materials and methods

Eight polycrystalline samples with different atomic compositions, as listed in Table 1, were synthesized by a home-made arc furnace. The constituent elements of Al (99.99 %), Nb (99.9 %), Ti (99.9 %), V (99.9 %), and Zr (99.5%), were arc-melted on a water-cooled Cu hearth in an Ar atmosphere. The samples received no heat treatment.

The X-ray diffraction (XRD) patterns of prepared samples were checked by an X-ray diffractometer (XRD-7000L, Shimadzu, Kyoto, Japan) with Cu-Kα radiation. We used thin slabs cut from the as-cast samples due to their high ductility. The microstructure of each sample was investigated by a field emission scanning electron microscope (FE-SEM, JSM-7100F; JEOL, Akishima, Japan). The atomic compositions of the samples were determined by an energy dispersive X-ray (EDX) spectrometer equipped to the FE-SEM.

Table 1 Atomic composition determined by EDX measurement, lattice parameter a, δ, and ΔS_{mix}/R of prepared samples.

Sample Atomic composition a (Å) δ ΔS_{mix}/R Al_5Nb_{24}Ti_{40} V_5Zr_{26} Al_{5.1(3)}Nb_{25(1)} Ti_{38.6(6)} V_{4.6(2)} Zr_{27(1)} 3.349(3) 5.28 1.359 Al_5Nb_{14}Ti_{35} V_5Zr_{41} Al_{5.1(3)} Nb_{14.6(5)} Ti_{33.6(3)} V_{4.9(4)} Zr_{41.8(4)} 3.407(4) 5.72 1.308 Al_5Nb_{24}Ti_{35} V_5Zr_{31} Al_{4.8(2)} Nb_{25.7(7)} Ti_{33.6(3)} V_{4.5(5)} Zr_{31.4(3)} 3.368(1) 5.53 1.373 Al_5Nb_{34}Ti_{35} V_5Zr_{21} Al_{5.0(1)} Nb_{33.5(6)} Ti_{33.5(3)} V_{5.2(3)} Zr_{22.9(5)} 3.342(2) 5.06 1.362 Al_5Nb_{44}Ti_{35} V_5Zr_{11} Al_{4.6(2)} Nb_{45.1(8)} Ti_{34.1(3)} V_{4.7(1)} Zr_{11.5(7)} 3.314(2) 4.18 1.271 Al_5Nb_{14}Ti_{45} V_5Zr_{31} Al_{4.7(2)} Nb_{12.9(4)} Ti_{47.7(5)} V_{5.5(3)} Zr_{29.2(5)} 3.372(1) 5.40 1.297 Al_5Nb_{34}Ti_{25} V_5Zr_{31} Al_{4.9(2)} Nb_{32.7(5)} Ti_{27.7(3)} V_{6.0(4)} Zr_{28.7(7)} 3.371(2) 5.65 1.376 Al_5Nb_{44}Ti_{15} V_5Zr_{31} Al_{5.0(2)} Nb_{40.9(7)} Ti_{17.6(2)} V_{5.8(3)} Zr_{30.6(7)} 3.371(1) 5.77 1.308

The temperature dependence of ac magnetic susceptibility χac (T ) in an alternating field of 5 Oe at 800 Hz, between 2.8 K and 300 K, was measured by a mutual inductance method using a GM refrigerator (UW404, Ulvac cryogenics, Kyoto, Japan). The temperature dependence of electrical resistivity ρ (T ) between 2.8 K and 300 K was measured by the conventional dc four-probe method using the GM refrigerator.

3 Results and discussion

The XRD pattern of Al5Nb24Ti40V5Zr26 is characterized by a single-phase bcc with the lattice parameter a =3.349 Å, which is consistent with the reported value 3.350 Å[27] (see Table 1 and the inset of Figure 1(a)). Al5Nb24Ti40V5Zr26 exhibits the diamagnetic signal and the zero resistivity as shown in Figs. 1(a) and 1(b), respectively. In the measurement of the real part of ac magnetic susceptibility χ^′_{ac} (T ), the superconducting critical temperature Tc is determined as being the intercept of the linearly extrapolated diamagnetic slope with the normal state signal[10, 28] (see the broken lines in Fig. 1(a)). Tc in ρ (T ) measurement is determined from the onset of the transition. The inset of Fig. 1(b) shows the ρ data in the whole measured temperature range, which indicates the weak temperature dependence in the normal state due to the atomic disorder.

Figures 2(a) and 2(b) show the XRD patterns of Al5NbxTi35V5Zr55−x and Al5NbxTi59−xV5Zr31, respectively. In each sample, the diffraction peaks can be

Fig. 1 (a) Temperature dependence of real part of χ_{ac} for Al_5Nb_{24}Ti_{40}V_5Zr_{26}. The inset is the XRD pattern of Al_5Nb_{24}Ti_{40}V_5Zr_{26}. (b) Temperature dependence of ρ for Al_5Nb_{24}Ti_{40} V_5Zr_{26} at low temperatures. The inset is ρ in the whole measured temperature range.

well indexed by a bcc structure. The lattice parameters are obtained by a leastmean square method (see Table 1) and plotted as a function of Nb content x in Fig. 2(c). For Al5NbxTi35V5Zr55−x, the lattice parameter shrinks with increasing x, which is contrasted with the almost x-independent lattice parameters in Al5NbxTi59−xV5Zr31. The SEM images of representative samples are displayed in Figures 3(a) and 3(b), indicating no apparent impurity phase. Each elemental mapping also supports the homogeneous elemental distribution. Table 1 shows the atomic compositions of the samples determined by EDX measurements. The respective composition agrees with the stating composition.

Shown in Figs. 4(a) and 4(b) are χ^′_{ac} (T ) of Al5NbxTi35V5Zr55−x and Al5NbxTi59−xV5Zr31, respectively. All samples exhibit diamagnetic signals. In both alloy systems, Tc systematically increases with increasing Nb concentration. Figures 5(a) and 5(b) exhibit ρ (T ) of Al5NbxTi35V5Zr55−x and Al5NbxTi59−xV5Zr31, respectively, which are normalized by the room temperature values listed in Table 2. The temperature dependence in the normal state tends to be weaker with decreasing Nb content. In each alloy system, the x=14 sample exhibit a negative temperature coefficient of resistivity, suggesting an occurrence of carrier localization. The insets are ρ (T )

Fig. 2 X-ray diffraction patterns of (a) Al_5Nb_xTi_{35} V_5Zr_{55−x} and (b) Al_5Nb_xTi_{59−x}V_5Zr_{31}, respectively. The origin of each pattern is shifted by an integer value for clarity. (c) Nb content dependences of lattice parameter of Al_5Nb_xTi_{35}V_5Zr_{55−x} and Al_5Nb_xTi_{59−x}V_5Zr_{31}.

at low temperatures, all showing drops to zero resistivity. Table 2 summarizes Tc’s in χ^′_{ac} (T ) and ρ (T ) measurements, which are determined by the same methods in Al5Nb24Ti40V5Zr26.

Here we discuss the relationship between Tc and the parameter δ or mixing entropy ΔS_{mix}. The parameter δ is employed in the material design of HEAs and means the degree of the atomic size difference among the constituent elements[1,

Fig. 3 SEM images of (a) Al_5Nb_{24}Ti_{35}V_5Zr_{31} and (b) Al_5Nb_{34} Ti_{25}V_5Zr_{31}, respectively. The elemental mappings are also shown.

Fig. 4 Temperature dependences of real part of χ_{ac} for (a) Al_5Nb_xTi_{35} V_5Zr_{55−x} and (b) Al_5Nb_xTi_{59−x}V_5Zr_{31}, respectively.

Fig. 5 Temperature dependences of ρ normalized by room temperature (RT) values for (a) Al_5Nb_xTi_{35} V_5Zr_{55−x} and (b) Al_5Nb_xTi_{59−x}V_5Zr_{31}, respectively. The insets are ρ (T ) at low temperatures.

Table 2 VEC, T_c’s determined by χ_{ac} and ρ measurements, and ρ at room temperature of prepared samples.

Sample VEC T_c (K) T_c (K) ρ at room by χ_{ac} by ρ temperature (μΩcm) Al_5Nb_{24}Ti_{40} V_5Zr_{26} 4.24 5.50 5.36 102.3 Al_5Nb_{14}Ti_{35} V_5Zr_{41} 4.14 4.73 4.40 88.3 Al_5Nb_{24}Ti_{35} V_5Zr_{31} 4.24 5.45 5.43 111.5 Al_5Nb_{34}Ti_{35} V_5Zr_{21} 4.34 6.47 6.48 105.2 Al_5Nb_{44}Ti_{35} V_5Zr_{11} 4.44 6.75 6.66 69.4 Al_5Nb_{14}Ti_{45} V_5Zr_{31} 4.14 4.96 4.65 111.6 Al_5Nb_{34}Ti_{25} V_5Zr_{31} 4.34 6.18 6.38 61.3 Al_5Nb_{44}Ti_{15} V_5Zr_{31} 4.44 6.98 7.01 76.6

2]. This was calculated for an n-component alloy as follows:

δ = 100 × n ∑ i=1 ci ( 1 − ri r̄ )_2 , (1)

where ci and ri are the atomic fraction and the atomic radius of the i-th element, respectively, and r̄ is the composition-weighted average atomic radius. The values

Fig. 6 (a)T_c vs δ plot and (b)T_c vs ΔS_{mix}/R plot for Al_5Nb_xTi_{35} V_5Zr_{55−x} and Al_5Nb_xTi_{59−x}V_5Zr_{31}.

of ri are taken from ref.[29]. ΔS_{mix} is given by

ΔS_{mix} = −R n∑ i=1 cilnci, (2) where R is the gas constant. As mentioned in the introduction, there are two wellaccepted definitions[1,2] for HEAs. Although the three alloys Al5Nb24Ti35V5Zr31, Al5Nb34Ti35V5Zr21, and Al5Nb34Ti25V5Zr31 fulfill the definition by the atomic percentage, each having 5 % ≤ ci ≤ 35 %, ΔS_{mix}’s of all alloys investigated are rather smaller than 1.60R (see also Table 1). Figures 6(a) and 6(b) explain the δ or ΔS_{mix}/R dependences of Tc for both alloy systems. For Al5NbxTi35V5Zr55−x, Tc increases with decreasing δ, which is contrasted with the δ dependence of Tc in Al5NbxTi59−xV5Zr31. This means the robustness of superconductivity against the lattice distortion, which would be one of the characteristics of bcc HEA superconductors. In both alloy systems, Tc shows the non-monotonous ΔS_{mix} dependences. Therefore, Tc does not severely rely on the high-entropy effect.

Figure 7 shows the VEC dependence of Tc for Al-Nb-Ti-V-Zr multicomponent alloys, which is compared to those of crystalline 4d metal solid solutions[9] (the dotted line) and typical superconducting bcc HEAs[10,12,14,15] (Ta-Nb-Hf-Zr-Ti, Nb20Re20Zr20Hf20Ti20, and Hf21Nb25Ti15V15Zr24). Although Tc’s of these HEAs are relatively lower than those of 4d metal solid solutions at a fixed VEC, the VEC

Fig. 7 VEC dependences of T_c for alloys denoted in figure legend. The same dependence is also shown for crystalline 4d metal solid solutions by the dotted line. Data for the dotted line is from ref.[9].

dependence is similar to each other; Tc seems to form a broad maximum at approximately VEC=4.7. The VEC dependence of Tc of Al-Nb-Ti-V-Zr multicomponent alloy falls on those of bcc HEAs, whereas ΔS_{mix}’s of the present alloys are lower. Ternary alloys Nb-Ti-Zr are also superconductors[30], and the data is plotted in Figure 7 (Nb50Ti10Zr40: Tc =10.3 K, Nb35Ti15Zr50: Tc =8.95 K, Nb35Ti60Zr5: Tc =8.6 K, and Nb21Ti61Zr18: Tc =6.8 K). The plot well agrees with the Matthias rule of 4d metal solid solutions. Therefore, a multicomponent alloy composed of five elements might generally show the lowered Tc compared to simple 4d metal solid solutions.

Several superconductors maintain the superconducting state after the cold rolling process[31,32,33]. Thus we can expect the same result for the present alloys. It would be important to elucidate the relationship between the mechanical properties of Al-Nb-Ti-V-Zr alloys, including gum-metal composition, and the superconducting properties in order to know whether the gum-metal HEA superconductors can be candidate for the next-generation superconducting wire or not.

4 Summary

We have characterized new multicomponent alloy superconductors Al-Nb-Ti-V- Zr including Al5Nb24Ti40V5Zr26 which exhibits a gum-metal-like behavior after the cold rolling. All as-cast samples crystallize into the bcc structure with no obvious secondary phase. The lattice parameters of Al5NbxTi35V5Zr55−x and Al5NbxTi59−xV5Zr31 exhibit the different x dependences. Al5NbxTi35V5Zr55−x shows the shrink of lattice parameter with increasing x, whereas the almost xindependent lattice parameters are observed in Al5NbxTi59−xV5Zr31. Nonetheless, the similar VEC dependence of Tc is confirmed for both alloy systems. Although the ternary superconducting Nb-Ti-Zr alloys well obey the Matthias rule of crystalline 4d metal solid solutions, the present alloys show lower Tc’s compared to ternary Nb-Ti-Zr alloys. However, the VEC dependence of Tc of Al-Nb-Ti-V-Zr alloys falls on those of the typical bcc HEA superconductors. Therefore, a multicomponent alloy composed of five elements might generally behave as an HEA superconductor, even if the mixing entropy is rather smaller than 1.60R. This study will be useful for the fundamental understanding of superconductivity in gum metals.

Acknowledgements J.K. is grateful for the support provided by Comprehensive Research Organization of Fukuoka Institute of Technology.

References

1. Gao,M. C., Yeh, J. -W., Liaw, P. K., Zhang, Y.: High-Entropy Alloys: Fundamentals and Applications, (Swizerland: Springer, 2015) 2. Murty, B. S. Yeh, J. -W., Ranganathan, S., Bhattacharjee, P. P.: High-Entropy Alloys.

2nd ed., (Amsterdam: Elsevier, 2019) 3. Kitagawa, J., Hamamoto, S., Ishizu, N.: Cutting Edge of High-Entropy Alloy Superconductors from the Perspective of Materials Research, Metals 10, 1078 (2020) 4. Musicó, B. L., Gilbert, D., Ward, L. Z., Page, K., George, E., Yan, J., Mandrus, D., Keppens, V.: The emergent field of high entropy oxides: Design, prospects, challenges, and opportunities for tailoring material properties, APL Materials 8, 040912 (2020)

5. Jiang, B., Yu, Y., Cui, J., Liu, X., Xie, L., Liao, J., Zhang, Q., Huang, Y., Ning, S., Jia, B., Zhu, B., Bai, S., Chen, L., Pennycook, S. J., He, J.: High-entropy-stabilized chalcogenides with high thermoelectric performance, Science 371, 830-834 (2021) 6. Otto, F., Yang, Y., Bei, H., George, E. P.: Relative effects of enthalpy and entropy on the phase stability of equiatomic high-entropy alloys, Acta Mater. 61 2628-2638 (2013) 7. Sun, L., Luo, Y., Ren, X., Gao, Z., Du, T., Wu, Z., Wang, J.: A multicomponent γ-type (Gd_{1/6} Tb_{1/6}Dy_{1/6}Tm_{1/6}Yb_{1/6}Lu_{1/6})_2Si_2 O_7 disilicate with outstanding thermal stability, Mater. Res. Lett. 8 424-430 (2020) 8. Marik, S., Singh, D., Gonano, B., Veillon, F., Pelloquin, D., Bréard, Y.: Enhanced magnetic frustration in a new high entropy diamond lattice spinel oxide. Scr. Mater.186, 366-369 (2020) 9. Sun, L., Cava, R. J.: High-entropy alloy superconductors: Status, opportunities, and challenges, Phys. Rev. Mater. 3, 090301 (2019) 10. von Rohr, F. O., Winiarski, M. J., Tao, J., Klimczuk, T., Cava, R. J.: Effect of electron count and chemical complexity in the Ta-Nb-Hf-Zr-Ti high-entropy alloy superconductor, Proc. Natl. Acad. Sci.113, E7144-E7150 (2016) 11. Guo, J., Wang, H., von Rohr, F., Wang, Z., Cai, S., Zhou, Y., Yang, K., Li, A., Jiang, S., Wu, Q., Cava, R. J., Sun, L.: Robust zero resistance in a superconducting high-entropy alloy at pressures up to 190 GPa, Proc. Natl. Acad. Sci. 114, 13144-13147 (2017) 12. Koželj, P., Vrtnik, S., Jelen, A., Jazbec, S., Jagličić, Z., Maiti, S., Feuerbacher, M., Steurer, W, Dolinšek, J.: Discovery of a superconducting high-entropy alloy, Phys. Rev. Lett. 113, 107001 (2014) 13. von Rohr, F. O., Cava, R. J.: Isoelectronic substitutions and aluminium alloying in the Ta-Nb-Hf-Zr-Ti high-entropy alloy superconductor, Phys. Rev. Mater. 2, 034801 (2018) 14. Marik, S., Varghese, M., Sajilesh, K. P., Singh, D., Singh, R. P.: Superconductivity in equimolar Nb-Re-Hf-Zr-Ti high entropy alloy, J. Alloys and Compd. 769, 1059-1063 (2018) 15. Ishizu, N., Kitagawa, J.: New high-entropy alloy superconductor Hf_{21}Nb_{25}Ti_{15} V_{15}Zr_{24}, Res. Phys. 13, 102275 (2019) 16. Nelson, W. L., Chemey, A. T., Hertz, M., Choi, E., Graf, D. E., Latturner, S., Albrecht- Schmitt, T. E., Wei, K., Baumbach, R. E.: Superconductivity in a uranium containing high entropy alloy, Sci. Rep. 10, 4717 (2020) 17. Zhang, X., Winter, N., Witteveen, C., Moehl, T., Xiao, Y., Krogh, F., Schilling, A., von Rohr, F. O.: Preparation and characterization of high-entropy alloy (TaNb)_{1−x}(ZrHfTi)_x superconducting films, Phys. Rev. Res. 2, 013375 (2020) 18. Kim, G., Lee, M. -H., Yun, J. H., Rawat, P., Jung, S. -G., Choi, W., You, T. -S., Kim, S. J., Rhyee, J. -S.: Strongly correlated and strongly coupled s-wave superconductivity of the high entropy alloy Ta_{1/6}Nb_{2/6}Hf_{1/6}Zr_{1/6}Ti_{1/6} compound, Acta Mater. 186, 250-256 (2020) 19. Stolze, K., Tao, J., von Rohr, F. O., Kong, T., Cava, R. J.: Sc-Zr-Nb-Rh-Pd and Sc-Zr- Nb-Ta-Rh-Pd high-entropy alloy superconductors on a CsCl-type lattice, Chem. Mater. 30, 906-914 (2018)

20. Wu, J., Liu, B., Cui, Y., Zhu, Q., Xiao, G., Wang, H., Wu, S., Cao, G., Ren, Z.: Polymorphism and superconductivity in the V-Nb-Mo-Al-Ga high-entropy alloys, Sci. China Mater. 63, 823-831 (2020) 21. Mizuguchi, Y.: Superconductivity in high-entropy-alloy telluride AgInSnPbBiTe_5 , J. Phys.

Soc. Jpn. 88, 124708 (2019) 22. Yamashita, A., Jha, R., Goto, Y., Matsuda, T. D., Aoki, Y., Mizuguchi, Y.: An Efficient way of increasing the total entropy of mixing in high-entropy-alloy compounds: a case of NaCl-type (Ag,In,Pb,Bi)Te1 − xSe_x (x = 0.0, 0.25, 0.5) superconductors, Dalton Trans. 49, 9118-9122 (2020) 23. Liu, B., Wu, J., Cui, Y., Zhu, Q., Xiao, G., Wu, S., Cao, G., Ren, Z.: Superconductivity and paramagnetism in Cr-containing tetragonal high-entropy alloys, J. Alloys and Compd. 159293 869, (2021) 24. Sogabe, R., Goto, Y., Mizuguchi, Y.: Superconductivity in REO_{0.5}F_{0.5}BiS_2 with high entropy-alloy-type blocking layers, Appl. Phys. Express 11, 053102 (2018) 25. Sogabe, R., Goto, Y., Abe, T., Moriyoshi, C., Kuroiwa, Y., Miura, A., Tadanaga, K., Mizuguchi, Y.: Improvement of superconducting properties by high mixing entropy at blocking layers in BiS_2-based superconductor REO_{0.5}F_{0.5}BiS_2, Solid State Commun. 295, 43-49 (2019) 26. Saito, T., Furuta, T., Hwang, J. -H., Kuramoto, S., Nishino, K., Suzuki, N., Chen, R., Yamada, A., Ito, K., Seno, Y., Nonaka, T., Ikehata, H., Nagasako, N., Iwamoto, C., Ikuhara, Y., Sakuma, T.: Multifunctional alloys obtained via a dislocation free plastic deformation mechanism. Science 300, 464-467 (2003) 27. Zherebtsov, S., Yurchenko, N., Panina, E., Tikhonovsky, M., Stepanov, N.: Gum-like mechanical behavior of a partially ordered Al_5Nb_{24}Ti_{40}V_5Zr_{26} high entropy alloy, Intermetallics 116, 106652 (2020) 28. Hamamoto, S., Kitagawa, J.: Superconductivity in oxygen-added Zr_5Pt_3, Mater. Res.

Express 5, 106001 (2018) 29. Miracle, D. B., Senkov, O. N.: A critical review of high entropy alloys and related concepts, Acta Mater. 122, 448-511 (2017) 30. Roberts, B. W.: Survey of superconductive materials and critical evaluation of selected properties, J. Phys. Chem. Ref. Data 5, 581-821 (1976) 31. Raabe, D., Hangen, U.: Correlation of microstructure and type II superconductivity of a heavily cold rolled Cu-20mass% Nb in situ composite, Acta Mater. 44, 953-961 (1996) 32. Guryev, V. V., Shavkin, S. V., Kruglov, V. S., Volkov, P. V., Vasiliev, A. L., Ovcharov, A. V., Likhachev, I. A., Pashaev, E. M., Svetogorov, R. D., Zubavichus, Y. V.: Apparent anisotropy effects of upper critical field in high-textured superconducting Nb-Ti tapes, J. Phys.: Conf. Ser. 747, 012034 (2016) 33. Idczak, R., Nowak, W., Babij, M., Tran, V. H.: Type-II superconductivity in cold-rolled tantalum, Phys. Lett. A 384, 126750 (2020)