arXiv:2206.05433v1 [physics.optics] 11 Jun 2022

Gigahertz-rate random speckle projection for high-speed single-pixel image classification

Jinsei Hanawa^1, Tomoaki Niiyama^2, Yutaka Endo^2, and Satoshi Sunada^{2,3∗} 1Graduate School of Natural Science and Technology, Kanazawa University, Kakuma-machi, Kanazawa, Ishikawa 920-1192, Japan 2Faculty of Mechanical Engineering, Institute of Science and Engineering, Kanazawa University Kakuma-machi, Kanazawa, Ishikawa 920-1192, Japan 3Japan Science and Technology Agency (JST), PRESTO, 4-1-8 Honcho, Kawaguchi, Saitama 332-0012, Japan

Imaging techniques based on single-pixel detection, such as ghost imaging, can reconstruct or recognize a target scene from multiple measurements using a sequence of random mask patterns. However, the processing speed is limited by the low rate of the pattern generation. In this study, we propose an ultrafast method for random speckle pattern generation, which has the potential to overcome the limited processing speed. The proposed approach is based on multimode fiber speckles induced by fast optical phase modulation. We experimentally demonstrate dynamic speckle projection with phase modulation at 10 GHz rates, which is five to six orders of magnitude higher than conventional modulation approaches using spatial light modulators. Moreover, we combine the proposed generation approach with a wavelength-division multiplexing technique and apply it for image classification. As a proof-of-concept demonstration, we show that 28×28-pixel images of digits acquired at GHz rates can be accurately classified using a simple neural network. The proposed approach opens a novel pathway for an all-optical image processor.

I. INTRODUCTION

Random pattern generation has garnered considerable interest because it has a wide range of potential applications, including imaging technologies based on single-pixel detection [1–4], such as ghost imaging [5–7], as well as remote sensing [8] and photonic computing [9–11]. Spatial light modulators (SLMs) have been commonly used to generate optical random patterns. While SLMs with a large number of pixels enable a wide variety of illumination pattern controls, the low refresh rate, which is typically on the order of ∼10 kHz, ultimately limits the image processing speed. In response, significant effort has been devoted to increasing the refresh rate of the pattern illumination for high-speed ghost imaging and singlepixel image processing [12–18].

Owing to the high speed wavelength-to-time mapping and modulation techniques developed recently, multimode fibers (MMFs) and scattering media have been widely utilized to generate random speckle patterns. For example, Wang et al. proposed fast speckle generation based on a single MMF and a photonic time stretch technique [14]. In that study, a pulse laser was used to produce a short optical pulse with a broadband spectrum, and the pulse signal was stretched in the temporal domain and converted into speckle patterns via the MMF. They demonstrated the reconstruction of a 27×27-pixel image with 500 speckle patterns. In addition, Shi et al. proposed a random speckle encoding scheme based on a hybrid wavelength and spatial phase modulation, which has the potential for high-speed pattern generation of up to gigahertz rates [15]. Furthermore, Fukui et al. proposed the use of a chip-scale integrated optical phased array for imaging through

∗ sunada@se.kanazawa-u.ac.jp

an MMF [16]. Using the speckles generated from the method, they obtained fine 2D images of a target object. These approaches have suggested great potential for accelerating random pattern illumination. However, to the best of our knowledge, the experimental demonstration of high-speed random pattern illumination at GHz rates has not been reported.

In this study, we propose and experimentally demonstrate an ultrafast method for random speckle pattern generation. The proposed generation approach is based on MMF speckles induced by fast phase modulation at 10 GHz rates, which is a five to six orders of magnitude higher than conventional modulation approaches using SLMs. While a similar modulation approach has been used for compressive sensing of sparse radio-frequency signals [19], this study represents the first experimental demonstration of high-speed speckle-based information processing. In contrast to existing generation schemes that are based on using a pulse-laser as a broadband spectrum source, the proposed approach is simple, versatile, and has the capability of generating a continuous stream of speckle patterns. Thus, in principle, information processing without dead time (i.e., the time during which the system cannot operate) is possible. As a proof-of-concept demonstration of a simple ultrafast random pattern generator, we show that 28×28-pixel images of digits (hereafter, digit images) acquired at gigahertz rates can be accurately classified using a simple neural network. This suggests that the proposed generator has the potential to act as a photonic preprocessor for fully photonic information processing.

II. MULTIMODE FIBER SPECKLES

The proposed random pattern generation is based on dynamic speckles produced from a single and long MMF.

MMFs generally support numerous guided modes with different phase velocities. When monochromatic coherent light is input to an MMF, it can produce a pseudorandom speckle pattern in the intensity distribution at the end facet of the MMF due to the interference between guided modes with different phase velocities. Because the phase velocities of the guided modes depend on the frequency (wavelength) of the input light, the speckle pattern is highly sensitive to the input frequency. Moreover, the sensitivity of the MMF speckle to the input frequency increases as the MMF length increases [20, 21]. Accordingly, dynamic speckles can be easily generated with a long MMF by modulating the phase ϕ(t) of the input light and inducing an instantaneous input frequency, f (t) ∼ dϕ(t)/dt. The variety of the generated speckles depends on the instantaneous input frequency. In our previous work, we have utilized fast optical phase modulation at 12.5 gigasamples per second (GS/s) to induce fast spatiotemporal speckle dynamics in a long MMF for photonic reservoir computing [9]. In this study, we use similar techniques for generating fast random speckle patterns.

Figure 1 shows the speckle generation system used in our experiment. It primarily consists of a coherent light source, a waveform generator, an optical phase modulator, and an MMF. In the experiment, a narrow linewidth tunable laser (Alnair Labs, TLG-220, linewidth <100 kHz, 30 mW) was used as a coherent light source. To dynamically vary the input frequency for the speckle modulation, the laser light was phase-modulated using a lithium niobate phase modulator (EO Space, PM-5S5-20-PFA-PFA-UV-UL, 16 GHz bandwidth) with a uniformly distributed pseudorandom sequence generated using an arbitrary waveform generator (Tektronix, AWG70002A, 25 GS/s). The pseudorandom sequence can induce a variety of instantaneous input frequencies for generating speckles. The modulated light was sent from a polarization-maintaining single-mode fiber to an MMF. We used a commercially available step-index multimode fiber with a core diameter of 200 μm, numerical aperture (NA) of 0.39, and lengths varying from 1 m to 100 m. According to a theoretical estimation [22], a 100-m MMF is expected to support over ∼10^4 guided modes at an input wavelength of λ_0 =1550 nm.

III. RESULTS

A. Speckle contrast measurement

First, we observed the MMF speckle patterns to evaluate the pattern generation capability of the proposed system. In the experiment, the end facet of the MMF was imaged onto an In- GaAs camera (SYNOS, ISA041H2) with a 20× near-infrared microscope objective (M Plan Apo NIR 20X). The exposure time of the camera was set to 10 ms. Figure 2(a) shows a representative example of the measured MMF speckle pattern for an input wavelength of 1550 nm. When the input light was phase-modulated at a GHz rate in the system [Fig. 1], a number of speckle patterns could be dynamically generated. Thus, the time-averaged pattern with a low contrast was measured

FIG. 1. Schematic of speckle pattern generation system. ISO represents the optical isolator, Amp represents the electric amplifier, AWG represents the arbitrary waveform generator, PM represents the phase modulator, and MMF represents the multimode fiber. A polarizationmaintaining single-mode fiber was coupled to the MMF with a standard FC/PC connector.

with the camera [Fig. 2(b)]. Considering that the dynamically changing speckle patterns could not be directly captured by a camera with a relatively low frame rate, we used the speckle contrast C = σ/Ī (where Ī and σ are the mean value and standard deviation of the measured intensity patterns, respectively) to characterize the variety of the generated speckle patterns. A value of C = 1 indicates that only a single speckle pattern was involved with the measured pattern if it was well developed. If a number of speckle patterns are involved in the measured pattern, C decreases due to the time-averaging during the exposure time of the camera (for instance, C was approximated as M^{−1/2} for M independent speckle patterns with equal intensities [20]). Figure 2(c) shows C as a function of the MMF length. As expected, C decreased as the MMF length increased, suggesting that the sensitivity of the speckle pattern to the length of the MMF could be enhanced [20]. The modulation speed or modulation bandwidth is also a crucial parameter for decreasing the speckle contrast because the input frequency f (t) for dynamic speckle generation can be characterized as f (t) = 1/(2π)dϕ(t)/dt. To investigate the modulation dependence of the speckle contrast, we changed the bandwidth of the pseudorandom signal used for the phase modulation using a low-pass filter and measured the speckle contrast. As shown in Fig. 2(c), as the cutoff frequency of the low-pass filter increased (i.e., as modulation bandwidth increased), C decreased. This result suggests that the number of speckle patterns generated in the system is scalable to the MMF length and modulation speed. In the remaining experiments, we used the 100-m MMF for dynamic speckle generation.

B. High-speed random speckle projection

We applied the proposed random speckle projection to encode the image of an object as a time-domain signal. The experimental setup is shown in Fig. 3(a). The speckle patterns were generated using the MMF from the phase-modulated in-

FIG. 2. Measured MMF speckle patterns (a) for non-modulated light input and (b) for phase-modulated light input at 25 GS/s. The exposure time of the InGaAs camera was set to 10 ms. In (b), the phase-modulated light dynamically induced a number of speckle patterns, and the time-averaged pattern was measured during the exposure time. Thus, the speckle contrast C was reduced to 0.13. The MMF length was set at 100 m. (c) Speckle contrast C as a function of the MMF length. To investigate the dependence of the modulation bandwidth on C, the modulation signal was low-pass filtered using various cut-off frequencies. In the experiment, we used a Butterworth filter as the low-pass filter.

put light at a rate of 12.5 GS/s. The speckle patterns were then used as illumination to encode a target image, which was displayed on a digital micromirror device (DMD). The reflected light from the DMD was collected with two lenses, coupled to a multimode fiber with a core diameter of 50 μm, and sent to a fast photodetector (Thorlabs, RXM25BF, 500 kHz-25 GHz). The signal waveform was measured with a digital oscilloscope (Tektronix, DPO72504DX, 25 GHz bandwidth, 50 GS/s).

Figure 4 shows examples of the time-domain signals generated in the experiment, which encoded the Modified National Institute of Standards and Technology (MNIST) handwritten digit images (“0”,”1”, “2”, and “3”) [23, 24]. The figure shows that different digit images can be successfully encoded as different waveforms, depending on the shapes, locations, and sizes of the digits. In these examples, the acquisition time T_N was set to 6 ns, wherein N = T_N /τ_s =300-pattern-encoded signal was obtained with a sampling time interval of τ_s = 0.02 ns in the oscilloscope.

To demonstrate the capability of capturing dynamic scenes, we encoded the transient switching behavior of the images shown on the DMD display from digit “0” to digit “5” as the time-domain signal. The result is shown in Fig. 5(a), where the laser light was repeatedly phase-modulated with the same pseudorandom signal of T_N = 20 ns. The switching behavior was analyzed through the correlation measurement of the time-domain signal. We computed the correlation between the signal I(t) shown in Fig. 5(a) and the signal I_i(t) with encoding digit ”i” (i = 0 or 5) [Figs. 5(b) and 5(c)], which is defined as C_i( jT_N ) = ⟨I(t + jT_N )I_i(t)⟩_{TN} /(σσ_i), where ⟨·⟩_{TN} denotes the time average from t = 0 to t = T_N , and σ and σ_i denote the standard deviations of I and I_i, respectively. In Fig. 5(d), the correlation C_i is plotted as a function of discrete time t_j = jT_N ( j = 0, 1, · · · ), where T_N was set to 20 ns. Fig. 5(d) clearly shows that, when the DMD display was switched, the correlation C_5 suddenly decreased and C_0 suddenly increased. This correlation analysis reveals that the proposed approach allows capturing the fast dynamical behavior of the microsecond switching phenomenon. Faster dynamical behavior can be captured with our approach by setting a shorter T_N .

FIG. 3. (a) Experimental setup for speckle projection. The output from the end facet of the MMF was collimated with a lens (L1). The target image was displayed on the digital micro mirror device (DMD). The reflected light from the DMD was coupled to the receiver fiber (MMF) via two lenses (L2 and L3). PD represents the photodetector, Amp represents the electric amplifier, and OSC represents the digital oscilloscope. (b) Schematic of neural network for digit recognition. The image-encoded time-domain signal was used as an input to the network with a fully connected layer of 100 units.

C. Application to fast single-pixel image classification

As mentioned in Section I, the proposed random speckle generation can be used for accelerating information processing based on a single-pixel detection. While many studies have mostly focused on signal and image reconstruction, the reconstruction is frequently not the ultimate goal. Because the feature information of an object image is compressively

FIG. 4. Experimental demonstration of the proposed speckle projection. (a)–(h) show the time-domain signals (voltage signals acquired by the oscilloscope), which encode the image information corresponding to each inserted digit image. The signal waveforms depend strongly on the digit images.

encoded into a time-domain signal, the acquired data can be directly utilized for classification or recognition. Such imagefree classification can eliminate redundant image acquisition, enable higher data efficiency [25], and be used in an application requiring real-time and high-speed control, such as flow cytometry cell sorting [26]. Although many image-free classification schemes based on single-pixel detection have been proposed and demonstrated [27–29], this study represents the first demonstration of high-speed (potentially at GHz frame rates) image-free classification using the proposed speckle generation method.

The experimental setup was the same as that shown in Fig. 3(a). In the experiment, we set the acquisition time T_N to 6 ns to encode a digit image with a sampling time interval τ_s = 0.02 ns (N = T_N /τ_s = 300 points was used for the purpose of classification). As a classifier, we chose a simple neural network that had a single fully connected layer of 100 nodes with a rectified linear unit (ReLU) activation function [Fig. 3(b)]. We did not use convolutional neural network (CNN) layers, which have frequently been used for high-performance recognition, because we focused on the effectiveness of the speckle projection approach for classification purposes. Additionally, we note that a simple neural network can be implemented in an application-specific circuit for low latency operation. For the proof-of-concept experiment, we chose the MNIST handwritten digit database [23, 24], and used a subset of the original database consisting of 10000 handwritten images of digits from “0” to “3” as our four-class classification database. Each digit image was separated into 9000 (2250×4) images for training and 1000 (250×4) images for testing. In the training process, cross entropy was chosen as the loss function, and it was minimized with the adaptive moment estimation gradient descent algorithm (ADAM) [30].

The confusion matrix in Fig. 6(a) shows the distribution of predicted labels for each class. Most predicted labels were distributed along the diagonal line and matched the true labels. The total classification accuracy was 92.6 %. However, a significant error arose as a result of mistaking digit “3” for “2” and vice versa, as shown in the confusion matrix. For comparison, we performed numerical simulations, for which an N×784 Gaussian random mask matrix was used to generate N features for a digit image (with 28×28 = 784 pixels), and the same neural network was used for the classifier. The result is shown in Fig. 6(b). A similar error tendency was observed, but the total accuracy (98.4 %) was better than that obtained from the experiment. This discrepancy may be attributed to the MMF-based speckle generation, which was highly sensitive to external environmental fluctuations and measurement errors, particularly quantization errors of the 8-bit digital oscilloscope used in the experiment. See Sec. IV for discussion on the stability of the MMF-based speckle generation.

D. Wavelength-division multiplexing

As shown in the previous subsection, our approach enables high-speed projection operations at an acquisition rate of 1/T_N ≈ 167 megaframes per second (Mfps). For further acceleration of the projection operation, our approach can incorporate the wavelength-division multiplexing scheme, as illustrated in Figs. 7(a) and 7(b). To verify the effect of the wavelength-division multiplexing, we used a tunable laser to produce laser light with different wavelengths ranging from 1547 to 1553 nm at 1 nm intervals, and we acquired the imageencoded time-domain signals with these wavelengths instead of the parallel acquisition using a multiplexer and demultiplexer. Figures 7(c) and 7(d) show the classification accuracy as a function of acquisition time T_N and the number of wavelengths L, respectively. The accuracy improved as T_N and L increased. For instance, an accuracy of nearly 95% was achieved with L ≥ 6 at the acquisition rate of up to 1/T_N = 1 Gfps [Fig. 7(d)].

FIG. 5. (a) The time-domain signal encoding the switching behavior of the DMD display images from digit “5” to digit “0”. The switching process occurred around 50 μs. In this demonstration, we set T_N = 20 ns for a clear display. The waveforms before and after the switching process are shown in (b) and (c), respectively. (d) Correlation value C_i(t_j) for digit “i” (i = 0 and 5) as a function of discrete time t_j = jT_N ( j = 0, 1, · · · ). The correlation analysis clearly reveals the fast switching of the DMD display images from “5” to “0” with a relaxation oscillation.

FIG. 6. Performance of the single-pixel image classification for the testing database, as demonstrated by normalized confusion matrices for (a) the experimental results and (b) the numerical results. In the experiment, we set the acquisition time T_N to 6 ns (corresponding to N = 300, the number of the features used for classification). In the numerical simulations, we used a Gaussian random matrix as a measurement matrix and generated N =300 features for the input to the neural network classifier. The neural network model for the classification was the same as that used for the experimental results. The classification accuracies for the experiment and numerical simulations were 92.6 % and 98.4 %, respectively.

IV. SUMMARY AND DISCUSSION

The main contribution of this work is the experimental demonstration of an ultrafast method for dynamic speckle pattern generation based on high-speed phase modulation. The generation of the speckle patterns can be controlled with the phase modulation rate. The speckle generation at over 10 GS/s-modulation rates is much faster than the conventional approach using SLMs. We also demonstrated a single-pixel image classification using the proposed speckle pattern generation approach, and we showed that our approach can overcome the major bottleneck of image capture and achieve an acquisition rate of nearly 1 Gfps. Further improvement is possible by combining this technique with various multiplexing techniques. We expect that the proposed approach of fast speckle generation is potentially applicable not only for highspeed image classification but also for frame rate improvement of imaging [2, 13] or dynamic target tracking [31–33].

Despite the advantages of the proposed approach, there is room for further improvement. One such improvement would be better system stability for the speckle pattern generation. Because speckle pattern generation utilizes a long MMF, it is highly sensitive to thermal, vibrational, and phonic noises, which can fluctuate the speckle patterns and thereby degrade the classification performance. One way to minimize these external perturbations is to isolate the MMF from the external environment by placing it inside an isolation box [34]. Considering that the modal distortions induced in an MMF are essentially linear phenomena, they can be compensated for by controlling the fiber geometry (i.e., the fiber bending) [35]. Another way is to use a more compact photonic scattering device, such as an on-chip disordered photonic chip [36], or the combination of a photonic chip and a shorter MMF instead of solely using a long MMF.

Secondly, it is important to increase the number of independent speckle patterns M generated from the system for applications in image reconstruction. We roughly estimated M = C^{−2} ≈ 59 from the speckle contrast shown in Fig. 2(b). Although this estimation is based on the assumption that the speckle patterns were independent and had equal intensities, the estimated number M is far fewer than expected from the number of the guided modes (∼ 10^4) in the MMF. This may be

FIG. 7. Top two panels: schematics of (a) parallel speckle pattern generation system based on wavelength-division multiplexing and (b) measurement system for wavelength-demultiplexing. MUX and DEMUX represent the optical multiplexer and optical demultiplexer, respectively. Bottom two panels: classification accuracy as a function of (c) acquisition time T_N and (d) the number of multiplexed wavelengths L. For L ≥ 6 and T_N > 1 ns, the accuracy exceeded 97%, which is comparable to the numerical result shown in Fig. 6(b). The inset in (c) shows the accuracy in the range of T_N <1 ns.

attributed to the fact that (i) not all guided modes are excited in the present system and/or (ii) the generated speckles are correlated with each other. This weakness may be alleviated using an algorithm that imposes no strict limitation on uncorrelated speckles [17]. In addition, the wavelength-division multiplexing techniques will be effective for the generation of more independent speckle patterns in parallel. Therefore, for an input wavelength of L, the number of the patterns is LM. For instance, we can generate LM =1200 patterns for M = 60 and L = 20 (with 1 nm intervals ranging from 1540 nm to 1560 nm), which is sufficient for the reconstruction of an MNIST image (with 28×28 pixels). Further improvement can be made by incorporating a space-division multiplexing using multicore fiber receivers in the proposed approach. The imageencoding based on space- and wavelength-division multiplexing techniques will be reported in a future paper.

An interesting future study could involve combining the proposed approach with photonic reservoir computing circuits [37–39], which enable high-speed processing for timedependent signals. In conventional schemes, the image information is electrically converted into time-domain signals with a mask [39], but with our approach, the process can be accomplished optically. In other words, the proposed system can be utilized as a photonic preprocessor of reservoir computing for high-speed dynamic scene capture. This opens a novel pathway toward the realization of all-optical computing. ACKNOWLEDGMENTS

This work was partly supported by JST PRESTO (JP- MJPR19M4), JSPS KAKENHI (20H04255), Grant for Basic Science Research Projects from the Sumitomo Foundation (210495), and JKA promotion funds from KEIRIN RACE (2022M-208).

[1] G. M. Gibson, S. D. Johnson, and M. J. Padgett, Single-pixel

imaging 12 years on: a review, Opt. Express 28, 28190 (2020). [2] C. F. Higham, R. Murray-Smith, M. J. Padgett, and M. P. Edgar,

Deep learning for real-time single-pixel video, Scientific Reports 8, 2369 (2018).

[3] M. F. Duarte, M. A. Davenport, D. Takhar, J. N. Laska, T. Sun,

K. F. Kelly, and R. G. Baraniuk, Single-pixel imaging via compressive sampling, IEEE Signal Processing Magazine 25, 83 (2008).

[4] B. Sun, M. P. Edgar, R. Bowman, L. E. Vittert, S. Welsh, A. Bowman, and M. J. Padgett, 3d computational imaging with single-pixel detectors, Science 340, 844 (2013).

[5] Y. Bromberg, O. Katz, and Y. Silberberg, Ghost imaging with a single detector, Phys. Rev. A 79, 053840 (2009).

[6] Z. Ye, H.-C. Liu, and J. Xiong, Computational ghost imaging with spatiotemporal encoding pseudo-random binary patterns, Opt. Express 28, 31163 (2020).

[7] X.-H. Chen, Q. Liu, K.-H. Luo, and L.-A. Wu, Lensless ghost imaging with true thermal light, Opt. Lett. 34, 695 (2009).

[8] B. I. Erkmen, Computational ghost imaging for remote sensing, J. Opt. Soc. Am. A 29, 782 (2012).

[9] S. Sunada, K. Kanno, and A. Uchida, Using multidimensional speckle dynamics for high-speed, large-scale, parallel photonic computing, Opt. Express 28, 30349 (2020).

[10] A. Saade, F. Caltagirone, I. Carron, L. Daudet, A. Drémeau, S. Gigan, and F. Krzakala, in 2016 IEEE International Conference on Acoustics, Speech and Signal Processing (ICASSP) (2016), p. 6215, ISSN 2379-190X.

[11] X. Gao, Y. Li, Y. Qiu, B. Mao, M. Chen, Y. Meng, C. Zhao, J. Kang, Y. Guo, and C. Shen, Improvement of image classification by multiple optical scattering, IEEE Photonics Journal 13, 1 (2021).

[12] E. Hahamovich, S. Monin, Y. Hazan, and A. Rosenthal, Single pixel imaging at megahertz switching rates via cyclic hadamard masks, Nature Communications 12, 4516 (2021).

[13] Z.-H. Xu, W. Chen, J. Penuelas, M. Padgett, and M.-J. Sun, 1000 fps computational ghost imaging using led-based structured illumination, Opt. Express 26, 2427 (2018).

[14] G. Wang, C. K. Mididoddi, F. Bai, S. Gibson, L. Su, J. Liu, and C. Wang, Ultrafast optical imaging using multimode fiber based compressed sensing and photonic time stretch, arXiv:1803.03061.

[15] W. Shi, C. Hu, S. Yang, M. Chen, and H. Chen, Optical random speckle encoding based on hybrid wavelength and phase modulation, Opt. Lett. 46, 3745 (2021).

[16] T. Fukui, Y. Kohno, R. Tang, Y. Nakano, and T. Tanemura, Single-pixel imaging using multimode fiber and silicon photonic phased array, J. Lightwave Technol. 39, 839 (2021).

[17] C. Deng, J. Suo, Y. Wang, Z. Zhang, and Q. Dai, Single-shot thermal ghost imaging using wavelength-division multiplexing, Applied Physics Letters 112, 051107 (2018).

[18] Y. Wang, Y. Liu, J. Suo, G. Situ, C. Qiao, and Q. Dai, High speed computational ghost imaging via spatial sweeping, Scientific Reports 7, 45325 (2017).

[19] G. C. Valley, G. A. Sefler, and T. J. Shaw, Multimode waveguide speckle patterns for compressive sensing, Opt. Lett. 41, 2529 (2016).

[20] E. G. Rawson, J. W. Goodman, and R. E. Norton, Frequency dependence of modal noise in multimode optical fibers, J. Opt. Soc. Am. 70, 968 (1980).

[21] B. Redding, S. M. Popoff, and H. Cao, All-fiber spectrometer based on speckle pattern reconstruction, Opt. Express 21, 6584 (2013).

[22] J. W. Goodman, Speckle phenomena in optics: theory and applications (Roberts and Company Publishers, 2007).

[23] Y. LeCun, C. Cortes, and C. J. C. Burges, The mnist database of handwritten digits.

[24] Y. Lecun, L. Bottou, Y. Bengio, and P. Haffner, Gradient-based learning applied to document recognition, Proceedings of the

IEEE 86, 2278 (1998).

[25] J. Bacca, C. V. Correa, E. Vargas, S. Castillo, and H. Arguello, in 2019 IEEE 29th International Workshop on Machine Learning for Signal Processing (MLSP) (2019), p. 1, ISSN 1551- 2541.

[26] S. Ota, R. Horisaki, Y. Kawamura, M. Ugawa, I. Sato, K. Hashimoto, R. Kamesawa, K. Setoyama, S. Yamaguchi, K. Fujiu, et al., Ghost cytometry, Science 360, 1246 (2018).

[27] Z. Zhang, X. Li, S. Zheng, M. Yao, G. Zheng, and J. Zhong, Image-free classification of fast-moving objects using “learned” structured illumination and single-pixel detection, Opt. Express 28, 13269 (2020).

[28] S. Jiao, J. Feng, Y. Gao, T. Lei, Z. Xie, and X. Yuan, Optical machine learning with incoherent light and a single-pixel detector, Opt. Lett. 44, 5186 (2019).

[29] S. Kumar, T. Bu, H. Zhang, I. Huang, and Y. Huang, Robust and efficient single-pixel image classification with nonlinear optics, Opt. Lett. 46, 1848 (2021).

[30] D. P. Kingma and J. Ba, Adam: A method for stochastic optimization, arXiv preprint arXiv:1412.6980 (2014).

[31] L. Zha, D. Shi, J. Huang, K. Yuan, W. Meng, W. Yang, R. Jiang, Y. Chen, and Y. Wang, Single-pixel tracking of fast-moving object using geometric moment detection, Opt. Express 29, 30327 (2021).

[32] D. Shi, K. Yin, J. Huang, K. Yuan, W. Zhu, C. Xie, D. Liu, and Y. Wang, Fast tracking of moving objects using single-pixel imaging, Optics Communications 440, 155 (2019).

[33] L. Zha, W. Meng, D. Shi, J. Huang, K. Yuan, W. Yang, Y. Chen, and Y. Wang, Complementary moment detection for tracking a fast-moving object using dual single-pixel detectors, Opt. Lett. 47, 870 (2022).

[34] Q. Vinckier, F. Duport, A. Smerieri, K. Vandoorne, P. Bienstman, M. Haelterman, and S. Massar, High-performance photonic reservoir computer based on a coherently driven passive cavity, Optica 2, 438 (2015).

[35] D. Z. Anderson, M. A. Bolshtyansky, and B. Y. Zel’dovich, Stabilization of the speckle pattern of a multimode fiber undergoing bending, Opt. Lett. 21, 785 (1996).

[36] B. Redding, S. F. Liew, R. Sarma, and H. Cao, Compact spectrometer based on a disordered photonic chip, Nature Photonics 7, 746 (2013).

[37] K. Vandoorne, P. Mechet, T. Van Vaerenbergh, M. Fiers, G. Morthier, D. Verstraeten, B. Schrauwen, J. Dambre, and P. Bienstman, Experimental demonstration of reservoir computing on a silicon photonics chip, Nature Communications 5, 3541 (2014).

[38] S. Sunada and A. Uchida, Photonic neural field on a silicon chip: large-scale, high-speed neuro-inspired computing and sensing, Optica 8, 1388 (2021).

[39] M. Nakajima, K. Tanaka, and T. Hashimoto, Scalable reservoir computing on coherent linear photonic processor, Communications Physics 4, 20 (2021).