arXiv:2306.02032v1 [cs.IT] 3 Jun 2023

ADMM-based Detector for Large-scale MIMO Code-domain NOMA Systems

Vinjamoori Vikas^1, Kuntal Deka^1, Sanjeev Sharma^2, and A. Rajesh^1 1Indian Institute of Technology Guwahati, India,^2Indian Institute of Technology (BHU) Varanasi, India

Abstract

Large-scale multi-input multi-output (MIMO) code domain non-orthogonal multiple access (CD-NOMA) techniques are one of the potential candidates to address the next-generation wireless needs such as massive connectivity, and high reliability. This work focuses on two primary CD-NOMA techniques: sparse-code multiple access (SCMA) and dense-code multiple access (DCMA). One of the primary challenges in implementing MIMO-CD-NOMA systems is designing the optimal detector with affordable computation cost and complexity. This paper proposes an iterative linear detector based on the alternating direction method of multipliers (ADMM). First, the maximum likelihood (ML) detection problem is converted into a sharing optimization problem. The set constraint in the ML detection problem is relaxed into the box constraint sharing problem. An alternative variable is introduced via the penalty term, which compensates for the loss incurred by the constraint relaxation. The system models, i.e., the relation between the input signal and the received signal, are reformulated so that the proposed sharing optimization problem can be readily applied. The ADMM is a robust algorithm to solve the sharing problem in a distributed manner. The proposed detector leverages the distributive nature to reduce per-iteration cost and time. An ADMM-based linear detector is designed for three MIMO-CD-NOMA systems: single input multi output CD-NOMA (SIMO-CD-NOMA), spatial multiplexing CD-NOMA (SMX-CD-NOMA), and spatial modulated CD-NOMA (SM-CD-NOMA). The impact of various system parameters and ADMM parameters on computational complexity and symbol error rate (SER) has been thoroughly examined through extensive Monte Carlo simulations.

Index Terms

Code domain-NOMA (CD-NOMA), dense code multiple access (DCMA), sparse code multiple access (SCMA), alternating direction method of multipliers (ADMM), single input multi output (SIMO), spatial multiplexing MIMO (SMX-MIMO), spatial modulation MIMO (SM-MIMO).

I. INTRODUCTION A. Motivation

The existing literature extensively studies two types of code domain non-orthogonal multiple access (CD-NOMA) systems. The first type is sparse coded CD-NOMA systems, which utilize low-density spreading sequence design (e.g., low-density signatures (LDS)) or sparse codebook design (e.g., sparse code multiple access (SCMA)) [1]. The second type is densely coded CD- NOMA systems, which utilize dense spreading sequence design (e.g., overloaded code-division multiple access (CDMA)) or dense codebook design (e.g., dense code multiple access (DCMA)) [2]. Throughout the paper, dense codebook-based NOMA is referred to as DCMA, and dense spreading sequence-based NOMA is referred to as overloaded CDMA.

SCMA and DCMA are critical enabling technologies to improve spectral efficiency and massive connectivity by overloading multiple user equipment’s (UEs) data on a single resource element (RE). These techniques exploit the codebooks’ multi-dimensional constellation (MDC) coding gain. Spreading sequence-based NOMA (LDS, overloaded CDMA) does not benefit from the coding gain of the MDC. Thus, codebook-based NOMA techniques offer substantial error rate performance gains over the spreading sequence-based NOMA.

Multi-input multi-output (MIMO) technology is another crucial enabler in improving spectral efficiency and system reliability [3]. CD-NOMA systems using a MIMO system (MIMO-CD- NOMA) offer even greater spectral efficiency, reliability, and massive connectivity improvements. This paper considers three types of uplink (UL) MIMO-CD-NOMA systems: (1) Single-input multi-output (SIMO) aided CD-NOMA, where each UE has a single antenna [4]; (2) Spatial multiplexing-CD-NOMA (SMX-CD-NOMA), where each UE is equipped with multiple transmit antennas [5]; and (3) Spatial modulated CD-NOMA (SM-CD-NOMA), where each UE activates a single transmit antenna out of multiple transmit antennas at the UE [6]. The primary challenge in implementing MIMO-CD-NOMA systems lies in designing a multiuser signal detector that offers excellent performance while maintaining affordable complexity.

The message passing algorithm (MPA) is usually used in SCMA detection [7], [8]. However, the MPA for MIMO-SCMA signal detection [9], [10] needs to improve its computational complexity. MPA detection over the MIMO-SCMA system uses an extended factor graph due to the additional antennas at the UEs and the BS [11]. The MPA exhibits exponential complexity with the codebook size (M), the number of UEs (J), and the number of transmit antennas. Thus, MPA becomes impractical for highly overloaded SCMA systems over large-scale MIMO systems. Further, MPA often faces convergence issues when the factor graph contains cycles. To overcome the limited diversity issues (due to sparsity) in SCMA, researchers have recently started designing the DCMA systems [2]. However, MPA demands sparsity for the accurate detection of codewords. DCMA codewords do not hold sparsity properties. Due to enormous short cycles in the DCMA factor graph, MPA is no longer a suitable detector for DCMA systems. Thus, an alternate detection algorithm must be developed to achieve the full diversity offered by DCMA with minimal detection complexity.

DRAFT June 6, 2023

The generalized sphere decoder (GSD) is used as a detector for a spread sequence-based DCMA system by considering a single antenna at both the base station (BS) and the UE [2]. The GSD works on principles of the tree search algorithm. Its complexity depends on the number of tree nodes and floating point operations (FLOPs) at each node. The number of tree nodes will increase multifold in the codebook-based DCMA systems. Moreover, the complexity of GSD increases rapidly for large-scale MIMO DCMA systems. So, it is not an efficient detector for large-scale MIMO CD-NOMA systems. Designing a low-complexity multiuser detector (MUD) for large-scale MIMOaided CD-NOMA systems with higher overloading factors (λ) and modulation order/codebook-size (M) is becoming essential. The existing research studies mainly nonlinear detectors (MPA and sphere decoder) for CD-NOMA systems [7], [12]. On the other hand, minimum mean square error (MMSE) and zeros forcing (ZF) are commonly used linear detectors in standalone MIMO systems [13]. These detectors are simple to implement and they exhibit low computational complexity over nonlinear detectors. However, these detectors show poor symbol error rate (SER) performance over CD-NOMA systems with high λ values. In addition, they fail to detect the CD-NOMA signals as M increases. Thus, designing an efficient detector with low complexity is mandatory to fully unfurl the benefits of MIMO CD-NOMA systems with a practically viable approach. Further, the detector must perform better than the existing linear detectors for large-scale CD-NOMA parameters (λ, M).

B. Related prior works

Recently, the ADMM has been widely used to solve convex and non-convex problems in a distributed manner [14]. Glowinski and Marrocco first proposed the ADMM in the mid-1970s. Later on, Boyd et al. rigorously discussed various complex optimization problems that can be solved using ADMM in their tutorial [14]. The ADMM is formed by the composition of dual ascent and the method of multipliers. The dual decomposition properties of dual ascent make the ADMM solve in a distributed manner. ADMM has superior convergence properties and often is able to converge without the requirement of strict convexity. A comprehensive treatment of ADMM and its advancements are detailed in [15].

The ADMM is extensively applied to solve the linear programming (LP) problem in low-density parity-check code’s (LDPC) decoding [16], [17]. The authors here have also shown that the ADMM significantly reduces the complexity of the decoder compared to the belief propagation (BP) methods. The MUD problem of UL grant-free NOMA is solved by using ADMM [18]. The ADMMbased infinity norm (ADMIN) iterative linear detector is proposed for massive MIMO systems [19]. The authors have also proposed VLSI architecture for the ADMIN detector. The results show that ADMIN outperforms all the linear detectors in terms of SER performance and low hardware cost compared to the nonlinear BP-based detectors. Similarly, an ADMM-based QAM signal detector for massive MIMO systems is proposed [20]. A distributed penalty sharing (DPS) ADMM method is designed to convert the maximum-likelihood (ML) detection problem into sharing optimization problem. This method shows good performance and complexity trade-offs for massive MIMO systems. The authors in [19], [20] show that the ADMM-based detector performs MMSE equalization in the first iteration. The performance of the ADMM improves over MMSE as iterations progress.

C. Contributions:

This paper proposes an ADMM-based iterative linear detector that solves the MUD problem of large-scale MIMO-aided CD-NOMA systems. It exhibits the best trade-off between the SER performance and computational complexity for SCMA and DCMA systems. We have formulated the highly computationally complex ML detection problem of large-scale MIMO-CD-NOMA systems as the non-convex distributed optimization problem. To the best of the authors’ knowledge, this is the first attempt to convert the ML detection problem of CD-NOMA into a sharing problem. Further, the ADMM approach is applied to solve the proposed sharing problem using distributed optimization. The proposed ADMM-based detector is guaranteed to improve the error rate performance over linear detectors with lower computational complexity than nonlinear detectors. The main contributions of this work are listed below:

• The ML MUD problem is nondeterministic polynomial-time hard (NP-hard) and can be solved using exhaustive search [21]. However, the complexity of the exhaustive search increases exponentially as the number of UEs and codebook size increase. The ML problem is transformed into a non-convex sharing optimization problem to overcome this challenge. An efficient distributed optimization method is then applied to solve the proposed sharing problem.

• The CD-NOMA system models, i.e., the relationships between the input signal and received signal, are reformulated so that the sharing ADMM algorithm can be readily applied for detection. For SIMO-CD-NOMA, the signal received by multiple antennas at BS is considered as a single observation vector for detection. For SMX-CD-NOMA and SM-CD-NOMA, resourcewise processing of the received signal is carried out during ADMM detection.

• A low-complexity iterative linear detector is designed via the ADMM approach to solve the sharing optimization problem for large-scale MIMO-CD-NOMA systems. ADMM solves the sharing optimization problem through a distribution optimization framework. Indeed, distributive nature of sharing ADMM allows parallel processing in multiuser detection, reducing periteration computational time.

DRAFT June 6, 2023

• The proposed ADMM-based detector is applied to large-scale MIMO (SIMO, SMX-MIMO, and SM-MIMO) aided CD-NOMA systems. Thus, the proposed single ADMM-based MUD is capable of solving the detection problem of various CD-NOMA systems.

• The complexity of the proposed ADMM-based detector is independent of the CD-NOMA system’s codebook size/modulation order (M), unlike the conventional MPA detector. Thus, it can be applied to large-size codebooks. The impact of the different MIMO-CD-NOMA system parameters is also thoroughly examined. The ADMM-based detector exhibits polynomial complexity with all other parameters, such as the numbers of antennas, UEs, and REs.

• The comparison of the error rate performance and receiver complexity of the proposed ADMMbased detector with all other conventional detectors is thoroughly examined. Comprehensive Monte Carlo simulations indicate that the ADMM-based detector substantially reduces the computational complexity while maintaining an error performance comparable to the MPA in SCMA detection. For spread sequence-based DCMA, the ADMM gives superior performance than GSD.

D. Organization:

The paper is organized as follows. The preliminaries of the existing CD-NOMA system models and sharing ADMM problem are discussed in Section II. The proposed system models and ADMMbased detection for UL MIMO-CD-NOMA systems are provided in Section III. Section IV presents a detailed computational complexity analysis. The simulation results for different MIMO-CD- NOMA systems are discussed in Section V. Section VI concludes the paper and mentions future scopes.

Notations: Lower case, bold lower case, and bold upper case letters denote scalars, vectors, and matrices, respectively. (·)^T and (·)^H denote transpose and Hermitian transpose, respectively. ‖(·)‖ denotes the Euclidean norm of a vector. ∏ [−α,α](·) denotes the Euclidean projection onto the interval

[−α, α]. ⟨·, ·⟩ denotes the inner product, and Re(·) denotes the real part of a complex variable. R^n and C^n denote n-dimensional real and complex vector spaces, respectively. CN (0, σ^2) denotes complex Gaussian distribution with zero mean and variance σ^2.

II. PRELIMINARIES This section mainly discusses the existing CD-NOMA system models and steps to solve the sharing optimization problem via the ADMM approach. The CD-NOMA techniques can be broadly divided into sparse-coded and dense-coded NOMA. Low-density signature (LDS) [22] and SCMA [23] belong to the first group, whereas overloaded CDMA [2] and DCMA [2] belong to the second group. LDS and overloaded CDMA are sequence-based CD-NOMA techniques where mapping and spreading are performed separately. LDS utilizes sparse sequences, while overloaded CDMA employs dense sequences. These techniques suffer from error performance loss due to limited coding gain. On the other hand, SCMA and DCMA are codebook-based CD-NOMA techniques. In these systems, the data of each UE is mapped to a multi-dimensional codeword. SCMA utilizes sparse codewords, while DCMA applies dense codewords. These techniques offer error performance benefits through the use of MDCs [24]. A. SCMA system model

SCMA is a sparse codebook-based NOMA technique. Each UE’s data is sent in the form of sparse codewords. Consider a CD-NOMA system having J UEs accessing K REs, where J > K ensures the overloading nature of SCMA. Each UE in the SCMA system has access to d_v < K active REs among K REs. Thus, d_v non-zero elements are present in the K-dimensional sparse codewords. The SCMA encoder maps each UE bitstream to a sparse codeword x^{K×1} in a pre-designed SCMA codebook X^{K×M} of the respective UE. The sparse nature of SCMA codewords enforces d_f < J number of overlapping UEs on each RE. The diversity order of SCMA is essentially limited to d_v, i.e., far less than the maximum possible diversity order K. For example, the codebook structure for 150 % overloaded SCMA system (d_v = 2, and d_f = 3) is shown in Fig. 1(a). The received signal vector is given by r = J∑ j=1 diag(h_j )x_j + w, (1)

where

• w ∼ CN (0, σ^2I_K ) denotes the additive white Gaussian noise (AWGN) at the receiver. • h_j ∼ CN (0, I_K ) denotes the Rayleigh fading channel vector for the jth UE. • diag(h = [h[1], . . . , h[k], . . . , h[K]]^T ) denotes diagonal matrix and h[k] is the kth diagonal element.

• x_j is the K-dimensional codeword of jth UE. B. DCMA system model

The error performance of SCMA suffers from limited diversity order. This limitation of SCMA can be overcome by using dense codebooks in the DCMA system [2]. Each UE in the DCMA system has access to all K REs. No zero entries are present in the K-dimensional dense codewords. Therefore, the DCMA system exploits the full diversity of multi-dimensional codewords. For example, the codebook structure of 150 % overloaded DCMA system is shown in Fig. 1(b). The received signal vector for the DCMA system is similar to that of the SCMA system, as described in (1). In addition to the codebook-based DCMA system, the spread sequence-based DCMA can be designed with non-orthogonal spreading sequences. The idea is similar to the overloaded CDMA systems. The number of UEs is larger than the length of the spreading sequence. Uni-modular spreading sequences have been used in this paper to achieve full diversity of the dense sequences [2].

DRAFT June 6, 2023

(a) SCMA codebook structure (b) DCMA codebook structure

Fig. 1: CD-NOMA codebook structure for J = 6 and K = 4. C. Shared ADMM problem

This subsection introduces the fundamental concepts of solving sharing problems using ADMM within a distributed optimization framework. A novel method, referred to as ADMM, was proposed to address both convex and non-convex sharing optimization problems [14]. The subsequent subsection delves into the details and ideas behind the sharing ADMM problem. The ADMM is formed by combining the superior properties of dual ascent and the method of multipliers. This combination ensures the robustness of ADMM [14]. The generic sharing problem is

min N∑ i=1 f_i(x_i) + g (_N ∑ i=1 x_i ) , (2)

where x_i ∈ R^n , i = 1, . . . , N, the associated local cost function f_i(x_i)(f_i : R^n → R) of subsystem i is handled by processor i, and g (g : R^n → R) is the shared objective, whose argument is the sum of N variables. Each variable x_i is involved in minimizing the individual cost f_i(x_i), as well as the shared objective g (∑_N i=1 x_i ) . The sharing problem can be converted into an ADMM problem by introducing an alternative variable, z_i ∈ R^n . Thus, the cost function is minimized over x_i and z_i, alternatively. The problem (2) is converted to the following problem:

min N∑ i=1 f_i(x_i) + g (_N ∑ i=1 z_i ) (3) s.t. x_i − z_i = 0 i = 1, . . . , N.

The augmented Lagrangian function for (3) can be written as

L ( {x_i, z_i, y_i}^N_{i=1} ) = N∑ i=1 f_i(x_i) + g (_N ∑ i=1 z_i ) + N∑ i=1 ⟨x_i − z_i, y_i⟩ + ρ 2 N∑ i=1 ‖x_i − z_i‖^2 (4) where x_i, z_i are called primal variables, y_i ∈ R^n is the Lagrangian variable and ρ > 0 is called the penalty parameter. The function in (4) can be minimized by the ADMM steps [14]

x^{t+1}_i := argmin_{xi} ( f_i(x_i) + ρ 2 ‖x_i − z^t_i + u^t_i‖^2 ) (5)

z^{t+1}_i := argmin_{zi} g (_N ∑ i=1 z_i ) + ρ 2 N∑ i=1 ‖z_i − u^t_i − x^{t+1}_i ‖^2 (6)

u^{t+1}_i := u^t_i + x^{t+1}_i − z^{t+1}_i (7)

where u_i is called a dual variable (scaled version of Lagrangian variable, u_i =^{yi}_ρ ). The problems (5) and (7) can be solved in parallel for i = 1, . . . , N. Let q_i = u^t_i + x^{t+1}_i . Then (6) can be rewritten as

min g (_N ∑ i=1 z_i ) + ρ 2 N∑ i=1 ‖z_i − q_i‖^2 (8)

s.t z̄ = 1 N N∑ i=1 z_i

with fixed variable z̄ ∈ R^n . The problem (8) has the following solution

z_i = q_i + z̄ − q̄, where q̄ = 1 N N∑ i=1 q_i = ū^t + x̄^{t+1}, (9)

ū^t = 1 N N∑ i=1 u^t_i, and x̄^{t+1} = 1 N N∑ i=1 x^{t+1}_i .

From (8) and (9), the z̄-update step can be simplified to the following unconstrained problem:

min g(Nz̄) + ρ 2 N∑ i=1 ‖z̄ − q̄|. (10)

Substituting (9) for z^{t+1}_i into (7), the ū-update step is

u^{t+1}_i = ū^t + x̄^{t+1} − z̄^{t+1} (11)

The dual variables {u^t_i}^N_{i=1} are equal and can be replaced by a single variable u^t. The ADMM steps are simplified as follows

x^{t+1}_i := argmin_{xi} ( f_i(x_i) + ρ 2 ‖x_i − x^t_i + x̄^t − z̄^t + u^t‖^2 ) (12)

z̄^{t+1} := argmin_{z̄} ( g(Nz̄) + Nρ 2 ‖z̄ − u^t − x̄^{t+1}‖^2 ) (13)

u^{t+1} := u^t + x̄^{t+1} − z̄^{t+1} (14)

The original sharing problem (2) is decomposed into a three-step iterative optimization problem. The problem (12) can be solved in parallel for i = 1, . . . , N. The step (13) solves the shared objective, and (14) is the dual variable update step.

DRAFT June 6, 2023

III. ADMM-BASED DETECTION FOR UL CD-NOMA SYSTEMS This section focuses on reformulating the relation between the input and received signals of three multi-antenna CD-NOMA system models. These models are 1. SIMO-CD-NOMA, 2. Spatial multiplexing CD-NOMA (SMX-CD-NOMA), and 3. Spatial modulated CD-NOMA (SM-CD-NOMA). The reformulated models are readily applied for sharing ADMM-based detection process. These models, along with the derivation of the ADMM steps, are described in the following.

A. SIMO CD-NOMA

Consider a UL scenario with the BS equipped with N_r antennas and each UE having a single antenna. The idea is to exploit the spatial diversity gain offered by multiple receive antennas at BS [25]. The error rate performance of the CD-NOMA system with N_r antennas at the receiver is significantly improved [4] due to higher diversity gain. The K × 1 observation vector at n_rth BS antenna can be expressed as

r^{(nr)} = J∑ j=1 diag ( h^{(nr)}_j ) x_j + w^{(nr)}, n_r = 1, . . . , N_r

where

• w^{(nr)} ∼ CN (0, σ^2I_K ), K × 1 vector assumed to be independent and identically distributed (i.i.d.), AWGN at the n_rth BS antenna.

• h^{(nr)}_j ∼ CN (0, I_K), K × 1 vector assumed to be i.i.d. complex Gaussian random vector, denotes Rayleigh fading channel coefficients between the jth UE and n_rth BS antenna. h^{(nr)}_j = [h[1] . . . h[k] . . . h[K]]^T and diag ( h^{(nr)}_j ) denotes diagonal matrix with h[k] being the kth diagonal element.

• x_j = [x_j [1] . . . x_j [k] . . . x_j [K]]^T is a codeword from the jth UE’s codebook, X^{K×M}_j . The overall KN_r × 1 observation vector at the BS for the SIMO CD-NOMA system is given by

r = Hx_{mu} + w, (15)

where

• r = [r^{(1)T} . . . r^{(nr)T} , . . . , r^{(Nr)T} ]^T .

• w ∼ CN (0, σ^2I_{KNr} ), N_rK × 1 vector denotes the AWGN vector at the BS. • x_{mu} is the JN_e × 1 multi-user concatenated transmitted signal.

x_{mu} = [x_1[1] . . . x_1[N_e] . . . x_j [1] . . . x_j [N_e] . . . x_J [1] . . . x_J [N_e]]^T , where N_e is the number of nonzero elements in codeword. We have N_e = K and N_e = d_v for DCMA and SCMA, respectively. The transmitted signal x_{mu} can be rewritten to facilitate the sharing-based detection problem in Section III-D i.e., x_{mu} = ∑_J j=1 x_{0j} . The variable x_{0j} = [0 . . . 0 x_j [1] x_j [2] . . . x_j [N_e] 0 . . . 0]^T represents the jth UE codeword.

• The channel matrix for DCMA system of size KN_r × JK is given by

H = diag(h^{(1)}_1 ) . . . diag(h^{(1)}_j ) . . . diag(h^{(1)}_J ) diag(h^{(2)}_1 ) . . . diag(h^{(2)}_j ) . . . diag(h^{(2)}_J ) . . . . . . . . . . . . diag(h^{(Nr)}_1 ) . . . diag(h^{(Nr)}_j ) . . . diag(h^{(Nr)}_J ) .

• The channel matrix for SCMA system of size KN_r × Jd_v is given by

H = diag(h^{(1)}_1 ) . . . diag(h^{(1)}_j ) . . . diag(h^{(1)}_J ) diag(h^{(2)}_1 ) . . . diag(h^{(2)}_j ) . . . diag(h^{(2)}_J ) . . . . . . . . . . . . diag(h^{(Nr)}_1 ) . . . diag(h^{(Nr)}_j ) . . . diag(h^{(Nr)}_J ) .

where diag ( h^{(Nr)}_j ) is K × d_v matrix after removing the columns in diag(h^{(Nr)}_j ) corresponding to zero elements of jth UE codeword x_j (inactive REs of jth UE).

Example 1. Consider the factor graph matrix for the 150 % overloading SCMA system with K = 4, J = 6, d_f = 3, d_v = 2:

F = 1 0 1 0 1 0 0 1 1 0 0 1 1 0 0 1 0 1 0 1 0 1 1 0

. (16)

For the 1st UE and the n_rth receiving antenna, the channel matrix is given below:

diag(h^{(nr)}_1 ) = h^{(nr)}_1 [1] 0 0 0 0 h^{(nr)}_1 [3] 0 0 .

The transmitted signal from all UEs is given by

x_{mu} = x_1[1] x_1[3]

UE 1

x_2[2] x_2[4]

UE 2

x_3[1] x_3[2]

UE 3

x_4[3] x_4[4]

UE 4

x_5[1] x_5[4]

UE 5

x_6[2] x_6[3]

UE 6

T . (17)

The 3rd UE codeword x_{03} in x_{mu} is given by

x_{03} = 0 0 UE_1 0 0_{UE 2} x^3[1] x^3[2]

UE 3 0 0 UE 4 0 0 UE 5 0 0 UE 6

T . (18)

The variables {x_{0j} }^J_{j=1} are similarly represented as x_{03}. Note that, the transmitted signal x_{mu} can be written as, x_{mu} =

∑_6 j=1 x_{0j} .

DRAFT June 6, 2023

B. SMX-CD-NOMA

The spectral efficiency of the UL CD-NOMA system is further enhanced by placing multiple antennas at the transmitter [5]. Multiple antennas at both transmitter and receiver of the CD-NOMA system are considered in this section. Multiple antennas at the transmitter exploit multiplexing gain offered by spatially multiplexing several data streams onto the MIMO channel. Consider a scenario where each UE is equipped with N_t transmitting antennas, and the BS is equipped with N_r receiving antennas. The total input data at each UE, N_tlog_2(M) bits, are divided into N_t parallel data streams. Each data stream is fed to the CD-NOMA encoder, as shown in Fig. 2. Note that in the SMX-CD-NOMA system, all the UE antennas transmit data simultaneously. The main challenge of SMX-CD-NOMA in practical implementation is the computational complexity at both transmitter and receiver. Further, detecting the data transmitted from multiple antennas of multiple UEs is a complex operation. The proposed method performs resource-wise processing at the BS via the ADMM algorithm, as shown in Fig. 3.

Fig. 2: SMX-CD-NOMA system model in the UL.

The received signal at the BS over the kth RE is given by

r_k = H_kx_{smx,k} + w_k, (19)

where

• r_k = [r^1_k . . . r^{nr}_k . . . r^{Nr}_k ]^T , N_r × 1 observation vector.

• w_k ∼ CN (0, σ^2I_{Nr} ), N_r × 1 vector denotes the AWGN at the BS over kth RE. • x_{smx,k} is the N_uN_t ×1 transmitted vector on kth RE. x_{smx,k} = [x^T_{1,k} . . . x^T_{j,k} . . . x^T_{Nu,k}]^T , and each x_{j,k} = [x_{j,k,1} . . . x_{j,k,nt} . . . x_{j,k,Nt} ]^T is N_t ×1 vector corresponding to jth UE. Each x_{j,k,nt} ∈ x^{nt}_j is the symbol transmitted from n_tth antenna of jth UE over kth RE, where x^{nt}_j is the codeword of jth UE transmitted from n_tth antenna. The set ζ_k represents the set of UEs overlapping on kth RE given by ζ_k = {j : x_j[k] ≠ 0; 1 ≤ j ≤ J}, and |ζ_k| = N_u,

where N_u = d_f and N_u = J for SCMA and DCMA, respectively.

The transmitted signal x_{smx,k} can be rewritten to formulate the sharing-based detection problem in Section III-D i.e., x_{smx,k} = ∑_{Nu} j=1 x_{0j,k}. The variable x_{0j,k} = [0 . . . 0 x_{j,k,1} x_{j,k,2} . . . x_{j,k,Nt} 0 . . . 0]^T is the N_uN_t ×1 vector, and represents the jth overlapped UE on kth RE. The nonzero elements in x_{0j,k} are symbols transmitted from N_t antennas.

• H_k is the N_r × N_uN_t matrix given by

H_k = [H_{1,k} . . . H_{j,k} . . . H_{Nu,k}]

where H_{j,k} represents the jth UE MIMO channel matrix of size N_r × N_t.

Fig. 3: Processing at kth RE of SMX-CD-NOMA system.

Example 2. Consider N_t = 2, and according to the factor graph matrix given in (16). The transmitted signal over the first RE in the SCMA system is

x_{smx,1} = [ x^T_{1,1} x^T_{3,1} x^T_{5,1} ]_T . (20)

For DCMA, due to the dense structure of codebooks, all J UEs overlap on each RE [2]. The transmitted signal over the first RE is given by

x_{smx,1} = [ x^T_{1,1} x^T_{2,1} . . . x^T_{5,1} x^T_{6,1} ]_T , (21)

where each x_{j,1} is a 2 × 1 (N_t × 1) vector given by

x_{j,1} = [ x_{j,1,1} x_{j,1,2} ]_T . The transmitted signal over each remaining RE (x_{smx,k}, k = 2, . . . , K) has a similar representation as in (20) and (21) for SCMA and DCMA, respectively.

DRAFT June 6, 2023

For SCMA, x_{03,1} represents the 3rd UE’s symbols as given by

x_{03,1} = 0 0 UE_1 x^{3,1,1} x^{3,1,2} UE 3 0 0 UE 5

T . (22)

For DCMA, x_{03,1} can be written as

x_{03,1} = 0 0 UE_1 0 0_{UE 2} x^{3,1,1} x^{3,1,2} UE 3 0 0 UE 4 0 0 UE 5 0 0 UE 6

T . (23)

The variables {x_{0j,k}}^K_{k=1} are similarly represented as x_{03,1}. The transmitted signal x_{smx,k} can be written as, x_{smx,k} =

∑_3

j=1 x_{0j,k} and x_{smx,k} =

∑_6 j=1 x_{0j,k} for SCMA and DCMA, respectively.

C. SM-CD-NOMA

Due to the requirement of multiple radio frequency (RF) chains, the SMX-CD-NOMA system is not affordable for various applications. Further, inter-channel interference is the main limitation of this system. Spatial modulation (SM) MIMO systems are promising technology to overcome the limitations of SMX MIMO systems. SM for single-UE communications is well studied in the literature [26]. Due to the demands of future wireless networks, it is important to study and analyze SM in multiuser scenarios. In [27], the authors studied and analyzed SM sparse CDMA. SM-aided CD-NOMA (SM-CD-NOMA) is guaranteed to improve the spectral efficiency of the CD-NOMA with feasible complexity at both transmitter and receiver [6], [28]. Fig. 4 shows the system model for the SM-CD-NOMA system. Each UE is equipped with N_t transmitting antennas, in which only one antenna is active at any time, as shown in Fig. 4. The active antenna index of the jth UE is denoted by n^j_a. All other antennas remain silent in that particular time slot. Thus, the active antenna index is a spatial modulation symbol to transmit extra information bits. The information bit stream b_j of the jth UE, is split into two parts [b_{ja},b_{jc}] having log_2(N_t) and log_2(M) bits, respectively. Each UE transmits an overall log_2(N_t) + log_2(M) bits from the active antenna.

The observation vector over the kth RE at the BS is an N_r × 1 vector given by

r_k = H_kx_{sm,k} + w_k, (24)

where

• r_k, w_k, and H_k have the similar forms as in SMX-CD-NOMA for both DCMA and SCMA systems.

• x_{sm,k} is the N_uN_t×1 vector x_{sm,k} = [x^T_{1,k} . . . x^T_{j,k} . . . x^T_{Nu,k}]^T , and each x_{j,k} = [0 . . . x_{j,k,n}j_a . . . 0]^T is N_t × 1 vector corresponding to jth UE. The nonzero element x_{j,k,n}j_a is the symbol transmitted from n^j_ath active antenna. The transmitted signal x_{sm,k} can be rewritten to formulate the sharing-based detection problem in Section III-D i.e., x_{sm,k} = ∑_{Nu} j=1 x^{nja}_{0j,k}. The variable

Fig. 4: SM-CD-NOMA system model in the UL.

x^{nja}_{0j,k} = [0 . . . 0 . . . x_{j,k,n}j_a 0 . . . 0 . . . 0]^T represents the jth overlapped UE on kth RE. The nonzero element in x^{nja}_{0j,k} is the symbol transmitted from n^j_ath active antenna.

Fig. 5 depicts the kth RE processing at the BS through the extended factor graph. The thick and dotted lines correspond to the active and inactive antennas, respectively.

Fig. 5: Processing at kth RE of SM-CD-NOMA system.

Example 3. Consider N_t = 2, and the factor graph matrix given in (16). Suppose the active antenna indices of the 6-users are {2,1,2,2,1,1}. The structure of transmit codewords from J UEs for SM-CD-NOMA is as follows [28]:

x_{tx} = [ 0_{K×1} x^1_{2K×1} 0_{K×1} 0_{K×1} x^1_{5K×1} x^1_{6K×1} x^2_{1K×1} 0_{K×1} x^2_{3K×1} x^2_{4K×1} 0_{K×1} 0_{K×1} ] N_tK×J=8×6 . (25)

Each x^{nja}_{jK×1} in x_{tx} represents the transmitted codeword from jth UE, and each column of x_{tx} carries information about active transmit antenna (n^j_a) as well as the codeword. In (25), 0_{K×1} indicates zero power transmitted by a deactivated antenna. To facilitate the resource-wise processing at the receiver via ADMM, the transmitted signal over the first RE in the SCMA system is modeled as x_{sm,1} = [ x^T_{1,1} x^T_{3,1} x^T_{5,1} ]_T . (26)

DRAFT June 6, 2023

The transmitted signal over the first RE in the DCMA system is modeled as x_{sm,1} = [ x^T_{1,1} x^T_{2,1} . . . x^T_{5,1} x^T_{6,1} ]_T , (27) where x_{1,1} = [0 x_{1,1,2}]^T , x_{2,1} = [x_{2,1,1} 0]^T , x_{3,1} = [0 x_{3,1,2}]^T , x_{4,1} = [0 x_{4,1,2}]^T , x_{5,1} = [x_{5,1,1} 0]^T , and x_{6,1} = [x_{6,1,1} 0]^T . The transmitted signals over the remaining REs (x_{sm,k}, k = 2, . . . , K ) have similar representations as (26) and (27) for SCMA and DCMA, respectively. For SCMA, x^2_{03,1} represents the symbol transmitted from 2nd active antenna of 3rd UE on 1st RE. x^2_{03,1} can be written as

x^2_{03,1} = 0 0 UE_1 0 x^{3,1,2} UE 3 0 0 UE 5

T . (28)

For DCMA, x^2_{03,1} can be written as

x^2_{03,1} = 0 0 UE_1 0 0_{UE 2} 0 x^{3,1,2} UE 3 0 0 UE 4 0 0 UE 5 0 0 UE 6

T . (29)

The variables {x^{nja}_{0j} }^K_{k=1} are similarly represented as x^2_{03,1}. The transmitted signal x_{sm,k} can be written as, x_{sm,k} =

∑_3 j=1 x^{nja}_{0j,k} and x_{sm,k} =

∑_6 j=1 x^{nja}_{0j,k} for SCMA and DCMA, respectively

Observe from equations (15), (19), and (24) that the system models of three MIMO-CD-NOMA systems are similar to those of the conventional MIMO system model. This model is given by r = Hx + w, x ∈ X^{Nt} , (30) where X is the signal constellation, r is the N_r ×1 observation vector, H is N_r ×N_t channel matrix (N_r > N_t), x is N_t × 1 transmitted vector and w is i.i.d. AWGN vector with each component being distributed as CN (0, σ^2). The ML detection problem can be formulated as min_{x∈X} N_t ‖r − Hx‖^2.

The ML detection problem for SIMO CD-NOMA system in (15) is given by min x_{mu}∈X^{JNe}_{mu}

‖r − Hx_{mu}‖^2, (31)

where X^{JNe}_{mu} denotes the multi-user signal constellation and it consists of J-UEs concatenated codewords. However, solving ML detection problems, in general, is NP-hard. The exhaustive search method can be used to solve the ML detection problem. However, the exhaustive search is exponentially complex as per O(M^J ) [13] and thus it is not feasible. The ML detection problem (31) can be solved with a polynomial complexity using a distributed optimization framework. The above problem needs to be converted into a sharing problem that can be solved using distributed optimization methods. In the next section, we apply an efficient method based on the ADMM algorithm to solve the sharing-based detection problem in a distributed manner.

D. Large-scale UL multi-antenna CD-NOMA detection via ADMM

This section discusses the design of ADMM-based MUD for two CD-NOMA techniques, i.e., SCMA and DCMA. The ADMM-based detector is applied to three different MIMO systems, namely, SIMO-CD-NOMA, spatial multiplexed CD-NOMA (SMX-CD-NOMA), and spatially modulated CD-NOMA (SM-CD-NOMA). The implications of the proposed method are discussed in subsequent sections.

1) SIMO CD-NOMA : The ML detection problem in (31) can be converted into a sharing problem. Further, this problem can be solved in a distributed manner via the ADMM approach, as discussed in Section II-C. ADMM allows parallel processing in MUD problems, guaranteeing a minimal computational time at the receiver. Recall from Section III-A, the transmitted signal x_{mu} is given by x_{mu} = ∑_J j=1 x_{0j}. The problem (31) can be rewritten as

min_{x0j} ‖r − H (_J ∑ j=1 x_{0j} ) ‖^2 (32)

s.t x_{0j} ∈ X^{JNe}_{mu} j = 1, . . . , J.

Here, for the channel matrix H^{NrK×JNe} , we consider N_rK > JN_e. Each entry’s real and imaginary parts in x_{0j} are restricted by set constraints. The set constraint must be converted into an interval constraint to convert (32) into a sharing problem. Box constraint relaxation (BCR) is used to relax the set constraints of each entry in the codeword [20]. Hence, each entry’s real and imaginary parts in the jth UE codeword belong to [−α_j , α_j ] and [−β_j , β_j]. After relaxation, each element in the jth UE codebook is defined as X̃_j = {x_j = x_{jR} + ix_{jI} |x_{jR} ∈ [−α_j , α_j], x_{jI} ∈ [−β_j , β_j]}, α_j = max |R(X_j )|, β_j = max |I(X_j )|. The highly complex MIMO-CD-NOMA ML detection problem in (32) is now ready to be converted into a non-convex distributed optimization problem. However, the constraint relaxation degrades the detection performance due to the losses introduced by the interval constraints. The losses can be compensated by adding a set of quadratic penalty functions ∑_J j=1 γ_j 2 ‖x_{0j}‖^2 to the objective function where γ_j ≥ 0 is a penalty parameter. The penalty functions are selected so that each variable, x_{0j} , in the penalty term minimizes the individual penalty and the shared objective. The added penalty term makes the solution as sparse as possible. However, the sparse vectors with specific numbers (d_v for SCMA and K for DCMA) of non-zero entries only will minimize the shared objective function. The favorable solutions are the sparse vectors with d_v and K non-zero elements for SCMA and DCMA, respectively. The sharing ADMM problem can be written as

min_{x0j} ‖r − H (_J ∑ j=1 x_{0j} ) ‖^2 + J∑ j=1 γ_j 2 ‖x_{0j}‖^2 (33)

s.t x_{0j} ∈ X̃^{JNe}_{mu} , j = 1, . . . , J.

DRAFT June 6, 2023

The problem in (33) is similar to the sharing ADMM problem in (2). Proceeding similarly as in Section II-C, (33) can be written as min x_{0j} ,z_{0j} ‖r − H (_J ∑ j=1 x_{0j} ) ‖^2 + J∑ j=1 γ_j 2 ‖z_{0j}‖^2 (34)

s.t x_{0j} = z_{0j}, x_{0j} ∈ X̃^{JNe}_{mu} , ∀j = 1, . . . , J For the formulation of the ADMM steps, the augmented Lagrangian function for the problem (34) is considered as shown below: L ( {x_{0j} , z_{0j}, y_j}^J_{j=1} ) = ‖r − H (_J ∑ j=1 x_{0j} ) ‖^2 + J∑ j=1 γ_j 2 ‖z_{0j}‖^2 (35)

+ J∑ j=1 Re⟨x_{0j} − z_{0j} , y_j ⟩ + ρ 2 J∑ j=1 ‖x_{0j} − z_{0j} ‖^2

where y_j ∈ C^{JNe} is Lagrangian multiplier of the jth UE. Letting u_j =^{yj}_ρ , the scaled form of ADMM steps are as follows [14] : z^{t+1}_{0j} := argmin

z_{0j} ∈X̃^{JNe}_{mu} γ_j 2 ‖z_{0j}‖^2 + ρ 2 ‖z_{0j} − x^t_{0j} + u^t_j ‖^2 (36)

x^{t+1}_{0j} := argmin

x_{0j} ∈X̃^{JNe}_{mu} ‖r − H (_J ∑ j=1 x_{0j} ) ‖^2 + ρ 2 J∑ j=1 ‖z^{t+1}_{0j} − x_{0j} + u^k_j ‖^2 (37)

u^{t+1}_j :=u^k_j + (z^{t+1}_{0j} − x^{t+1}_{0j} ) (38)

Algorithm 1 SIMO CD-NOMA detection via sharing ADMM

1: Input: Noise variance (N_0), average codebook energy (E_s) and initialize {z_{0j} }^J_{j=1}, x̄_0, u, z̄_0 with zero vectors. 2: Output: x̄^{(T )}_0 , where T is the maximum number of iterations. 3: From (39) and (40), obtain optimal solutions (42) and (43), respectively. 4: Preprocessing 5: ρ = N_0/E_s 6: G = (H^H HJ + ρI)^{−1} 7: M = H^H r 8: for t = 1, 2, , . . . T do 9: Step:1 Update {z^{t+1}_{0j} }^J_{j=1} in parallel via (42) and compute x̄_1. 10: Step:2 11: Update x̄^{t+1}_0 via (43). 12: Update u^{t+1} via (41) 13: end for 14: Compute x̂_{mu} = Jx̄^{(T )}_0 .

15: After extracting each UE codeword from x̂_{mu}, apply the MED rule according to (44).

The variables z_{0j} and u_j can be updated independently in parallel for each j = 1, . . . , J. Following a similar sequence of steps as discussed in Section II-C, the steps in (36), (37), and (38) are simplified as

z^{t+1}_{0j} := argmin

z_{0j} ∈X̃^{JNe}_{mu} γ_j 2 ‖z_{0j}‖^2 + ρ 2 ‖z_{0j} − z^t_{0j} − x̄^t_0 + u^t + z̄^t_0‖^2 (39)

x̄^{t+1}_0 := argmin_{x̄0} ‖r − JHx̄_0‖^2 + ρJ 2 ‖x̄_0 − x̄^{t+1}_1 − u^t‖^2 (40)

u^{t+1} :=u^t + z̄^{t+1}_0 − x̄^{t+1}_0 (41)

where x̄_0 =^1_J ∑_J j=1 x_{0j} and z̄_0 =^1_J ∑_J j=1 z_{0j} . The solutions obtained by solving (39) and (40) are as follows

z^{t+1}_{0j} = ∏ [−α_j ,α_j ]&[−β_j ,β_j ] ρ (ρ + γ_j)

(z^t_{0j} + x̄^t_0 − u^t − z̄^t_0), ∀j = 1, . . . , J. (42)

x̄^{t+1}_0 = (H^H HJ + ρI)^{−1}(H^H r + ρ(z̄^{t+1}_0 + u^t)), (43)

where ∏ [−α_j ,α_j ]&[−β_j ,β_j ](.) denotes the projection of the real part of each entry of the vector onto

[−α_j , α_j] and imaginary part of each entry of the vector onto [−β_j , β_j]. The step in (42) can be solved in parallel, for j = 1, . . . , J. I is identity matrix of size Jd_v × Jd_v and JK × JK for SCMA and DCMA, respectively. From the definition of x̄_0 given above, the estimated multi-user codeword is given by, x̂_{mu} = Jx̄_0. Each UE’s concatenated sparse codeword x̂_{0j} can be extracted from the x̂_{mu} . Let x̃_{0j} be the jth UE codeword after removing zeros from x̂_{0j} . The minimum Euclidean distance (MED) rule is applied to detect the transmitted codeword index corresponding to each UE,

p̂_j = argmin_p ‖x̃_{0j} − x_{j,p}‖, j = 1, . . . , J (44)

where x_{j,p} represents pth codeword of the jth UE codebook x_{j,p} ∈ X^{K×M}_j . Note that for SCMA, the zeros from x_{j,p} are removed to find p̂_j . Algorithm 1 details the steps for detection.

2) SMX-CD-NOMA : The detector of SMX-CD-NOMA needs to detect the signals transmitted from N_t antennas of J UEs. Here, the detection is more complex than the SIMO case. The resourcewise processing is adapted to simplify the ADMM-based detection problem. Recall from Section III-B, that the SMX codeword is given by, x_{smx,k} = ∑_{Nu} j=1 x_{0j,k}. The ADMM processing first estimates the resource-wise spatial multiplexed transmitted vector x̂_{smx,k}, for k = 1, . . . , K. Then, the transmitted codeword indices are detected via the MED rule. The ML detection problem is converted into sharing problem as follows

min_{x0j,k} ‖r_k − H_k(

N_u∑

j=1 x_{0j,k})‖^2 +

N_u∑

j=1 γ_j 2 ‖x_{0j,k}‖^2 (45)

s.t. x_{0j,k} ∈ X̃^{NuNt}_{j,smx}

DRAFT June 6, 2023

Algorithm 2 SMX CD-NOMA detection via sharing ADMM

1: Input: N_0, E_s and initialize {z_{0j,k}}^{Nu}_{j=1}, x̄_{0,k}, u, z̄_{0,k} with zero vectors. 2: Output: x̄^{(T )}_0 .

3: From (47) and (48), obtain optimal solutions (49) and (50) respectively. 4: Preprocessing 5: ρ = N_0/E_s 6: G = (H^H_k H_kJ + ρI)^{−1} 7: M = H^H_k r_k 8: for t = 1, 2, , . . . T do 9: Step:1 Update {z^{t+1}_{0j,k}}^J_{j=1} in parallel via (49) and compute x̄_1. 10: Step:2 11: Update x̄^{t+1}_{0,k} via (50). 12: Update u^{t+1} via (48) 13: end for 14: Compute x̂_{smx,k} = Jx̄^{(T )}_{0,k} (for DCMA), and x̂_{smx,k} = d_fx̄^{(T )}_{0,k} (for SCMA). 15: After extracting x̂_{j,Nt} , apply the MED rule according to (52).

where γ_j ≥ 0 is the penalty parameter. By introducing alternative variable z_{0j,k} = x_{0j,k}, the ADMM steps for (45) are as follows:

z^{t+1}_{0j,k} := argmin z_{0j,k} ∈X̃^{NuNt}_{j,smx} γ_j 2 ‖z_{0j,k}‖^2 + ρ 2 ‖z_{0j,k} − x^t_{0j,k} + u^t_j ‖^2 (46)

x^{t+1}_{0j,k} := argmin_{x0j,k} ‖r_k − H_k (_{Nu} ∑ j=1 x_{0j,k} ) ‖^2 + ρ 2 J∑ j=1 ‖z^{t+1}_{0j,k} − x_{0j,k} + u^k_j ‖^2 (47)

u^{t+1}_j :=u^k_j + ( z^{t+1}_{0j,k} − x^{t+1}_{0j,k} ) . (48)

The solutions for (46) and (47) are as follows:

z^{t+1}_{0j,k} = ∏ [−α_j ,α_j ]&[−β_j ,β_j ] ρ (ρ + γ_j)

(z^t_{0j,k} + x̄^t_{0,k} − u^t − z̄^t_{0,k}) (49)

x̄^{t+1}_{0,k} =(H^H_k H_kN_u + ρI)^{−1}(H^H_k r_k + ρ(z̄^{t+1}_{0,k} + u^t)) (50)

where I is identity matrix of size N_uN_t × N_uN_t and the definitions of x̄_{0,k} and z̄_{0,k} are given below

x̄_{0,k} = 1 N_u

N_u∑

j=1 x_{0j,k} z̄_{0,k} = 1 N_u

N_u∑

j=1 z_{0j,k}. (51)

From the definition of x̄_{0,k}, the estimated codeword corresponding to the kth RE is given by x̂_{smx,k} = N_ux̄_{0,k}. The sparse vector x̂_{0j,k} corresponding to jth UE can be extracted from x̂_{smx,k}. Let x̃_{j,k} be a N_t × 1 vector formed after removing the zeros from sparse vector x̂_{0j,k}. Let x̂^{nt}_j be the estimated codeword of jth UE corresponding to n_tth transmit antenna. x̂^{nt}_j is formed after resource-wise processing is finished. MED rule is applied to detect the transmitted codeword index corresponding to each UE and transmit antenna as follows: p̂^{nt}_j = argmin_p ‖x̂^{nt}_j − x_{j,p}‖, j = 1, . . . , J, n_t = 1, . . . , N_t. (52)

where x_{j,p} represents the pth codeword of the jth UE codebook X^{K×M}_j . The detailed ADMM-based detection procedure is given in Algorithm 2.

3) SM-CD-NOMA: This section discusses the formulation of the ADMM-based detection problem for the SM-CD-NOMA system. The modulation happens in both the signal domain and the spatial domain. The SM-CD-NOMA system transmits information on the codeword and active antenna indices simultaneously. The receiver needs to estimate these two quantities. The variable x_{sm,k} from Section III-A, is given by x_{sm,k} = ∑_{Nu} j=1 x^{nja}_{0j,k}. The proposed method estimates the resource-wise spatial modulated transmitted vector x̂_{sm,k} for k = 1, . . . , K via ADMM processing. Then, the L1-norm rule is applied to detect the antenna index, and the MED rule is applied to detect the transmitted codeword index. The sharing problem of the SM-CD-NOMA system is similar to the problem in (45). Following the steps (46), (47), and (48), the sharing ADMM problem of SM- CD-NOMA can be solved. The solutions obtained for the sharing ADMM problem are similar to (49) and (50) and are repeated here for clarity: z^{t+1}_{0j,sm,k} = ∏ [−α_j ,α_j ]&[−β_j ,β_j ] ρ (ρ + γ_j)

(z^t_{0j,sm,k} + x̄^t_{0,sm,k} − u^t − z̄^t_{0,sm,k}) (53)

x̄^{t+1}_{0,sm,k} =(H^H_k H_kN_u + ρI)^{−1}(H^H_k r_k + ρ(z̄^{t+1}_{0,sm,k} + u^t)). (54) The definitions of x̄_{0,sm,k} and z̄_{0,sm,k} are similar to (51). The estimated SM codeword corresponding to kth RE is x̂_{sm,k} = N_ux̄_{0,sm,k}. After resource-wise processing, the structure of the transmitted codewords for J UEs can be retrieved. For Example 3, the detected codewords for 6 UEs is given by x̂_{tx} = [ x̂^1 x̂^1_2 x̂^1_3 x̂^1_4 x̂^1_5 x̂^1_6 x̂^2_1 x̂^2 x̂^2_3 x̂^2_4 x̂^2_5 x̂^2_6 ] N_tK×J(8×6) where x̂^{nt}_j indicates the estimated codeword of jth UE over the n_tth transmit antenna. In the presence of noise, the detected active transmit antenna index is given by n̂^j_a = argmax_{nt} (‖x̂^{nt}_j ‖_1), ∀j (55)

where ‖(·)‖_1 denotes the L1-norm of (·). Let x̂^{n̂ja}_j be the estimated codeword of the jth UE transmitted from n̂^j_a active antenna. The MED rule is applied to detect the codeword index corresponding to each UE p̂_j = argmin_p ‖x̂^{n̂ja}_j − x_{j,p}‖, ∀j. (56) Similar steps of Algorithm 2 are followed in the detection of the SM-CD-NOMA system.

DRAFT June 6, 2023

IV. COMPUTATIONAL COMPLEXITY This section analyses the computational complexity of the SIMO-CD-NOMA system. The detection algorithm’s computational complexity determines its practical viability. The number of FLOPs (mainly complex multiplications) is a useful metric to analyze the complexity of the detector [12]. The number of calculations in the proposed CD-NOMA detection via ADMM consists of two parts. Part-1 is iteration-independent (Pre-processing) steps, described in lines 6 and 7 in Algorithm 1, and Part-2 is iteration-dependent steps, from lines 9 to 12. The calculations in Part- 1 are performed only once, i.e., before the ADMM iterations. In the SIMO-CD-NOMA system, Part-1 contains three steps of calculations such as H^H H, (H^H H + ρI)^{−1}, and H^H r. The size of H is N_rK × Jd_v and N_rK × JK for SCMA and DCMA, respectively. Further, the numbers of FLOPs required to perform these three steps over the SCMA system are (N_rK)(Jd_v)^2, (Jd_v)^3 and (N_rK)(Jd_v). The numbers of FLOPs required to perform the same steps over the DCMA system are (N_rK)(JK)^2, (JK)^3, and (N_rK)(JK). The calculations in Part-2 need to be repeated in every iteration and contain mainly two steps. For SCMA system, these steps involve scalar multiplication of Jd_v × 1 vector for J UEs parallelly in (42), multiplication of Jd_v × Jd_v matrix with Jd_v ×1 and scalar multiplication with Jd_v ×1 vector in (43), in total J^2d_v+(Jd_v)^2+Jd_v FLOPs approximately. For DCMA system, (J^2K + (JK)^2 + JK) FLOPs are required. The approximate total computational cost to implement the ADMM-based detector over the SIMO-SCMA system and SIMO-DCMA system are (N_rK)(Jd_v)^2 + (Jd_v)^3 + (N_rK)(Jd_v) + T (J^2d_v + (Jd_v)^2 + Jd_v) and (N_rK)(JK)^2 + (JK)^3 + (N_rK)(JK) + T (J^2K + (JK)^2 + JK) respectively. TABLE I compares the total complexity of the sharing ADMM-based detection problem with other known detection schemes. In TABLE I, NA stands for ‘Not applicable’.

MPA is widely used for SCMA systems, and its complexity is exponential with M and d_f , as mentioned in TABLE I [12]. The computational burden will grow further for large-scale SCMA systems. Further, due to exponential complexity, MPA is not feasible in large-scale MIMO systems. Additionally, the lack of sparsity in DCMA makes MPA impractical for detection.

A single tree search (STS) based soft-in soft-out (SISO) GSD [29] is applied to detect the signals of a spreading sequence-based DCMA system, also known as an overloaded CDMA system [2]. GSD performs key pre-processing steps to convert the rank deficient system into full rank one [30]. These steps include H^H H in (Q = H^H H + λI_J ), Cholesky decomposition Q = D^H D, and (HD^{−1})^H r. These steps require (N_rK)J^2, J^3/3, and (J^3 +(N_rK)J^2 +JN_rK) FLOPs, respectively. The rank-deficient linear system is thus converted into a full-rank one, and standard sphere decoding (SD) can be readily applied. The SD performs pre-processing steps, including QR decomposition and Q^H r. Further, the numbers of FLOPs to perform these steps are J^3 and 2J^2, respectively. The major complexity of the SD lies in the tree search algorithm [31]. The expected complexity of SD

TABLE I: Computational complexity of different detectors for SIMO CD-NOMA systems

Detector Spreading sequence based Codebook based LDS DCMA SCMA DCMA MPA NA NA (Kd^2_f M^{df} N_r + Nd_f Md_v)T NA GSD NA (N_rK)J^2 +J^3/3+(J^3 +(N_rK)J^2 + JN_rK) + J^3 + 2J^2 + E_{FLOPS}

NA NA

MMSE NA (N_rK)J^2 + J^3 + (N_rK)J (N_rK)(Jd_v)^2 + (Jd_v)^3 + (N_rK)(Jd_v) (N_rK)(JK)^2 + (JK)^3 + (N_rK)(JK) Sharing ADMM

NA (N_rK)J^2 +J^3+ (N_rK)J +T (2J^2 + J) N_rK(Jd_v)^2 + (Jd_v )^3+ (N_rK)(Jd_v ) + T (J^2d_v + (Jd_v)^2 + Jd_v)

N_rK(JK)^2+(JK)^3 +(N_rK)(JK) +T (J^2K + (JK)^2 + JK) SCMADCMA Spreading sequence based DCMA 05,000 10,000 15,000 20,000 25,000

Number of FLOPS

ADMM MPA MMSE GSD

Fig. 6: Computational complexity comparison of various detectors. is E_{FLOPS} = ∑_J j=1 f_p(j)N_j, where N_j is the average number of nodes visited in level-j of the tree and f_p(j) is the number of FLOPs needed in level-j. It is given in [31], f_p(j) = 2j + 11, and N_j is roughly cubic in the number J of unknowns to be solved. Fig. 6 depicts the computational complexity comparison of various detection schemes for different CD-NOMA systems with N_r = 4, K = 4, J = 6, d_v = 2, and M = 4. It can be observed that the complexity of ADMM-based detector is almost equal to that of the low-complexity MMSE detector.

V. SIMULATIONS AND DISCUSSIONS This section presents wide-ranging simulation results of various MIMO-CD-NOMA systems, including SER performance and selection of ADMM parameters ( T, {γ}^J_{j=1} ) . The simulations are performed for various MIMO-CD-NOMA systems described in Section III with varying parameters λ, M, N_r, and N_t. Further, the performance of the ADMM-based detector is compared with that of the MPA detector with ten iterations (T = 10) in the case of the SCMA system. The DCMA and overloaded CDMA systems’ detection is carried out using the MMSE and the GSD detectors, respectively. The codebooks designed in [32] and [2] are considered, for SCMA and DCMA, respectively. Table II further details the simulation parameters. The sample simulation codes for this work are available at https://github.com/vikas2020-del/ADMM-based-detector-for-NOMA. A. SER performance of SIMO CD-NOMA system

Fig. 7(a) and Fig. 7(b) show the SER performance of SIMO-SCMA system for 150 % and 200 % overloading, respectively. Each curve represents the SER performance for a specific number N_r

DRAFT June 6, 2023

Parameter Value Modulation order (M) 4, 8, 16 Number of UEs (J) 6, 10 Number of resources (K) 4, 5 Number of transmit antenna (Nt) 2, 4, 8 Number of receive antenna (Nr) 4, 8, 32, 64 Overloading factor (λ) 150 %, 200 % Detectors ADMM, MPA, MMSE, GSD Number of iterations (T ) 30 (ADMM), 10 (MPA)

TABLE II: Simulation parameters.

−4−2024 10^{−6} 10^{−5} 10^{−4} 10^{−3} 10^{−2} 10^{−1}100

E_b/N_0 (dB)

SER

Nr=16, M=8 Nr=4, M=4 Nr=4, M=8 Nr=8, M=8 Nr=8, M=4 Nr=4, M=4 Nr=8, M=4

λ = 150 %

(a) SER vs. SNR performance for λ = 150 %.

−5051015 10^{−7} 10^{−6} 10^{−5} 10^{−4} 10^{−3} 10^{−2} 10^{−1}10^0

E_b/N_0 (dB)

SER

Nr = 4, M = 4 Nr = 8, M = 4 Nr = 8, M = 8 Nr = 4, M = 8 Nr = 16, M = 8 Nr = 4, M = 4 Nr = 8, M = 4

λ = 200 %

(b) SER vs. SNR performance for λ = 200 %.

Fig. 7: SER performance SIMO SCMA system. Solid and dotted lines denote the ADMM and MMSE performance, respectively. of the receive antennas at the BS and codebook size M. Fig. 7(a) and Fig. 7(b) show that the SER performance improves as N_r increases. Thus, the proposed ADMM-based detector is able to exploit the diversity gain provided by the SIMO-CD-NOMA system. However, for M = 8, the SER performance is slightly worse than M = 4 due to the inevitable decrease in the minimum Euclidean and minimum product distance [32]. Fig. 7(a) and Fig. 7(b) also compare the SER performance of the MMSE and ADMM-based detectors. For a small-scale SCMA system (M = 4, λ = 150 %), the performance of the MMSE detector is close to that of the ADMM-based detector. However, for λ = 200 %, the MMSE performance is inferior to ADMM. Observe from (15) that as the number J of UEs increases, the number Jd_v of unknowns approaches the number KN_r of observations. The MMSE performance degrades when the KN_r to Jd_v ratio approaches unity. ADMM provides approximately 2 dB SNR gain at SER = 10^{−3} over the MMSE detector for 200 % overloaded SCMA system, as observed from Fig. 7(b). Fig. 8(a) and Fig. 8(b) show the SER performance of M = 4 and M = 16 overloaded SIMO-DCMA systems, respectively. Fig. 8(a) compares the SER performance of the MMSE and ADMM-based detectors. ADMM provides approximately 2 dB SNR gain at SER = 10^{−3} over the MMSE detector for the 200 % overloaded DCMA system, as observed from Fig. 8(a). Therefore, ADMM is a more suitable detector compared with MMSE for 200 % overloaded CD-NOMA systems. Furthermore, simulation attempts indicate that MMSE cannot detect the CD-NOMA signals for M = 8 and M = 16 size codebooks. Therefore, these plots are not shown in Fig. 7 and Fig. 8.

−4−20246810 10^{−6} 10^{−5} 10^{−4} 10^{−3} 10^{−2} 10^{−1}100

E_b/N_0(dB)

SER

200 % 150 % 150 % 150 % 200 %

Nr=8

Nr=16

(a) Codebook size M = 4.

05101520 10^{−7} 10^{−6} 10^{−5} 10^{−4} 10^{−3} 10^{−2} 10^{−1}10^0

E_b/N_0 (dB)

SER

200 % 150 % 150 %

Nr = 16

Nr=8

(b) Codebook size M = 16.

Fig. 8: SER performance of SIMO DCMA system for 150 % and 200 % overloading. Solid and dotted lines denote the ADMM

and MMSE performance, respectively.

B. SER performance of SMX CD-NOMA systems

Fig. 9(a) and Fig. 9(b) show the SER performance of SMX-SCMA system for 150 % and 200 % overloading, respectively. Observe from Fig. 9(a) and Fig. 9(b), that the higher the value of N_r, the better is the SER performance. As the value of N_t increases, N_r is increased to maintain N_r > d_f N_t in (19). The improvement in the SER performance is maximum for N_r = 64 case due to more observations at the BS. This improvement comes at the cost of a marginal computational complexity increment (TABLE I) in ADMM detection. Fig. 9(c) depicts the SER performance of SMX-DCMA systems. For SCMA, N_u = d_f UEs overlap on each RE. On the other hand, for DCMA N_u = J (J > d_f ) UEs overlap on each RE, as shown in Fig. 1(b). This significant overlapping increases the number of unknowns in a DCMA system compared to the SCMA one, as observed in (19). To maintain the number of observations higher than the number of unknowns (N_r > JN_t), DCMA requires larger N_r at the BS as compared to SCMA for a fixed N_t. As a result, the computational complexity of DCMA detection significantly increases. The tree search-based SD algorithms are highly complex in codebook-based DCMA, as explained in Section IV. Further, the ADMM-based detector shows similar complexity as that of MMSE, as shown in Fig. 6. Therefore, compared with MMSE, the ADMM-based detector performs well with almost the same complexity.

DRAFT June 6, 2023

25 −15−10−5051015 10^{−6} 10^{−4} 10^{−2}100

E_b/N_0 (dB)

SER

Nr = 16, Nt = 4 Nr = 16, Nt = 4 Nr = 8, Nt = 2 Nr = 8, Nt = 2 Nr = 64, Nt = 8 Nr = 32, Nt = 8

λ=150 % M=4M=8

(a) SMX-SCMA with λ = 150 %

−1001020 10^{−7} 10^{−5} 10^{−3} 10^{−1}101

E_b/N_0 (dB)

SER

Nr =8, Nt=2 Nr =8, Nt=2 Nr =16, Nt=4 Nr =16, Nt=4 Nr =32, Nt=8 Nr =64, Nt=8

λ=200 % M=4M=8

(b) SMX-SCMA with λ = 200 %

−15−10−5051015 10^{−6} 10^{−5} 10^{−4} 10^{−3} 10^{−2} 10^{−1}100

E_b/N_0 (dB)

SER

Nr = 16, λ = 150 % Nr = 32, λ = 200 % Nr = 32, λ = 200 % Nr = 16, λ = 150 %

Nt=2

M=4M=16

(c) SMX-DCMA

Fig. 9: SER vs. SNR performance of SMX-CD-NOMA system by varying Nt, Nr, M using the ADMM-based detector. C. SER performance of SM CD-NOMA systems

Fig. 10(a) and Fig. 10(b) show the SER performance of SM-SCMA system for 150 % and 200 % overloading, respectively. The performance of the ADMM-based detector mainly depends on N_t, N_r, and M, as we have seen in the previous subsections. The M = 4 size codebook exhibits superior performance over M = 8 due to its better distance properties (Euclidean distance and product distance). In SM-CD-NOMA systems, each UE’s codeword contains the active antenna and codeword index information of that particular UE, as given in (25). Fig. 10(a) and Fig. 10(b) depict the efficiency of ADMM in detecting the information both in the signal domain and space domain. Note that the codewords in (25) contain zero-column vectors to indicate zero power transmission from the inactive antenna. As a result, the number of observations goes below the number of unknowns (N_r < N_uN_t). Thus, it leads to performance loss for an ADMM-based detector. However, increasing the number of observations (N_r) at the BS can compensate for this loss. Therefore, the performance of the ADMM-based detector can be maintained by a marginal increment in the computational complexity as given in TABLE I. The observations mentioned above for SMX-

DCMA and SM-SCMA systems apply to SM-DCMA systems, as shown in Fig. 10(c). Further, N_r = 32, λ = 200 % provides significantly better performance than N_r = 16, λ = 150 %, as the former has more observations (N_r) than the latter. So the ADMM-based detector is more appropriate for highly overloaded DCMA systems equipped with large-scale MIMO parameters.

−15−10−505101520 10^{−6} 10^{−5} 10^{−4} 10^{−3} 10^{−2} 10^{−1}100

E_b/N_0 (dB)

SER

Nr = 32, Nt = 8 Nr = 16, Nt = 4 Nr = 16, Nt = 4 Nr = 32, Nt = 8 Nr = 64, Nt = 8

λ=150 % M=4M=8

(a) SM-SCMA with λ = 150 %

−100102030 10^{−7} 10^{−6} 10^{−5} 10^{−4} 10^{−3} 10^{−2} 10^{−1}10^0

E_b/N_0 (dB)

SER

Nt=16, Nt =4 Nr=32, Nt =8 Nr=16, Nt =4 Nr=32, Nt =8 Nr=64, Nt =8

λ=200 % M=4M=8

(b) SM-SCMA with λ = 200 %

−15−10−505101520 10^{−6} 10^{−5} 10^{−4} 10^{−3} 10^{−2} 10^{−1}100

E_b/N_0 (dB)

SER

Nr=16, λ = 150 % Nr=16, λ = 150 % Nr=32, λ = 200 % Nr=32, λ = 200 %

M=4M = 16 Nt=2

(c) SM-DCMA

Fig. 10: SER vs. SNR performance for SM-MIMO CD-NOMA system using the proposed ADMM-based detector.

D. SER performance: ADMM vs. MPA

Fig. 11(a) shows the SER performance comparison between the ADMM and MPA detectors for the SIMO-SCMA system. Existing research shows that the MPA is a near-optimal detection with high computational complexity [7]. MPA gives a maximum SNR gain of around 2.5 dB over ADMM at SER = 10^{−2} for N_r = 4 and M = 4, as shown in Fig. 11(a). As the modulation order M increases, the performance of ADMM becomes close to MPA, as observed for N_r = 4, M = 8 in Fig. 11(a). Therefore, for M = 8, codebook distance properties influence MPA and ADMM-based detectors similarly. Further, for N_r = 8, M = 8, the ADMM-based detector shows approximately 2 dB SNR gain at SER = 10^{−3} over the MPA detector. The increase in the number of observations

DRAFT June 6, 2023

27

significantly improves the ADMM performance compared to MPA for large-size codebooks (i.e. with large M).

−4−2024 10^{−6} 10^{−5} 10^{−4} 10^{−3} 10^{−2} 10^{−1}100

E_b/N_0 (dB)

SER

Nr = 4, M = 4, ADMM Nr = 4, M = 8, ADMM Nr = 8, M = 8, ADMM Nr = 8, M = 4, ADMM Nr = 4, M = 4, MPA Nr = 4, M = 8, MPA Nr = 8, M = 8, MPA Nr = 8, M = 4, MPA

(a) SIMO SCMA: ADMM vs. MPA with λ=150 %

−4−2024 10^{−7} 10^{−6} 10^{−5} 10^{−4} 10^{−3} 10^{−2} 10^{−1}10^0

E_b/N_0 (dB)

SER

Nr = 8, M = 16, GSD Nr = 8, M = 16, ADMM Nr = 4, M = 4, ADMM Nr = 4, M = 4, GSD

λ=150 %

(b) SIMO Overloaded CDMA: ADMM vs. GSD

Fig. 11: Comparison of SER performance using the proposed ADMM and the conventional MPA and GSD detectors.

E. SER performance: ADMM vs. GSD

Fig. 11(b) shows the SER performance comparison between ADMM and GSD detectors for the SIMO-overloaded CDMA system. Observe from Fig. 11(b) that, at low SNR regions, GSD outperforms the ADMM with a maximum of around 2 dB SNR gain at SER=10^{−4}. As the SNR increases, GSD performance degrades compared to ADMM. Unlike GSD, as M increases, ADMM performance is enhanced by doubling the number of received antennas as shown in Fig. 11(b). Note that ADMM performance improves as the number of observations increases. F. SER performance: Imperfect channel state information (CSI)

All the above simulations are analyzed by considering perfect CSI at the receiver. In practical scenarios, obtaining perfect CSI at the receiver is not feasible due to channel estimation errors (CEEs). Thus, the proposed detector’s performance in the presence of CEEs is an important metric to show its practical feasibility. An imperfect channel can be modeled as [33] Ĥ = H + e Ω (57)

where Ω is the CEE and is considered to be uncorrelated with H. The entries of Ω are independent and i.i.d. complex Gaussian random variables with zero mean and unit variance, i.e., CN (0, 1). The quantity e in (57) determines the variance of the CEE. Fig. 12 depicts the performance of the proposed ADMM-based detector for the imperfect CSI with e = 0 %, e = 5 %, e = 10 %, and e = 20 %. The simulations for SCMA and DCMA systems are shown in Fig. 12(a) and Fig. 12(b), respectively. Observe that the impact of the CEE on the ADMM-based detector’s performance is minimal. Therefore, the ADMM-based detector can be applied in imperfect CSI scenarios.

28 −4−202 10^{−5} 10^{−4} 10^{−3} 10^{−2} 10^{−1}100

E_b/N_0 (dB)

SER

e=0 %

e=5 %

e=10 %

e=20 %

λ=150 %

(a) SIMO SCMA system with Nr = 8, M = 4

−4−2024 10^{−5} 10^{−4} 10^{−3} 10^{−2} 10^{−1}100

E_b/N_0 (dB)

SER

e=0 %

e=5 %

e=10 %

e=20 %

λ=150 %

(b) SIMO-DCMA system with Nr = 8, M = 4

Fig. 12: SER performance of CD-NOMA system in imperfect CSI for e = 0 %, e = 5 %, e = 10 %, e = 20 %.

G. Convergence of ADMM and selection of parameters

The convergence analysis of the ADMM-based detector in the DCMA system is performed based

on the Monte Carlo simulations. Fig. 13(a) shows the impact of ADMM iterations on the SER

performance. The proposed detector exploits the iterative nature of ADMM to converge. The SER

510152025 10^{−7} 10^{−6} 10^{−5} 10^{−4}

Number of iterations (T )

SER

Eb N0 =15dB Eb N0 =18dB Eb N0 =20dB

(a) Iterations vs. SER with λ = 150 %, M = 4, Nr = 4

050100150200250300 10^{−8} 10^{−7} 10^{−6} 10^{−5} 10^{−4} γ

SER

Eb N0 =15dB Eb N0 =18dB Eb N0 =20dB

(b) γ vs. SER with λ = 150 %, M = 4, Nr = 4

Fig. 13: Impact of T and γ on the ADMM-based detector’s SER performance.

performance improves as the number of iterations (T ) increases. The improvement in SER becomes

marginal after a certain number of iterations. For all considered^{Eb}_{N0} values, ADMM converges after

15 iterations, as shown in Fig. 13(a). The penalty parameters {γ_j}^J_{j=1} and ρ are selected to maximize

the SER performance. The augmented Lagrangian parameter ρ is selected as the reciprocal of

SNR [19]. The impact of γ on SER performance in the ADMM-based detector is analyzed through

Monte Carlo simulations, and the results are given in Fig. 13(b). For low values of γ, the ADMM

performance degrades, and for large values, the variation in SER becomes inconsequential. When

γ is close to zero, the impact of penalty terms is nullified. Thus, the alternative variables in the

DRAFT June 6, 2023

penalty function lose importance in minimizing the objective function. Observe from the Fig. 13(b) that the ADMM performs better in the range {γ_j}^J_{j=1} ∈ [50 100].

VI. CONCLUSIONS AND FUTURE SCOPES This paper proposed new system models and a low-complexity iterative linear detector for largescale MIMO-CD-NOMA systems. The optimal ML detection is converted into a sharing problem, which is efficiently solved via the ADMM algorithm using distributed optimization framework. The proposed ADMM-based detector enables the detection of large-scale MIMO-CD-NOMA systems with high overloading factors (λ) and modulation orders (M) while maintaining low complexity. By leveraging the proposed ADMM, the CD-NOMA systems achieve significantly increased connectivity. Further, the impact of ADMM parameters, such as the number of iterations and penalty parameters, is analyzed. Exhaustive simulation results are presented to validate the effectiveness of the proposed ADMM-based detector when compared to conventional detectors such as MPA, GSD, and MMSE detectors. In addition, the results demonstrate that the ADMM-based detector offers excellent performance with low complexity across various CD-NOMA system variants. This paper has explored the concept of ADMM detection specifically for uncoded CD-NOMA systems. Designing a soft decision detector using the ADMM algorithm for coded CD-NOMA systems is an interesting future work.

REFERENCES

[1] M. Taherzadeh, H. Nikopour, A. Bayesteh, and H. Baligh, “SCMA codebook design,” in Proc, IEEE 80th Veh. Technol. Conf.

(VTC-Fall), 2014, pp. 1–5.

[2] Y. L.-L. Liu, Zilong, “Sparse or Dense: A comparative study of code-domain NOMA systems,” IEEE Trans. Wireless Commun., vol. 20, no. 8, pp. 4768–4780, 2021.

[3] A. Chockalingam and B. S. Rajan, Large MIMO Systems. Cambridge University Press, 2014. [4] S.-C. Lim, N. Kim, and H. Park, “Uplink SCMA system with multiple antennas,” IEEE Trans. Veh. Technol., vol. 66, no. 8, pp. 6982–6992, 2017.

[5] S. Elkawafi, A. Younis, and R. Mesleh, “Performance analysis of sparse code multiple access MIMO systems,” in 2019 IEEE 30th Int. Symp. Per. Indoor Mobile Radio Commun (PIMRC), 2019, pp. 1–6.

[6] Z. Pan, J. Luo, J. Lei, L. Wen, and C. Tang, “Uplink spatial modulation SCMA system,” IEEE Commun. Lett., vol. 23, no. 1, pp. 184–187, 2019.

[7] C. Zhang, Y. Luo, and Y. Chen, “A Low-complexity SCMA Detector based on Discretization,” IEEE Trans. Wireless Commun., vol. 17, no. 4, pp. 2333–2345, 2018.

[8] L. Yang, Y. Liu, and Y. Siu, “Low complexity message passing algorithm for SCMA system,” IEEE Commun. Lett., vol. 20, no. 12, pp. 2466–2469, 2016.

[9] J. Dai, G. Chen, K. Niu, and J. Lin, “Partially active message passing receiver for MIMO-SCMA systems,” IEEE Wireless Commun. Lett., vol. 7, no. 2, pp. 222–225, 2018.

[10] Y. Du, B. Dong, Z. Chen, P. Gao, and J. Fang, “Joint sparse graph-detector design for downlink MIMO-SCMA systems,” IEEE Wireless Commun. Lett., vol. 6, no. 1, pp. 14–17, 2017.

[11] S. Sharma, K. Deka, and B. B. Lozano, “Low-complexity Detection for Uplink Massive MIMO SCMA Systems,” IET Communications, vol. 15, no. 1, pp. 51–59, 2021.

[12] F. Wei and W. Chen, “Low complexity iterative receiver design for sparse code multiple access,” IEEE Trans. Commun., vol. 65, no. 2, pp. 621–634, 2017.

[13] S. Yang and L. Hanzo, “Fifty years of MIMO detection: The road to large-scale MIMOs,” IEEE Commun. Surveys Tuts., vol. 17, no. 4, pp. 1941–1988, 2015.

[14] S. Boyd, N. Parikh, E. Chu, B. Peleato, and J. Eckstein, Distributed Optimization and Statistical Learning via the Alternating Direction Method of Multipliers. Now Foundations and Trends, 2011.

[15] C. F. Zhouchen Lin, Huan Li, Alternating Direction Method of Multipliers for Machine Learning. Springer, 2022. [16] S. Barman, X. Liu, S. C. Draper, and B. Recht, “Decomposition methods for large scale LP decoding,” IEEE Trans. Inf.

Theory, vol. 59, no. 12, pp. 7870–7886, 2013.

[17] H. Wei and A. H. Banihashemi, “ADMM check node penalized decoders for LDPC codes,” IEEE Trans. Commun., vol. 69, no. 6, pp. 3528–3540, 2021.

[18] A. C. Cirik, N. Mysore Balasubramanya, and L. Lampe, “Multi-user detection using ADMM-based compressive sensing for uplink grant-free NOMA,” IEEE Wireless Commun. Lett., vol. 7, no. 1, pp. 46–49, 2018.

[19] S. Shahabuddin, I. Hautala, M. Juntti, and C. Studer, “ADMM-based infinity-norm detection for massive MIMO: Algorithm and VLSI architecture,” IEEE IEEE Trans. Very Large Scale Integr. (VLSI) Syst., vol. 29, no. 4, pp. 747–759, 2021.

[20] Q. Zhang, J. Wang, and Y. Wang, “Efficient QAM signal detector for Massive MIMO systems via PS/DPS-ADMM approaches,” IEEE Trans. Wireless Commun., vol. 21, no. 10, pp. 8859–8871, 2022.

[21] W.-K. Ma, T. Davidson, K. M. Wong, Z.-Q. Luo, and P.-C. Ching, “Quasi-maximum-likelihood multiuser detection using semi-definite relaxation with application to synchronous CDMA,” IEEE Trans. Signal Process., vol. 50, no. 4, pp. 912–922, 2002.

[22] R. Hoshyar, F. P. Wathan, and R. Tafazolli, “Novel low-density signature for synchronous CDMA systems over AWGN channel,” IEEE Trans. Signal Process., vol. 56, no. 4, pp. 1616–1626, 2008.

[23] H. Nikopour and H. Baligh, “Sparse code multiple access,” in 2013 IEEE 24th Annual Int. Symp. Per. Indoor Mobile Radio Commun (PIMRC), 2013, pp. 332–336.

[24] J. Boutros and E. Viterbo, “Signal space diversity: a power- and bandwidth-efficient diversity technique for the rayleigh fading channel,” IEEE Trans. Inf. Theory, vol. 44, no. 4, pp. 1453–1467, 1998.

[25] T. L. Marzetta and H. Yang, Fundamentals of massive MIMO. Cambridge University Press, 2016. [26] R. Y. Mesleh, H. Haas, S. Sinanovic, C. W. Ahn, and S. Yun, “Spatial modulation,” IEEE Trans. Veh. Technol., vol. 57, no. 4, pp. 2228–2241, 2008.

[27] Y. Liu, L.-L. Yang, and L. Hanzo, “Spatial modulation aided sparse code-division multiple access,” IEEE Trans. Wireless Commun., vol. 17, no. 3, pp. 1474–1487, 2018.

[28] H. Yaoyue, P. Zhiwen, L. Nan, and Y. Xiaohu, “Multidimensional constellation design for spatial modulated SCMA systems,” IEEE Trans. Veh. Technol., vol. 70, no. 9, pp. 8795–8810, 2021.

[29] C. Studer, A. Burg, and H. Bolcskei, “Soft-output sphere decoding: algorithms and VLSI implementation,” IEEE J. Sel. Areas Commun., vol. 26, no. 2, pp. 290–300, 2008.

[30] T. Cui and C. Tellambura, “An efficient generalized sphere decoder for rank-deficient MIMO systems,” IEEE Commun. Lett., vol. 9, no. 5, pp. 423–425, 2005.

[31] B. Hassibi and H. Vikalo, “On the sphere-decoding algorithm I. Expected complexity,” IEEE Trans. Signal Process., vol. 53, no. 8, pp. 2806–2818, 2005.

[32] V. Vikas, A. Rajesh, K. Deka, and S. Sharma, “A comprehensive technique to design SCMA codebooks,” IEEE Commun.

Lett., vol. 26, no. 8, pp. 1735–1739, 2022.

[33] C. Wang, E. K. Au, R. D. Murch, W. H. Mow, R. S. Cheng, and V. Lau, “On the performance of the MIMO zero-forcing receiver in the presence of channel estimation error,” IEEE Trans. Wireless Commun., vol. 6, no. 3, pp. 805–810, 2007.

DRAFT June 6, 2023