arXiv:2311.10885v1 [cs.CV] 17 Nov 2023

A Video-Based Activity Classification of Human Pickers in Agriculture

Abhishesh Pal^1, Antonio C. Leite^1, Jon G. O. Gjevestad^1, Pål J. From^{1,2}

Abstract— In farming systems, harvesting operations are tedious, time- and resource-consuming tasks. Based on this, deploying a fleet of autonomous robots to work alongside farmworkers may provide vast productivity and logistics benefits. Then, an intelligent robotic system should monitor human behavior, identify the ongoing activities and anticipate the worker’s needs. In this work, the main contribution consists of creating a benchmark model for video-based human pickers detection, classifying their activities to serve in harvesting operations for different agricultural scenarios. Our solution uses the combination of a Mask Region-based Convolutional Neural Network (Mask R-CNN) for object detection and optical flow for motion estimation with newly added statistical attributes of flow motion descriptors, named as Correlation Sensitivity (CS). A classification criterion is defined based on the Kernel Density Estimation (KDE) analysis and K-means clustering algorithm, which are implemented upon in-house collected dataset from different crop fields like strawberry polytunnels and apple tree orchards. The proposed framework is quantitatively analyzed using sensitivity, specificity, and accuracy measures and shows satisfactory results amidst various dataset challenges such as lighting variation, blur, and occlusions.

I. INTRODUCTION

The agricultural field has emerged as a promising application for human activity recognition (HAR) towards the development and optimization of efficient robot fleet operations and human-robot collaboration in farming and harvesting operations [1]. According to [2], an HAR system must deal with many technical challenges related to the extraction of distinguishable features, scarcity of annotations, the complexity of data association, the heterogeneity of the sensory data, and the interpretability in sensory data. The use of HAR systems in agriculture is relatively new, especially when it comes to recognizing human pickers’ field operational activities, such as distinguishing between harvesting, unloading, and transportation of trays, where not much research is done in the past. For example, training and testing of machine learning-based methods require the availability of large annotated data sets as well as a baseline model to compare them. However, collecting and manually annotating sensory activity data are expensive and time-consuming tasks, especially in agricultural fields. The video or images captured from a real-time soft-fruit picking operation basically contains features of the actions and events (i.e., the duration of an activity). Usually, these visual

1Abhishesh Pal, Antonio C. Leite, Jon G. O. Gjevestad and Pål J. From are with the Faculty of Science and Technology, Norwegian University of Life Sciences, Universitetstunet 3, 1433 Ås, Norway. E-mail: [abhishesh.pal, pal.johan.from]@nmbu.no

2Pål J. From is with the Lincoln Institute for Agri-Food Technology, University of Lincoln, Lincoln LN6 7TS, United Kingdom. E-mail: pfrom@lincoln.ac.uk

features might carry different noise sources (Fig. 1), such as dynamic background interference, partial or total occlusion, and distinct viewpoints. Moreover, it is still a laborious task to identify motions and objects from a content-based video analysis. Then, it may be quite challenging to obtain efficient and accurate motion representation for humans working in agricultural fields.

Fig. 1: Dataset collecting challenges in agricultural fields: blur (left), lighting variation (center), and occlusion (right).

In general, an HAR process includes two main steps: feature extraction based on image/video information, and image/video classification based on the extracted feature vectors [3]. In static images, visual (spatial) features are for example pixel values, corners, blobs and edge histograms. Thus, a feature extraction method must compute a reliable descriptor from the pixels around each interest point, such as SIFT, SURF and BRIEF. In dynamic scenes, along with static images, visual features also include temporal features as interest points, displacement and trajectories. A spatiotemporal interest point encodes the video information at a specific location in space and time. On the other hand, a trajectory tracks a certain spatial point over time and, thus, captures the motion information [4].

Global features describe an image as a whole entity and can generalize an entire object within a scene with a single vector. In contrast, local features represent image patches and are computed at multiple points in the image, being more robust to occlusion and cluttering. Thus, local spacetime features may provide a successful representation for the recognition of human activity [5]. There are several feature extraction approaches for extracting local spatio-temporal features in videos, such as Gabor filters, Hessian matrix, higher-order derivatives, gradient information, optical flow [6], and brightness information.

This work proposes a video-based benchmark model that identifies human pickers in a scene with visual noises and classifies which agricultural activities the identified workers are performing on the crop field. For this, we will extract the visual feature map from image sequences of the pickers’ activities in different fruit picking scenarios (Fig. 2). The classification model consists of 4 (four) main modules with distinct functions per each, namely: Object Detection Module (ODM), Motion Estimation Module (MEM), Motion Classification Module (MCM), and Robot Scheduler Module (RSM), as shown in Fig. 3. In a nutshell, our classification framework uses a mask salient object detection approach based on the combination of a Mask Region-based Convolutional Neural Network (Mask R-CNN) architecture to extract visual features and, optical flow motion descriptors to understand behavioral activity patterns, with the help of newly added statistical attributes defined as mean of Correlation Sensitivity (CS) along with other attributes such as minimum (min.), maximum (max.) and range of descriptors.

To decipher the underlying patterns in motion descriptor’s statistical attributes and to create class labels, we explore the synergy between the Kernel Density Estimation (KDE) analysis and the K-means clustering algorithm. We apply both methods on the same dataset, collected in distinct crop fields, and discuss their performance based on data characteristics. In view of that, we set the classification criteria by choosing the thresholding parameters to the identified statistical attributes of the motion descriptor. To evaluate the relevance of the CS attribute in pattern recognition and classification of activities, we compare the practical results obtained with the proposed video-based activity classification algorithm, which includes mean CS, against other variants of the same algorithm that does not have CS.

Fig. 2: Data collection setup in a strawberry polytunnel (left side) and an apple tree orchard (right side).

II. DATA COLLECTION AND CHALLENGES The data is collected in-house with two human pickers working in different fruit picking scenarios, viz. polytunnel and open field, located at the Norwegian University of Life Sciences (NMBU), Campus Ås, Norway. The setup for data collection is shown in Fig. 2, where we have installed the Intel® RealSense™ depth camera D435 (pixel size: 3μ × 3μ; focal length: 1.93mm; RGB frame rate: 30fps) at an approximate height of 1−1.5m on a fixed platform, using a tripod stand or the Thorvald robot [7], located at the headland of a given crop row of the experimental field.

The image data was bagged at 30fps rate, where a series of actions were recorded in an orderly manner. In [8], the authors explain a harvesting protocol for real-time soft-fruit harvesting operation in strawberry production fields. There were five activities mentioned, namely idle, picking, loading, unloading, and transportation. We have similarly demonstrated the harvesting operation in an agricultural environment, focusing on mainly two activities, i.e., Picking, and Not

Picking. Picking activity deals with actions involving human picker motions, occurring while picking up fruits from crops, and Not Picking activity includes all other activities, such as idle, unloading, loading and transportation. From now on, we call the Not Picking activity as unloading throughout the manuscript.

Multiple video data were collected for different agricultural scenarios (Fig. 2) with varying combinations of both activities to promote randomness in the dataset. Then, we have manually processed the raw video data into three types of classified video dataset: picking dataset with both pickers picking, unloading dataset with both pickers unloading, and mixed dataset with both pickers doing different activities. In the mixed dataset, several combinations of activities are considered for both pickers. For example, in a single video clip, one picker might be picking first, then switch to unloading, while another picker might only be picking (or unloading) in the whole video. Each classified dataset consists of 6−7 videos, with a frame rate of 10 fps and a resolution of 640×480 pixels, and 4−6 seconds video chunks (.avi or .MP4) for each activity, wherein every single video consists of 40−60 frames in total.

III. PROPOSED ALGORITHM OVERVIEW

This section will briefly explain each module of our proposed activity recognition and classification architecture based on the video dataset collected in distinct crop fields.

Fig. 3: Overview of the proposed video-based activity recognition and classification architecture.

Object Detection Module (ODM) using Mask R-CNN This module is used to extract moving targets in frame sequences under various visual challenges in datasets such as noise, shadows, poor illumination, and low frame resolution. We emphasize the use of Mask R-CNN architecture [9] due to its ability to robustly handle scene challenges and work precisely at pixel-level instance segmentation of moving objects in the images. This network framework provides class labels, bounding boxes, and segmentation masks for each detected object. We have performed transfer learning on the pre-trained model on COCO (Common Objects in Context) dataset. The CNN model was trained on our dataset using GPU (GTX 1080Ti, Nvidia, Corp.) Desktop with CUDA 9.0. The trained weights were saved and used in the OpenCV library in Python for further application in the classification pipeline. Next, each inference input frame fed in the trained network provides instance segmentation for foreground class ‘person’, with its predicted box, overlay colored and binary masks contours inside the boxes (see Fig. 4). The extracted foreground mask is called Moving Object Region (MOR), that is used by the MEM block.

Fig. 4: From left to right: original frame with two pickers; using Mask R-CNN for consecutively detecting pickers, then fetching a MOR in each frame with its colored and binary masks; finally, applying optical flow on selected grids.

Motion Estimation Module (MEM) based on Optical flow This module estimates motion using an optical flow algorithm on a MOR to obtain the flow motion descriptors (i.e., magnitude and orientation) and analyze them using statistical attributes. We use the Gunnar-Farneback optical flow method [10] because of its ability to look at all of the feature vectors at pixel-level and its intensity changes between the two consecutive frames. Motion descriptors are feature vectors calculated for each frame, or several consecutive frames, and used for analysis. We have combined the use of Kernel Density Estimation (KDE) analysis [11] and K-means clustering algorithm to identify the underlying critical classes in motion descriptors data. Then, we have applied the univariate KDE with Gaussian kernel, and the parameter bandwidth is determined automatically using the adaptive bandwidth selection method based on a linear diffusion process.

The basis of evaluation in the K-means clustering algorithm is the silhouette coefficient method, which has values within the interval [−1,1] [12]. Then, we want the coefficients to be as high as possible and close to the unit to have representative clusters. We have analysed motion descriptor data distribution statistically by calculating their mean value (mean), standard deviation (std.), range (range), minimum (min.), maximum (max.), and root mean square (rms). Moreover, we have also calculated another feature vector by defining a relation between flow magnitude and orientation. Thus, any significant changes in motion descriptors can be evidently noticed, which would otherwise not be possible. In this way, we make our algorithm classification criteria more sensitive to be able to sparse different patterns effectively. This motion descriptor is named in the paper as Correlation Sensitivity (CS), and it is defined as:

CS = F ∑_{f =1}^{mag f · θ f}

2 · S(V_f ,θ_f )

, (1)

where, for a set of input MOR frames F in a video, S(V_f ,θ_f ), V_f , mag_f and θ_f are respectively the total number of flow features, the flow magnitude and the flow orientation for each frame f . We have chosen only those statistical attributes of motion descriptors that show a sparse representation of different patterns in KDE analysis. Therefore, among several statistical attributes for each motion descriptor, we have relied upon a 4 (four) parameters vector, such as range values for flow magnitude, (max.) and (min.) values for flow orientation and mean value for CS. Finally, we set the threshold value for each parameters vector of the identified clusters to provide class labels to different activities.

Motion Classification Module (MCM)

Here, we introduce a hierarchical approach to separate the picker’s actions to increase the effectiveness of the classification, wherein we are investigating the activity classification at two levels: (i) Frame-level (FL) classification, that classifies each frame into two pre-classes as Picking (P) and Not Picking (NP); (ii) Batch-Frame level (BFL) classification, that classifies further batch of FL annotation into two classes for showing the continuity of an activity as: if P, then Wait to Finish; otherwise, if NP, then Call a robot. To achieve this, we have developed a classification correction algorithm that uses the list of FL class labels in a rolling window spanning the last five frames. Then, we choose the most occurred FL class label from the sequence of labels to create the respective BFL class label. For convenience, we named it as rolling mode method. The BFL labels are part of the RSM block in the proposed video-based recognition and classification framework, indicating future research to solve the field logistic problem by scheduling the fleet of robots from picker’s activity predictions.

IV. EXPERIMENTAL RESULTS AND DISCUSSION This section presents the experimental tests and the numerical results obtained with the proposed video-based classification framework for picker’s activity classification on a mixed activity dataset consisting of 600 frames with 2 pickers in each, makes in total 1200 MOR frames.

Activity Classification Analysis

For a given statistical attribute, the combination of the KDE distribution analysis and the best evaluation of the Kmeans silhouette score suggests mainly two clusters (k =2), as shown respectively in Fig. 5 and Table I. The corresponding K-means cluster centers are shown in Table II, where NP is Not Picking (or unloading) and P is Picking. Accordingly, the threshold values are set for all four parameters vectors. Next, the FL classification performance is evaluated using statistical measures of sensitivity (TPR), specificity (TNR), and accuracy (ACC) of the activity detection as the average values over the number of frames.

TABLE I: Activity classification: K-means silhouette coefficients for different statistical attributes and size of clusters.

k range mean max. min.

(flow mag.) (CS) (flow ori.) (flow ori.) 2 0.65 0.90 0.87 0.87 3 0.60 0.87 0.87 0.85 4 0.57 0.60 0.85 0.85

Fig. 5: KDE distribution analysis of the four parameters vectors, where evidently two local maxima are found in each plot considered as two natural clusters: (blue) range of magnitude; (red) mean of CS; (yellow) max. of flow orientation; (green) min. of flow orientation.

TABLE II: Activity classification: K-means cluster center.

k range mean max. min.

(flow mag.) (CS) (flow ori.) (flow ori.) NP 1550.49 3433.18 176.55 3.47 P 708.78 675.95 104.82 79.65 units pixel pixel degree degree

TABLE III: Activity classification using the proposed classification algorithm and its different variants.

classification methods ACC % TNR % TPR% proposed solution 84.18 89.06 75.00 variant (i) 50.51 90.23 40.12 variant (ii) 66.33 94.52 49.59 variant (iii) 60.20 82.72 44.35

We have also analysed our classification framework with various combinations of all four parameters vectors named as variants and listed as: variant (i), which includes range value of the flow magnitude, as well as min. and max. values of the flow orientation, that is, (range) flow magnitude + (min., max.) flow orientation; variant (ii), which includes (range) value of the flow magnitude; and variant (iii), which includes (min., max.) values of the flow orientation. The proposed solution presents the higher ACC and TPR values respectively as 84% and 75 %, as shown in Table III, revealing the added advantage of including the CS feature vector for activity classification compared to other algorithm variants without using CS. An example of the performance analysis of our proposed FL and BFL classification algorithm on test videos is shown in Figures 6a and 6b, which depict the human pickers as picker ID00 and picker ID01 respectively. The BFL classification for the corresponding FL classification shows an overall improvement in classifying the activity duration. Meanwhile, we argue that the MOR mask has successfully detected the foreground moving object amidst various scene challenges.

V. CONCLUDING REMARKS In this work, a video-based activity classification framework is proposed that uses the combination of Mask R-CNN architecture and optical flow motion descriptors. We have defined four modules in this framework with their distinct functions in classification pipeline. The proposed classifica-

(a) Picker 00 (b) Picker 01

Fig. 6: Experimental results of activity classification with FL and BLF approaches from test dataset.

tion criteria with a newly derived Correlation Sensitivity (CS) shows satisfactory classification results at a Frame Level (FL) with accuracy, specificity and sensitivity as close as 84%, 89% and 75%, respectively. A running-mode algorithm also shows a good classification correction at a Batch Frame Level (BFL). The developed video-based benchmark model shows satisfactory overall results under variability in shading, brightness, blur of images, and occlusion. The accuracy analysis of the classification framework in a multiple pickers scenario using Deep Neural Networks (DNNs) can be explored in future research.

REFERENCES

[1] P. J. From, L. Grimstad, M. Hanheide, S. Pearson, and G. Cielniak, “RASberry - Robotic and Autonomous Systems for Berry Production,” ASME, Mechanical Engineering., vol. 140, no. 06, pp. S14–S18, 2018.

[2] J. Wang, Y. Chen, S. Hao, X. Peng, and L. Hu, “Deep Learning for Sensor-based Activity Recognition: A Survey,” Pattern Recognition Letters, vol. 119, pp. 3–11, 2019.

[3] S. Ranasinghe, F. A. Machot, and H. C. Mayr, “A Review on Applications of Activity Recognition Systems with Regard to Performance and Evaluation,” International Journal of Distributed Sensor Networks, vol. 12, no. 8, pp. 1–22, 2016.

[4] H. Wang, A. Kläser, C. Schmid, and C.-L. Liu, “Dense Trajectories and Motion Boundary Descriptors for Action Recognition,” International Journal of Computer Vision, vol. 103, pp. 60–79, 2013.

[5] A. B. Vasudevan, S. Muralidharan, S. P. Chintapalli, and S. Raman, “Dynamic Scene Classification Using Spatial and Temporal Cues,” in IEEE International Conference on Computer Vision Workshops, 2013, pp. 803–810.

[6] D. J. Fleet and Y. Weiss, “Optical Flow Estimation,” in Handbook of Mathematical Models in Computer Vision, N. Paragios, Y. Chen, and O. Faugeras, Eds. Springer Boston MA, 2006, pp. 237–257.

[7] L. Grimstad and P. J. F. From, “The Thorvald II Agricultural Robotic System,” Robotics, vol. 6, no. 4, pp. 1–24, 2017.

[8] G. Das, G. Cielniak, P. From, and M. Hanheide, “Discrete Event Simulations for Scalability Analysis of Robotic In-field Logistics in Agriculture–a Case Study,” in IEEE International Conference on Robotics and Automation, Workshop on Robotic Vision and Action in Agriculture, 2018.

[9] K. He, G. Gkioxari, P. Dollár, and R. Girshick, “Mask R-CNN,” in Proceedings of the IEEE International Conference on Computer Vision, 2017, pp. 2961–2969.

[10] G. Farnebäck, “Two-frame Motion Estimation based on Polynomial Expansion,” in Scandinavian Conference on Image Analysis, 2003, pp. 363–370.

[11] A. Khosrowpour, I. Fedorov, A. Holynski, J. C. Niebles, and M. Golparvar-Fard, “Automated Worker Activity Analysis in Indoor Environments for Direct-Work Rate Improvement from Long Sequences of RGB-D Images,” in Construction Research Congress 2014, 2014, pp. 729–738.

[12] F. Wang, H.-H. Franco-Penya, J. D. Kelleher, J. Pugh, and R. Ross, “An Analysis of the Application of Simplified Silhouette to the Evaluation of k-means Clustering Validity,” in 13th International Conference on Machine Learning and Data Mining in Pattern Recognition, 2017, pp. 291–305.