arXiv:2403.07355v2 [eess.SP] 13 Mar 2024

Vector Quantization for Deep-Learning-Based CSI Feedback in Massive MIMO Systems

Junyong Shin, Yujin Kang, and Yo-Seb Jeon

Abstract

This paper presents a finite-rate deep-learning (DL)-based channel state information (CSI) feedback method for massive multiple-input multiple-output (MIMO) systems. The presented method provides a finite-bit representation of the latent vector based on a vector-quantized variational autoencoder (VQ-VAE) framework while reducing its computational complexity based on shape-gain vector quantization. In this method, the magnitude of the latent vector is quantized using a non-uniform scalar codebook with a proper transformation function, while the direction of the latent vector is quantized using a trainable Grassmannian codebook. A multi-rate codebook design strategy is also developed by introducing a codeword selection rule for a nested codebook along with the design of a loss function. Simulation results demonstrate that the proposed method reduces the computational complexity associated with VQ-VAE while improving CSI reconstruction performance under a given feedback overhead.

Index Terms

Channel state information (CSI) feedback, vector-quantized variational autoencoder (VQ-VAE), finite-rate feedback, shape-gain vector quantization

I. INTRODUCTION Massive multiple-input multiple-output (MIMO) stands out as a crucial technique for enhancing spectral efficiency in wireless communication systems. In frequency division duplexing (FDD) systems, achieving this improvement necessitates accurate knowledge of the channel state information (CSI) at the base station (BS). However, as the dimension of CSI grows substantially in massive MIMO systems, there emerges a significant burden on user equipment (UE) to feed the CSI back to a BS. To address this challenge, CSI feedback methods based on recent advancements in deep learning (DL) have been introduced [1]– [3]. The common idea of the DL-based CSI feedback methods, which is based on an autoencoder (AE) framework, is to compress the CSI using an encoder network and then feed the latent vector (i.e., the output of the encoder) back to the BS with reduced overheads. With appropriate pre-processing of the CSI and

Junyong Shin, Yujin Kang, and Yo-Seb Jeon are with the Department of Electrical Engineering, POSTECH, Pohang, Gyeongbuk, Republic of Korea (e-mail: sjyong@postech.ac.kr, yujinkang@postech.ac.kr, yoseb.jeon@postech.ac.kr).

meticulous design of the neural networks, the above methods have proven effective in mitigating the CSI feedback overhead, compared to conventional non-DL-based approaches such as compressive sensing and static codebook-based feedback [4], [5].

In practice, for compatibility with modern digital communication systems, the latent vector, corresponding to the UE’s feedback, needs to be transformed into a finite-length bit sequence. Motivated by this fact, scalar quantization methods for the DL-based CSI feedback have been developed to support the finite-bit representation of the latent vector. In [3], non-uniform scalar quantizer and dequantization module were developed. In this method, the entries of the latent vector were normalized according to their distributions, so that these entries can be quantized in a bounded range. In [6], [7], bounded activation functions were considered in order to use a non-uniform quantizer in a bounded range. All these methods assume independent quantization of the latent entries. This assumption, however, making them impossible to leverage the correlations among different latent entries, despite its potential to reduce quantization error as mentioned in [8]. Another limitation is that when employing scalar quantization, at least one bit is required for quantizing each entry. This requirement significantly restricts the dimension of the latent vector under a given feedback overhead, resulting in performance degradation.

The limitations of the scalar-quantization approach have been addressed in [9], [10] by incorporating the idea of vector quantization into the DL-based CSI feedback. The common strategy of these methods is to leverage the vector-quantized variational autoencoder (VQ-VAE) framework developed in [11] which allows a finite-bit representation of the latent vector based on a trainable vector codebook. However, these methods require comparing the distances from the latent vector to all codeword vectors, resulting in significant computational complexity that scales with the size of the codebook. Moreover, a vector codebook design for DL-based CSI feedback has not been explored in the literature, despite its importance and potential for minimizing quantization error.

In this letter, we propose a finite-rate DL-based CSI feedback method for massive MIMO systems, utilizing the VQ-VAE framework. Our key contribution is to design the codebook for VQ-VAE based on shape-gain vector quantization, which alleviates the computational complexity associated with VQ-VAE by separately quantizing the shape (direction) and gain (magnitude) of the latent vector. In particular, for the gain quantization, we adopt a non-uniform scalar codebook based on a clipped μ-law transformation which captures the behavior of the latent vector’s magnitude. For the shape quantization, we employ a trainable Grassmannian codebook under the unit-norm constraint. Beyond the design of a single-rate vector codebook, we also develop a multi-rate codebook design strategy for the proposed method to support multi-rate vector quantization using a single codebook. In this strategy, we modify a nested codebook design in [12], by developing a new codeword selection rule along with a revised loss function design. In simulations, we demonstrate that the proposed method significantly reduces the computational complexity of the quantization process while improving reconstruction performance under a given feedback overhead. Our simulation results also demonstrate that the use of our multi-rate codebook design further improves the performance of the proposed method.

II. SYSTEM MODEL AND PRELIMINARY A. FDD Massive MIMO System

Consider a single-cell massive MIMO system in which a BS equipped with N_t transmit antennas communicates with a UE equipped with a single antenna. The system employs orthogonal frequency division multiplexing (OFDM) with N_c subcarriers. CSI in the spatial-frequency domain is represented as a channel matrix H_{sf} ∈ C^{Nc ×Nt} . To exploit the sparsity of the CSI matrix in the angular-delay domain as in [1], it is transformed into a channel matrix H_{ad} ∈ C^{Nc ×Nt} by applying a 2D discrete Fourier transform (DFT). The transformation is formulated as H_{ad} = F_dH_{sf}F_a, where F_d and F_a are N_c × N_c and N_t × N_t DFT matrices, respectively. In the angular-delay domain, only the first Ñ_c(≤ N_c) delay components carry significant values because multipath delays are confined to a limited time interval. Motivated by this, a submatrix of H_{ad} which consists of the initial Ñ_c rows is defined as an effective channel matrix H̃_{ad} ∈ C^{Ñc ×Nt} .

In a typical DL-based CSI feedback method, the UE employs an encoder network to compress the CSI information into the form of a latent vector with dimension M. Meanwhile, the BS employs a decoder network to reconstruct the CSI information from the UE’s feedback. The UE initiates a CSI feedback process by utilizing the effective channel matrix H̃_{ad} as an input of the encoder network. This yields the latent vector z expressed as z = f_{enc}(H̃_{ad}), where f_{enc} represents the encoder network. Typically, the latent vector z is considered as a UE’s feedback that needs to be transmitted to the BS. Upon the reception of the UE’s feedback, the BS reconstructs the effective channel matrix by utilizing the latent vector as an input of the decoder network f_{dec}.

In practice, the latent vector z is transformed into a finite-length bit sequence before being transmitted to the BS. This transformation is achieved through quantizing the latent vector z under the constraint on feedback overhead. Subsequently, the BS reconstructs the effective channel matrix by utilizing the quantized latent vector, denoted as z_q, as an input for the decoder network (i.e., Ĥ = f_{dec}(z_q)).

B. Vector-Quantized Variational Autoencoder (VQ-VAE)

VQ-VAE is well-known for its ability to enable a discrete representation of the latent vector by incorporating vector quantization into the VAE framework [11]. This framework utilizes a trainable quantization codebook placed in the latent space and jointly trains the encoder, codebook, and decoder using a loss function that captures both the quantization and reconstruction errors.

A conventional way of employing the VQ-VAE is to divide the latent vector z into N sub-vectors each with dimension D (M = N × D) and then use a D-dimensional codebook for quantizing each subvector separately [9]–[11]. Let B be a vector codebook using B bits which consists of 2^B D-dimensional codewords, namely {b_k}^{2B}_{k=1}. Also, let z_i be the i-th sub-vector of z, defined as z_i = [z_{(i−1)D+1}, · · · , z_{iD}], where z_j is the j-th entry of z. Then each sub-vector z_i is quantized to z_{q,i} using the codebook B according to the minimum Euclidean distance criterion, i.e., z_{q,i} = argmin_{bk∈B}‖z_i − b_k‖. For jointly training the encoder, codebook, and decoder, in [11], the loss function is designed as

L_{vq} = ‖ ‖Ĥ − H̃_{ad} ‖ ‖^2_F + ‖sg(z) − z_q‖^2 + β ‖z − sg(z_q)‖^2 , (1)

where sg(·) denotes the stop-gradient operator that ignores gradient descent computation as a constant. The third term in (1) is called as commitment loss, regularized by a hyperparameter β [11]. After calculating the quantization errors, which are the second and third term above, a gradient correction of the decoder input is performed as z_q ← z + sg(z_q − z).

Unlike scalar quantization which ignores the correlations among the latent entries (e.g., [3], [6], [7]), the VQ-VAE approach is able to capture joint behavior of multiple latent entries and therefore has a potential to achieve a further reduction in the quantization error under the same feedback overhead. However, the above VQ-VAE approach often imposes significant computational complexity because it compares the distances from the latent vector to all codeword vectors. This limitation poses a potential obstacle to the practical adoption of VQ-VAE as a solution for finite-rate DL-based CSI feedback.

III. PROPOSED DL-BASED CSI FEEDBACK METHOD In this section, we propose a novel DL-based CSI feedback method which reduces the computational complexity of the original VQ-VAE approach by leveraging shape-gain vector quantization.

A. Basic Idea: Shape-Gain Quantization

The basic idea of the proposed method is to quantize the magnitude and direction of each latent sub-vector z_i using a gain and shape quantizer, respectively. To be more specific, we quantize the magnitude ‖z_i‖ of z_i using a gain quantizer Q_{mag}(·), while quantizing the direction z_i/‖z_i‖ of z_i using a shape quantizer Q_{dir}. Then, the quantized latent sub-vector is given by

z_{q,i} = Q_{mag}(‖z_i‖) · Q_{dir}(z_i/‖z_i‖). (2)

Fig. 1. An illustration of the proposed DL-based CSI feedback method using shape-gain vector quantization.

Our shape-gain quantization strategy is illustrated in Fig. 1.

A significant advantage of our quantization strategy is the reduced computational complexity in the quantization process. In our approach, the feedback bits per sub-vector are divided between the shape and gain quantizers. Let B_{mag} and B_{dir} denote the feedback bits for the gain and shape quantizers, respectively, implying that B_{mag} + B_{dir} = B, when the feedback overhead per sub-vector is B bits. It leads for the entire feedback overheads to be calculated as^M_D ×B. In this case, the computational complexity of our shape-gain quantization in (2) is of order O(2^{max{Bmag ,Bdir}}), significantly smaller than the complexity order O(2^B) of the original VQ-VAE approach. Therefore, for the same feedback overhead, our quantization approach significantly reduces the computational complexity compared to the VQ-VAE approach.

B. Gain (Magnitude) Quantization

We present the design of the gain quantizer Q_{mag}(·) used to quantize the magnitude ‖z_i‖ of each latent sub-vector z_i. It should first be noted that each latent sub-vector z_i has a bounded magnitude if the activation function of the output layer of the encoder is bounded. Without loss of generality, we shall assume that this output function is bounded by 1. Consequently, the magnitude ‖z_i‖ is constrained within √ D. Another crucial observation is that the magnitude of the sub-vector is often concentrated in a specific regime rather than evenly distributed across the range of [0, √ D]. This observation suggests that a simple uniform quantizer may not perform optimally for the quantization of ‖z_i‖. Motivated by this observation, we construct a nonuniform quantizer by mapping the magnitude ‖z_i‖ to the range of [0, A] with an appropriate transformation h(x) : [0, √ D] → [0, A] and perform uniform quantization as (3). Our gain quantizer is then expressed as

Q_{mag}(‖z_i‖) = h^{−1}(f_u(h(‖z_i‖))), where f_u(x) is a B_{mag}-bit uniform quantization function defined as

f_u(x) = A { round(2^{Bmag} x/A − 0.5) + 0.5 2^{Bmag} } . (3)

Next, for determining an appropriate transformation h(x), we consider the μ-law transformation expressed as h_{μ-law}(x) = ln ( 1 +^{μx√}_D ) /ln(1 + μ), which has been widely studied in the literature [3], [6], [7]. This method provides concentrated quantization levels near-zero values due to its concavity for positive inputs. To restrict the output of this method to focus only on a confined region [0, A], we modify the original μ-law transformation by introducing a clipping value, which limits the highest value for the output of the transformation. Our clipped μ-law transformation is expressed as follows:

ĥ_{μ-law}(x) = h_{μ-law}(x), 0 ≤ x ≤^{(1+μ)A −1}_μ √ D, A,^{(1+μ)A −1}_μ √ D < x ≤ √ D. (4)

When training the encoder and decoder, our gain quantizer does not allow a direct back propagation for gradient computing, because the round functions in (3) have a zero-gradient problem. To resolve this problem, we leverage a soft-gradient passing technique considered in [6], [13]. When executing the back propagation process, we replace round functions in (3) with the step-wise Tanh functions as follows:

f̃_u(x) = A 2 {∑_{2Bmag −1} i=1 tanh(τ(2^{Bmag} x/A − i)) + 1 2^{Bmag} } . (5)

C. Shape (Direction) Quantization

We introduce the design of the shape quantizer Q_{dir}(·) used to quantize the direction z̃_i = z_i/‖z_i‖ of each latent sub-vector z_i. Note that a distance between two unit-norm vectors c_1 and c_2 can be measured by the sine of the angle between these vectors, defined as d(c_1, c_2) = √ 1 − |c_1, c_2|^2. Utilizing this fact, we adopt the quantization function that determines the codeword with the minimum distance according to the above distance measure:

Q_{dir}(z̃_i) = argmin

b_k∈B_{dir}

d(z̃_i, b_k), (6)

where B_{dir} is a shape codebook which consists of 2^{Bdir} unit-norm vectors with dimension D.

We now focus on designing a proper shape codebook. At the beginning of a training process, we do not have any prior information about the direction of the latent sub-vectors. Hence we initialize the codebook by assuming that the directions of the latent sub-vectors are uniformly distributed. Under this assumption, minimizing the quantization error of our shape quantizer is achieved by determining the 2^{Bdir} codewords that maximize the minimum distance between any two codewords. This problem is well known as a Grassmannian line packing problem and can be solved efficiently by some existing algorithms [14]. Utilizing this fact, we initialize the codebook B_{dir} with the solution of the above problem, known as the Grassmannian codebook. As the training progresses, more information about the directions of the latent sub-vectors becomes available. Therefore, during the training process, we update the codewords in B_{dir} based on the gradient with respect to the loss function. It’s noteworthy that the vectors in the codebook may not have unit norm after a gradient descent update; therefore, we normalize the codebook vectors after their updates.

D. Multi-Rate Codebook Design

We also present a multi-rate codebook design strategy for the proposed CSI feedback method. A multi-rate VQ-VAE approach was studied in [12] for image classification tasks. In this approach, a nested codebook is constructed by successively increasing the codebook size through the addition of random codeword vectors. We modify this strategy for designing a nested shape codebook to support L different shape quantization rates. Unlike the existing approach in [12], our strategy involves constructing a nested shape codebook by successively reducing the codebook size from a large size to a small size. The resulting L shape codebooks can be expressed as B^{(1)}_{dir} ⊃ B^{(2)}_{dir} ⊃ · · · ⊃ B^{(L)}_{dir} with |B^{(l)}_{dir}| = 2^{B(l)dir} for l ∈ {1, ..., L}. The first codebook B^{(1)}_{dir} is initialized as our shape-gain vector codebook and then trained using the loss function in (1), as described earlier. Unlike the first codebook, the l-th codebook B^{(l)} for l > 1 is initialized by selecting the most frequently quantized 2^{B(l)dir} vectors from the (l − 1)-th codebook B^{(l−1)}. This strategy represents an important deviation from the approach in [12], as our strategy involves selecting vectors based on their frequency of quantization rather than simply adding random codeword vectors. Then, an initialized l-th codebook is trained using the following loss function:

L^{(l)}_{nvq} = 1 ∑_l k=1 γ^k l∑ j=1 γ^j (‖ ‖Ĥ^{(j)} − H̃_{ad}‖^2_F + ‖sg(z) − z^{(j)}_q ‖^2 + β‖z − sg(z^{(j)}_q )‖^2 ) , (7)

where z^{(j)}q is the latent vector quantized with B^{(j)}, Ĥ^{(j)} = f_{dec}(z^{(j)}q ), and γ ≤ 1 is a hyperparameter which regulates the portion of each quantization order’s loss in the nested codebook. Unlike the loss function in (7) which considers a simple summation of the losses of l codebooks, we consider a weighted combination of the losses of l codebooks by assigning a smaller weight to a codebook with a larger size. By doing so, the l-th codebook B^{(l)} is not only optimized for the l-th rate, but also regulated to preserve its effectiveness in higher rates. Our multi-rate codebook design strategy is summarized in Algorithm 1. Similarly to other DL-based CSI feedback methods, when the channel distribution undergoes significant changes from those

Algorithm 1: Training of the proposed CSI feedback method with multi-rate codebook design 1. Initialization:

Randomly initialize the parameters in f_{enc} and f_{dec}; Initialize B^{(1)}_{dir} with the Grassmannian codebook; 2. Training: for l = 1, ..., L do while not converged do

z ← f_{enc}(H̃_{ad}); for i = 1, ..., N do Q_{mag} ← h^{−1}_{μ-law}(f_u(ĥ_{μ-law}(‖z_i‖))); ∇Q_{mag} ← ∇h^{−1}_{μ-law}(f̃_u(ĥ_{μ-law}(‖z_i‖))); for j = 1, ..., l do Q_{dir} ← argmin_{bk∈B}(j)_{dir} d(z̃_i, b_k); z^{(j)}_{q,i} ← Q_{mag} · Q_{dir}; end end Ĥ^{(j)} ← f_{dec}(z^{(j)}_q ), ∀j ∈ {1, ..., l}; Calculate L^{(l)}nvq in (7);

Update all parameters with the gradient descent; end B^{(l+1)}_{dir} ← 2^{B(l+1)dir} most quantized vectors in B^{(l)}_{dir} ; end

assumed during offline training, our shape-gain codebooks can be updated jointly with the encoder/decoder weights as part of the re-training or fine-tuning process.

IV. SIMULATION RESULTS In this section, we evaluate the performance of the proposed finite-rate CSI feedback method. In our proposed model, network structure in [11] is considered. The channel dataset is generated using the COST2100 channel model for the indoor picocellular scenario at 5.3 GHz and outdoor rural scenario at the 300 MHz [15]. The BS is equipped with a uniform linear array (ULA) with N_t = 32 and N_c = 1024 in spatial-frequency domain. After transformation to angular-delay domain, we truncate the CSI image with Ñ_c = 32. The other parameters are described as the default setting in [15]. The dataset contains the training,

Fig. 2. Comparison of the NMSE performance of the proposed method with and without the multi-rate codebook design when L = 4.

validation, and testing sets with the size of 100000, 30000, and 20000 respectively. Also, the batch size is set to 200. The Adam optimizer with 0.001 learning rate, and 1000 training epochs are used. For performance comparison, we consider (i) the original VQ-VAE method in [11], (ii) the DL-based CSI feedback method in [3], (iii) the DL-based CSI feedback method in [16], and (iv) the DL-based CSI feedback method in [17]. The parameters related to the quantization process are set as A = 0.6, B_{mag} = 4, D = 16, μ = 255, β = 0.25, and τ = 8. A performance measure considered in our simulations is normalized mean squared error (NMSE) defined as NMSE = E {‖~ H_{ad} − Ĥ ‖ ‖^2_F/ ‖ ‖H̃_{ad} ‖ ‖^2_F}.

Table I compares the NMSE performance of various CSI feedback methods across different feedback overheads. For the proposed method with multi-rate codebook design, we set L = 2 and γ = 0.8, indicating that a single nested codebook covers two different rates. Table I demonstrates that, for the same feedback overhead, the proposed method outperforms other CSI feedback methods. This result indicates that the proposed method effectively enhances the performance of the original VQ-VAE approach through a judicious design of the vector codebook. Furthermore, it is shown that the proposed method with multirate codebook design achieves better performance than the proposed method with single-rate codebook design. This result demonstrates that our multi-rate codebook design strategy not only reduces the number of required codebooks but also facilitates the effective design of the codebook. A similar result is also depicted in Fig. 2, which compares the NMSE performance of the proposed method with and without multi-rate codebook design when L = 4. Fig. 2 shows that the proposed method with multi-rate codebook outperforms the proposed method with the separate design of the codebooks.

TABLE I COMPARISON OF THE NMSE (dB) PERFORMANCE OF VARIOUS CSI FEEDBACK METHODS ACROSS DIFFERENT FEEDBACK OVERHEADS.

Indoor Feedback Overheads (Bits) 384 512 640 768 Model in [3] (M = 128) -10.24 -12.58 -13.64 -14.02 Model in [16] (M = 128, 256, −, 256)

-10.72 -11.71 - -13.14

VQVAE (M = 1024) -12.31 -14.17 -14.63 -15.21 Proposed (Single-rate, L = 1) (M = 512, 512, 1024, 1024)

-13.06 -14.79 -15.33 -16.33

Proposed (Multi-rate, L = 2)

(M = 512 | M = 1024)

-13.15 -14.93 -15.5 -16.41

Outdoor Feedback Overheads (Bits) 768 1024 1536 2048 Model in [3] (M = 256, 256, 512, 512)

-6.67 -7.94 -9.96 -11.54

Model in [17] (M = 128, 256, 256, 512)

-5.51 -8.10 -8.35 -12.13

VQVAE (M = 2048, 2048, 3072, 4096)

-6.92 -7.32 -9.56 -10.98

Proposed (Single-rate, L = 1) (M = 1024, 1024, 2048, 2048)

-7.11 -9.06 -10.17 -12.7

Proposed (Multi-rate, L = 2) (M = 1024 | M = 2048)

-7.34 -9.15 -10.32 -13.13

Fig. 3 compares the trade-off between performance and complexity achieved by the proposed and original VQ-VAE methods. In this simulation, the computational complexity is measured by the number of multiplications in the quantization process. Fig. 3 demonstrates that, for the same complexity, the proposed method significantly outperforms the VQ-VAE method. This result verifies that the proposed method is a powerful solution to improve the performance-complexity trade-off in finite-rate CSI feedback.

V. CONCLUSION In this paper, we have presented a finite-rate DL-based CSI feedback method for massive MIMO systems, utilizing the VQ-VAE framework. By leveraging shape-gain vector quantization, we have successfully alleviated the computational complexity associated with VQ-VAE, while improving its reconstruction performance under a given feedback overhead. We have also demonstrated that the presented method can support multirate vector quantization by harnessing the principle of the nested quantization.

Fig. 3. Comparison of the performance-complexity trade-off achieved by the proposed and original VQ-VAE methods.

REFERENCES

[1] C.-K. Wen, W.-T. Shih, and S. Jin, “Deep learning for massive MIMO CSI feedback,” IEEE Wireless Commun. Lett., vol. 7, no. 5, pp.

748–751, Oct. 2018.

[2] Z. Lu, J. Wang, and J. Song, “Multi-resolution CSI feedback with deep learning in massive MIMO system,” in Proc. IEEE Int. Conf.

Commun. (ICC), June 2020, pp. 1–6.

[3] J. Guo, C.-K. Wen, S. Jin, and G. Y. Li, “Convolutional neural network-based multiple-rate compressive sensing for massive MIMO CSI feedback: Design, simulation, and analysis,” IEEE Trans. Wireless Commun., vol. 19, no. 4, pp. 2827–2840, Apr. 2020.

[4] D. J. Love, R. W. Heath, Jr., V. K. Lau, D. Gesbert, B. D. Rao, and M. Andrews, “An overview of limited feedback in wireless communication systems,” IEEE J. Sel. Areas Commun., vol. 26, no. 8, pp. 1341–1365, Oct. 2008.

[5] Z. Qin, J. Fan, Y. Liu, Y. Gao, and G. Y. Li, “Sparse representation for wireless communications: A compressive sensing approach,” IEEE Signal Process. Mag., vol. 35, no. 3, pp. 40–58, May 2018.

[6] X. Liang, H. Chang, H. Li, X. Gu, and L. Zhang, “Changeable rate and novel quantization for CSI feedback based on deep learning,” IEEE Trans. Wireless Commun., vol. 21, no. 12, pp. 10100–10114, Dec. 2022.

[7] Z. Liu, L. Zhang, and Z. Ding, “An efficient deep learning framework for low rate massive MIMO CSI reporting,” IEEE Trans. Commun., vol. 68, no. 8, pp. 4761–4772, Aug. 2020.

[8] A. Gersho and R. M. Gray, Vector Quantization and Signal Compression, USA: Kluwer Academic Publishers, Ch. 10, 1991. [9] V. Rizzello, M. Nerini, M. Joham, B. Clerckx, and W. Utschick, “User-driven adaptive CSI feedback with ordered vector quantization,” IEEE Wireless Commun. Lett., vol. 12, no. 11, pp. 1956–1960, Nov. 2023.

[10] J. Yang, X. Chen, H. Zou, D. Wang, Q. Xu, and L. Xie, “EfficientFi: toward large-scale lightweight WiFi sensing via CSI compression,” IEEE Internet of Things Journal, vol. 9, no. 15, pp. 13086–13095, Aug., 2022.

[11] A. van den Oord, O. Vinyals, and K. Kavukcuoglu, “Neural discrete representation learning,” Adv. Neural Inf. Process. Syst., Dec. 2017, pp. 6306–6315.

[12] M. Malka, S. Ginzach, and N. Shlezinger, “Learning multi-rate vector quantization for remote deep inference,” in Proc. IEEE Int. Conf.

Acoustics, Speech, Sig. Process. Workshops (ICASSPW), June 2023, pp. 1–5.

[13] N. Shlezinger and Y. C. Eldar, “Deep task-based quantization,” Entropy, vol. 23, no. 1, 104, Jan. 2021.

[14] Y. Linde, A. Buzo, and R. Gray, “An algorithm for vector quantizer design,” IEEE Trans. Commun., vol. 28, no. 1, pp. 84–95, Jan. 1980. [15] L. Liu et al., “The COST 2100 MIMO channel model,” IEEE Wireless Commun., vol. 19, no. 6, pp. 92–99, Dec. 2012. [16] X. Liang, Z. Jia, X. Gu, and L. Zhang, “Towards better low-rate deep learning-based CSI feedback: a test channel-based approach,” IEEE Trans. Wireless Commun., early access. doi: 10.1109/TWC.2024.3354238.

[17] X. Zhang, Z. Lu, R. Zeng and J. Wang, “Quantization Adaptor for Bit-Level Deep Learning-Based Massive MIMO CSI Feedback,” IEEE Trans. Veh. Technol., early access. doi: 10.1109/TVT.2023.3333358.