arXiv:2405.09200v1 [cs.IT] 15 May 2024

Performance Analysis of RIS-aided MISO Systems with EMI and Channel Aging

Taoyu Song, Enyu Shi, Yu Lu, Yiyang Zhu, Jiayi Zhang, and Bo Ai, Fellow, IEEE School of Electronic and Information Engineering, Beijing Jiaotong University, Beijing 100044, China

Abstract—In this paper, we investigate a reconfigurable intelligent surface (RIS)-aided multiple-input single-output (MISO) system in the presence of electromagnetic interference (EMI) and channel aging with a Rician fading channel model between the base station (BS) and user equipment (UE). Specifically, we derive the closed-form expression for downlink spectral efficiency (SE) with maximum ratio transmission (MRT) precoding. The Monte- Carlo simulation supports the theoretical results, demonstrating that amplifying the weight of the line-of-sight (LoS) component in Rician fading channels can boost SE, while EMI has a detrimental impact. Furthermore, continuously increasing the number of RIS elements is not an optimal choice when EMI exists. Nonetheless, RIS can be deployed to compensate for SE degradation caused by channel aging effects. Finally, enlarging the RIS elements size can significantly improve system performance.

I. INTRODUCTION With the evolution of wireless communication technology, it is anticipated that 5G may not meet future demands for ultra-high data rates, ultra-low latency, and extensive coverage [1]. Therefore, in recent years, the global industry has started preliminary research on 6G and brought about significant advancements in areas such as millimeter-wave (mmWave) communications [2], cell-free (CF) massive multiple-input multipleoutput (MIMO) [3], reconfigurable intelligent surface (RIS) [4], and ultra-dense network (UDN) [5]. RIS is a rising technology that can shape radio waves without using complex digital signal processing methods or active power amplifiers [6]. Thus, it has recently been considered a new way to create reconfigurable wireless channels in some scenarios with hostile communication environments [7], [8]. Due to the different fabrication, RIS exhibits distinct properties compared to traditional uniform linear arrays (ULAs).

However, [9] demonstrates that natural electromagnetic interference (EMI) can significantly affect the system performance, highlighting the importance of taking EMI into account in RISaided systems. In [10], the authors consider the effect of EMI on the uplink spectral efficiency (SE) of user equipment (UE) in CF massive MIMO systems and it indicates that EMI significantly affects SE, and the influence of EMI becomes more pronounced when the components of RIS are sufficiently large. Meanwhile, [11] highlights that the dynamic channel hasn’t been thoroughly explored in current research, and most setups rely on the block fading model with roughly uniform channel features within coherent blocks. The decline in performance

This work was supported by the Fundamental Research Funds for the Central Universities under Grants 2023YJS015.

stems from the disparity between the real channel and the estimated channel due to user position shifts, thus necessitating a reevaluation of the influence of channel aging in RIS-aided systems.

Building upon prior research, this paper explores closed-form expressions for the downlink SE of RIS-aided multiple-input single-output (MISO) system with EMI over spatially correlated channels. We assume a Rician fading channel between the RIS and the base station (BS) while the channels from UE to RIS and UE to BS are Rayleigh fading. We employ a minimum mean square error (MMSE) estimator for channel state information (CSI) from the pilot signal, and maximum ratio transmission (MRT) precoding is used at BS. Then, we analyze the impact of various parameters on SE and validate the equation through Monte Carlo simulation. The results show that increasing line-of-sight (LoS) weight in the Rician fading channel improves SE, RIS can alleviate the effects of channel aging, and enlarging the RIS size can enhance system performance. However, EMI will have a significant negative impact when there are more RIS elements. Moreover, increasing transmission time and user movement speed will amplify the effects of channel aging.

II. SYSTEM MODEL We assume that the BS has N_t antennas. The RIS consists of a controller and M elements capable of applying phase shifts to incoming signals. For the UE side, we consider a constant speed denoted as v for user movement while the BS and the RIS remain static. We assume that each coherence time block is represented as τ_c . In the uplink, we allocate τ_u symbols for channel estimation, while τ_d = τ_c − τ_u symbols are for data transmission in the downlink. The channels are assumed to remain unchanged over symbol duration but vary across symbol time gaps. We assume independent Rayleigh fading models between the BS and UE, as well as between the RIS and UE, and Rician fading model is used between RIS and BS.

A. Channel Model

At the time of transmitting the n-th symbol, the channel matrix of the direct link between the BS and the UE can be expressed as G_d [n] = [g_{d,1} [n] , ..., g_{d,k} [n] , ..., g_{d,K} [n]] ∈ C^{Nt ×K} where g_{d,k} [n] ∈ C^{Nt} denotes the channel between UE k and the BS. Specially, g_{d,k} [n] can be expressed as g_{d,k} [n] = √ β_{d,k}h_{d,k} [n] , ∀k ∈ {1, ..., K} where h_{d,k} [n] ∈ C^{Nt} denotes the small-scale fading coefficient between UE k and the BS, β_{d,k} denotes the path loss of the direct path. For the channel between the RIS and the BS, we can express as [12] G_{br} = √ β_{br} (√ κ κ + 1 ḡ_{br} + √ 1 κ + 1 g̃_{br} ) ∈ C^{Nt ×M} , (1) where ḡ_{br} = [ḡ_{br1}, ..., ḡ_{brm}, ..., ḡ_{brM} ] ∈ C^{Nt ×M} denotes the deterministic LoS component, while ḡ_{brm} ∈ C^{Nt} can be expressed as ḡ_{brm} = [α exp (jθ_1) , ..., α exp (jθ_n) , ..., α exp (jθ_{Nt} )]^T where α ∈ [0, 1] and θ_n ∈ [0, 2π] represents the amplitude and phase of the signal. We assume that the amplitude of the signal reaches its maximum. Meanwhile, g̃_{br} is the non-line of sight (NLoS) component. β_{br} denotes the corresponding path loss. At the time of transmitting the n-th symbol, the channel matrix of the direct link between the UE and the RIS can be expressed as g_{r,k} [n] = [g_{r,k1} [n] , ..., g_{r,kM} [n]]^T ∈ C^M where g_{r,km} [n] = √ β_{r,k}h_{r,km} [n] denotes the channel between UE k and m-th element of RIS. We denote the channel between the RIS and the UE as G_{r,ue} [n] = [g_{r,1} [n] , ..., g_{r,k} [n]] ∈ C^{M ×K} . And g_{r,k} ∼ N (0, Aβ_{r,k}R), where β_{r,k} denotes the corresponding path loss. d_H and d_V represent the horizontal width and the vertical height of a RIS element, and A = d_H d_V denotes the area of the RIS element. R ∈ C^{M ×M} denotes the correlation matrix which has the (n, m)-th element as [R]_{n,m} = sinc (2‖u_n − u_m‖/λ) where sinc (x) = sin (πx) / (πx) and λ denotes the carrier wavelength. The position of the m-th element with respect to the origin is u_m = (0, mod (m − 1, M_H ) d_H , ⌊(m − 1) /M_H ⌋d_V )^T , m ∈ [0, M] , where M_H and M_V are the numbers of elements at RIS in each row and column, such that M = M_H × M_V [13]. Therefore, the cascade channel can be represented as G_{c,k} [n] = G_{br}Φ [n] g_{r,k} [n] , where Φ [n] = diag {ϕ exp (jθ_1) , ..., ϕ exp (jθ_M )} ∈ C^{M ×M} denotes the RIS reflection matrix, ϕ ∈ [0, 1] and θ_m ∈ [0, 2π] represents the amplitude and phase of the reflected signal. Due to the sparsity and serious path loss of the mmWave channel, we only consider the signal reflected by the RIS for the first time [11]. Same as above, we assume that α = 1. We can also express G_{c,k} [n] as G_{c,k} [n] = g_{ck} [n] v [n], where G_{ck} [n] = [g_{ck1} [n] , ..., g_{ckM} [n]] ∈ C^{Nt ×M} represents the cascade channel matrix and v [n] = [ϕ exp (jθ_1) , ..., ϕ exp (jθ_M )] ∈ C^{M×1} denotes the RIS reflection matrix . Moreover, g_{ckm} [n] can be expressed as g_{ckm} [n] = g_{brm}g_{r,km} [n]. B. Electromagnetic Interference Model

The EMI is an uncontrolled electromagnetic wave generated by electronic devices, which can cause interference to other devices. In [9], the author demonstrates that the EMI at the RIS significantly affects communication quality. Especially, the EMI is donated as n ∼ N ( 0, Aσ^2_e R ) where σ^2_e is the EMI power at RIS. To further investigate the effects of EMI, we define ρ = P_{τp} β_{br}/σ^2_e which corresponds to the ratio between the received signal power and EMI power at each element of the RIS [9].

Remark 1. For the sinc function, the output is zero only when the argument is a non-zero integer, implying that the magnitude of ‖u_n − u_m‖ must be an integer multiple of λ/2. This means that the RIS elements should be aligned along a straight line with intervals that are integer multiples of λ/2, which is impossible to achieve with a two-dimensional RIS in practice. Thus, it is essential to take into account the impact of EMI with spatial correlation at the RIS elements.

C. Channel Estimation

We use τ_p pilot sequences to estimate channel, in every coherence time block. The pilot signal emitted by UE k, which is represented by φ_k ∈ C^{τp} , meets the condition that ‖φ_k‖^2 = 1. Thus, the pilot matrix transmitted by the K UE is mutually orthogonal as Ψ = [φ_1, ..., φ_k] ∈ C^{τp ×K} , which satisfies Ψ^H Ψ = I_K . The pilot signals from different UE satisfy φ^H_i φ_j = 0, ∀i ≠ j. Considering the EMI, the received signal G_{r,k} [n] at the RIS is G_{r,k} [n] = g_{r,k} [n] φ^T_k [n] + N where N ∈ C^{M ×τp} represents the additive EMI at RIS. We perform linear MMSE estimates for direct and cascade links. Initially, we obtain channel vector estimates, then we derive channel characteristics at subsequent time points based on temporal correlation. During pilot signal transmission, we assume constant direct and cascade channels, allowing us to disregard the effects of channel aging [11]. For the channels between UE and BS, the signal received by the BS can be presented as

Y^p_d [0] = √ P_{τp} G_d [0] Ψ^H + Z^p_d [0] , (2) where P_{τp} = τ_pP_{τu} represents the pilot signal power, P_{τu} is the average uplink transmission power per UE. Z^p_d [0] ∼ N ( 0, σ^2_dI_{Nt} ) ∈ C^{Nt ×τp} represents the noise received at the BS at the initial state, where σ^2_d represents the variance of the noise. Then, we multiply (2) by 1/ √ P_{τp} φ_k and we get the direct link as ỹ^p_{d,k} [0] = g_{d,k} [0] + 1 √ P_{τp} Z^p_d [0] φ_k. (3)

The optimal g_{d,k} [0] can be obtained using the MMSE estimation method, which minimizes the mean squared error E ( ‖g_{d,k} [0] − ĝ_{d,k} [0]‖^2 ) [14]. So the estimated g_{d,k} [0] can be expressed as [11]

ĝ_{d,k} [0] = ( 1 + σ^2_d P_{τp} β_{d,k} )_{−1} ỹ^p_{d,k} [0] . (4)

Thus, g_{d,k} [0] can be expressed as g_{d,k} [0] = ĝ_{d,k} [0] + g̃_{d,k} [0] where ĝ_{d,k} [0] ∼ N ( 0,^{Pτp β2d,k} σ^2_d+P_{τp} β_{d,k} IN^t ) . And g̃_{d,k} [0] ∼ N ( 0,^{σ2dβd,k} σ^2_d +P_{τp} β_{d,k} IN^t ) is the estimation error which is uncorrelated with ĝ_{d,k} [0]. We can get the cascade link between the BS and UE without the reflection matrix as

Y^p_c [0] = √ P_{τp} ( G_d [0] Ψ^H + G_{br}G_r [0] ) + Z^p_c [0] , (5)

where G_r [0] can be expressed as G_r [0] = G_{r,ue} [0] Ψ^H + N. Then, we multiply (5) by1/ √ P_{τp} φ_k and we get the cascade link as

ỹ^p_{c,k}[0]=g_{d,k}[0]+g_{ck}[0]+G_{br}Nφ_k + 1 √ P_{τp} Z^p_c [0] φ_k. (6)

Here, Z^p_c [0] ∼ N ( 0, σ^2_c I_{Nt} ) ∈ C^{Nt ×τp} represents the noise received at the BS at the initial state, where σ^2_c represents the variance of the noise. After ignoring the channel estimation error, we obtain the cascade link as

ỹ^p_{c,k} [0] = g̃_{d,k} [0]+g_{ck} [0]+G_{br}Nφ_k + 1 √ P_{τp} Z^p_c [0] φ_k. (7)

So the MMSE estimation of g_{ck} [0] can be expressed as ĝ_{ck} [0] = ξ_{c,k} ( σ^2_dβ_{d,k} σ^2_d + P_{τp} β_{d,k} + ξ_{c,k} + Q + σ^2_c P_{τp} )_{−1} ỹ^p_{c,k} [0] , (8) where ξ_{c,k} = Aβ_{r,k}β_{br} (κ/ (κ + 1) + A/ (κ + 1)) and Q = Aσ^2_e tr (R_e) β_{br} (κ/ (κ + 1) + A/ (κ + 1)). Similarly, g_{ck} [0] can be expressed as g_{ck} [0] = ĝ_{ck} [0] + g̃_{ck} [0] where ĝ_{ck} [0] ∼ N ( 0,^{ξc,k σ2e1,k} σ^2_{e1,k} +σ^2_{e2,k} +σ^2_{e3,k} +σ^2_dσ^2_c IN^t ) . And

g̃_{ck} [0] ∼ N ( 0,^{ξc,k} (^{σ2e2,k +σ2e3,k} ) σ^2_{e1,k} +σ^2_{e2,k} +σ^2_{e3,k} +σ^2_dσ^2_c IN^t ) is the estima-

tion error which is uncorrelated with ĝ_{ck} [0], where σ^2_{e1,k} ≜ P_{τp} ξ_{c,k} ( σ^2_d + P_{τp} β_{d,k} ) , σ^2_{e2,k} ≜ P_{τp} β_{d,k} ( σ^2_d + σ^2_c ) , σ^2_{e3,k} ≜ Q ( σ^2_d + P_{τp} β_{d,k} ) . D. Channel Aging

Due to the relative position change between the UE and the BS causing channel aging, the CSI is usually not perfectly estimated. Therefore, we must consider the impact of outdated CSI on system performance. According to [11], g_{d,k} [n] and g_{r,k} [n] can be represented by their initial state, respectively g_{d,k} [n] = ρ_0 [n] g_{d,k} [0] + ρ̄_0 [n] e_{d,k} [n] , (9) g_{r,km} [n] = ρ_1 [n] g_{r,km} [0] + ρ̄_1 [n] e_{r,km} [n] . (10) According to the Jakes’ model [11], the temporal correlation coefficient is donated as ρ_i [n] = J_0 (2πnf_DT_s) (i ∈ {0, 1}) [15], where J_0 (·) is the initial class of zeroth-order Bessel function, f_c is the carrier frequency, c is the velocity of light, so f_D = f_cv/c is the maximum Doppler shift and T_s is the sample interval. We assume ρ_i [n] is known at the BS. Moreover, ρ̄_i [n] = √ 1 − ρ^2_i [n] donates the coefficient of the current channel part independent of the initial state of the channel. This part satisfies that e_{d,k} [n] ∼ N (0, β_{d,k}I_{Nt} ), and e_{r,km} [n] ∼ N (0, 1), respectively. Thus, g_{ckm} [0] can be written as g_{ckm} [0] = ρ_1 [n] g_{brm}g_{r,km} [0] + ρ̄_1 [n] g_{brm}e_{r,km} [n]. We define that e_{ckm} [n] ≜ g_{brm}e_{r,km} [n], so e_{ck} [n] ∼ N (0, ξ_{c,k}I_{Nt} ). After considering the combined effect of estimation error and channel aging we can obtain the expressions for cascading links as g_{ck} [0] = ρ_1 [n] (ĝ_{ck} [0] + g̃_{ck} [0]) + ρ̄_1 [n] e_{ck} [n] , (11) where ẽ_{ck} [n] ≜ ρ_1 [n] g̃_{ck} [0] + ρ̄_1 [n] e_{ck} [n], and ẽ_{ck} [n] ∼ N ( 0, ( ξ_{c,k} −^{ρ21 [n]ξc,k σ2e1,k} σ^2_{e1,k} +σ^2_{e2,k} +σ^2_{e3,k} +σ^2_d σ^2_c ) I_{Nt} ) . Similarly, the direct link can be expressed as g_{d,k} [0] = ρ_0 [n] ĝ_{d,k} [0] + ẽ_{d,k} [n] , (12) where ẽ_{d,k} [n] ≜ ρ_0 [n] g̃_{d,k} [0] + ρ̄_0 [n] e_{d,k} [n], and ẽ_{d,k} [n] ∼ N ( 0, ( β_{d,k} −^{ρ20[n]Pτp β2d,k} σ^2_d +P_{τp} β_{d,k} ) I_{Nt} ) .

III. PERFORMANCE ANALYSIS AND USEFUL INSIGHTS

Based on the channel reciprocity [16] and combined with the channel aging, we can express the received signal at UE k in the phase of downlink signal transmission as

y_k [n] = ( g^H_{d,k} [n] + v^H [n] g^H_{ck} [n] ) x [n] + g^H_{r,k} [n] Φ^H [n] u + ω_k [n] , (13) where x [n] = F [n] s [n]represents the signal transmitted by the BS with power P_T ⩾ tr ( F^H [n] F [n] ) = E ( ‖x [n]‖^2 ) , and u ∼ N ( 0, Aσ^2R ) ∈ C^M denotes the additive EMI noise.

F [n] = [f_1 [n] , ..., f_K [n]] ∈ C^{Nt ×K} denotes the precoding matrix and s [n] = [s_1 [n] , ..., s_K [n]]^T ∈ C^K donates received signal vector at UE, which satisfies E (s [n]) = 0 and E ( s [n] s^H [n] ) = I_K . ω_k [n] denotes additive white Gaussian noise at UE k, which satisfies ω_k [n] ∼ N ( 0, σ^2_k ) . We define G_k [n] ≜ g^H_{d,k} [n] + v^H [n] g^H_{ck} [n], so we can get

G_k [n] = ρ_0 [n] ĝ^H_{d,k} [0] + ẽ^H_{d,k} [n] + v^H [n] ( ρ_1 [n] ĝ^H_{ck} [0] + ẽ^H_{ck} [n] ) , (14) where we define Ḡ_k [n] ≜ ρ_0 [n] ĝ^H_{d,k} [0] + ρ_1 [n] v^H [n] ĝ^H_{ck} [0] and G_{e,k} [n] ≜ ẽ^H_{d,k} [n]+v^H [n] ẽ^H_{ck} [n]. Therefore, the received signal at UE k can be expressed as

y_k [n] = E (G_k [n] f_k [n]) s_k [n] + K∑ j=1,j≠k G_k [n] f_j [n] s_j [n]

+ G_k [n] f_k [n] s_k [n] − E (G_k [n] f_k [n]) s_k [n] + g^H_{r,k} [n] Φ^H [n] u + ω_k [n] . (15) Using the MRT precoding algorithm, we assume that the CSI known at the BS at time n is G_k [n]. The precoding matrix can be expressed as [11] F [n] = ζ [n] (¯ G [n] )_H , where ζ^2 [n] ≜ 1/tr ( Ḡ [n] (Ḡ [n])^H ) denotes the normalized coefficient of

the precoding matrix and Ḡ [n] = [¯ G_1 [n] , ..., Ḡ_K [n] ]_T . According to the use-and-then-forget capacity bound [11], the minimum SE achievable by UE k is limited by R_k = 1 τ_c ∑_{τc−τu} n=1 log_2 (1 + γ_k [n]), where γ_k [n] is the SINR of the UE k at time n. γ_k [n] can be expressed as (16) at the top of the next page.

Corollary 1:

I_{0.kn} = ζ^2 [n] ( N_t ( ρ^2_0 [n] P_{τp} β^2_{d,k} σ^2_d + P_{τp} β_{d,k} + Mρ^2_1 [n] ξ_{c,k}σ^2_{e1,k} σ^2_{e1,k} + σ^2_{e2,k} + σ^2_{e3,k} + σ^2_dσ^2_c ))_2 , (17)

I_{1.kn} = ζ^2 [n] N_t ( Mρ^2_1 [n] ξ_{c,k}σ^2_{e1,k} σ^2_{e1,k} + σ^2_{e2,k} + σ^2_{e3,k} + σ^2_dσ^2_c + ρ^2_0 [n] P_{τp} β^2_{d,k} σ^2_d + P_{τp} β_{d,k} ) × (( β_{d,k} − ρ^2_0 [n] P_{τp} β^2_{d,k} σ^2_d + P_{τp} β_{d,k} )

+M ( ξ_{c,k} − ρ^2_1 [n] ξ_{c,k}σ^2_{e1,k} σ^2_{e1,k} + σ^2_{e2,k} + σ^2_{e3,k} + σ^2_dσ^2_c )) , (18) γ_k [n] =

|E (G_k [n] f_k [n])|^2 I_{0.kn} V ar (G_k [n] f_k [n]) I_{1,kn} + K∑ j=1,j≠k E ( |G_k [n] f_j [n]|^2 )

I_{2,kn} + E (| |g^H_{r,k} [n] Φ^H [n] u|^2 ) I_{3,kn} + E ( |ω_k [n]|^2 ) I_{4.kn}

. (16)

I_{2.kn} = K∑ j=1,j≠k ζ^2 [n] N_t ( Mρ^2_1 [n] ξ_{c,k}σ^2_{e1,j} σ^2_{e1,j} + σ^2_{e2,j} + σ^2_{e3,j} + σ^2_dσ^2_c + ρ^2_0 [n] P_{τp} β^2_{d,j} σ^2_d + P_{τp} β_{d,j} ) × (( β_{d,k} − ρ^2_0 [n] P_{τp} β^2_{d,k} σ^2_d + P_{τp} β_{d,k} )

+M ( ξ_{c,k} − ρ^2_1 [n] ξ_{c,k}σ^2_{e1,k} σ^2_{e1,k} + σ^2_{e2,k} + σ^2_{e3,k} + σ^2_dσ^2_c )) , (19) I_{3.kn} = A^2β_{r,k}σ^2_e tr ( Φ^H [n] RΦ [n] R_e ) , (20) I_{4.kn} = σ^2_k . (21) Proof: The proof is given in Appendix A.

From the formula, we can see that with the increase of the pilot signal power P_{τp} and the number of BS antennas N_t, the SE will improve. When M = 0, (16) denotes the SINR of the system without RIS assistance.

IV. NUMERICAL RESULTS AND DISCUSSION In this section, we verify the correct lines of the expressions by comparing the results of Monte Carlo simulation with theoretical calculations. At the same time, we compare and analyze the influence of M, the Rician κ-factor and ρ_i [n] (i ∈ {0, 1}) on the SE. We denote the Rician κ-factor as κ = 10^{1.3−0.003dbr} , where d_{br} donates the distance between BS and RIS [10]. We set the carrier frequency to 2 GHz, the channel noise per UE to σ^2 = −96 dBm, and the dimension of the RIS element to d_H = d_V = λ/2. Moreover, the transmit pilot power is 25 dBm. Using a rectangular coordinate system, we set the positions of the BS and the RIS to (-50, 0, 30) and (0, 0, 15), respectively. The locations of the four UE is assumed to be (50, 0, 1.7), (50.5, 0, 1.7), (51, 0, 1.7) and (51.5, 0, 1.7).

Fig. 1 depicts the variations in the total SE due to different factors. The simulation results align closely with the experimental findings, indicating that the implementation of RIS significantly enhances system performance. Notably, SE tends to be stable when M tends to infinity without considering EMI. It can also be inferred from the equation that both the numerator and denominator increase simultaneously as M tends to infinity, leading the SE to approach a constant value. When considering EMI, the SE is negatively affected by the increase of M. This is consistent with the result in [9]. Furthermore, the higher the value of κ-factor, the greater the SE. When the M is small, the channel aging effect is more noticeable, and when the M is large, the EMI effect is more pronounced. For example, when M = 256, the effect of EMI reduces SE by approximately 8%, and channel aging reduces SE by approximately 6%.

We use f_DT_s to represent the impact of changes in ρ_i [n] on SE. It can be concluded from (9) and (10) that the faster

Fig. 1: Sum SE‘’ versus M and κ (N_t = 16, f_DT_s = 0. 001, τ_c = 100, τ_p = 4, ρ = 20 dB).

Fig. 2: Average SE versus time instant (N_t = 16, M = 64, τ_p = 4).

the user moves, the more serious the effect of aging on SE. Fig. 2 shows the relationship between the average SE and the transmission time under different f_DT_s and EMI. It can be seen that Increasing the value of f_DT_s will lead to a faster decline in the average SE. Similarly, an increase in EMI power will cause a decrease in SE. For f_DT_s = 0.002, the total transmission time τ_c should below 200, i. e. , τ_c < 200. When the EMI power increases by 20 dB, SE decreases by 22%. Additionally, we can observe that the alteration of ρ does not impact the change in time when SE decreases to 0.

Fig. 3 depicts the correlation of the relationship between f_DT_s and sum SE across different RIS element sizes and different transmission times. The system performance increases with the increase of RIS elements area. When f_DT_s = 0, τ_p = 4, a longer transmission time means a larger proportion of the downlink transmission time, resulting in a higher SE of the system. However, as f_DT_s increases, longer transmission time is associated with more dramatic declines in SE due to the worsening effects of channel aging. For example, when

Fig. 3: Sum SE versus normalized Doppler shift (N_t = 16, M = 64, τ_p = 4, ρ = 20 dB).

f_DT_s = 0.002, M = 64 and τ_c = 100, SE increases by 116% following a fourfold increase in the area of RIS elements. At this point, increasing the transmission time to τ_c = 200, SE will increase by 30%, indicating that expanding the area of RIS elements will restrain the negative effects of channel aging.

V. CONCLUSIONS

In this paper, we investigated the performance of the RISaided MISO system with the effect of channel aging and EMI. In particular, we consider the Ricican fading channel between the BS and RIS while the other paths are Rayleigh fading channels. The downlink SE closed-form expression is derived with the MRT precoding at the BS. The results indicate that the adoption of RIS can compensate for the negative effects of channel aging. However, when the number of RIS elements increases to a large number, EMI will deteriorate the system performance. In future work, we will design EMI-based precoding to mitigate the negative effects of EMI.

APPENDIX A

We can calculate each part as follows.

(1) For I_{0.kn}: According to (14), because G_{e,k} [n] and f_k [n] are independent on each other, we can obtain that E (G_k [n] f_k [n]) = ζ [n] E (¯ G_k [n] Ḡ^H_k [n] ) . According to the statistical properties of ĝ_{d,k} [0] and ĝ_{ck} [0], we can know that Ḡ_k [n] ∼ N ( 0, ( ρ^2_0 [n] P_{τp} β^2_{d,k} σ^2_d + P_{τp} β_{d,k} + Mρ^2_1 [n] ξ_{c,k}σ^2_{e1,k} σ^2_{e1,k} + σ^2_{e2,k} + σ^2_{e3,k} + σ^2_dσ^2_c )) , (22)

due to v^H [n] ĝ^H_{ck} [0] =^M ∑ m=1 v_m [n] ĝ^H_{ckm} [0]. Therefore, we

can obtain the expectation of Ḡ_k [n] Ḡ^H_k [n], because it has a Wishart distribution with complex-valued centers. Thus, we can get I_{0.kn}.

(2) For I_{1.kn}: Based on the property of the variance, we can obtain that V ar (G_k [n] f_k [n]) = E ( G_{e,k} [n] G^H_{e,k} [n] ) E ( f_k [n] f^H_k [n] ) . According to the (III), we can obtain that E ( f_k [n] f^H_k [n] ) = ζ^2 [n] N_t E (¯ G^H_k [n] Ḡ_k [n] ) . (23)

E ( G_{e,k} [n] G^H_{e,k} [n] ) can be written as E ( ẽ^H_{d,k} [n] ẽ_{d,k} [n] ) + E ( v^H [n] ẽ^H_{ck} [n] ẽ_{ck} [n] v [n] ) . (24) According to the properties of the Wishart distribution, we can get I_{1.kn} due to v^H [n] ẽ^H_{ck} [n] ẽ_{ck} [n] v [n] = M∑ m=1 M∑ l=1 exp (jθ_m [n] − jθ_l [n]) ẽ^H_{ck} [n] ẽ_{ck} [n].

(3) For I_{2.kn}:Because of E ( |G_k [n] f_j [n]|^2 ) = E ( G_{e,k} [n] f_j [n] f^H_j [n] G^H_{e,k} [n] ) , we can obtain I_{2.kn} in the same approach as above, (4) For I_{3.kn} and I_{4.kn} :We can easily prove the I_{3.kn} and I_{4.kn}. REFERENCES

[1] J. Zhang, E. Björnson, M. Matthaiou, D. W. K. Ng, H. Yang, and D. J.

Love, “Prospective multiple antenna technologies for beyond 5G,” IEEE J. Sel. Areas Commun., vol. 38, no. 8, pp. 1637–1660, Aug. 2020.

[2] T. S. Rappaport, Y. Xing, G. R. MacCartney, A. F. Molisch, E. Mellios, and J. Zhang, “Overview of millimeter wave communications for fifthgeneration (5G) wireless networks—with a focus on propagation models,” IEEE Trans. Antennas Propag., vol. 65, no. 12, pp. 6213–6230, Dec. 2017.

[3] E. Shi, J. Zhang, S. Chen, J. Zheng, Y. Zhang, D. W. Kwan Ng, and B. Ai, “Wireless energy transfer in RIS-aided cell-free massive MIMO systems: opportunities and challenges,” IEEE Commun. Mag., vol. 60, no. 3, pp. 26–32, Mar. 2022.

[4] E. Shi, J. Zhang, H. Du, B. Ai, C. Yuen, D. Niyato, K. B. Letaief et al., “RIS-aided cell-free massive MIMO systems for 6G: fundamentals, system design, and applications,” arXiv:2310.00263, 2023.

[5] J. G. Andrews, X. Zhang, G. D. Durgin, and A. K. Gupta, “Are we approaching the fundamental limits of wireless network densification?” IEEE Commun. Mag., vol. 54, no. 10, pp. 184–190, Oct. 2016.

[6] Y. Zhang, J. Zhang, M. Di Renzo, H. Xiao, and B. Ai, “Reconfigurable intelligent surfaces with outdated channel state information: centralized vs. distributed deployments,” IEEE Trans. Commun., vol. 70, no. 4, pp. 2742–2756, Apr. 2022.

[7] Q. Wu and R. Zhang, “Intelligent reflecting surface enhanced wireless network via joint active and passive beamforming,” IEEE Trans. Wireless Commun., vol. 18, no. 11, pp. 5394–5409, Nov. 2019.

[8] J. Zhang, H. Liu, Q. Wu, Y. Jin, Y. Chen, B. Ai, S. Jin, and T. J. Cui, “RISaided next-generation high-speed train communications: Challenges, solutions, and future directions,” IEEE Wireless Commun., vol. 28, no. 6, pp. 145–151, Jun. 2021.

[9] A. de Jesus Torres, L. Sanguinetti, and E. Björnson, “Electromagnetic interference in RIS-aided communications,” IEEE Wireless Commun. Lett., vol. 11, no. 4, pp. 668–672, Apr. 2022.

[10] E. Shi, J. Zhang, D. W. K. Ng, and B. Ai, “Uplink performance of RISaided cell-free massive MIMO system with electromagnetic interference,” IEEE J. Sel. Areas Commun., vol. 41, no. 8, pp. 2431–2445, Aug. 2023.

[11] Y. Lu, Y. Zhang, J. Zhang, and B. Ai, “Performance analysis of RISassisted wireless systems with channel aging and spatial correlation,” ITU J-FET, vol. 4, no. 1, pp. 1–12, Jan. 2023.

[12] Y. Zhang, J. Zhang, M. Di Renzo, H. Xiao, and B. Ai, “Reconfigurable intelligent surfaces with outdated channel state information: Centralized vs. distributed deployments,” IEEE Trans. Commun., vol. 70, no. 4, pp. 2742–2756, Apr. 2022.

[13] E. Björnson and L. Sanguinetti, “Rayleigh fading modeling and channel hardening for reconfigurable intelligent surfaces,” IEEE Wireless Commun. Lett., vol. 10, no. 4, pp. 830–834, Apr. 2020.

[14] N. K. Kundu and M. R. McKay, “Channel estimation for reconfigurable intelligent surface aided MISO communications: From LMMSE to deep learning solutions,” IEEE Open J. Commun. Society, vol. 2, no. 3, pp. 471–487, Mar. 2021.

[15] A. K. Papazafeiropoulos, “Impact of general channel aging conditions on the downlink performance of massive MIMO,” IEEE Trans. Veh. Technol., vol. 66, no. 2, pp. 1428–1442, Feb. 2017.

[16] K. T. Truong and R. W. Heath, “Effects of channel aging in massive MIMO systems,” J. Commun. Networks, vol. 15, no. 4, pp. 338–351, Aug. 2013.