astro-ph/9607022

First results from a second generation galactic axion experimentC. Hagmann, D. Kinion, W. Stoeffl, K. van BibberLawrence Livermore National Laboratory7000 East Ave, Livermore, CA 94550E. Daw, J. McBride, H. Peng, L.J. Rosenberg, H. XinDept of Physics, Massachusetts Institute of Technology77 Massachusetts Ave, Cambridge, MA 02139J. Laveigne, P. Sikivie, N.S. Sullivan, D.B. TannerDept of Physics, University of FloridaGainesville, FL 94720D. MoltzNuclear Science Division, Lawrence Berkeley Laboratory1 Cyclotron Rd, Berkeley, CA 94720F. Nezrick, M.S. TurnerFermi National Accelerator LaboratoryBatavia, IL 60510N. Golubev, L. KravchukInstitute for Nuclear Research of the Russian Academy of Sciences60th October Anniversary Prospekt 7a, Moscow 117312, RussiaWe report first results from a large-scale search for dark matter axions. The experiment probesaxion masses of 1.3-13 meV at a sensitivity which is about 50 times higher than previous pilotexperiments. We have already scanned part of this mass range at a sensitivity better than required tosee at least one generic axion model, the KSVZ axion. Data taking at full sensitivity commenced inFebruary 1996 and scanning the proposed mass range will require three years.1. INTRODUCTIONAt present, the hypothetical axion is one ofthe leading candidates for the dark matter inthe universe. The axion is a consequence of thePeccei-Quinn mechansim to solve the strongCP problem in QCD [1,2], and it has propertiessimilar to those of a light neutral pion, butwith much weaker couplings to ordinarymatter. Cosmological and astrophysicalarguments [3] constrain its mass to 10-6 < ma <10˚-3 eV. The relic axion density is roughlyinversely proportional to the axion mass andprovides critical density for ma = O(10-6 eV).These axions are cold dark matter (CDM) andhave never been in thermal equilibrium withother particles. CDM is a major ingredient oftheories of structure formation and inparticular could be the material that makes upthe dark halo of our galaxy.

2. TECHNIQUEGalactic axions are nonrelativistic and canbe converted into monochromatic microwavephotons (hf=mc2(1+O(10-6)) via the Primakoffeffect in a static magnetic field B. This processis resonantly enhanced in a high-Q microwavecavity tuned to the axion mass. The expectedsignal, normalized to our current experimentalparameters, is [4,5]

Pa→ γ ≈ 10^{− 21}W B7.7T^2 V200l C0.65 Q 90000 f 0.7 GHz ρ a ρ halo

(1)where V is the cavity volume, C is a modedependent form factor (maximal for thefundamental TM010 mode), Q is the loadedquality factor, and ra is the local axion density.This power is calculated for the hadronicKSVZ axion [6] and corresponds to a fewthousand converted axions per second. TheGUT inspired DSFZ axion [7] yields aboutseven times fewer conversions.The signature of an axion signal is a narrowpeak (of fractional width » 10-6 due to kineticenergy) above the thermal backgroundcomposed of cavity blackbody radiation andamplifier noise. The latter is usually expressedas a system noise temperature Ts=Tc+Ta, whereTc i s t h e c a v i t y t e m p e r a t u r e a n d T a is theamplifier noise temperature. Since the axion mass is not known, thecavity must be tunable, so it may be slowlyscanned in frequency. For a signal-to-noiseratio s/n and a signal power given by (1), thescan rate is

dfdt ≈ 25 MHzmonth 4s / n 2 6 KTs 2.

(2)3. DETECTOR Figure 1 shows the dewar, which contains themagnet and the insert comprising themicrowave cavity and amplifier. The magnethas its own helium reservoir and remains coldduring changes in the cavity/amplifierconfiguration. The cylindrical cavity isoperated in the TM010 mode. It is made ofcopper plated stainless steel and contains twotuning rods (alumina or copper) which aremoved transversely. Using differentcombinations of rods, the tuning range is (0.65-1.7)f0, where f0 is the resonance frequency ofthe empty cavity (460 MHz for the first singlecavity) . A pair of stepper motors on the dewartop drive 1:30000 worm gear reducersmounted on the cavity. The frequency tuningresolution is a few 100 Hz. The resonancefrequency (FWHM » 10 kHz) is typicallystepped by a few kHz.

cryostat vessel stepping motors

to vacuum pumpLHe reservoir for cavityLHe reservoir for magnetGaAs amplifiercavity tuning mechanismcopper plated RF cavityalumina tuning rodcopper tuning rodsuperconducting magnet360 cm

Fig 1 Drawing of axion dewar.We use a balanced, 30 dB gain, 2-stageHEMT amplifier built by the NRAO at ourfront end. Its nominal noise temperature is »4˚K for physical temperatures < 15 K. Thebalanced design makes the amplifier

insensitive to the cavity output impedance andavoids the use of a circulator.Both cavity and amplifier are cooled to1.4˚K with helium gas pumped by a rootsblower. A small reservoir of superfluid heliumis maintained at the bottom of the cancontaining the cavity. The liquid level isregulated by a computer controlled valveconnected to the main tank. The heliumconsumption of the cavity is about 7liters/day.The magnet is a high inductance (500 H),low current (225 A) NbTi solenoid. Thecurrent is provided by a computer controlledpower supply with a short term stability of5ppm. The current runs through a pair ofoptimized vapor cooled current leads madefrom copper foil. The dewar has a LN2 jacketand three intermediate temperature layers at80, 50, and 30 K. The helium usage of themagnet is 50 liters/day.IF section10.7 MHzLF section100 kHzMW section0.3-3.1 GHz

LOLOCesium clock400 pt FFT106 pt FFTFig.2 Electronic block diagram.4. SIGNAL PROCESSINGThe signal processing chain is shown inFigure 2. It consists of several amplificationand mixing stages. The low frequency signal isspectrum analyzed at two differentresolutions: a medium resolution (Df=100 Hz,Df/f»10-7, 10000 averages), and a highresolution channel (Df=0.02 Hz, Df/f»10-11,noaverages). The latter was implemented to lookfor possible fine structure [8,9] in the galacticaxion line. The integration time per tuning rodsetting was set to about 50 seconds in order too b t a i n t h e s c a n r a t e i n ( 2 ) . E a c h f r e q u e n c y range is scanned three times to minimize thec o n t r i b u t i o n s o f s p u r i o u s n o i s e . T h e F F T spectra are periodically logged to disk for offline analysis and peak search. The experimenti s f u l l y c o m p u t e r c o n t r o l l e d b y a M a c i n t o s h c o m p u t e r r u n n i n g L a b v i e w . S i n c e 2 / 9 6 , w e have been running with a duty cycle of > 90 %.5. CALIBRATION OF SENSITIVITYThe sensitivity of the axion detector ismeasured with the variable temperaturemethod. The cavity, which is criticallycoupled, acts as a 50 W termination and emits anoise power Pc = k B T B , w h e r e B i s t h e bandwidth and kB is Boltzmann�s constant.The noise power at the output of the amplifierwith gain G is P=kB B G ( T c + T a). The amplifiertemperature Ta can be determined bymeasuring P while varying the cavitytemperature Tc, since B, G, and Ta are constant.Figure 3 shows the data from a calibration runat f=700MHz. The system noise temperature istherefore Ts=Ta+Tc=4.3 K+1.4 K =5.7 K.

012345

Noise Power (arbitrary units)-6-4-2024Cavity Temperature (K)6Ta=4.3K810

Fig.3 Calibration of amplifier noise temperature bythe cavity heating method.6. REACH OF EXPERIMENTWe intend to cover a decade of axionmasses (1.3-13 meV) in about three years. Oursensitivity is sufficient to probe the halo for

axions with theoretically predicted couplings.The proposed mass region is shown inFigure˚4. Also shown is the already excludedparameter space from previous pilotexperiments [10,11]. To date (5/96), we havescanned the region 660-720 MHz (2.7-3.0 meV),indicated in the plot. Data analysis is still inprogress.For frequencies above 800 MHz (3.3 meV),an array of 4 or 16 identical cavities will beused. These cavities must be synchronouslystepped and their ouput power-combined inphase. The hardware is already underconstruction and the switchover to the 4-arraywill occur in early 1997.

10-3210-3110-3010-2910-28

gagg2 (GeV -2)10-2710-2610-25maRBFUFThis experimentKSVZDFSZ10-2410-6 eV10-5 eV(0.24 GHz)(2.4 GHz)

5/96sensitivity

Fig.4 Exclusion plot for galactic axions, assuming ahalo density ra= 300 MeV/cm3. The heavy darkline indicates where we have already scanneddown to KSVZ sensitivity, but data analysis is stillin progress.ACKNOWLEDGEMENTSThis work was performed under theauspices of the U.S. Department of Energyunder contracts no. W-7405-ENG-48 (LLNL),DE-AC03-76SF00098 (LBL), DE-AC02-76CH03000 (FNAL), DE-FC02-94ER40818(MIT), DE-FG05-86ER40272 (UF), and FG02-90ER-40560 (U Chicago).REFERENCES1. R. Peccei and H. Quinn, Phys. Rev. Lett. 38(1977) 1440.2. S. Weinberg, Phys. Rev. Lett. 40 (1978) 223; F.Wilczek, Phys. Rev. Lett. 40 (1978) 279.3. For a review see M. Turner, Phys. Rep. 197(1990) 67.4. P. Sikivie, Phys. Rev. Lett. 51 (1983) 1415.5. L. Krauss et al., Phys. Rev. Lett. 55 (1985)1797.6. J. Kim, Phys. Rev. Lett. 43 (1979) 103; M.Shifman et al., Nucl. Phys. B166 (1980) 493.7. M. Dine et al., Phys. Lett. 104B (1981) 199; A.Zhitnitskii, Sov. J. Nucl. Phys. 31 (1980) 260.8. P. Sikivie and J. Ipser, Phys. Lett. B291 (1992)288.9. P. Sikivie et al., Phys. Rev. Lett. 75 (1995)2911.10. W. Wuensch et al., Phys. Rev. D40 (1989)3153.11. C. Hagmann et al., Phys. Rev. D42 (1990)1297.