arXiv:astro-ph/9912167v1 8 Dec 1999

Accepted for publication in the Astronomical Journal, February 2000

The Hubble Deep Field South – STIS Imaging^1.

Jonathan P. Gardner^2, Stefi A. Baum^3, Thomas M. Brown^{2,7}, C. Marcella Carollo^{4,8,9}, Jennifer Christensen^3, Ilana Dashevsky^3, Mark E. Dickinson^3, Brian R. Espey^{3,10}, Henry C. Ferguson^3, Andrew S. Fruchter^3, Anne M. Gonnella^3, Rosa A. Gonzalez-Lopezlira^3, Richard N. Hook^5, Mary Elizabeth Kaiser^{2,4}, Crystal L. Martin^{3,8}, Kailash C. Sahu^3, Sandra Savaglio^{3,10}, T. Ed Smith^3, Harry I. Teplitz^{2,7}, Robert E. Williams^3, Jennifer Wilson^{3,11}

ABSTRACT

We present the imaging observations made with the Space Telescope Imaging Spectrograph of the Hubble Deep Field – South. The field was imaged in 4 bandpasses: a clear CCD bandpass for 156 ksec, a long-pass filter for 22–25 ksec per pixel typical exposure, a near-UV bandpass for 23 ksec, and a far-UV bandpass for 52 ksec. The clear visible image is the deepest observation ever made in the UV-optical wavelength region, reaching a 10σ AB magnitude of 29.4 for an object of area 0.2 square arcseconds. The field contains QSO J2233-606, the target of the STIS spectroscopy, and extends 50^{′′} × 50^{′′} for the visible images, and 25^{′′} × 25^{′′} for the ultraviolet images. We present the images, catalog of objects, and galaxy counts obtained in the field.

1Based on observations made with the NASA/ESA Hubble Space Telescope, obtained from the Space Telescope Science Institute, which is operated by the Association of Universities for Research in Astronomy, Inc., under NASA contract NAS 5-26555.

2Laboratory for Astronomy and Solar Physics, Code 681, Goddard Space Flight Center, Greenbelt MD 20771

3Space Telescope Science Institute, 3700 San Martin Drive, Baltimore MD 21218

4Dept. of Physics and Astronomy, Johns Hopkins University, Baltimore MD 21218

5Space Telescope-European Coordinating Facility, Karl Schwarzschild Strasse 2, D-85748, Garching bei München, Germany

6European Southern Observatory, Karl-Schwarzschild-Strasse 2, D-85748 Garching bei München, Germany

7NOAO Research Associate

8Hubble Fellow

9Currently at Columbia University, Department of Astronomy, Mail Code 5246 Pupin Hall, 550 West 120th Street, New York NY 10027

10On assignment from the Astrophysics Division, Space Science Department, European Space Agency

11Currently at The Observatories of the Carnegie Institution of Washington, 813 Santa Barbara, Pasadena, CA 91101

– 2 –

1. Introduction

The Space Telescope Imaging Spectrograph (STIS) (Kimble et al. 1997; Woodgate et al. 1998; Walborn & Baum 1998) was used during the Hubble Deep Field – South (HDF–S) (Williams et al. 1999) observations for ultraviolet spectroscopy (Ferguson et al. 1999) and ultraviolet and optical imaging. In this paper we present the imaging data.

The Hubble Deep Field – North (HDF–N) (Williams et al. 1996) is the best studied field on the sky, with >1 Msec of Hubble Space Telescope (HST) observing time (including follow-up observations by Thompson et al. 1999 and Dickinson et al. 1999), and countless observations with ground-based telescopes (e.g., Cohen et al. 1996; Connolly et al. 1997). Results obtained to date include a measurement of the ultraviolet luminosity density of the universe at z > 2 (Madau et al. 1996), the morphological distribution of faint galaxies (Abraham et al. 1996), galaxy-galaxy lensing (Hudson et al. 1998), and halo star counts (Elson, Santiago & Gilmore 1996). See Ferguson (1998) and Livio, Fall & Madau (1998) for reviews and further references. The HDF–S differs from the HDF–N in several ways. First, the installation of STIS and NICMOS on HST in 1997 February has enabled parallel observations with three cameras. In addition to the STIS data, the HDF–S dataset includes deep WFPC2 imaging (Casertano et al. 1999), deep near-infrared imaging (Fruchter et al. 1999), and wider-area flanking field observations (Lucas et al. 1999). Second, the STIS observations were centered on QSO J2233-606, at z ≈ 2.24, to obtain spectroscopy. Finally, the field was chosen in the southern HST continuous viewing zone in order to enable follow-up observations with ground-based telescopes in the southern hemisphere.

In section 2 we describe the observations. In section 3 we describe the techniques we used to reduce the CCD images. In section 4 we describe the reduction of the MAMA images. In section 5 we describe the procedures used to catalog the images. In section 6 we present some statistics of the data, including galaxy number counts and color distributions. Our purpose in this paper is to produce a useful reference for detailed analysis of the STIS images. Thus for the most part we refrain from model comparisons and speculation on the significance of the results. We expect the STIS images to be useful for addressing a wide variety of astronomical topics, including the sizes of the faintest galaxies, the ultraviolet-optical color evolution of galaxies, the number of faint stars and white dwarfs in the galactic halo, and the relation between absorption line systems seen in the QSO spectrum and galaxies near to the line of sight. We also expect the observations to be useful for studying sources very close to the quasar, and perhaps for detecting the host galaxy of the quasar. However, this may require a re-reduction of the images, as the quasar is saturated in all of the CCD exposures, and there are significant problems with scattered light and reflections.

– 3 –

2. Description of the observations

The images presented here were taken in 4 different modes, 50CCD (Figure 1), F28X50LP (Figure 2), NUVQTZ (Figure 3), and FUVQTZ (Figure 4). The 50CCD and F28X50LP modes used the Charge Coupled Device (CCD) detector. The 50CCD is a clear, filterless mode, while the F28X50LP mode uses a long-pass filter beginning at about 5500Å. The FUVQTZ and NUVQTZ used the Multi-Anode Microchannel Array (MAMA) detectors as imagers with the quartz filter. The quartz filter was selected to reduce the sky noise due to airglow to levels below the dark noise. The effective areas of the 4 modes are plotted in Figure 5, along with a pseudo-B_{430} bandpass constructed from the 50CCD and F28X50LP fluxes. The MAMA field of view is a square, 25^{′′} on a side, and was dithered so that the observations include data on a field approximately 30^{′′} square. The 50CCD mode is filterless imaging with a CCD. The field of view is a square 50^{′′} on a side, and the dithering extends to a square 60^{′′} on a side. The F28X50LP is a long-pass filter that vignettes the field of view of the CCD to a rectangle 28 × 50^{′′}. The observations were dithered to image the entire field of view of the 50CCD observations, although the exposure time per point on the sky is thus approximately half the total exposure time spent in this mode. The original pixel scale is 0.0244^{′′} pix^{−1} for the MAMA images, and 0.05071^{′′} pix^{−1} for the CCD images. The final combined images have a scale of 0.025^{′′} pix^{−1} in all cases. Table 1 describes the observations. The filterless 50CCD observations correspond roughly to V+I, and reach a depth of 29.4 AB magnitudes at 10σ in a 0.2 square arcsecond aperture (320 drizzled pixels). This is the deepest exposure ever made in the UV-optical wavelength region.

2.1. Selection of the Field

Selection of the field is described by Williams et al. (1999). The QSO is at RA = 22^h33^m37.5883^s, Dec = −60^∘33^′29.128^{′′} (J2000). The errors on this position are estimated to be less than 40 milli-arcseconds (Zacharias et al. 1998). The position of the QSO on the 50CCD and F28X50LP images is x=1206.61, y=1206.32, and on the MAMA images is x=806.61, y=806.32.

2.2. Test Data

Test observations of the field were made in 1997 October. These data are not used in the present analysis. While the test exposures do not add significantly to the exposure time, they would provide a one-year baseline for proper motion studies of the brighter objects.

– 4 –

2.3. Observing Plan

The STIS observations were scheduled so that the CCD was used in the orbits that were impacted by the South Atlantic Anomaly, and the MAMAs were used in the clear orbits. The observations were made in the continuous viewing zone, and therefore were all made close to the limb of the Earth. The G430M spectroscopy, all of which was read-noise limited, was done during the day or bright part of the orbit, while the CCD imaging was all done during the night or dark part of the orbit. The MAMA imaging, done with the quartz filter, is insensitive to scattered Earth light, and was therefore done during bright time. A more detailed discussion of the scheduling issues is given by Williams et al. (1999). The sky levels in the 50CCD images were approximately twice the square of the read noise, so these data are marginally sky noise limited. The MAMA images are limited by the dark noise.

2.4. Dithering and Rotation

The images were dithered in right ascension (RA) and declination (Dec) in order to sample the sky at the sub-pixel level. In addition, variations in rotation of about ±1 degree were used to provide additional dithering for the WFPC2 and NICMOS fields during the STIS spectroscopic observations. The STIS imaging observations were interspersed with the STIS spectroscopic observations; therefore, all of the images were dithered in rotation as well as RA and Dec.

2.5. CR-SPLIT and pointing strategy

The CCD exposures were split into 2 or 3 cr-splits that each have the same RA, Dec, and rotation. This facilitates cosmic ray removal, although as discussed below, this was only used in the first iteration of the data reduction. The final 50CCD image is the combination of 193 exposures making up 67 cr-split pointings. After standard pipeline processing, (including bias and dark subtraction, and flatfielding), each exposure is given a flt file extension, and the cosmic-ray rejected combinations of each cr-split is given a crj file extension. The final F28X50LP image is the combination of 66 exposures making up 23 cr-split pointings. The F28X50LP image included 12 pointings at the northern part of the field, one pointing at the middle of the field, and 10 pointings at the southern half of the field.

– 5 –

2.6. PSF observations

In order to allow for PSF subtraction of the QSO present in the center of the STIS 50CCD image, two SAO stars of about 10 mag were observed in the filterless 50CCD mode before and after the main HDF-S campaign. The stars are SAO 255267, a G2 star, and SAO 255271, an F8 star, respectively. These targets have spectral energy distributions in the STIS CCD sensitivity range similar to that of the QSO. For each star, 32 different cr-split exposures were taken. The following strategy was used: (i) four different exposure times between 0.1 s and 5 s for each cr-split frame, to ensure high signal-to-noise in the wings while not saturating the center; (ii) a four-position dither pattern with quarter-pixel sampling and cr-split at each pointing with each exposure time; (iii) use of gain=4, to insure no saturation in the A-to-D conversion. During the observations for SAO255267, a failure in the guide star acquisition procedure caused the loss of its long-exposure (5 s) images. Gain=4 has a well-documented large scale pattern noise that must be removed, e.g., by Fourier filtering, before a reliable PSF can be produced. These data are not discussed further in this paper, but are available from the HST archive for further analysis.

3. Reduction of the CCD Images

3.1. Bias, Darks, Flats and Masks

Standard processing of CCD images involves bias and dark subtraction, flatfielding, and masking of detector defects. The bias calibration file used for the HDF-S was constructed from 285 individual exposures, combined together with cosmic-ray and hot-pixel trail rejection.

The dark file was constructed from a “superdark” frame and a “delta” dark frame. The superdark is the cosmic-ray rejected combination of over 100 individual 1200 s dark exposures taken over the several months preceding the HDF-S campaign. The delta dark adds into this high S/N dark frame the pixels that are more than 5σ from the mean in the superdark-subtracted combination of 14 dark exposures taken during the HDF-S campaign. Calibration of the images with this dark frame removes most of the hot pixels but still leaves several hundred in each image.

An image mask was constructed to remove the remaining hot pixels and detector features. The individual cosmic-ray rejected HDF-S 50CCD exposures were averaged

– 6 –

together without registration. The remaining hot pixels were identified with the IRAF^{12} cosmicrays task. These pixels were included in a mask that was used to reject pixels during the drizzle phase. Pixels that were more than 5σ below the mean sky background were also masked, as were the 30 worst hot pixel trails, and the unilluminated portions of the detector around the edges. Hot pixel trails run along columns and are caused by high dark current in a single pixel along the column.

Flatfielding was carried out by the IRAF/STSDAS calstis pipeline using two reference files. The first, the pflat corrects for small-scale pixel-to-pixel sensitivity variations, but is smooth on large scales. This file was created from ground-test data but comparisons to a preliminary version of the on-orbit flat revealed only a few places where the difference was more than 1%. The CCD also shows a 5-10% decrease in sensitivity near the edges due to vignetting. This illumination pattern was corrected by a low-order fit to a sky flat constructed from the flanking field observations.

3.2. Shifts and rotations

After pipeline processing, the CCD images were reduced using the IRAF/STSDAS package dither, and test versions called xdither, and xditherii. These packages include the drizzle software (Fruchter & Hook 1998; Fruchter et al. 1998; Fruchter 1998). We used drizzle version 1.2, dated 1998 February. The test versions differ from the previously released version primarily in their ability to remove cosmic rays from each individual exposure, and include tasks that have not yet been released.

The xditherii package uses an iterative process to reject cosmic rays and determine the x and y sub-pixel shifts, which we summarize here. The standard pipeline rejects cosmic rays using each cr-split of 2 or 3 images. The resulting crj files are used as the first iteration, we determine the x and y shifts, and the files are median combined. The resulting preliminary combination is then shifted back into the frame of each of the original exposures (flt files), and a new cosmic ray mask is made. By comparing each exposure to a high signal-to-noise combination of all of the data, we are less likely to leave cosmic ray residuals. The x and y shifts are determined at each iteration as well.

The rotations used in combining the data were determined from the roll avg

12IRAF is distributed by the National Optical Astronomy Observatories, which are operated by the Association of Universities for Research in Astronomy, Inc., under cooperative agreement with the National Science Foundation.

– 7 –

parameter in the jitter files, using the program bearing. We did not seek to improve on these rotations via cross-correlation or any other method. We did use cross-correlation to determine the x and y shifts.

Determination of the sub-pixel x and y shifts was done with an iterative procedure. The first iteration was obtained by determining the centroid of the bright point source just west of the QSO, using the pipeline cosmic-ray rejected crj files. We could not use cross-correlation in this first iteration, because the very bright star on the southern edge of the field was present on images taken at some, but not all, dither positions, which corrupted the cross-correlation. The source we used for centroiding was clearly visible on all of the 50CCD and F28X50LP frames.

Using these shifts (which were accurate to better than 1 pixel), we created a preliminary combined image. After pipeline processing and cosmic ray rejection, the drizzle program was used to shift and rotate each sc crj file onto individual outputs, without combining them. We then used the task imcombine to create a median combination of the files. This preliminary image was then shifted and rotated back into the frame of each individual exposure using the xdither task, blot, ready for the next iteration of the cosmic-ray rejection procedure.

3.3. Cosmic ray rejection

In this iteration, we discarded the crj files, and went back to the flt files, in which each exposure had undergone bias and dark subtraction and flatfielding, but not cosmic-ray rejection. Each exposure was compared to the blotted image, and a cosmic-ray mask for that exposure was created from all of the pixels that differed (positively or negatively) by more than a given threshold from the blotted image. In the version 1.0 released 50CCD image, this threshold was set to be 5σ. However, we believe that a small error in the sky level determination, introduced by the amplifier ringing correction discussed below, meant that our rejection was approximately at the 3σ level. The cosmic ray masks were multiplied by the hot pixel masks discussed above, and resulted in about 8% of the pixels being masked as either cosmic rays or hot pixels. This is, perhaps, overly conservative. A less conservative cut (after correcting the error in the sky value) would result in slightly higher exposure time per pixel, and thus an improvement of 1-2% in the signal to noise ratio. The cosmic ray mask was combined with the hot pixel and cosmetic defect mask.

This problem with the sky value was corrected in the F28X50LP image, and a 3σ level was used in the cosmic ray rejection.

– 8 –

3.4. Amplifier ringing correction

Horizontal features due to amplifier ringing, varying in pattern from image to image, were present in most of the STIS CCD frames. When a pixel saw a highly saturated signal, the bias level was depressed in the readout for the next few rows. The very high signals causing this ringing came from hot pixels and from the saturated QSO. The signal-to-noise ratio in the overscan region of the detector was not sufficient to remove these features well. We removed them with a procedure that subtracted on a row-by-row basis, from each individual image, the weighted average of the background as derived from the innermost 800 columns after masking and rejecting “contaminated” pixels. The masks included all visible sources, hot pixels, and cosmic-ray hits. The source mask was determined from the initial registered median-combined image, shifted back to the reference frame of each of the individual images. For the unmasked pixels in each row, the 50 highest and lowest were rejected and the mean of the remaining pixels was subtracted from the each pixel in that row.

Heavily smoothing the images reveals very slight horizontal residuals that were not removed by the present choice of parameters in this process.

3.5. Drizzling it all together

The final image combination was done by drizzling the amplifier-ringing corrected pipeline products together onto a single output image. The exposures were weighted by the square of the exposure time, divided by the variance, which is (sky+rn^2+dark). The rotations were corrected so that North is in the +y direction, and the scale used was 0.492999 original CCD pixels per output pixel so that the final pixel scale is exactly 0.025 arcsec/pixel. For the 50CCD data we used a pixfrac=0.1, which is approximately equivalent to interleaving, where each input pixel falls on a single output pixel. For the F28X50LP data we used pixfrac=0.6, as a smaller pixfrac left visible holes in the final image. See Fruchter & Hook (1998) for a discussion of the meaning of the drizzle parameters. The point spread functions of bright, non-saturated point sources are shown in Figure 6. The sources selected are the point source just to the west of the quasar in the 50CCD and F28X50LP images, and the QSO in the MAMA images.

The final image is given in counts per second, which can be converted to magnitudes on the stmag system using the photometric zeropoints given by the photflam parameter supplied in the image headers. We used the pipeline photometric zeropoints for the 50CCD and MAMA images, but revised the F28X50LP zeropoint by 0.1 magnitude based on

– 9 –

a comparison of STIS photometry of the HST calibration field in ω Centauri with the ground-based photometry of Walker (1994). The zeropoints in the AB magnitude system which we used are 26.386, 25.291, 23.887, and 21.539, for the 50CCD, F28X50LP, NUVQTZ and FUVQTZ respectively. We also supply the weight image, which is the sum of the weights falling on each pixel. For the F28X50LP image, we supply an exposure-time image, which is the total exposure time contributing to each pixel. We have multiplied this image by the area of the output pixels. The world coordinate system in the headers was corrected so that North is exactly in the +y direction, and the pixel scale is exactly 0.025 arcsec/pixel.

3.6. Window reflection

A window in the STIS CCD reflects slightly out-of-focus light from bright sources to the +x, −y direction (SW on the HDF-S images). The QSO is saturated in every 50CCD and F28X50LP exposure. The window reflection of the QSO is clearly visible in the F28X50LP image, but has been partially removed from the 50CCD image by the cosmic-ray rejection procedure. We wish to emphasize that it has only been partially removed, and there are remaining residuals. These residuals should not be mistaken for galaxies near the QSO, nor should they be mistaken for the host galaxy of the QSO. There is additional reflected light from the QSO (and from the bright star at the southern edge) evident in the images. We believe that the version 1.0 released images are not appropriate for searching for objects very close to or underlying the QSO, and that such a search would require re-processing the raw data with particular attention paid to the window reflection, other reflected light, and to the PSF of the QSO. The diffraction spikes of the QSO are smeared in the final images by the rotation of the individual exposures.

4. Reduction of the MAMA Images

The near-UV and far-UV images are respectively the weighted averages of 12 and 25 registered frames, with total exposure times of 22616 s and 52124 s. The MAMAs do not suffer from read noise or cosmic rays, and the quasar is not saturated in any of the UV data. However, the MAMAs do have calibration issues that must be addressed.

– 10 –

4.1. Flats, Dark Counts, and Geometric Correction

Prior to combination, all frames were processed with CALSTIS, including updated high-resolution pixel-to-pixel flat field files for both UV detectors. Geometric correction and rescaling were applied in the final combinations via the drizzle program. The quartz filter changes the far-UV plate scale relative to that in the far-UV clear mode, and so the relative scale between MAMA imaging modes was determined from calibration images of the globular cluster NGC 6681.

Dark subtraction for the near-UV image was done by subtracting a scaled and flat-fielded dark image from each near-UV frame. The scale for the dark image was determined by inspection of the right-hand corners of the near-UV image, because these portions of the detector are occulted by the aperture mask and thus only register dark counts. For the far-UV images, calstis removes a nearly flat dark frame, but the upper left-hand quadrant of STIS far-UV frames contains a residual glow in the dark current after nominal calibration. This glow varies from frame to frame and also appears to change shape slightly with time. To remove the residual dark current, the 16 far-UV frames with the highest count rates in the glow region were co-added without object registration but with individual object masks for the only two obvious objects in the far-UV frames (the quasar and bright spiral NNE of the quasar). We then fit the result with a cubic spline to produce a glow profile. This profile was then scaled to the residual glow in each processed frame and subtracted prior to the final drizzle. Even during observations with a strong dark glow, where the dark count rate is an order of magnitude higher than normal, it is still very low, reaching rates no higher than 6 × 10^{−5}cts sec^{−1} pix^{−1}. The glow thus appears as a higher concentration of ones in a sea of zeros, and the subtraction of a smooth glow profile from such quantized data over-subtracts from the zeros and under-subtracts from the ones. These effects are visible in the corrected data, even when smoothed out considerably in the final drizzled far-UV image. A low-resolution flat-field correction was applied to the far-UV frames after subtraction of the residual dark glow. The near-UV frames require no low-resolution flat field correction.

4.2. Shifts and Rotations

Currently, geometrically corrected NUVQTZ and FUVQTZ frames do not have the same plate scale. Although geometric correction, rotation, and rescaling is applied during the final summation of individual calibrated frames, we first produced a set of calibrated frames that included these corrections, in order to accurately determine the relative shifts between them; this information was then used in conjunction with these corrections in

– 11 –

the final drizzle. All near-UV and far-UV frames were geometrically corrected, rescaled to 0.025^{′′} pix^{−1}, and rotated to align North with the +y image axis. The roll angle specified in the jitter files was used to determine the relative roll between frames, and the mean difference between the planned roll and the jitter roll determined the absolute rotation. It is difficult to determine accurate roll angles from the images themselves, because of the scarcity of objects in the MAMA images. All near-UV and far-UV frames were then cross-correlated against one of the far-UV frames to provide shifts in the output coordinate system. Note that centroiding on the quasar in all far-UV and near-UV frames yields the same shifts as cross-correlation, within 0.1 pixel.

4.3. Drizzling

The calibrated frames were drizzled to a 1600 × 1600 pixel image, including the above corrections, rescaling, rotations, and shifts. We updated the world coordinate system in the image headers to exactly reflect the plate scale, alignment, and the astrometry of the quasar.

For both the far-UV and near-UV frames, individual pixels in each frame were weighted by the ratio of the exposure time squared to the dark count variance; this weights the exposures by (S/N)^2 for sources that are fainter than the background. Although the variations in the far-UV dark profile are smooth, the near-UV dark profile is an actual sum of dark frames, and so we smoothed the near-UV dark profile to determine the weights. With this weighting algorithm, pixels in the upper left-hand quadrant of a given far-UV image contribute less when the dark glow is high, and contribute more when it is low. The statistical errors (cts s^{−1}) in the final drizzled image, for objects below the background (e.g., objects other than the quasar), are given by the square root of the final drizzled weights file.

The drizzle “dropsize” (pixfrac) was 0.6, thus improving the resolution over a pixfrac of 1.0 (which would be equivalent to simple shift-and-add). The 1600 × 1600 pixel format contains all dither positions, and pixels outside of the dither pattern are at a count rate of zero. The pixel mask for each near-UV input frame included the occulted corners of the detector, a small number of hot pixels, and pixels with relatively low response (those with values ≤ 0.75 in the high-resolution flat field). The pixel mask for each far-UV frame included hot pixels and all pixels flagged in the data quality file for that frame. When every input pixel drizzled onto a given output pixel was masked, that pixel was set to zero.

– 12 –

4.4. Window Reflection

As with the CCD, a window reflection of the QSO appears in the near-UV image. This reflection appears ≈ 0.2^{′′} east of the QSO itself, and should not be considered an astronomical object.

5. Cataloging

5.1. Cataloging the Optical Images

The catalog was created using the SExtractor package (Bertin & Arnouts 1996), revision of 1998 November 19, with some minor modifications that were done for this application. We used two separate runs of SExtractor, and manually merged the resulting output catalogs. The first run used a set of parameters selected to optimize the detection of faint sources while not splitting what appeared to the eye to be substructure in a single object. We varied the parameters detect thresh, deblend mincont, back size, and back filtersize. We decided to use a detection threshold corresponding to an isophote of 0.65σ. Sources were required a minimum area of 16 connected pixels above this threshold. Deblending was done when the flux in the fainter object was a minimum of 0.03 times the flux in the brighter object. The background map was constructed on a grid of 60 pixels, and subsequently filtered with a 3 × 3 median filter. Prior to cataloging, the image was convolved with a Gaussian kernel with full width half maximum of 3.4 pixels. As discussed in Fruchter & Hook (1998), the effects of drizzling on the photometry is no more than 2%, and in our well-sampled 50CCD field, the effects should be much less than this. This effect is smaller than other uncertainties in the photometry of extended objects.

The second run of SExtractor was optimized to detect objects that lay near the QSO and the bright star at the southern edge of the image. These objects tend to be blended in with the point source at the lower detection threshold. Although our catalog might include galaxies that are associated with absorption lines in the quasar spectrum, we did not attempt to subtract the quasar light from the image, and so the catalog does not include objects within 3^{′′} of the quasar. The parameters used for the second run were the same as for the first run, with the exception of the detect thresh parameter, which was set to 3.25σ. This parameter not only sets the minimum flux level for detection, but also is the isophote used to determine the extent of the object. Several objects fall between the 0.65σ isophote and the 3.25σ isophote of the quasar. These are not deblended on the first SExtractor run, because their fluxes are below 0.03 of the quasar flux, but are detected (without the need for deblending) on the second run. Objects near the quasar

– 13 –

detected in the second run were added to the catalog generated by the first run, and flagged accordingly. Objects from the second run that were not confused with the quasar or the bright star were not included. The isophotal photometry of objects from the second run will not be consistent with the photometry of objects from the first run, because a different isophote was used. Eight objects were added to the catalog in this way.

In addition, 26 objects from the first SExtractor run were clearly spurious due to the diffraction spikes of the QSO and the bright star. These were manually deleted from the catalog.

Photometry of the F28X50LP image was done with SExtractor run in two-image mode, in which the objects were detected and identified on the 50CCD image, but the photometry was done in the other band. Isophotes and elliptical apertures are thus determined by the extent of the objects on the 50CCD images. Objects detected in the F28X50LP image but not on the 50CCD image are impossible, since it has a lower throughput and shorter exposure time.

5.2. Cataloging the Ultraviolet Images

Fluxes in the UV were calculated outside of SExtractor because it had some problems handling quantized low-signal data. To determine the gross flux, we summed the countrate within the area for each object appearing in the SExtractor 50CCD segmentation map. We then created an object mask by “growing” each object in the segmentation map, using the IDL routine dilate, until it subtended an area three times its original size. The resulting mask excludes faint emission outside of the SExtractor isophotes for all known objects in the field. The sky was calculated from those exposed pixels within a 151 × 151 pixel box centered on each object, excluding pixels from the mask. The mean countrate per pixel in this sky region was used to determine the background for each object (the median is not a useful quantity when dealing with very low quantized signals), and thus the net flux. Statistical errors per pixel for objects at or below the background are determined from the drizzle weight image raised to the −1/2 power. The statistical errors for the gross flux and sky flux were calculated using this pixel map of statistical errors, and thus underestimate the errors for bright objects such as the quasar.

Some objects that are fully-exposed in the CCD image do not fall entirely within the exposed area of the MAMA images; for these objects, we calculated the UV flux in the exposed area only, without correcting for the incomplete exposure, and flagged such objects accordingly. Objects were also flagged if the sky-box described above did not contain at

– 14 –

least 100 pixels (e.g., the quasar). For these objects, we calculated a global sky value from a larger 685 × 670 pixel box, roughly centered in each MAMA image, that only includes areas fully exposed in the dither pattern, and excludes pixels in the object mask. When the net flux incorporates this global sky value, they have been flagged accordingly. We do not expect or see any evidence for objects in the ultraviolet images that do not appear on the 50CCD image.

5.3. The Catalog

The catalog is presented in Table 2, which contains a subset of the photometry. The full catalogs are available on the World Wide Web. For each object we report the following parameters:

ID: The SExtractor identification number. The objects in the list have been sorted by right ascension (first) and declination (second), and thus are no longer in catalog order. In addition, the numbers are no longer continuous, as some of the object identifications from the first SExtractor run have been removed. Objects from the second SExtractor run have had 10000 added to their identification numbers. These identification numbers provide a cross-reference to the segmentation maps.

HDFS J22r−60d: The minutes and seconds of right ascension and declination, from which can be constructed the catalog name of each object. To these must be added 22 hours (RA) and −60 degrees (Dec). The first object in the catalog is HDFS J223333.69−603346.0, at RA 22^h 33^m 33.69^s, Dec 60deg 33^′ 46.0^{′′}, epoch J2000.

x, y: The x and y pixel positions of the object on the 50CCD and F28X50LP images. To get the x and y pixel positions on the MAMA images, subtract 400 from each.

m_i, m_a: The isophotal (m_i) and “mag auto” (m_a) 50CCD magnitudes. The magnitudes are given in the AB system (Oke 1971), where m = −2.5logf_ν − 48.60. The isophotal magnitude is determined from the sum of the counts within the detection isophote, set to be 0.65σ. The “mag auto” is an elliptical Kron (1980) magnitude, determined from the sum of the counts in an elliptical aperture. The semi-major axis of this aperture is defined by 2.5 times the first moments of the flux distribution within an ellipse roughly twice the isophotal radius. However if the aperture defined this way would have a semi-major axis smaller than than 3.5 pixels, a 3.5 pixel value is used.

clr-lp: Isophotal color, 50CCD−F28X50LP, in the AB magnitude system, as determined in the 50CCD isophote. SExtractor was run in two-image mode to determine

– 15 –

the photometry in the F28X50LP image, using the 50CCD image as the detection image. When the measured F28X50LP flux is less than 2σ, we determine an upper limit to the color using the flux plus 2σ when the measured flux is positive, and 2σ when the measured flux is negative. We did not clip the 50CCD photometry.

nuv-clr, fuv-clr: Isophotal colors, NUVQTZ-50CCD and FUVQTZ-50CCD, in the AB magnitude system. Photometry in the MAMA images are discussed above. Photometry of objects falling partially outside the MAMA image are flagged and should not be considered reliable. When the measured flux is less than 2σ, we give lower limits to the color as discussed above.

r_h: The half-light radius of the object in the 50CCD image, given in milli-arcseconds. The half-light radius was determined by SExtractor to be the radius at which a circular aperture contains half of the flux in the “mag auto” elliptical aperture.

s/g: A star-galaxy classification parameter determined by a neural network within SExtractor, and based upon the morphology of the object in the 50CCD images (see Bertin & Arnouts 1996 for a detailed description of the neural network). Classifications near 1.0 are more like a point source, while classifications near 0.0 are more extended.

flags: Flags are explained in the table notes, and include both the flags returned by SExtractor, and additional flags we added while constructing the catalog.

6. Statistics

In this section we present several statistics of the data compiled from the catalog.

6.1. Source Counts

The source counts in the 50CCD image are given in Table 3, and plotted as a function of AB magnitude in Figure 7, where they are compared with the galaxy counts from the HDF-N WFPC2 observations, as compiled by Williams et al. (1996). The counts are compiled directly from the catalog, although all flagged regions have been excluded, so that the counts do not include objects near the edge of the image, or near the quasar. We plot only the Poissonian errors, although there might be an additional component due to large-scale structure. We plot all sources, including both galaxies and stars, although we do not expect stars to contribute substantially to the source counts. No corrections for detection completeness have been made, and the counts continue to rise until fainter than

– 16 –

30 mag. The turnover fainter than this is due to incompleteness; the counts do not turn over for astrophysical or cosmological reasons.

6.2. Colors and Dropouts

The 50CCD-F28X50LP colors of objects in the STIS images are plotted as points in Figure 8. Flagged objects have been removed from the sample. For comparison, we plot K–corrected (no-evolution) colors of the template galaxies in the Kinney et al. (1996) sample as a function of redshift on the left of the figure. The LP filter is able to distinguish blue galaxies at z < 2.5, but becomes dominated by the noise for blue galaxies fainter than 28 mag, and loses color resolution at z > 3, where the Lyα forest dominates the color in these bandpasses.

Because the F28X50LP bandpass is entirely contained within the 50CCD bandpass, it is possible, by subtracting an appropriately scaled version of the measured F28X50LP flux from the 50CCD flux, to construct a pseudo-B_{430} measurement (see Figure 5). This pseudo-B_{430} is combined with the NUVQTZ and the F28X50LP measurements in a color-color diagram in Figure 9. NUV drop-outs, indicated on this figure by the dashed line, are those objects with blue colors in the visible, but red colors in the UV, indicative of galaxies at z >∼ 1.5. These galaxies show blue colors characteristic of rapid star formation, while the red NUV to optical color is due to the Lyman break and absorption by the Lyα forest. The selection criteria were determined using the models of Madau et al. (1996). In an inset to Figure 9, we plot the efficiency of these criteria for selecting galaxies of high redshift. The solid line is the fraction of all of the models that meet these criteria, while the dotted line is the fraction of those models with ages < 10^8 years and foreground-screen extinction less than A_B = 2. These criteria are very efficient at finding young, star-forming galaxies at 1.5 < z < 3.5. We have removed point sources from this figure, including the bright object just west of the QSO, which is extremely red and is likely to be an M star.

In Figure 10 we give a FUV-NUV vs NUV-50CCD color-color plot showing FUV dropouts, where the Lyman break is passing through the FUV bandpass at z > 0.6. Of the 17 galaxies in the MAMA field with NUV magnitudes brighter than 28.4, only 3 have a clear signature of a Lyman break at 0.6 < z < 1.5. However, the upper limits are sufficiently weak that roughly half the sample could be at z > 0.6.

– 17 –

7. Conclusions

We have presented the STIS imaging observations that were done as part of the Hubble Deep Field – South campaign. The 50CCD image is the deepest image ever made in the UV-optical wavelength region, and achieves a point source resolution near the diffraction limit of the HST. We have presented the catalog, and some statistics of the data. These data will be useful for the study of the number and sizes of faint galaxies, the UV-optical color evolution of galaxies, the number of faint stars and white dwarfs in the galactic halo, and the relation between absorption line systems seen in the QSO spectrum and galaxies near to the line of sight. Follow-up observations of the HDF-South fields by southern hemisphere ground-based telescopes, by HST, and by other space missions will also greatly increase our understanding of the processes of galaxy formation and evolution.

The images and catalog presented here are available on the World Wide Web at: <http://www.stsci.edu/ftp/science/hdfsouth/hdfs.html>.

We would like to thank all of the people who contributed to making the HDF-South campaign a success, including those who helped to identify a target quasar in the southern CVZ, and those who helped in planning and scheduling the observations. JPG, TMB, and HIT wish to acknowledge funding by the Space Telescope Imaging Spectrograph Investigation Definition Team through the National Optical Astronomical Observatories, and by the Goddard Space Flight Center. CLM and CMC wish to acknowledge support by NASA through Hubble Fellowship grants awarded by STScI.

REFERENCES

Abraham, R. G., Tanvir, N. R., Santiago, B. X., Ellis, R. S., Glazebrook, K., & van den Bergh, S. 1996, MNRAS, 279, L47 Bertin, E., & Arnouts, S. 1996, A&AS, 117, 393 Casertano, S., et al. 1999, in preparation Cohen, J. G., Cowie, L. L., Hogg, D. W., Songaila, A., Blandford, R., Hu, E. M., Shopbell, P. 1996, ApJ, 471, L5 Connolly, A. J., Szalay, A. S., Dickinson, M., SubbaRao, M. U., & Brunner, R. J. 1997, ApJ, 486, L11 Dickinson et al. 1999, ApJ, in press, astro-ph/9908083

– 18 –

Elson, R. A. W., Santiago, B. X., & Gilmore, G. F. 1996, New Astronomy, 1, 1 Ferguson, H. C., 1998, Reviews in Modern Astronomy, 11, 83 Ferguson, H. C., et al. 1999, in preparation Fruchter, A. S., & Hook, R. N. 1998, astro-ph/9808087 Fruchter, A. S. et al. 1998, in 1997 HST Calibration Workshop, ed. S. Casertano et al.

(STScI) Fruchter, A. S. 1998, http://www.stsci.edu/∼fruchter/dither/dither.html Fruchter, A. S. et al. 1999, in preparation Hudson, M. J., Gwyn, S. D. J., Dahle, H., & Kaiser, N. 1998, ApJ, 503, 531 Kimble, R. A., et al. 1997, ApJ, 492, L83 Kinney, A. L., Calzetti, D., Bohlin, R. C., McQuade, K., Storchi-Bergmann, T., & Schmitt, H. R. 1996, ApJ, 467, 38 Kron, R. G. 1980, ApJS, 43, 305 Livio, M., Fall, S. M., & Madau, P. (eds.) 1998, The Hubble Deep Field : proceedings of the Space Telescope Science Institute Symposium 11, (New York : Cambridge University Press) Lucas, R. A., et al. 1999, in preparation Madau, P., Ferguson, H. C., Dickinson, M. E., Giavalisco, M., Steidel, C. C. & Fruchter, A.

1996, MNRAS, 283, 1388 Oke, J. B. 1971, ApJ, 170, 193 Thompson, R. I., Storrie-Lombardi, L. J., Weymann, R. J., Rieke, M. J., Schneider, G., Stobie, E., & Lytle, D. 1999, 117, 17 Walborn, N., & Baum, S. 1998, STIS Instrument Handbook, version 2.0, (Baltimore:

STScI), http://www.stsci.edu/instruments/stis. Walker, A. R. 1994, PASP, 104, 828 Williams, R. E., et al. 1996, AJ, 112, 1335 Williams, R. E., et al. 1999, in preparation Woodgate, B. E., et al. 1998, PASP, 110, 1183 Zacharias, N., et al. 1998, BAAS, 193, 75.09

This preprint was prepared with the AAS L^ATEX macros v4.0.

– 19 –

NOTE: The resolution of this image has been reduced. Full resolution images are available at: http://hires.gsfc.nasa.gov/∼gardner/hdfs/stispaper.

Fig. 1.— The 50CCD image. The image is displayed on a log scale, and has been clipped between 1 × 10^{−5} and 5 × 10^{−2} counts per second. The field of view of the image is 0.8357 square arcminutes.

– 20 –

NOTE: The resolution of this image has been reduced. Full resolution images are available at: http://hires.gsfc.nasa.gov/∼gardner/hdfs/stispaper.

Fig. 2.— The F28X50LP image. The image is displayed on a log scale, and has been clipped between 1 × 10^{−5} and 5 × 10^{−2} counts per second. The field of view of the image is 0.8326 square arcminutes.

– 21 –

NOTE: The resolution of this image has been reduced. Full resolution images are available at: http://hires.gsfc.nasa.gov/∼gardner/hdfs/stispaper.

Fig. 3.— The NUVQTZ image. The image is displayed on a log scale, and has been clipped between 1 × 10^{−6} and 5 × 10^{−3} counts per second, and has been smoothed with a 5 × 5 pixel box average. The field of view of the image is 0.2221 square arcminutes.

– 22 –

NOTE: The resolution of this image has been reduced. Full resolution images are available at: http://hires.gsfc.nasa.gov/∼gardner/hdfs/stispaper.

Fig. 4.— The FUVQTZ image. The image is displayed on a log scale, and has been clipped between 1 × 10^{−8} and 5 × 10^{−5} counts per second, and has been smoothed with a 5 × 5 pixel box average. The field of view of the image is 0.2438 square arcminutes.

– 23 –

Fig. 5.— Effective areas of the 4 imaging modes. The 50CCD mode is filterless imaging with a CCD, and this curve represents the response of the detector. The other three modes are a combination of the throughput of the filter with the response functions of the CCD and the two MAMA detectors. Also plotted is a pseudo-B_{430} bandpass, constructed from the fluxes by 50CCD - 1.31(F28X50LP).

– 24 –

Fig. 6.— Point spread functions of the final images. The points plotted are each pixel value as a function of distance from the centroid of the point source. The lines are a Gaussian with the same full width half maximum as the PSF. The objects plotted are the red point source just to the west of the quasar in the optical images, and the quasar itself in the ultraviolet images.

– 25 –

Fig. 7.— The source counts in the 50CCD image scaled to objects per square degree per magnitude as a function of AB magnitude. We plot both the mag auto and mag iso counts, binned at different magnitudes to show the points. We plot Poissonian errors on the points. For comparison, we plot the WFPC2 HDF-N galaxy counts, in B_{450}, V_{606}, and I_{814}, based upon the total magnitude as given by Williams et al. (1996). The error bars reflect √ N counting statistics and do not include systematic errors in the photometry or galaxy clustering.

– 26 –

Fig. 8.— 50CCD-F28X50LP AB magnitudes plotted as a function of 50CCD magnitude. The magnitudes and colors are isophotal. On the left we plot the K–corrected colors of the template galaxies in the Kinney et al. (1996) sample as a function of redshift. The “normal” galaxies from that sample are plotted as solid lines, and the starburst galaxies are plotted as dotted lines. The templates do not include data shortward of Lyα, so the plots converge when this limit is redshifted into the F28X50LP filter. In real high-z galaxies, a similar effect would be caused by the Lyα forest.

– 27 –

Fig. 9.— A color-color plot of the STIS NUV - B_{430} vs. B_{430} - F28X50LP, where B_{430} is a pseudo bandpass obtained by subtracting a scaled F28X50LP flux from the 50CCD flux. The dashed line shows the selection boundary for objects with 1.5 < z < 3.5. The size of the symbols indicates their magnitudes, and the symbol size of an object with F28X50LP = 26 is indicated in the inset at the upper right. Circular symbols are detected at the 1 sigma level in all bands, while triangles are undetected in the NUV, providing lower limits to the color. In the inset figure at right, we plot the selection efficiency of the NUV drop-out technique. This shows the fraction of models from the Madau et al. (1996) grid meeting the color selection criteria. The selection criteria are NUV−B_{430} > 1.75(B_{430} − F 28X50LP ) + 1.3, AND B_{430} − F 28X50LP < 1.5. The solid line is the full set of models (including old and highly reddened galaxies). The dotted line is just those model galaxies with ages < 10^8 years and foreground-screen extinction less than A_B = 2.

– 28 –

Fig. 10.— A color-color plot of the STIS FUV - NUV vs. NUV - 50CCD. The dashed line shows the selection boundary for objects with 0.6 < z < 1.5. The symbols are as in Figure 9; in addition, the square symbols represent objects which are not detected at the 1σ level in either the NUV or the FUV.

– 29 –

Table 1. Description of the Observations

Mode Central Width Detector Total Depth Resolution Wavelength FOV Exposure

FUVQTZ 1590 Å 220 Å 25^{′′} × 25^{′′} 52124 sec 27.8 0.057^{′′} NUVQTZ 2320 Å 1010 Å 25^{′′} × 25^{′′} 22616 sec 27.5 0.055^{′′} 50CCD 5850 Å 4410 Å 52^{′′} × 52^{′′} 155590 sec 29.4 0.083^{′′} F28X50LP 7230 Å 2720 Å 28^{′′} × 52^{′′} 49768 sec 27.5 0.085^{′′}

Note. — The detector fields of view have been clipped slightly to remove vignetting. The total exposure time for the F28X50LP mode is split into two fields of view with 23202 seconds exposure in the southern half, 25806 sec exposure in the northern half, and 760 seconds exposure in the central part of the field. The observations overlap, so that the region containing the QSO has full exposure. Depths are AB magnitudes at 10σ in a 0.2 square arcsecond aperture for the deepest part of the image. The resolution given is the full-width-half-maximum of point sources, as shown in Figure 6

– 30 –

Table 2. The catalog

ID HDFS J22r−60d x y m_i m_a clr-lp nuv-clr fuv-clr r_h s/g flags

552 3333.69 3346.0 2354.86 530.80 28.73 27.71 -0.11 · · · · · · 175 0.21 adehkn 576 3333.81 3347.3 2320.27 479.99 29.03 28.90 <0.46 · · · · · · 69 0.12 ekn 491 3333.91 3341.2 2292.26 723.83 30.91 29.89 <1.43 · · · · · · 95 0.97 ekn 531 3333.91 3343.9 2292.27 615.84 30.68 30.01 <1.04 · · · · · · 85 0.98 hkn 572 3333.93 3346.9 2284.00 493.81 30.76 30.22 <0.70 · · · · · · 73 0.96 kn 419 3333.97 3336.4 2275.12 916.66 27.07 27.11 0.16 · · · · · · 121 0.03 ekn 650 3333.99 3353.6 2268.43 226.34 30.76 30.23 0.52 · · · · · · 55 0.89 ehkn 293 3334.08 3327.6 2241.08 1265.37 30.13 30.02 <0.70 · · · · · · 57 0.59 kn 278 3334.12 3323.7 2230.81 1424.99 28.85 28.88 -0.05 · · · · · · 51 0.85 ehkn 345 3334.13 3331.2 2227.79 1122.83 30.01 29.55 <0.77 · · · · · · 79 0.66 kn 454 3334.13 3338.9 2227.56 816.29 30.23 29.43 <0.96 · · · · · · 148 0.78 kn 557 3334.13 3346.0 2226.26 531.39 31.65 30.63 <1.17 · · · · · · 74 0.81 kn 600 3334.17 3350.1 2213.57 367.28 31.42 30.17 <0.85 · · · · · · 117 0.76 kn 287 3334.18 3327.3 2212.17 1279.84 29.41 29.09 0.06 · · · · · · 91 0.06 kn 153 3334.20 3316.4 2206.50 1713.55 28.76 28.73 1.25 · · · · · · 83 0.02 ekn 476 3334.20 3340.5 2206.71 752.90 31.28 30.80 <1.18 · · · · · · 60 0.90 kn 67 3334.23 3309.4 2197.32 1995.20 30.86 31.43 <1.26 · · · · · · 26 0.94 ekn 504 3334.24 3342.2 2194.78 683.83 28.01 27.83 0.82 · · · · · · 117 0.02 kn 368 3334.25 3333.1 2190.29 1045.95 30.25 29.44 <1.15 · · · · · · 136 0.07 kn 627 3334.29 3352.3 2179.91 280.70 31.27 30.31 <0.74 · · · · · · 65 0.88 kn 652 3334.30 3348.3 2175.89 439.09 31.57 31.11 <0.90 · · · · · · 46 0.77 kn 366 3334.34 3332.6 2163.37 1065.86 31.41 30.48 <1.38 · · · · · · 88 0.86 kn 110 3334.35 3312.7 2160.87 1861.57 30.50 30.13 1.22 · · · · · · 58 0.96 hkn 35 3334.36 3306.2 2159.44 2122.56 29.90 29.60 0.51 · · · · · · 87 0.52 kn 448 3334.37 3338.2 2156.12 841.93 29.57 28.99 0.19 · · · · · · 128 0.01 kn 688 3334.39 3300.2 2150.41 2361.54 26.18 25.66 0.27 · · · · · · 143 0.25 adehkn 565 3334.41 3346.5 2143.93 510.94 28.84 28.78 0.19 · · · · · · 61 0.78 kn 172 3334.42 3317.3 2141.37 1680.09 29.47 29.19 0.43 · · · · · · 98 0.04 kn 439 3334.43 3337.4 2137.45 875.82 30.42 30.31 <0.28 · · · · · · 52 0.81 kn 644 3334.44 3355.0 2133.56 172.93 24.47 23.60 -1.56 · · · · · · 375 0.03 abehkn 200 3334.45 3318.9 2133.51 1616.24 28.43 28.31 -0.25 · · · · · · 107 0.02 kn 625 3334.45 3352.1 2131.66 287.95 30.86 29.93 <0.99 · · · · · · 96 0.96 kn 409 3334.46 3335.5 2128.74 949.42 31.52 30.06 1.06 · · · · · · 118 0.89 kn 591 3334.48 3349.9 2124.37 377.26 28.19 28.02 0.69 · · · · · · 151 0.02 kn 643 3334.49 3353.6 2120.62 229.30 26.60 24.64 0.43 · · · · · · 1641 0.03 abehkn 118 3334.50 3314.2 2118.99 1801.42 25.70 25.58 0.23 · · · · · · 348 0.03 kn 546 3334.50 3345.5 2116.83 552.59 30.09 30.10 <0.35 · · · · · · 65 0.12 kn 647 3334.50 3348.5 2117.43 431.79 26.25 26.26 -0.03 · · · · · · 76 0.76 kn 521 3334.52 3343.1 2111.12 647.07 30.41 29.91 <0.67 · · · · · · 155 0.15 kn 286 3334.53 3327.4 2107.82 1275.49 26.74 26.70 0.17 · · · · · · 132 0.03 kn 571 3334.53 3347.0 2108.80 493.06 28.68 28.57 0.28 · · · · · · 93 0.04 kn 435 3334.54 3337.0 2106.43 890.93 31.24 29.55 0.85 · · · · · · 175 0.86 kn 637 3334.54 3352.7 2106.20 261.96 29.76 29.18 <0.09 · · · · · · 110 0.23 kn 21 3334.55 3304.8 2102.49 2178.34 29.42 29.03 -0.21 · · · · · · 79 0.82 kn 66 3334.55 3309.1 2104.17 2008.66 29.15 28.84 0.52 · · · · · · 138 0.01 kn 554 3334.57 3346.0 2097.22 531.69 30.59 30.17 0.45 · · · · · · 84 0.79 kn 577 3334.59 3259.8 2089.82 2378.98 28.63 27.71 0.02 · · · · · · 88 0.95 dehkn 217 3334.59 3320.2 2090.39 1562.33 29.47 28.89 0.75 · · · · · · 147 0.01 kn 340 3334.61 3331.0 2083.86 1131.74 30.62 30.02 <1.10 · · · · · · 100 0.74 kn 210 3334.62 3319.9 2081.06 1575.17 30.60 29.72 0.88 · · · · · · 109 0.25 akn 319 3334.65 3329.7 2074.17 1182.91 24.34 24.37 0.82 · · · · · · 64 0.98 kn 194 3334.68 3319.5 2064.18 1591.88 28.46 27.88 0.22 · · · · · · 193 0.02 abkn

– 31 –

Table 2—Continued

ID HDFS J22r−60d x y m_i m_a clr-lp nuv-clr fuv-clr r_h s/g flags

39 3334.69 3306.4 2062.38 2115.16 30.40 30.31 0.39 · · · · · · 61 0.76 kn 407 3334.69 3335.5 2061.73 950.35 28.72 28.66 0.80 · · · · · · 74 0.39 kn 151 3334.71 3316.2 2057.00 1724.42 31.59 31.18 <1.44 · · · · · · 49 0.82 kn 537 3334.73 3344.8 2049.93 580.21 29.91 29.60 <0.82 · · · · · · 114 0.01 kn 193 3334.74 3319.0 2046.89 1612.56 28.29 27.26 -0.01 · · · · · · 522 0.00 bkn 381 3334.77 3333.6 2038.35 1027.26 31.23 29.96 <1.20 · · · · · · 135 0.90 kn 489 3334.78 3341.0 2034.33 729.71 31.60 31.31 0.94 · · · · · · 44 0.86 kn 305 3334.81 3328.6 2025.49 1226.92 29.63 29.50 <0.36 · · · · · · 89 0.16 kn 316 3334.84 3329.1 2015.84 1206.72 31.11 30.34 <1.15 · · · · · · 88 0.90 kn 472 3334.84 3340.3 2016.13 759.59 31.15 30.80 <0.94 · · · · · · 65 0.92 kn 606 3334.85 3350.8 2013.56 339.75 27.88 27.71 0.18 · · · · · · 139 0.03 kn 219 3334.87 3320.7 2009.03 1544.97 26.30 26.29 0.61 · · · · · · 113 0.03 kn 375 3334.87 3333.4 2007.04 1033.79 30.79 30.38 <1.26 · · · · · · 107 0.41 kn 615 3334.87 3351.2 2007.40 322.97 31.07 30.57 <0.54 · · · · · · 59 0.95 akn 295 3334.88 3327.7 2004.25 1264.65 31.48 31.05 <0.49 · · · · · · 63 0.81 kn 418 3334.88 3336.2 2004.32 925.16 31.78 30.81 <1.01 · · · · · · 86 0.77 kn 613 3334.89 3351.1 2001.05 329.15 30.13 29.81 0.56 · · · · · · 82 0.48 akn 447 3334.91 3338.1 1997.04 849.33 29.03 28.95 <-0.13 · · · · · · 61 0.82 kn 18 3334.94 3304.8 1986.64 2181.27 29.95 29.71 0.74 · · · · · · 82 0.25 kn 86 3334.94 3310.9 1987.52 1936.48 29.67 29.46 0.67 · · · · · · 91 0.02 kn 227 3334.94 3320.9 1986.43 1534.93 30.85 30.17 0.67 · · · · · · 106 0.48 akn 585 3334.94 3349.2 1986.74 403.84 30.37 29.95 <0.23 · · · · · · 74 0.95 kn 335 3334.95 3331.2 1983.88 1123.76 24.31 24.29 0.38 · · · · · · 386 0.03 kn 325 3334.96 3329.8 1981.73 1179.54 31.45 31.08 <1.58 · · · · · · 51 0.92 kn 596 3334.96 3350.0 1981.11 373.15 30.27 29.99 0.40 · · · · · · 94 0.15 kn 85 3335.00 3308.7 1969.95 2022.72 30.81 30.09 <1.29 · · · · · · 111 0.45 kn 651 3335.01 3353.8 1966.30 219.85 29.55 29.32 <-0.06 · · · · · · 74 0.81 kn 44 3335.02 3307.2 1963.48 2084.38 28.31 27.95 0.16 · · · · · · 152 0.02 abkn 202 3335.02 3319.1 1964.16 1607.11 29.55 29.30 0.48 · · · · · · 99 0.03 kn 43 3335.05 3307.0 1954.77 2091.07 28.47 28.27 0.40 · · · · · · 105 0.02 abkn 61 3335.05 3308.3 1956.41 2038.86 30.72 30.10 <0.88 · · · · · · 91 0.44 kn 611 3335.05 3352.3 1954.88 279.42 28.11 27.87 -0.12 · · · · · · 106 0.03 abkn 672 3335.06 3348.4 1952.76 434.94 31.08 30.84 <0.68 · · · · · · 64 0.64 kn 185 3335.07 3317.9 1950.30 1656.38 29.51 29.27 0.64 · · · · · · 71 0.20 kn 542 3335.07 3345.3 1949.22 557.86 31.13 30.44 <1.20 · · · · · · 93 0.92 kn 137 3335.08 3315.3 1945.67 1759.58 26.82 26.76 0.05 · · · · · · 235 0.03 kn 490 3335.08 3341.2 1946.35 722.51 28.81 28.63 <-0.05 · · · · · · 115 0.01 kn 475 3335.09 3340.5 1944.33 751.19 28.94 28.78 0.14 · · · · · · 126 0.01 kn 610 3335.09 3351.4 1943.56 316.90 26.59 26.36 -0.15 · · · · · · 295 0.03 bkn 242 3335.10 3318.2 1941.78 1643.60 30.80 30.48 <1.16 · · · · · · 63 0.78 kn 92 3335.12 3311.6 1934.06 1909.17 31.58 30.65 <1.17 · · · · · · 74 0.83 kn 234 3335.15 3321.6 1926.94 1508.92 29.09 29.07 0.02 · · · · · · 77 0.02 kn 245 3335.19 3325.9 1912.74 1336.84 23.41 23.36 0.51 · · · · · · 544 0.03 abkn 441 3335.19 3338.2 1913.07 843.58 25.93 25.85 0.67 · · · · · · 315 0.03 kn 187 3335.20 3318.1 1911.98 1649.17 28.38 28.27 -0.44 · · · · · · 116 0.02 kn 327 3335.21 3330.1 1907.49 1166.09 29.35 29.00 0.82 · · · · · · 99 0.02 kn 426 3335.21 3336.9 1906.65 893.69 30.21 29.88 <0.58 · · · · · · 101 0.31 abkn 41 3335.22 3307.1 1904.44 2086.71 26.86 26.80 0.31 · · · · · · 168 0.03 kn 288 3335.22 3324.2 1905.53 1403.51 23.49 23.40 0.42 · · · · · · 537 0.03 abkn 298 3335.23 3327.9 1903.49 1254.11 31.21 30.62 <0.98 · · · · · · 81 0.93 kn 425 3335.23 3336.7 1900.88 903.79 29.68 29.15 <0.59 · · · · · · 152 0.00 abkn 420 3335.24 3336.3 1899.75 920.25 30.65 29.70 0.62 · · · · · · 140 0.13 akn

– 32 –

Table 2—Continued

ID HDFS J22r−60d x y m_i m_a clr-lp nuv-clr fuv-clr r_h s/g flags

291 3335.28 3327.7 1887.55 1262.31 28.86 28.69 0.76 · · · · · · 105 0.02 kn 477 3335.30 3340.5 1882.17 751.06 31.44 30.64 <0.95 · · · · · · 76 0.82 kn 364 3335.31 3332.7 1877.23 1063.65 28.62 28.59 0.12 · · · · · · 65 0.38 abkn 365 3335.32 3333.2 1874.77 1043.81 28.40 28.28 0.31 · · · · · · 95 0.02 abkn 461 3335.32 3339.4 1876.55 796.37 31.28 31.15 <0.73 · · · · · · 47 0.90 kn 70 3335.38 3309.8 1858.29 1978.24 30.57 30.18 <0.89 · · · · · · 66 0.86 kn 620 3335.38 3351.7 1858.82 304.05 30.00 30.41 0.25 · · · · · · 55 0.97 kn 487 3335.41 3341.1 1848.95 727.26 27.66 27.64 -0.14 · · · · · · 83 0.04 kn 317 3335.42 3329.4 1847.33 1196.27 26.41 26.41 0.37 · · · · · · 106 0.04 kn 338 3335.42 3330.9 1846.76 1135.23 29.66 29.17 <0.34 · · · · · · 127 0.01 kn 223 3335.44 3320.7 1841.36 1543.56 30.50 29.66 <0.63 · · · · · · 128 0.02 kn 626 3335.45 3348.0 1836.68 450.26 28.14 28.03 0.25 · · · · · · 193 0.00 kn 412 3335.50 3335.2 1822.64 964.45 28.26 28.10 -0.08 · · · · · · 112 0.03 kn 446 3335.51 3338.0 1818.46 850.97 30.10 29.96 <0.70 · · · · · · 77 0.19 kn 149 3335.52 3316.1 1816.45 1725.55 31.60 31.26 <0.85 · · · · · · 49 0.86 kn 281 3335.53 3322.8 1813.72 1460.07 28.70 28.54 0.25 · · · · · · 173 0.00 kn 274 3335.54 3325.9 1809.67 1337.02 30.07 29.92 0.45 · · · · · · 122 0.15 bkn 189 3335.55 3318.2 1807.28 1643.69 26.53 26.53 0.32 · · · · · · 140 0.03 kn 162 3335.57 3316.8 1803.18 1699.17 31.12 30.38 <1.27 · · · · · · 92 0.90 kn 199 3335.57 3318.7 1802.69 1623.57 31.79 31.29 <1.42 · · · · · · 49 0.74 kn 355 3335.57 3324.4 1802.11 1394.03 31.16 30.84 <0.75 · · · · · · 68 0.86 kn 275 3335.57 3326.0 1800.73 1331.60 30.47 30.34 <0.74 · · · · · · 85 0.16 abkn 159 3335.59 3316.6 1794.94 1706.89 31.60 30.49 <1.64 · · · · · · 95 0.81 akn 105 3335.64 3313.1 1782.55 1848.08 26.01 25.97 0.21 · · · · · · 224 0.03 kn 277 3335.70 3326.0 1762.65 1333.04 29.62 29.25 0.58 >-0.68 · · · 102 0.01 ln 346 3335.70 3330.8 1764.00 1137.55 29.16 28.91 0.10 >-0.21 >0.19 113 0.01 503 3335.70 3342.0 1764.28 692.79 30.99 30.47 <1.06 · · · · · · 86 0.84 kn 692 3335.71 3302.0 1760.29 2292.15 30.97 30.77 <0.19 · · · · · · 43 0.88 kn 455 3335.71 3338.9 1761.54 817.02 32.13 31.19 <1.45 · · · >-1.51 61 0.67 k 154 3335.73 3316.5 1755.73 1712.69 29.39 29.29 <0.33 · · · · · · 95 0.03 kn 192 3335.73 3318.3 1753.83 1640.63 29.35 29.28 <0.19 · · · · · · 89 0.01 kn 75 3335.74 3310.1 1751.50 1968.62 31.05 30.41 <0.60 · · · · · · 73 0.93 kn 283 3335.74 3326.7 1751.98 1302.21 29.47 29.24 0.35 >-0.30 >-0.13 83 0.09 566 3335.74 3346.7 1752.61 501.73 30.74 30.37 0.88 · · · · · · 65 0.82 kn 34 3335.75 3307.2 1747.64 2083.59 24.48 24.45 0.36 · · · · · · 439 0.03 kn 104 3335.75 3312.4 1748.77 1875.44 30.48 29.76 <0.42 · · · · · · 117 0.18 kn 635 3335.76 3352.7 1746.81 265.36 31.02 30.82 <0.68 · · · · · · 64 0.79 kn 509 3335.77 3343.0 1743.06 652.60 25.01 24.99 0.06 · · · >6.55 260 0.03 ko 228 3335.78 3321.1 1739.34 1528.22 28.99 29.12 -0.05 >-1.42 >-0.06 153 0.00 alo 474 3335.83 3340.7 1723.84 744.28 29.50 29.34 0.37 · · · >0.14 84 0.04 abk 88 3335.84 3311.2 1721.11 1921.99 28.76 28.56 0.06 · · · · · · 120 0.18 kn 640 3335.84 3353.0 1720.97 250.97 28.57 28.22 0.13 · · · · · · 196 0.02 kn 284 3335.85 3326.7 1719.83 1302.44 30.89 30.56 0.85 >-0.97 >-0.75 68 0.96 623 3335.85 3352.0 1720.19 290.03 30.71 29.69 <0.88 · · · · · · 174 0.69 kn 167 3335.86 3317.0 1715.14 1691.58 29.25 29.09 0.56 >-0.12 0.21 87 0.05 abo 201 3335.87 3320.0 1713.95 1572.67 25.94 25.81 0.05 >1.63 >1.62 699 0.00 lo 358 3335.87 3332.0 1714.35 1091.36 31.54 31.04 0.86 >-1.07 -1.37 70 0.87 473 3335.87 3340.4 1713.85 754.28 28.67 28.61 0.15 >0.22 >0.93 81 0.02 abl 168 3335.89 3317.3 1707.01 1679.65 30.04 29.61 0.31 >-0.81 >-1.05 119 0.03 ab 181 3335.89 3317.6 1707.72 1669.03 30.67 30.23 0.54 >-0.75 >-0.72 91 0.13 382 3335.90 3333.6 1705.03 1027.98 31.61 30.73 <1.57 >-1.29 >-1.23 76 0.86 551 3335.91 3345.7 1702.81 542.80 31.14 30.82 <0.65 · · · · · · 50 0.93 kn

– 33 –

Table 2—Continued

ID HDFS J22r−60d x y m_i m_a clr-lp nuv-clr fuv-clr r_h s/g flags

101 3335.93 3311.9 1695.71 1896.15 30.22 29.65 <0.90 · · · · · · 118 0.01 kn 601 3335.94 3350.3 1691.30 358.51 31.61 30.80 <0.92 · · · · · · 70 0.87 kn 329 3335.96 3324.1 1687.50 1408.15 29.49 29.07 0.06 >-0.38 >-0.26 133 0.00 690 3335.97 3301.7 1683.06 2302.89 30.01 29.92 <0.21 · · · · · · 69 0.75 kn 12 3335.97 3303.5 1684.54 2232.71 31.11 30.64 <0.50 · · · · · · 61 0.94 kn 49 3335.97 3307.5 1684.47 2072.93 30.31 30.03 0.58 · · · · · · 112 0.12 kn 157 3335.98 3315.6 1680.19 1746.31 29.85 29.05 <0.55 >-0.78 · · · 204 0.06 bn 142 3335.98 3315.9 1680.62 1736.09 30.08 29.40 0.18 >-0.81 · · · 117 0.12 abn 569 3335.99 3346.8 1679.00 500.49 31.06 30.97 <0.88 · · · · · · 63 0.95 kn 453 3336.02 3339.0 1670.38 811.30 28.53 28.32 0.28 >0.36 >1.68 109 0.02 a 459 3336.02 3339.6 1668.64 787.15 28.63 28.42 0.58 >0.00 >0.57 183 0.00 330 3336.04 3330.3 1662.20 1161.28 29.96 29.86 0.65 >-0.02 >0.53 77 0.07 233 3336.07 3321.5 1654.51 1510.85 30.36 30.17 0.44 >-0.90 >-0.35 67 0.49 530 3336.07 3343.4 1654.62 633.93 31.35 30.53 <1.61 · · · >-0.57 79 0.77 k 428 3336.10 3336.8 1644.75 901.31 28.40 28.25 0.50 >0.90 >1.41 115 0.02 247 3336.11 3323.0 1643.76 1449.43 30.85 30.37 <1.09 >-0.92 >-0.91 83 0.60 370 3336.12 3333.2 1641.00 1041.96 30.64 30.04 <0.93 >-0.98 >-0.05 102 0.43 290 3336.15 3327.3 1629.77 1277.84 31.11 30.74 <0.58 >-0.73 >0.14 75 0.73 460 3336.15 3339.4 1631.24 797.15 29.71 29.60 0.37 -0.63 >0.89 87 0.01 408 3336.16 3335.5 1627.40 953.12 31.69 30.68 <1.55 >-1.67 >-0.23 89 0.84 525 3336.16 3341.7 1628.25 704.89 31.16 30.74 <1.35 · · · >-0.51 62 0.94 k 538 3336.16 3344.6 1626.35 586.85 30.85 30.23 <0.99 · · · · · · 73 0.97 kn 612 3336.16 3351.1 1629.19 328.20 28.57 28.46 0.07 · · · · · · 98 0.03 kn 324 3336.17 3330.0 1626.05 1171.79 26.97 26.89 0.11 0.80 >2.27 138 0.03 60 3336.18 3308.8 1620.60 2018.97 27.15 27.02 0.45 · · · · · · 244 0.01 kn 254 3336.18 3323.4 1620.90 1436.95 30.13 29.69 0.76 >-0.34 >0.70 97 0.20 100 3336.19 3311.8 1618.88 1900.86 31.93 30.20 <1.61 · · · · · · 144 0.77 kn 416 3336.19 3336.1 1618.91 925.62 30.92 30.82 <1.30 >-0.56 >0.30 59 0.33 243 3336.21 3322.6 1613.08 1466.61 28.02 27.92 0.66 >1.12 >1.41 107 0.02 691 3336.22 3302.0 1609.97 2292.63 30.12 29.53 0.92 · · · · · · 105 0.73 kn 150 3336.22 3316.2 1608.99 1723.88 31.19 30.16 1.16 >-0.76 >-1.02 114 0.71 334 3336.22 3330.5 1609.42 1152.36 30.42 29.39 <0.81 >-1.14 >-0.29 189 0.03 a 385 3336.22 3333.7 1610.49 1022.62 31.31 30.63 <0.88 >-1.30 -0.36 74 0.92 510 3336.23 3342.4 1608.08 674.19 30.02 29.56 <0.93 · · · >0.00 128 0.12 k 134 3336.25 3314.8 1601.43 1780.56 30.18 29.89 <0.59 >-0.98 >-1.24 109 0.02 256 3336.25 3324.7 1601.85 1384.83 30.42 30.18 0.93 >-0.31 >0.52 75 0.23 367 3336.25 3332.7 1601.08 1063.49 31.26 31.03 <1.12 >-0.64 >0.20 49 0.84 528 3336.25 3341.7 1602.53 701.69 29.64 29.37 0.38 · · · >0.36 113 0.01 k 237 3336.28 3321.9 1591.87 1494.82 28.99 28.76 -0.69 >0.74 >1.30 82 0.24 211 3336.30 3319.9 1586.91 1576.16 31.12 30.58 <0.52 >-0.83 >0.27 83 0.94 230 3336.30 3321.3 1586.32 1519.24 30.52 29.48 0.92 >-1.14 >0.40 175 0.23 536 3336.31 3344.7 1582.53 585.23 28.59 28.56 -0.09 · · · >1.97 165 0.00 afiko 532 3336.32 3344.1 1580.92 607.35 29.43 29.56 <0.37 · · · >0.22 108 0.00 ak 25 3336.33 3305.3 1578.82 2160.86 31.73 30.89 <1.28 · · · · · · 66 0.85 kn 270 3336.33 3326.3 1576.68 1321.14 24.79 24.79 0.31 >3.14 >4.08 238 0.03 517 3336.33 3343.3 1576.24 641.31 27.74 27.16 0.54 · · · >1.13 311 0.00 abk 659 3336.35 3354.4 1571.17 196.50 29.77 29.03 0.52 · · · · · · 126 0.72 kn 16 3336.36 3304.6 1569.82 2185.89 30.03 29.24 0.27 · · · · · · 145 0.02 kn 486 3336.36 3341.0 1569.82 731.33 30.02 29.38 0.76 · · · >-0.03 130 0.13 k 176 3336.38 3317.9 1563.44 1656.37 26.53 26.42 0.58 1.55 2.02 202 0.03 b 518 3336.38 3343.5 1563.97 631.17 27.72 27.39 0.52 · · · >0.71 233 0.03 abk 373 3336.39 3333.7 1559.26 1022.90 29.85 29.40 0.59 >0.05 >0.83 128 0.12 ab

– 34 –

Table 2—Continued

ID HDFS J22r−60d x y m_i m_a clr-lp nuv-clr fuv-clr r_h s/g flags

389 3336.39 3334.0 1558.95 1010.61 31.23 30.71 <0.79 >-0.77 >-0.45 69 0.92 a 27 3336.40 3305.5 1557.43 2150.33 30.11 29.75 <0.53 · · · · · · 119 0.66 kn 289 3336.41 3327.3 1554.92 1277.73 29.99 29.94 <0.03 0.08 >0.91 60 0.77 396 3336.41 3333.4 1554.56 1033.82 29.65 29.46 <0.69 >-0.14 >0.73 116 0.00 b 534 3336.41 3344.1 1554.46 606.77 30.72 30.21 <0.63 · · · >-0.74 80 0.04 k 10 3336.44 3302.8 1546.57 2259.61 30.08 29.25 <0.54 · · · · · · 145 0.68 kn 177 3336.44 3317.8 1545.96 1659.35 28.79 28.45 0.26 >0.80 >1.37 107 0.01 ab 205 3336.44 3319.3 1545.92 1599.82 31.16 31.22 <0.88 >-0.96 >-0.05 56 0.88 590 3336.44 3349.7 1545.80 383.97 30.66 30.26 0.77 · · · · · · 85 0.87 kn 26 3336.48 3305.5 1534.95 2152.75 30.23 29.76 <0.43 · · · · · · 92 0.76 kn 282 3336.53 3326.7 1520.08 1301.56 29.88 29.71 0.27 >-0.31 >0.75 92 0.08 645 3336.53 3353.3 1518.65 241.02 25.75 25.74 0.39 · · · · · · 159 0.04 kn 438 3336.54 3337.5 1514.73 873.00 28.99 28.91 0.12 >0.65 >1.47 91 0.02 444 3336.57 3338.3 1505.68 840.74 26.79 26.69 0.25 >1.31 2.68 237 0.03 622 3336.57 3351.9 1506.84 295.35 30.46 30.09 <0.94 · · · · · · 82 0.96 kn 271 3336.58 3325.7 1502.91 1343.95 28.66 28.64 0.42 >0.88 >1.63 105 0.02 404 3336.58 3335.2 1504.80 962.79 30.57 30.48 <0.96 >-0.39 >-0.35 101 0.73 fi 116 3336.60 3313.6 1497.55 1827.81 28.43 28.30 0.54 >-1.98 · · · 179 0.00 ln 376 3336.61 3324.8 1496.31 1380.10 27.66 27.60 0.22 >1.33 >2.38 115 0.03 524 3336.61 3343.3 1495.43 640.79 29.42 29.33 0.11 · · · >0.57 100 0.01 k 597 3336.62 3350.2 1493.57 364.15 27.73 27.69 0.70 · · · · · · 152 0.03 kn 667 3336.62 3354.7 1492.56 182.39 30.38 30.04 <0.77 · · · · · · 76 0.97 bkn 670 3336.65 3355.1 1482.69 165.62 29.92 29.63 0.47 · · · · · · 96 0.85 aehkn 58 3336.66 3308.7 1480.82 2023.96 25.17 25.13 0.24 · · · · · · 409 0.02 kn 309 3336.67 3328.7 1478.84 1222.44 29.80 29.47 0.72 >-0.13 >0.79 108 0.01 630 3336.69 3352.7 1472.29 264.45 28.95 28.10 0.44 · · · · · · 274 0.01 kn 545 3336.70 3345.4 1469.15 555.36 31.47 30.47 <1.54 · · · · · · 96 0.86 kn 664 3336.70 3354.6 1467.25 186.26 30.00 28.70 <0.33 · · · · · · 177 0.60 kn 9 3336.71 3303.4 1466.92 2233.90 25.89 25.84 0.47 · · · · · · 198 0.03 kn 326 3336.73 3330.0 1459.98 1171.57 29.97 29.54 0.28 >0.01 >0.39 111 0.01 583 3336.73 3349.2 1460.44 404.18 27.21 27.16 0.00 · · · · · · 127 0.03 abkn 442 3336.74 3337.8 1457.47 860.58 31.22 30.75 <0.82 -0.82 >0.06 74 0.87 584 3336.74 3349.6 1456.79 386.52 27.59 27.49 0.35 · · · · · · 141 0.03 abkn 238 3336.75 3321.8 1453.36 1499.22 32.05 30.66 <1.26 >-1.14 >-0.38 88 0.72 fi 348 3336.75 3324.1 1452.97 1408.30 30.47 30.30 <0.85 >-0.18 >0.12 69 0.71 204 3336.76 3319.3 1450.99 1598.76 30.17 29.79 <0.82 >0.00 >0.52 92 0.10 559 3336.78 3346.1 1446.27 527.94 30.51 30.36 0.48 · · · · · · 58 0.63 kn 567 3336.78 3346.8 1446.03 498.77 29.36 29.20 0.37 · · · · · · 90 0.01 abkn 673 3336.80 3355.3 1439.18 159.39 30.13 · · · 0.79 · · · · · · · · · 0.84 abhkn 568 3336.81 3346.9 1435.98 496.62 29.02 28.78 -0.00 · · · · · · 103 0.01 abkn 668 3336.81 3355.0 1436.58 172.68 29.01 29.78 0.48 · · · · · · 81 0.01 abhkn 663 3336.82 3354.7 1432.72 184.82 29.22 27.32 -0.35 · · · · · · 373 0.01 akn 133 3336.83 3314.4 1431.62 1796.90 29.40 29.29 -0.02 >-1.44 >-0.24 104 0.01 o 431 3336.83 3336.9 1431.19 895.67 28.78 28.54 0.12 >0.11 >1.30 108 0.02 541 3336.83 3345.2 1430.27 561.62 31.36 30.49 <1.05 · · · · · · 88 0.72 kn 331 3336.84 3330.2 1428.73 1162.93 31.38 30.79 <0.89 >-0.88 >-0.15 79 0.59 642 3336.86 3353.0 1421.19 252.49 31.22 30.69 <0.93 · · · · · · 52 0.94 kn 117 3336.87 3313.4 1418.90 1833.58 28.89 28.86 0.75 · · · · · · 81 0.02 kn 495 3336.87 3341.9 1418.91 693.61 24.87 24.84 0.18 >5.45 >3.86 195 0.03 abl 657 3336.87 3354.2 1417.70 204.46 30.45 28.96 <0.13 · · · · · · 155 0.98 kn 665 3336.88 3354.7 1416.46 181.84 29.92 28.11 <0.52 · · · · · · 249 0.54 akn 445 3336.89 3337.9 1411.11 857.24 31.28 30.27 <1.01 >-0.79 -0.02 119 0.56

– 35 –

Table 2—Continued

ID HDFS J22r−60d x y m_i m_a clr-lp nuv-clr fuv-clr r_h s/g flags

466 3336.89 3339.7 1411.73 781.81 30.18 29.96 <0.57 >-0.62 >0.61 76 0.15 616 3336.89 3351.3 1411.65 318.13 29.86 29.70 0.16 · · · · · · 98 0.32 kn 675 3336.89 3355.6 1411.84 146.41 30.72 32.47 <0.95 · · · · · · 25 0.98 aehkn 485 3336.90 3341.3 1411.05 720.91 30.55 29.89 <0.92 >-1.87 >0.34 106 0.13 abl 496 3336.91 3342.9 1406.27 655.60 22.79 22.79 0.23 >6.59 >3.80 267 0.03 abl 152 3336.92 3316.3 1404.02 1718.89 30.54 30.42 <0.65 >-0.32 >-1.14 55 0.76 484 3336.92 3341.0 1404.07 731.85 29.17 28.87 -0.08 >-0.82 >0.78 101 0.03 bl 78 3336.94 3310.4 1397.10 1955.40 27.80 27.74 0.45 · · · · · · 95 0.02 kn 379 3336.94 3333.5 1397.56 1029.79 31.99 31.26 <1.35 >-1.27 >-0.57 60 0.84 afi 225 3336.95 3320.8 1395.27 1539.40 30.05 29.79 0.52 >-0.11 >0.46 96 0.09 432 3336.96 3336.9 1392.34 896.55 29.88 29.65 <0.22 >-0.20 >0.83 114 0.00 95 3336.98 3311.7 1385.69 1902.29 29.77 29.63 0.30 · · · · · · 73 0.12 kn 155 3336.99 3316.4 1383.03 1715.84 30.85 30.32 0.47 >-0.89 -0.93 76 0.83 216 3336.99 3320.1 1384.06 1566.08 28.79 28.67 0.59 >0.84 >1.60 115 0.01 10123 3336.99 3333.0 1384.14 1052.53 29.21 27.94 -0.24 >0.92 >1.71 138 0.00 fgij 628 3337.01 3352.4 1377.37 275.48 30.18 28.87 <0.37 · · · · · · 216 0.66 kn 686 3337.01 3356.6 1376.68 107.11 29.38 27.48 <0.51 · · · · · · 158 0.96 aehkn 339 3337.02 3330.9 1374.67 1135.01 30.36 30.13 <0.92 >-0.15 >0.45 78 0.18 259 3337.03 3324.7 1372.02 1381.92 31.43 30.86 <1.54 >-0.85 >-0.29 77 0.52 a 10120 3337.03 3332.5 1371.47 1073.39 28.80 27.15 -0.24 >1.18 >1.81 228 0.00 fgij 377 3337.04 3333.6 1367.36 1029.05 31.24 30.98 <1.02 >-0.91 >-0.25 69 0.30 32 3337.05 3306.2 1364.03 2124.64 29.27 29.16 0.58 · · · · · · 92 0.01 kn 160 3337.08 3316.8 1357.51 1700.39 28.40 28.24 -0.26 >0.51 >0.77 130 0.03 300 3337.08 3328.7 1357.69 1223.56 22.58 22.62 0.80 >5.14 >5.73 69 0.96 175 3337.09 3317.5 1353.75 1673.37 30.57 29.61 0.92 >-0.82 >0.12 147 0.18 587 3337.09 3349.7 1353.24 384.76 27.26 27.22 -0.19 · · · · · · 163 0.03 afikn 661 3337.10 3353.3 1351.61 240.76 29.93 29.72 <0.02 · · · · · · 77 0.08 kn 226 3337.11 3320.9 1346.30 1536.36 30.63 30.29 <1.16 >-0.62 >-0.06 95 0.64 10121 3337.11 3332.6 1347.46 1066.91 26.65 26.03 0.19 0.67 2.42 251 0.00 fgij 102 3337.12 3312.4 1343.86 1876.39 27.39 27.30 0.34 · · · · · · 162 0.03 kn 131 3337.17 3314.3 1329.54 1799.17 29.37 29.11 0.85 >-0.80 >-1.02 100 0.01 o 91 3337.18 3310.3 1325.60 1960.39 24.91 24.89 0.39 · · · · · · 420 0.03 kn 212 3337.19 3319.9 1324.57 1575.35 31.18 29.77 <1.41 -0.82 >0.09 161 0.79 10100 3337.19 3325.5 1323.08 1351.80 27.98 26.69 0.63 >1.32 >2.19 297 0.00 fgij 374 3337.19 3333.4 1324.15 1035.28 31.34 31.06 <1.45 >-0.80 >-0.70 67 0.89 592 3337.22 3349.8 1315.43 381.24 30.30 29.64 0.45 · · · · · · 107 0.74 kn 10119 3337.23 3332.3 1312.78 1077.46 29.35 28.78 0.34 >0.88 >1.68 70 0.04 gj 511 3337.23 3342.5 1312.27 671.04 30.63 30.84 <0.89 · · · >-0.14 72 0.89 k 38 3337.24 3306.3 1309.08 2119.19 29.70 29.53 <0.31 · · · · · · 92 0.03 kn 65 3337.24 3308.8 1308.07 2019.25 30.89 29.59 <1.06 · · · · · · 180 0.14 akn 261 3337.24 3324.9 1309.02 1374.83 29.18 28.83 0.47 >0.79 >0.53 95 0.25 ab 433 3337.24 3336.9 1309.03 895.09 30.72 29.72 <0.74 >-0.40 >0.02 162 0.17 28 3337.26 3305.6 1304.81 2148.89 30.14 29.86 <0.38 · · · · · · 87 0.08 kn 500 3337.27 3341.5 1300.04 710.33 29.07 28.74 <0.41 >-1.28 >0.90 163 0.00 l 262 3337.28 3325.2 1298.56 1365.20 29.67 29.32 0.72 >0.02 >0.54 122 0.01 ab 462 3337.28 3339.6 1297.19 789.20 30.32 29.72 <0.68 >-0.93 >0.54 124 0.03 169 3337.32 3317.0 1285.98 1689.73 29.97 29.10 0.68 >0.02 >-0.08 199 0.01 222 3337.33 3320.2 1282.27 1564.49 26.00 26.00 0.41 >2.65 >3.29 146 0.03 180 3337.34 3317.5 1278.89 1670.58 30.90 30.13 <0.58 >-0.57 >0.04 142 0.81 467 3337.34 3340.3 1279.99 759.57 25.35 25.36 0.21 >1.63 >4.02 111 0.03 98 3337.37 3311.8 1271.82 1898.75 29.19 29.20 -0.00 · · · · · · 73 0.01 kn 186 3337.39 3317.9 1264.37 1656.14 28.28 28.21 0.50 >1.32 1.31 88 0.02

– 36 –

Table 2—Continued

ID HDFS J22r−60d x y m_i m_a clr-lp nuv-clr fuv-clr r_h s/g flags

413 3337.39 3335.9 1264.59 933.94 30.24 30.26 <0.54 >-0.12 >0.45 79 0.18 231 3337.40 3321.6 1262.78 1505.60 25.36 25.37 0.14 2.01 >3.49 109 0.06 393 3337.40 3334.7 1263.62 984.31 28.37 28.27 0.40 >1.15 >1.62 87 0.05 46 3337.43 3307.1 1252.79 2087.90 30.00 29.77 <0.47 · · · · · · 101 0.07 kn 24 3337.44 3305.3 1250.18 2157.66 28.15 28.10 0.31 · · · · · · 87 0.02 kn 555 3337.44 3345.9 1248.95 534.12 31.55 31.17 <1.12 · · · · · · 43 0.86 kn 580 3337.44 3348.7 1251.15 423.90 30.73 30.01 <0.90 · · · · · · 101 0.70 kn 48 3337.50 3307.4 1232.24 2074.60 29.26 29.00 0.17 · · · · · · 107 0.01 kn 482 3337.50 3340.9 1232.48 734.35 28.05 28.04 -0.32 0.65 >1.59 115 0.02 519 3337.51 3342.8 1229.87 657.98 29.80 29.63 <0.43 · · · -0.25 72 0.13 k 602 3337.52 3350.4 1225.46 355.92 30.79 30.23 <1.10 · · · · · · 82 0.91 kn 40 3337.58 3306.5 1210.51 2111.76 31.21 29.68 <1.42 · · · · · · 187 0.91 kn 141 3337.58 3315.7 1209.18 1742.61 26.00 25.96 0.36 0.77 >1.75 204 0.03 10103 3337.59 3329.1 1205.73 1206.06 17.78 17.83 0.34 1.77 2.53 188 0.85 cfgijmpq 607 3337.60 3350.9 1202.68 337.39 28.13 27.97 0.44 · · · · · · 137 0.02 kn 1 3337.60 3355.3 1204.05 161.27 17.14 17.16 0.79 · · · · · · 274 0.85 acefhikn 51 3337.62 3307.6 1196.36 2068.34 29.72 29.70 0.49 · · · · · · 64 0.19 kn 588 3337.62 3349.9 1198.57 376.67 26.31 26.25 0.56 · · · · · · 229 0.03 kn 179 3337.64 3318.0 1190.31 1652.84 26.05 25.98 0.22 1.89 >2.07 321 0.03 a 456 3337.68 3339.0 1178.40 810.44 29.59 29.17 <0.19 >-0.15 >0.86 155 0.01 469 3337.68 3340.0 1179.28 770.44 30.16 29.81 <0.51 >-0.67 >0.32 78 0.06 273 3337.71 3325.9 1171.99 1337.34 29.10 28.88 0.17 >0.64 >0.57 139 0.01 a 639 3337.71 3347.7 1170.28 462.49 31.95 31.09 <2.00 · · · · · · 62 0.81 kn 103 3337.72 3312.3 1167.35 1880.72 30.18 30.15 <0.34 · · · · · · 68 0.19 kn 236 3337.73 3321.8 1164.70 1500.23 30.02 28.92 <0.93 >-0.12 >0.09 235 0.13 423 3337.73 3336.4 1165.86 916.07 29.88 29.48 <0.37 >-0.07 >0.55 126 0.00 130 3337.75 3314.2 1157.76 1803.03 30.65 29.89 <1.18 · · · · · · 153 0.96 kn 7 3337.77 3302.3 1153.69 2279.29 27.41 27.13 0.30 · · · · · · 147 0.03 aehkn 417 3337.79 3336.2 1146.51 923.23 30.53 29.98 <1.10 >-0.47 >0.27 97 0.63 173 3337.81 3317.7 1140.67 1665.26 25.68 25.66 0.40 0.78 >2.67 187 0.03 253 3337.81 3324.4 1142.48 1394.05 22.85 22.84 0.48 0.89 1.86 553 0.03 a 403 3337.83 3335.2 1136.64 962.58 28.84 28.81 -0.00 >0.41 >1.06 68 0.07 52 3337.86 3307.6 1125.02 2067.53 30.89 29.38 0.75 · · · · · · 208 0.52 kn 573 3337.86 3347.0 1126.62 489.92 31.58 30.97 <0.93 · · · · · · 66 0.84 kn 493 3337.87 3341.3 1122.37 718.20 31.75 31.32 <1.08 >-2.15 >-0.14 55 0.73 512 3337.88 3342.6 1119.29 669.06 29.03 28.92 0.33 · · · >1.05 66 0.46 k 383 3337.90 3334.1 1115.72 1006.97 26.18 26.17 0.23 1.80 >2.31 167 0.03 548 3337.91 3345.7 1111.09 543.58 29.91 29.52 <0.92 · · · · · · 148 0.00 kn 19 3337.92 3304.8 1107.90 2178.81 28.67 28.56 0.31 · · · · · · 93 0.01 kn 543 3337.93 3345.3 1106.44 557.65 30.59 29.71 <0.41 · · · >-0.86 168 0.95 ako 497 3337.95 3341.7 1101.35 701.55 30.73 30.19 0.87 >-1.38 >0.17 75 0.91 146 3337.98 3314.6 1092.48 1786.73 26.48 26.36 0.69 >0.73 >1.39 465 0.00 lo 483 3337.99 3340.9 1088.85 736.59 31.57 31.04 <1.07 >-1.48 >-0.34 64 0.84 89 3338.00 3311.8 1083.88 1900.90 27.89 27.86 -0.12 · · · · · · 196 0.03 kn 126 3338.00 3313.6 1085.19 1826.33 30.86 30.00 <0.72 · · · · · · 122 0.47 akn 457 3338.01 3339.4 1082.25 797.05 27.95 27.77 -0.20 1.11 >1.53 123 0.03 ab 272 3338.02 3325.7 1077.92 1345.30 29.07 28.89 -0.27 >0.60 >0.58 118 0.01 344 3338.02 3331.2 1078.20 1125.29 31.35 30.82 <1.14 >-0.81 >-0.45 72 0.81 a 47 3338.04 3307.0 1073.68 2090.40 30.79 29.56 <1.04 · · · · · · 181 0.58 kn 135 3338.04 3313.8 1073.69 1820.19 30.63 30.05 <0.96 · · · · · · 115 0.21 akn 235 3338.05 3321.6 1070.58 1508.27 31.52 30.89 <0.82 >-0.95 >-0.73 62 0.86 269 3338.06 3325.4 1068.91 1355.69 31.03 30.15 <0.93 >-0.46 >-0.23 135 0.89 a

– 37 –

Table 2—Continued

ID HDFS J22r−60d x y m_i m_a clr-lp nuv-clr fuv-clr r_h s/g flags

575 3338.06 3347.1 1066.68 485.60 29.68 29.29 <0.28 · · · · · · 154 0.01 kn 8 3338.07 3302.6 1065.55 2267.19 26.11 25.86 0.59 · · · · · · 341 0.03 aehkn 132 3338.07 3314.3 1065.57 1800.68 31.70 32.00 <1.07 · · · · · · 42 0.87 kn 50 3338.08 3308.4 1062.58 2035.87 24.03 23.99 0.45 · · · · · · 566 0.03 bkn 458 3338.08 3339.5 1060.67 791.19 27.25 27.05 0.04 1.01 >2.33 275 0.01 ab 11 3338.10 3303.4 1054.64 2233.59 30.65 30.00 0.41 · · · · · · 77 0.97 kn 221 3338.11 3320.5 1053.91 1551.57 30.34 30.08 <0.29 >-0.56 >0.34 82 0.04 354 3338.11 3324.4 1053.36 1393.63 29.04 29.04 0.15 >0.62 >0.99 96 0.01 77 3338.14 3310.0 1044.17 1970.11 24.94 24.93 0.21 · · · · · · 215 0.03 abkn 111 3338.14 3312.9 1043.80 1856.05 30.78 30.58 <0.86 · · · · · · 83 0.10 kn 203 3338.14 3319.4 1044.18 1595.08 27.59 27.48 0.21 0.56 >1.42 200 0.02 535 3338.14 3344.5 1043.29 592.01 29.29 29.07 0.13 · · · 0.31 153 0.00 k 646 3338.15 3353.5 1040.86 232.87 29.88 29.02 <0.10 · · · · · · 181 0.02 akn 631 3338.17 3352.6 1035.05 268.60 31.03 31.14 <1.23 · · · · · · 48 0.74 kn 465 3338.18 3339.3 1030.87 797.70 29.19 28.94 0.24 >0.33 >1.00 140 0.00 a 123 3338.19 3313.7 1027.88 1824.38 28.58 28.21 -0.32 · · · · · · 209 0.00 kn 307 3338.19 3328.7 1030.23 1221.62 29.34 28.66 0.46 >0.34 >0.58 162 0.00 369 3338.20 3333.2 1025.41 1042.94 30.11 29.91 1.04 >0.05 >0.41 68 0.23 266 3338.21 3325.3 1024.59 1357.52 30.54 30.05 <0.46 >-0.65 >0.02 104 0.14 abfi 353 3338.21 3331.9 1023.14 1094.84 28.77 28.72 0.52 >0.43 >0.78 80 0.19 147 3338.23 3316.3 1017.34 1719.35 27.52 27.44 0.35 1.31 >1.20 119 0.06 232 3338.23 3321.4 1018.00 1514.52 27.35 27.29 0.47 >1.75 >2.22 151 0.03 333 3338.23 3330.4 1016.84 1154.10 30.22 29.30 0.70 >-0.13 >0.18 164 0.04 20 3338.24 3304.8 1014.60 2179.79 30.71 30.13 <0.75 · · · · · · 71 0.97 kn 301 3338.24 3323.7 1015.11 1422.88 31.55 30.94 <1.09 >-0.82 >-0.44 58 0.85 371 3338.24 3333.3 1015.04 1039.74 31.12 30.12 <1.60 >-0.70 >-0.35 108 0.93 a 164 3338.25 3317.2 1010.81 1683.34 29.95 29.50 <0.71 >-0.80 >-0.66 103 0.19 ab 653 3338.25 3353.8 1011.08 219.04 29.97 30.08 <0.02 · · · · · · 69 0.78 kn 163 3338.26 3317.0 1009.62 1692.95 30.30 29.26 0.37 >-0.47 >-0.73 165 0.11 ab 165 3338.26 3317.4 1007.70 1674.55 29.78 29.44 0.24 >0.18 >-0.28 100 0.03 ab 347 3338.27 3331.5 1004.42 1109.49 29.87 29.61 0.14 >-0.49 >0.21 97 0.00 494 3338.27 3341.4 1006.29 716.28 30.06 29.78 <0.05 >-0.60 >0.26 84 0.23 224 3338.28 3320.7 1002.07 1542.24 30.46 29.74 <1.05 >-0.30 >0.19 126 0.10 352 3338.30 3324.7 996.84 1382.40 29.65 28.77 0.49 >-0.15 >0.47 229 0.01 abfi 678 3338.33 3355.7 988.82 142.13 29.21 28.18 0.40 · · · · · · 211 0.02 akn 499 3338.34 3341.9 983.88 695.85 28.31 28.28 0.28 >0.02 1.12 86 0.03 682 3338.34 3356.2 985.63 121.93 28.83 · · · 0.69 · · · · · · · · · 0.02 ahkn 684 3338.36 3356.6 979.46 107.72 28.96 26.56 0.42 · · · · · · 610 0.01 aehkn 79 3338.37 3310.7 975.35 1941.55 26.73 26.64 0.12 · · · · · · 192 0.03 bkn 2 3338.37 3357.2 976.59 81.48 28.43 25.50 <1.85 · · · · · · 1004 0.01 aehkn 506 3338.39 3342.3 971.48 678.64 30.27 29.85 0.62 >-0.74 >0.05 88 0.22 l 195 3338.41 3318.8 965.31 1618.55 28.55 27.94 0.49 >0.75 >1.13 276 0.00 b 263 3338.41 3325.0 964.34 1370.61 31.10 30.56 <0.78 >-1.26 >-0.39 98 0.82 5 3338.41 3357.4 965.10 76.01 29.96 27.16 <1.08 · · · · · · 382 0.90 adehkn 196 3338.42 3319.2 961.53 1604.55 30.04 29.52 0.52 >-0.12 >0.25 120 0.00 ab 279 3338.42 3326.4 960.27 1317.40 30.95 30.62 0.83 >-0.58 >-0.17 68 0.89 452 3338.42 3338.6 961.44 825.72 29.61 29.49 0.51 0.26 >0.92 73 0.09 80 3338.43 3310.8 958.11 1937.99 28.72 28.68 -0.64 · · · · · · 76 0.02 abkn 687 3338.43 3356.8 957.39 98.48 30.29 28.09 <1.12 · · · · · · 257 0.98 ehkn 605 3338.44 3351.1 956.25 326.08 26.45 26.40 0.38 · · · · · · 216 0.03 akn 685 3338.44 3356.5 956.49 112.84 30.50 · · · 0.51 · · · · · · · · · 0.93 hkn 660 3338.45 3354.4 951.39 194.64 30.88 30.00 1.01 · · · · · · 104 0.83 kn

– 38 –

Table 2—Continued

ID HDFS J22r−60d x y m_i m_a clr-lp nuv-clr fuv-clr r_h s/g flags

161 3338.47 3316.8 947.06 1697.76 29.43 29.02 -0.16 >-0.76 >-0.24 123 0.01 681 3338.47 3355.9 947.45 137.27 30.78 29.32 <0.37 · · · · · · 164 0.98 kn 10097 3338.48 3324.0 944.86 1411.95 30.02 29.04 0.11 >0.26 >0.87 75 0.80 fgij 128 3338.49 3314.2 940.74 1804.13 28.61 28.37 0.08 · · · · · · 115 0.02 abkn 68 3338.50 3309.6 938.16 1988.42 31.15 30.75 <1.28 · · · · · · 63 0.88 kn 99 3338.50 3311.8 938.23 1897.62 29.55 29.05 0.51 · · · · · · 154 0.04 kn 53 3338.51 3307.6 934.03 2066.79 30.42 29.72 <0.99 · · · · · · 117 0.34 kn 656 3338.51 3353.2 933.84 244.10 29.92 29.25 0.66 · · · · · · 137 0.20 kn 6 3338.51 3357.5 934.69 69.53 27.68 26.29 <-0.27 · · · · · · 287 0.04 abdehkn 129 3338.53 3314.5 928.29 1793.00 27.34 27.16 0.08 · · · · · · 197 0.03 bkn 514 3338.55 3342.5 922.92 671.21 30.34 29.85 0.81 · · · >0.36 98 0.20 k 411 3338.56 3335.7 919.41 943.77 31.26 30.48 <1.58 >-0.87 >-0.40 82 0.90 529 3338.60 3344.3 909.40 600.07 24.75 24.73 0.35 · · · >0.97 296 0.03 k 662 3338.60 3354.5 909.61 190.59 29.74 29.33 <0.53 · · · · · · 94 0.10 kn 36 3338.63 3306.5 899.28 2109.88 27.82 27.70 0.18 · · · · · · 156 0.03 bkn 182 3338.63 3317.6 900.26 1669.16 31.12 30.69 <1.25 >-0.87 >-1.39 71 0.90 a 599 3338.63 3350.1 898.17 368.97 29.06 28.98 0.14 · · · · · · 83 0.02 kn 654 3338.63 3353.8 898.31 219.64 31.23 30.69 <0.71 · · · · · · 76 0.87 kn 515 3338.64 3342.7 897.84 661.59 30.57 30.24 0.84 · · · >-0.21 88 0.39 k 395 3338.65 3334.8 894.14 980.68 27.79 27.77 0.04 1.63 >1.58 79 0.07 37 3338.66 3306.8 890.33 2099.85 28.96 28.83 0.31 · · · · · · 95 0.01 abkn 178 3338.67 3317.5 888.57 1671.46 30.52 30.12 0.72 >-0.56 >-0.82 97 0.13 669 3338.67 3348.3 887.25 437.76 31.69 30.55 <1.16 · · · · · · 98 0.78 afikn 145 3338.68 3315.9 883.27 1737.12 31.63 30.44 0.99 >-1.13 >-1.27 109 0.84 4 3338.68 3357.4 885.05 75.76 29.07 28.79 <0.66 · · · · · · 96 0.02 dehkn 96 3338.69 3311.9 880.31 1896.85 27.62 27.58 0.16 · · · · · · 157 0.03 kn 10173 3338.70 3349.5 879.48 392.73 29.65 28.17 0.71 · · · · · · 133 0.00 gjkn 119 3338.75 3313.7 864.69 1822.33 30.05 29.85 <0.49 · · · · · · 89 0.08 kn 394 3338.76 3334.7 860.24 984.43 28.98 28.90 0.65 >0.75 >1.16 90 0.01 648 3338.76 3348.3 861.34 438.66 30.46 29.27 <1.18 · · · · · · 195 0.11 afikn 207 3338.77 3319.9 858.45 1575.85 25.22 25.20 0.49 >2.89 >3.02 284 0.03 306 3338.77 3328.6 857.58 1226.35 29.59 29.56 <0.41 >0.33 >0.62 83 0.01 45 3338.78 3307.6 855.48 2068.22 25.69 25.65 0.57 · · · · · · 212 0.03 akn 174 3338.79 3317.4 851.49 1675.68 29.23 29.20 0.13 >0.45 >0.07 76 0.12 641 3338.79 3347.9 851.45 456.67 31.45 29.58 1.06 · · · · · · 193 0.87 fikn 349 3338.82 3331.9 844.17 1097.26 27.21 27.16 0.17 0.47 1.58 239 0.02 a 90 3338.83 3311.6 841.70 1908.16 30.76 30.79 0.90 · · · · · · 40 0.97 kn 533 3338.83 3344.1 839.92 607.89 28.72 28.67 -0.22 · · · >0.47 61 0.85 k 138 3338.84 3315.0 836.56 1772.30 31.14 30.52 <1.46 · · · · · · 73 0.93 kn 424 3338.84 3337.2 836.60 882.61 25.25 25.20 0.27 1.52 >3.30 359 0.03 562 3338.86 3346.4 831.81 517.32 30.21 30.09 <0.72 · · · · · · 63 0.44 kn 550 3338.87 3345.7 829.29 542.75 32.01 31.16 <1.26 · · · >-2.06 71 0.78 k 593 3338.87 3349.9 828.05 374.32 26.46 26.45 0.07 · · · · · · 102 0.03 kn 64 3338.89 3310.1 823.04 1968.47 23.68 23.65 0.45 · · · · · · 544 0.03 kn 478 3338.91 3340.6 815.88 748.79 30.83 29.86 <1.24 · · · >0.10 158 0.11 k 619 3338.91 3347.4 817.38 473.57 30.63 30.43 <1.19 · · · · · · 139 0.86 bfikn 363 3338.94 3332.6 806.89 1067.48 29.01 28.50 0.46 >-0.25 >0.85 181 0.01 a 563 3338.94 3346.5 807.81 512.45 29.99 29.36 0.25 · · · · · · 139 0.01 fikn 481 3338.95 3340.7 805.97 741.56 31.15 30.05 <1.41 · · · >-0.46 160 0.80 k 33 3338.97 3304.2 798.19 2203.79 30.05 29.73 <0.28 · · · · · · 59 0.97 kn 629 3339.00 3347.7 790.07 464.36 30.88 30.56 <1.15 · · · · · · 77 0.90 kn 581 3339.00 3348.7 788.96 421.97 30.47 30.23 <0.91 · · · · · · 75 0.34 kn

– 39 –

Table 2—Continued

ID HDFS J22r−60d x y m_i m_a clr-lp nuv-clr fuv-clr r_h s/g flags

121 3339.01 3313.8 788.74 1819.80 29.79 29.65 <0.30 · · · · · · 69 0.28 kn 356 3339.01 3332.2 788.74 1081.48 28.82 28.29 0.80 >-0.09 >0.25 227 0.00 410 3339.01 3335.7 786.52 942.93 30.40 29.83 0.49 >-1.25 >0.02 108 0.01 292 3339.03 3327.5 782.57 1269.76 31.56 30.80 <1.00 >-0.97 >-0.68 71 0.76 343 3339.03 3331.2 781.93 1124.79 28.79 28.65 0.63 >0.52 >1.07 93 0.02 632 3339.03 3352.5 782.90 270.34 31.51 31.31 <0.83 · · · · · · 57 0.90 kn 666 3339.05 3354.7 774.46 185.12 31.05 30.79 <0.65 · · · · · · 66 0.94 kn 31 3339.06 3306.2 771.22 2122.41 25.33 25.31 0.69 · · · · · · 175 0.03 kn 436 3339.06 3337.2 773.22 884.12 30.47 30.34 <0.91 >-0.67 >0.33 67 0.14 214 3339.09 3320.1 763.34 1566.80 30.44 29.83 <0.63 >-0.86 >-0.15 148 0.94 ab 148 3339.10 3316.2 761.05 1722.30 28.69 28.60 0.37 0.56 >-0.14 74 0.55 299 3339.11 3323.6 757.17 1426.22 31.25 30.82 <1.18 >-1.09 >-0.43 66 0.90 258 3339.11 3325.0 758.66 1372.64 28.19 27.78 0.16 >0.27 >1.15 277 0.00 314 3339.11 3329.0 758.29 1209.82 30.82 30.38 <0.57 >-1.22 >-0.45 102 0.95 b 549 3339.13 3345.6 752.21 547.19 31.42 29.88 <0.94 · · · >-0.64 157 0.90 k 633 3339.13 3347.9 751.54 454.26 27.20 27.18 0.58 · · · · · · 130 0.03 kn 676 3339.14 3355.7 749.43 141.60 26.96 26.91 0.23 · · · · · · 96 0.03 kn 209 3339.15 3320.9 747.39 1536.73 27.03 26.98 0.20 0.46 >2.05 170 0.03 ab 42 3339.16 3303.9 741.58 2216.66 29.88 29.72 0.66 · · · · · · 72 0.23 ehkn 208 3339.16 3320.2 744.27 1564.31 28.11 27.79 0.17 >0.60 1.37 196 0.02 ab 125 3339.19 3314.3 733.72 1797.47 25.82 25.78 0.09 · · · · · · 267 0.03 kn 405 3339.19 3335.3 732.98 958.53 31.45 30.96 1.22 >-1.28 >-1.04 55 0.88 360 3339.20 3332.2 730.66 1085.23 31.64 30.32 <1.31 >-1.39 >-1.29 143 0.86 351 3339.21 3331.7 728.15 1101.85 30.40 30.18 <0.66 >-0.99 >-0.90 71 0.14 539 3339.21 3345.1 728.01 566.21 30.79 30.17 0.68 · · · >-2.25 85 0.95 ko 56 3339.22 3304.1 723.98 2207.54 29.89 29.55 0.46 · · · · · · 92 0.52 kn 384 3339.23 3324.4 723.28 1396.72 31.31 30.70 0.95 >-1.05 -0.42 67 0.91 471 3339.23 3340.1 722.34 766.96 30.91 30.48 <0.75 >-1.04 >0.15 104 0.88 614 3339.23 3350.0 723.62 372.01 30.96 30.67 <0.67 · · · · · · 74 0.19 kn 62 3339.24 3308.5 718.09 2030.21 28.53 28.41 -0.02 · · · · · · 86 0.10 kn 679 3339.26 3355.9 713.49 137.22 27.98 27.87 0.42 · · · · · · 101 0.03 abkn 390 3339.28 3334.1 707.45 1008.86 30.87 30.60 <0.68 >-0.91 >0.21 58 0.94 30 3339.29 3306.7 705.88 2102.39 26.55 26.46 0.47 · · · · · · 147 0.03 abkn 463 3339.30 3339.5 702.65 789.86 29.79 29.86 0.03 >-0.67 -0.88 56 0.25 680 3339.31 3356.0 699.02 132.96 27.08 26.98 0.50 · · · · · · 156 0.03 abkn 13 3339.32 3303.4 694.40 2235.75 26.29 26.08 0.77 · · · · · · 261 0.03 aehkn 332 3339.32 3330.3 695.56 1158.14 29.36 29.24 0.23 >0.04 >-0.06 78 0.01 342 3339.35 3323.1 686.36 1446.03 26.31 26.30 0.09 >2.01 >2.40 86 0.60 ab 359 3339.35 3332.2 687.41 1084.87 30.88 30.09 <1.18 >-1.40 >-0.95 99 0.95 388 3339.35 3333.9 688.44 1014.05 29.77 29.76 <0.34 >-0.60 >-0.19 55 0.42 450 3339.35 3338.6 687.77 828.67 27.81 27.77 0.23 >0.45 >0.76 135 0.03 29 3339.36 3306.2 684.68 2122.86 24.94 24.76 0.43 · · · · · · 488 0.03 abkn 106 3339.39 3312.6 674.86 1866.37 30.19 29.98 <0.43 · · · · · · 82 0.01 kn 198 3339.41 3318.6 670.76 1625.66 31.06 30.40 <0.96 >-1.06 >-1.19 80 0.58 624 3339.41 3352.0 670.09 290.57 31.36 30.81 1.57 · · · · · · 72 0.88 kn 323 3339.42 3329.5 667.50 1191.38 29.88 29.74 <0.26 >-0.79 >-1.48 84 0.11 415 3339.42 3336.2 666.88 924.02 28.71 28.52 -0.47 >-0.50 >-0.17 131 0.01 328 3339.43 3330.1 662.45 1168.22 31.29 31.03 <0.87 >-2.17 >-2.32 49 0.90 241 3339.44 3322.8 661.27 1459.97 25.19 25.17 0.37 >1.52 >1.65 318 0.03 b 310 3339.44 3328.7 661.70 1224.06 30.54 30.41 0.55 >-1.87 -2.17 81 0.24 451 3339.45 3338.6 657.88 828.66 30.94 30.12 <1.14 >-1.97 >-1.22 115 0.92 81 3339.46 3310.7 654.80 1942.59 27.22 27.20 0.41 · · · · · · 107 0.05 kn

– 40 –

Table 2—Continued

ID HDFS J22r−60d x y m_i m_a clr-lp nuv-clr fuv-clr r_h s/g flags

108 3339.46 3312.7 653.69 1861.52 29.26 29.11 0.31 · · · · · · 82 0.33 kn 183 3339.46 3318.0 653.60 1650.67 26.86 26.83 0.38 >1.10 1.37 137 0.03 526 3339.48 3343.4 649.14 634.34 30.98 30.98 <1.00 · · · >-1.28 74 0.85 ak 689 3339.48 3357.2 648.67 83.78 30.63 29.71 <0.22 · · · · · · 97 0.97 hkn 114 3339.50 3313.0 641.60 1851.70 31.02 30.14 <0.63 · · · · · · 103 0.87 akn 621 3339.51 3351.7 640.55 301.57 30.96 30.45 <1.21 · · · · · · 77 0.18 kn 220 3339.52 3320.4 637.32 1553.93 30.49 29.64 <1.03 >-1.25 >-0.35 135 0.46 594 3339.53 3350.1 634.82 366.80 26.72 26.68 0.42 · · · · · · 146 0.03 kn 617 3339.54 3351.3 631.45 319.60 29.95 29.47 <0.71 · · · · · · 112 0.01 kn 107 3339.55 3312.6 627.50 1869.26 31.26 30.65 0.99 · · · · · · 80 0.79 kn 470 3339.55 3340.1 628.32 769.17 30.14 29.82 0.30 >-1.39 >-0.96 81 0.32 429 3339.56 3336.7 626.47 902.11 28.53 28.50 0.70 >-0.65 >0.41 73 0.78 320 3339.58 3328.1 618.27 1246.28 30.86 30.20 0.72 >-1.71 >-1.97 83 0.85 372 3339.58 3333.9 620.10 1013.64 26.88 26.67 0.19 0.19 >0.63 305 0.00 o 127 3339.59 3314.1 617.27 1805.63 29.21 29.01 0.65 · · · · · · 108 0.01 kn 604 3339.60 3350.7 613.83 344.51 28.27 28.04 -0.04 · · · · · · 145 0.02 akn 683 3339.60 3356.2 614.07 122.89 30.35 30.01 <0.84 · · · · · · 67 0.97 kn 158 3339.61 3316.7 611.41 1703.48 28.80 28.49 0.12 >-0.42 · · · 179 0.00 n 84 3339.62 3310.7 606.95 1944.88 31.16 30.54 <1.07 · · · · · · 96 0.85 kn 440 3339.62 3337.7 607.97 863.34 30.54 30.19 <0.41 >-2.01 >-1.42 92 0.60 lo 296 3339.64 3327.8 601.96 1259.65 30.73 30.47 0.93 >-2.20 >-1.80 74 0.62 505 3339.66 3342.1 594.44 685.98 31.17 30.35 <1.15 · · · · · · 100 0.87 kn 55 3339.67 3308.5 593.38 2030.70 25.88 25.66 0.33 · · · · · · 275 0.03 abkn 136 3339.68 3314.9 590.55 1776.20 29.68 28.92 0.66 · · · · · · 182 0.02 kn 94 3339.69 3311.8 585.52 1900.10 28.39 28.25 0.20 · · · · · · 152 0.01 kn 674 3339.69 3355.9 587.74 136.97 27.17 26.81 0.65 · · · · · · 249 0.03 kn 634 3339.70 3352.6 583.61 267.95 31.57 30.90 0.91 · · · · · · 65 0.85 kn 215 3339.71 3320.1 579.64 1568.17 30.38 29.87 <0.80 >-1.72 >-1.49 92 0.81 658 3339.73 3353.2 575.93 244.04 31.28 30.59 <1.28 · · · · · · 83 0.89 kn 54 3339.74 3308.5 571.35 2030.73 24.49 24.38 0.31 · · · · · · 471 0.03 abkn 361 3339.74 3332.2 571.26 1082.31 29.81 29.78 <0.02 · · · · · · 84 0.01 kn 553 3339.75 3345.9 568.06 534.99 31.38 30.77 <1.63 · · · · · · 72 0.81 kn 97 3339.77 3311.7 561.69 1903.07 30.07 29.83 <0.19 · · · · · · 71 0.25 kn 598 3339.77 3350.0 561.94 370.70 29.55 29.36 0.36 · · · · · · 77 0.02 kn 249 3339.78 3323.3 560.88 1439.02 26.04 26.05 0.76 >1.71 >1.97 64 0.99 516 3339.78 3342.8 559.97 658.98 29.38 29.22 0.79 · · · · · · 72 0.23 kn 197 3339.81 3318.1 551.41 1645.91 27.89 27.79 0.39 >-0.19 · · · 170 0.02 n 297 3339.82 3327.9 547.46 1254.69 31.55 30.79 <1.39 · · · · · · 82 0.85 kn 308 3339.83 3328.8 546.88 1218.37 27.69 27.69 -0.49 >1.91 >1.96 138 0.03 lo 93 3339.84 3311.7 543.08 1904.25 29.13 29.04 0.26 · · · · · · 88 0.01 kn 357 3339.86 3332.1 536.42 1089.18 30.93 30.04 <1.00 · · · · · · 129 0.59 kn 595 3339.87 3350.0 534.67 371.01 28.95 28.84 0.08 · · · · · · 80 0.03 kn 82 3339.91 3310.6 522.50 1945.41 29.69 29.27 0.28 · · · · · · 115 0.01 kn 304 3339.92 3324.0 520.16 1411.36 27.49 27.49 0.03 · · · · · · 81 0.04 kn 171 3339.93 3317.2 516.79 1684.95 31.49 30.59 <1.45 >-4.11 · · · 83 0.78 ln 391 3339.95 3334.2 510.86 1003.28 30.66 30.47 0.59 · · · · · · 70 0.84 kn 14 3339.98 3305.1 502.50 2167.46 21.40 21.39 0.73 · · · · · · 739 0.03 aehkn 492 3339.98 3341.2 501.85 722.24 31.13 30.89 <1.26 · · · · · · 55 0.89 kn 402 3339.99 3335.0 497.60 972.47 29.66 29.59 <0.52 · · · · · · 89 0.01 kn 479 3340.00 3340.7 496.46 743.32 31.46 30.78 <1.28 · · · · · · 78 0.88 kn 188 3340.01 3317.9 491.90 1655.27 31.47 31.04 <1.12 · · · · · · 58 0.89 kn 544 3340.01 3345.3 491.62 558.92 31.38 31.01 <1.10 · · · · · · 50 0.88 kn

– 41 –

Table 2—Continued

ID HDFS J22r−60d x y m_i m_a clr-lp nuv-clr fuv-clr r_h s/g flags

513 3340.02 3342.6 488.36 669.05 31.35 30.85 <1.18 · · · · · · 75 0.91 kn 671 3340.02 3355.2 489.89 162.65 30.98 30.45 <0.42 · · · · · · 80 0.95 kn 437 3340.04 3337.3 483.26 877.89 30.74 30.17 <0.55 · · · · · · 98 0.14 kn 246 3340.11 3323.2 463.05 1443.51 27.41 27.39 0.26 · · · · · · 109 0.03 kn 401 3340.11 3334.9 462.68 976.40 30.22 29.69 <0.42 · · · · · · 103 0.19 kn 362 3340.12 3332.4 458.77 1076.56 30.46 29.80 1.22 · · · · · · 122 0.05 kn 144 3340.13 3316.6 458.12 1708.07 25.18 25.20 0.72 · · · · · · 128 0.93 kn 337 3340.17 3330.8 444.75 1139.28 30.27 29.78 <0.22 · · · · · · 106 0.08 kn 540 3340.19 3345.3 439.25 560.23 29.41 29.23 0.24 · · · · · · 106 0.01 kn 582 3340.20 3348.9 437.05 413.71 28.17 27.91 0.13 · · · · · · 148 0.02 kn 561 3340.21 3346.6 434.70 508.99 26.23 26.18 0.61 · · · · · · 204 0.03 kn 677 3340.21 3355.8 433.23 139.83 28.87 28.64 0.35 · · · · · · 151 0.01 kn 609 3340.22 3351.4 430.35 315.36 26.27 26.13 0.04 · · · · · · 309 0.00 bkn 206 3340.25 3319.5 420.82 1591.13 30.20 29.71 <0.87 · · · · · · 115 0.09 kn 71 3340.28 3309.9 412.40 1977.10 31.20 31.15 <0.96 · · · · · · 78 0.82 bkn 586 3340.30 3349.4 405.99 395.08 31.60 31.29 <1.00 · · · · · · 48 0.86 kn 120 3340.33 3313.7 396.70 1824.45 31.37 31.20 <0.88 · · · · · · 57 0.93 kn 313 3340.33 3328.9 398.11 1214.14 29.25 29.18 -0.06 · · · · · · 102 0.01 kn 69 3340.35 3309.8 392.78 1978.63 30.45 29.82 <1.09 · · · · · · 117 0.14 kn 498 3340.35 3341.8 392.57 698.00 28.78 28.60 0.47 · · · · · · 107 0.03 kn 608 3340.35 3351.0 392.81 330.66 26.25 26.24 -0.03 · · · · · · 128 0.03 abkn 191 3340.38 3318.7 384.20 1621.99 25.17 25.15 0.29 · · · · · · 275 0.03 kn 464 3340.41 3339.8 375.42 779.82 28.63 28.53 0.61 · · · · · · 156 0.01 kn 520 3340.41 3343.2 373.60 645.20 26.68 26.55 0.28 · · · · · · 290 0.00 kn 264 3340.42 3325.1 371.80 1365.35 26.93 26.90 0.63 · · · · · · 102 0.03 kn 380 3340.42 3333.7 370.62 1023.09 27.88 27.68 0.28 · · · · · · 154 0.03 kn 507 3340.45 3342.3 363.99 680.14 31.55 31.56 <1.13 · · · · · · 49 0.83 kn 655 3340.45 3354.1 362.39 208.30 26.44 26.43 0.14 · · · · · · 97 0.03 kn 427 3340.47 3336.7 357.24 904.70 28.30 27.94 0.06 · · · · · · 205 0.01 kn 124 3340.50 3314.0 348.99 1813.25 31.96 30.91 <1.52 · · · · · · 73 0.82 kn 501 3340.50 3342.1 347.22 686.32 28.15 27.96 0.02 · · · · · · 177 0.02 kn 560 3340.50 3346.3 347.43 519.74 28.97 28.75 0.68 · · · · · · 112 0.01 kn 166 3340.51 3317.0 343.45 1693.28 30.60 30.18 <1.12 · · · · · · 88 0.19 kn 556 3340.52 3345.9 343.50 534.16 30.97 30.70 <1.16 · · · · · · 61 0.92 kn 268 3340.53 3325.4 337.57 1356.41 30.23 29.64 <0.90 · · · · · · 114 0.11 kn 315 3340.53 3329.1 339.90 1206.27 29.41 29.14 -0.02 · · · · · · 152 0.00 kn 23 3340.57 3305.2 327.26 2164.22 30.15 29.90 0.16 · · · · · · 67 0.92 kn 336 3340.57 3330.9 326.00 1136.77 28.86 28.79 0.07 · · · · · · 90 0.01 kn 122 3340.61 3313.8 314.68 1817.92 30.85 30.51 <0.59 · · · · · · 70 0.57 kn 218 3340.61 3320.1 315.35 1569.14 30.80 30.44 0.44 · · · · · · 67 0.93 kn 267 3340.61 3325.2 316.73 1363.68 30.77 30.86 <1.02 · · · · · · 40 0.96 kn 422 3340.61 3336.4 316.40 915.23 30.13 29.87 <0.43 · · · · · · 106 0.96 bkn 480 3340.63 3340.8 309.03 737.88 28.40 28.12 0.62 · · · · · · 148 0.02 kn 638 3340.65 3352.7 304.46 262.79 30.98 30.52 <1.23 · · · · · · 60 0.95 kn 397 3340.66 3334.7 301.88 984.73 29.47 29.33 <0.46 · · · · · · 102 0.02 kn 589 3340.66 3349.7 300.60 382.94 26.17 26.17 0.67 · · · · · · 66 0.98 kn 143 3340.67 3315.5 298.02 1749.95 30.09 29.85 <0.69 · · · · · · 89 0.40 kn 115 3340.69 3313.2 292.94 1843.22 30.20 30.03 <0.68 · · · · · · 61 0.70 kn 260 3340.69 3324.8 292.40 1380.84 30.07 30.00 <-0.07 · · · · · · 57 0.38 kn 312 3340.69 3328.7 293.12 1222.92 29.68 29.27 <0.77 · · · · · · 143 0.01 kn 649 3340.71 3353.4 284.73 234.05 30.88 30.25 <1.33 · · · · · · 63 0.95 kn 22 3340.72 3305.0 282.41 2172.15 30.80 30.55 <0.88 · · · · · · 54 0.97 kn

– 42 –

Table 2—Continued

ID HDFS J22r−60d x y m_i m_a clr-lp nuv-clr fuv-clr r_h s/g flags

468 3340.73 3339.6 280.77 788.99 30.11 29.80 <1.00 · · · · · · 99 0.25 kn 508 3340.73 3341.6 280.54 707.17 30.83 30.33 <1.31 · · · · · · 57 0.97 kn 57 3340.74 3307.9 275.84 2054.70 30.90 30.18 0.45 · · · · · · 78 0.95 kn 59 3340.74 3308.3 277.69 2037.43 30.85 30.21 <1.01 · · · · · · 81 0.95 kn 170 3340.75 3316.8 274.55 1699.60 30.70 30.39 <0.43 · · · · · · 108 0.25 kn 76 3340.76 3309.2 270.69 2004.14 29.90 29.56 1.21 · · · · · · 116 0.08 kn 502 3340.76 3341.8 272.46 697.71 30.70 29.63 <0.92 · · · · · · 135 0.93 kn 378 3340.78 3333.6 266.18 1027.66 28.64 28.57 0.10 · · · · · · 129 0.02 kn 636 3340.78 3352.7 266.31 264.62 30.28 29.65 <1.24 · · · · · · 95 0.95 kn 213 3340.81 3320.3 254.93 1557.44 26.04 26.00 0.29 · · · · · · 181 0.03 kn 341 3340.81 3331.1 256.46 1127.84 30.47 29.66 <0.91 · · · · · · 120 0.12 kn 434 3340.82 3337.0 252.96 893.32 29.82 30.07 <0.97 · · · · · · 69 0.60 kn 523 3340.82 3343.2 253.67 643.19 29.25 28.96 -0.08 · · · · · · 96 0.03 kn 547 3340.82 3345.5 252.54 549.64 28.84 28.53 <0.43 · · · · · · 93 0.04 kn 578 3340.82 3349.0 254.82 412.47 24.43 24.44 0.33 · · · · · · 157 0.03 kn 449 3340.83 3338.3 249.47 839.86 30.73 30.53 0.87 · · · · · · 57 0.96 kn 386 3340.85 3333.8 245.62 1018.59 29.78 29.43 <0.59 · · · · · · 93 0.13 kn 603 3340.85 3350.5 244.74 352.09 29.17 28.99 <0.32 · · · · · · 97 0.01 kn 3 3340.85 3357.3 245.73 80.81 28.43 28.54 0.60 · · · · · · 89 0.52 aekn 17 3340.86 3304.7 242.73 2184.57 30.17 30.22 0.25 · · · · · · 48 0.93 ehkn 184 3340.89 3317.7 231.63 1663.71 30.89 29.97 <1.19 · · · · · · 104 0.85 kn 63 3340.90 3308.6 231.06 2027.66 29.24 29.10 -0.26 · · · · · · 81 0.19 kn 488 3340.92 3341.1 225.04 728.68 29.32 28.53 <0.76 · · · · · · 145 0.03 kn 140 3340.93 3315.7 221.71 1744.80 28.56 28.28 0.49 · · · · · · 105 0.38 bkn 276 3340.93 3325.9 221.88 1335.38 28.20 28.17 0.58 · · · · · · 85 0.03 kn 579 3340.93 3348.7 221.51 425.17 29.85 29.48 <1.30 · · · · · · 86 0.71 ekn 139 3340.95 3315.2 213.77 1763.64 27.66 27.59 0.50 · · · · · · 83 0.37 abkn 72 3340.96 3309.9 213.51 1973.75 31.34 30.29 <0.90 · · · · · · 86 0.90 kn 257 3340.96 3324.7 213.21 1381.46 30.14 29.97 0.43 · · · · · · 124 0.05 kn 527 3340.97 3343.5 209.78 631.76 29.23 28.99 <1.04 · · · · · · 102 0.73 kn 522 3340.99 3343.1 202.09 647.88 30.98 30.21 <1.79 · · · · · · 77 0.97 kn 83 3341.03 3310.6 192.42 1949.03 31.29 31.23 <1.52 · · · · · · 44 0.91 kn 387 3341.06 3333.9 183.88 1016.69 28.84 28.57 -0.04 · · · · · · 90 0.37 kn 443 3341.11 3337.8 166.67 857.97 29.91 30.09 <1.27 · · · · · · 51 0.82 ehkn 15 3341.12 3304.6 165.61 2189.27 28.51 28.47 0.26 · · · · · · 71 0.07 ehkn 74 3341.15 3310.5 155.14 1952.26 27.47 27.33 0.29 · · · · · · 236 0.03 bkn 113 3341.15 3313.0 156.15 1852.35 30.69 30.20 <1.14 · · · · · · 79 0.97 kn 322 3341.19 3329.6 143.12 1188.50 29.29 29.04 0.57 · · · · · · 84 0.02 bekn 73 3341.21 3310.1 138.29 1968.22 28.72 28.28 0.30 · · · · · · 126 0.02 abkn 294 3341.21 3327.8 138.20 1259.52 26.60 26.58 0.61 · · · · · · 91 0.03 ekn 321 3341.21 3329.8 137.71 1180.86 30.44 30.25 <1.04 · · · · · · 65 0.97 abekn 112 3341.23 3313.0 133.45 1853.01 29.61 28.98 <0.51 · · · · · · 91 0.91 kn 156 3341.24 3316.4 130.68 1715.22 29.11 28.23 <0.45 · · · · · · 233 0.01 kn 311 3341.26 3328.7 122.92 1223.94 30.59 30.42 <1.30 · · · · · · 38 0.94 ehkn 285 3341.30 3327.0 110.67 1291.43 28.25 28.21 0.62 · · · · · · 93 0.02 ehkn 280 3341.33 3326.6 103.41 1306.47 28.47 28.47 0.65 · · · · · · 80 0.06 aehkn 240 3341.35 3322.0 95.88 1492.90 29.70 29.64 <0.30 · · · · · · 63 0.72 ehkn 87 3341.43 3311.1 73.39 1928.09 30.81 30.07 <0.80 · · · · · · 78 0.97 dekn 190 3341.44 3318.0 70.10 1650.50 30.56 30.43 <0.67 · · · · · · 49 0.96 dehkn 109 3341.52 3313.0 46.50 1852.47 25.99 25.73 0.22 · · · · · · 278 0.03 adehkn

– 43 –

Table 2—Continued

NOTE — Flags: a: Object has near neighbors (50CCD). b: Object was orignally blended with another (50CCD). c: At least one pixel is saturated (50CCD). d: Object’s aperture data is incomplete or corrupted (50CCD). e: Object is off the image, or within 30 pixels of the edge (50CCD). f: Object lies on top of a diffraction spike (50CCD). g: Photometry is from the second run of SExtractor (50CCD). h: Object is off the image, or within 30 pixels of the edge (F28X50LP). i: Object lies on top of a diffraction spike (F28X50LP). j: Photometry is from the second run of SExtractor (F28X50LP). k: Object is completely off the image (NUV). l: Object is partially off the image (NUV). m: Used global sky value (NUV). n: Object is completely off the image (FUV). o: Object is partially off the image (FUV). p: Used global sky value (FUV). q: Target QSO J2233-606.

– 44 –

Table 3. Source Counts

AB mag N_{auto} log(N_{auto}) N_{iso} log(N_{iso})

22.75 3 4.46 1 3.99 23.25 2 4.29 2 4.29 23.75 2 4.29 3 4.46 24.25 5 4.68 1 3.99 24.75 7 4.83 5 4.68 25.25 9 4.94 12 5.07 25.75 13 5.10 8 4.89 26.25 19 5.26 15 5.16 26.75 16 5.19 18 5.24 27.25 19 5.26 17 5.22 27.75 28 5.43 17 5.22 28.25 36 5.54 23 5.35 28.75 62 5.78 42 5.61 29.25 74 5.86 55 5.73 29.75 111 6.03 56 5.73 30.25 102 5.99 92 5.95 30.75 72 5.84 82 5.90 31.25 27 5.42 92 5.95 31.75 1 3.99 63 5.79 32.25 1 3.99 8 4.89

Note. — The 50CCD source counts. Magnitudes are in the AB magnitude system. The counts are given for the SExtractor mag auto, which uses an elliptical aperture set at 2.5 times the first moment of the semi-major and semi-minor axes. We also give the counts as determined using isophotal magnitudes. Column 1 is the center of the magnitude bin, columns 2 & 4 contain the raw number of objects per bin in the image, and columns 3 & 5 contain the log of the number per magnitude per square degree.