arXiv:cond-mat/0001016 v3 21 Jan 2000

Hysteresis measurement of anomalous microwave surface resistance in

superconducting thin films

X.S.Rao, C.K.Ong, B.B.Jin and Y.P.Feng

Centre for superconducting and Magnetic Materials and Department of Physics, National

University of Singapore, Singapore  119260

          The anomalous decrease in microwave surface resistance, R

s

, of superconducting YBa

2

Cu

3

O

7 -d
(YBCO) thin films in the presence of a low dc magnetic field is studied using a microstrip

resonator technique. We have done a dc field hysteresis measureme nt of R

s

 to study the effects of

vortex penetration on the anomalous effect. It is shown that the anomaly happens at a field level

far below the low critical field, H

                                                                                                              c1,strip

, of the superconducting microstrip and vortex (Abrikosov)

penetration would elimi nate the anomalous effect observed at low field . This implies that the

anomalous effect is not contributed by vortices.

          Recently, several low - field microwave

surface resistance (R

                                                                          s

                                                                            ) anomalies, i.e., R

s
decreases at low dc magnetic field (H

dc

) and

micro wave magnetic field (H

                                                                                                     mw

                                                                                                           ), has been

observed [1 - 5]. In a previous paper [5], we

studied the anomaly observed in YBCO thin

films and showed that the R

                                                                                                  s

                                                                                                    (H

                                                                                                            dc

                                                                                                                ) curve for

H

      dc

         // c - axis and H

                                                          dc

                                                             ^ c - axis can coincide with

each other through a normalization

procedure and the anomaly was qualitatively

independent of the dc field alignment.  It is

usually accepted that low - field microwave

responses of HTS are mainly related with

weak links and vortices [6,7]. As shown in [6],

vortex mechanisms would have a pronounced

angu lar dependence of the field effect on R

s

,

which comes from the anisotropy of YBCO.

On the other hand, the angular dependence of

the dc - field effect on R

                                                                                  s

                                                                                     for the weak - link

mechanism is negligible since weak links are

chaotically oriented [8]. Thus we suppo se that

the anomaly is not related to vortices and

may come from weak links. To further

confirm that vortices have no contribution on

the anomaly observed, we have done a  large

dc field hysteresis measurement of the R

s

. We

have shown that the anomaly happe ns at a

field level far below the lower critical field for
vortex generation and vortices cannot account

for the anomalous R

s

 decrease.

The sample preparation and measurement

were shown in [5]. The dc field is applied

perpendicular with the film surface (// c - axis)

using a Helmholtz coil configuration. The

sample is initially cooled down to 77 K in zero

field (ZFC). The dc field is ramped from zero

to 2000 Oe and then decreased back to zero.

The experimental results are shown in Fig.1

for the microstrip re sonator working at 1.1

GHz with the input microwave power P

mw

= - 10

dBm.

The R

s

(H

dc

) curve in increasing field is

characterized by a negative slope in the

lowest field range (H

dc

<6 Oe) where R

s

 drops

sharply as the dc field is increased. Then R

s
increases gr adually with elevated H

dc

. After

that, a plateau, where the R

s

 has a weaker

dependence on field, is reached. This region

extends roughly from R

s

(H

dc

) ~ 20 Oe to 70 Oe.

At higher fields (H

dc

>70 Oe) R

s

 increases

again and the slope of R

s

(H

dc

) curve is steep.

A fter reaching the largest dc field,

H

dc
max =2000 Oe, the dc field was subsequently

decreased. In the field range H

dc

>70 Oe the

R

s

(H

dc

) curve in decreasing field coincides

with that in increasing field and no hysteretic

                                        effect is found within the experimenta l error.

                                        When the dc field falls below 70 Oe, an

                                        obvious hysteretic loop can be observed in the

                                        figure where the R
                                                                                                       s

                                                                                                         (H
                                                                                                                 dc

                                                                                                                     ) curve in decreasing

                                        field strongly deviates from that in increasing

                                        field. The R
                                                                                 s

                                                                                   (H
                                                                                           dc

                                                                                              ) is almost constant in the

                                        region from 70 Oe to z ero field. The final R
s
                                        value at zero dc field is slightly larger than

                                        its initial value.

                                                 The lower critical field of the

                                        superconducting YBCO strip, H
c1,strip

~ 70 Oe,

                                        can be deduced from Fig.1. In the increasing

                                        field range, R
                                                                                      s

                                                                                        (H
                                                                                                dc

                                                                                                    ) is slightly dependent on

                                        the field below H
                                                                                                   c1,strip

                                                                                                                except the anomalous

                                        region (ranging from 0 to 20 Oe). At H
c1,strip

, dc

                                        vortices (Abrikosov) begin to penetrate into

                                        the films and cause the steep increase in

                                        R
                                            s

                                              (H
                                                      dc

                                                          ). When the field is increased up to 2000

                                        Oe and then decrease d below H
c1,strip

, some

                                        vortices are trapped in the films due to

                                        pinning effect. This is the cause for the

                                        plateau of the R
                                                                                           s

                                                                                            (H
                                                                                                     dc

                                                                                                        ) curve in decreasing field

                                        observed below 70 Oe. It is noticed that the

                                        H
                                             c1,strip

                                                           (~70 Oe) is different from the bulk H
c1
                                        for single crystalline YBCO measured by Wu

                                        et al . [9]. The difference may come from the

                                        large demagnetization effect [10] and the

                                        screening effect due to the superconducting

                                        ground plane. So it is clear that the

                                        anomalous decrease of R
s

 happens at a field
leve l ( ~ 6 Oe) far below the low critical field of

the superconducting microstrip, where no

vortex (Abrikosov) is formed. This is

consistent with our previous result that

shows the anomalous effect is qualitatively

independent of the dc field alignment at low

f ield [5].

The other important feature revealed by

Fig.1 is that the anomalous field dependence

of R
s

 in weak dc field can only be observed in

increasing field. In the R
s

(H
dc

) curve of

decreasing field, the pinned vortices totally

eliminate the anomalous ef fect observed in

increasing field.

From the above results, we can conclude

that the anomalous decrease of R
s

 at low dc

magnetic field is not contributed by vortices.

So one may expect that the anomalous effect

is related with weak links in the YBCO films.

In fact, we have carried out a comparison

study of two films with different film

qualities and our preliminary results show

that the film with more weak links has a

stronger anomalous effect. A systematic

study of the correlation between the

anomalous effe ct and the microstructure of

the YBCO thin films is in progress.

1. D. P. Choudhury et al., IEEE Trans. Appl.

Supercond., 7 (1997) 1260 .

2. M. A. Hein et al., J. Supercond., 10  (1997)

485.

3. A. P. Kharel et al., Phy. Rev. B , 58  (1998)

11189.

4. A. P. Kharel et al.,  IEEE Trans. Appl.

Supercond., 9 (1999) 2121.

5. X. S. Rao et al., Physica C, 328 (1999) 60.

6. M. A. Golosovsky, M. Tsindlekht, D.

Davidov,  Sueprcond. Sci. Technol. 9

(1996) 1.

7. J. Halbritter, J. Supercond. 8 (1995) 691.

8. M. A. Goloso vsky et al., Physica C 235 - 240

(1994) 3147.

9. D. - H. Wu and S. Sridhar, Phys. Rev. Lett.

65 (1990) 2074.

10. B. A. Willemsen, J. S. Derov, and S.

Sridhar, Phys. Rev. B56 (1997) 11989.

                                        Figure 1. Hysteretic response of R
s

(H
dc

) for

                                        H
                                             dc

                                                 max =2000 Oe.

                                                                1 10 100 1000

                                                     0.01

                                                        0.1

                                                             1

                                                          10

                                                       100

RS / R

S(0)

                                                                                                                 H
                                                                                                                       dc

 (Oe)

                                                                    0 40 80

-0.1

0.0

0.1