arXiv:cond-mat/0301081v1 [cond-mat.supr-con] 7 Jan 2003

Order parameter oscillations in Fe/Ag/Bi_2Sr_2CaCu_2O_{8+δ} tunnel junctions

Mario Freamat and K.-W. Ng Department of Physics and Astronomy, University of Kentucky, Lexington, KY 40506-0055, U.S.A. (Dated: January 15, 2022)

We have performed temperature dependent tunneling conductance spectroscopy on Fe/Ag/Bi2 Sr2CaCu2O_{8+δ} (BSCCO) planar junctions. The multilayered Fe counterelectrode was designed to probe the proximity region of the ab-plane of BSCCO. The spectra manifested a coherent oscillatory behavior with magnitude and sign dependent on the energy, decaying with increasing distance from the junction barrier, in conjunction with the theoretical predictions involving d-wave superconductors coupled with ferromagnets. The conductance oscillates in antiphase at E = 0 and E = ±Δ. Spectral features characteristic to a broken time-reversal pairing symmetry are detected and they do not depend on the geometrical characteristics of the ferromagnetic film.

PACS numbers: 74.45.+c, 74.50.+r, 75.70.-i

In recent years numerous theoretical and experimental studies have been devoted to the spin polarized transport in ferromagnet(FM)-superconductor(SC) structures. This interest is equally motivated by the rapidly developing applications, e.g. in quantum twolevel systems (qubits) based on phase shifts [1], as well as by the very interesting physics involving unconventional superconducting states. The exchange energy h in the ferromagnet leads to a spatially inhomogeneous state with the order parameter presenting phase changes by π in the proximity region at the interface with the SC. Such a modulated state is called Larkin-Ovchinnikov- Fulde-Ferrell (LOFF) from the names of the authors who first predicted it [2]. In the FM, the Cooper paired electrons have different energies and Fermi momenta, so they dephase on a scale of several ferromagnetic coherence lengths. Consequently, this region presents a diversity of intensely explored phenomena like spatially dumped oscillations of the density of states (DOS) and gapless superconductivity [3]-[6], oscillations of the superconducting critical temperature T_c and critical current I_c with the thickness of the FM electrode in layered systems [7, 8], or asymmetric zero-bias conductance peak (ZBCP) splitting [9].

An extensive attention was dedicated to the LOFF state arising in junctions between conventional SC’s and FM films of variable thickness. As example, the measurements on Al/Al_2O_3/PdNi/Nb junctions reported by the Orsay group [7] clearly show the difference in the conductance spectra at two different locations in the proximity region, indicating the order parameter change from positive (0-state) to negative values (π-state). However, the data originated from experiments involving high-Tc superconductors (HTSC) is rather scarce, even if it could be conclusive about the interaction between ferromagnetism and a more complex form of superconductivity. In particular, the superconductivity mechanism in the cuprates is far from being fully understood. According to a series of phase sensitive experiments [10] the symmetry of the order parameter is d-wave, pure or mixed with a secondary s or d component [11]. It also seems that the antiferromagnetic spin plays an important role in the pairing mechanism [12]. Therefore, it is constructive to consider that the LOFF state in the cuprates, while intrinsically interesting, may also offer information about what makes the high-Tc superconductivity different from the conventional one. A multitude of theoretical models were developed to calculate the specific transport properties, spin and charge relaxation in tunneling experiments involving d-wave HTSC with FM counterelectrodes. The most popular ones are those based on the Blonder-Tinkham- Klapwijk (BTK) approach [13, 14]. However, these models consider just the transmission and reflection processes at the interface with the FM film modeled as a semiinfinite domain. In this paper we will use a model [5] based on a ballistic quasiclassical formalism with the DOS averaged over all classical trajectories of multiple reflections in the FM domain of finite thickness d.

Hoping to contribute to the experimental information about this topic, we report in this paper the transport properties in a multilayered-Fe/Ag/Bi_2Sr_2CaCu_2O_{8−δ} (BSCCO) ab-plane oriented planar tunneling junction. The BSCCO ab-plane is probed successively from 5 overlapping Fe thin films with the same thickness, through an intermediate thin layer of Ag designed to minimize the barrier strength and avoid the appearance of a spinglass phase at the junction interface [15]. The spectra are collected on the thicker and thicker counterelectrodes and studied as function of the temperature and thickness of the FM domain. The planar junctions were built on freshly cleaved monocrystal samples of slightly underdoped BSCCO grown by the self-flux method. Two silver paste leads were attached to the crystal and its lower side was molded in epoxy resin. Before the epoxy dried, the upper side was fixed between two quartz glass slabs with coplanar surfaces. The epoxy penetrated between the sides of the slabs so that the crystal was caught between two smooth glass surfaces attached by

FIG. 1: Junction layout. The layered Fe/Ag conterelectrode is deposited perpendicular on the BSCCO ab-plane.

thin epoxy walls. While the surface of the glass was protected, we performed a clean mechanical polishing along the ab-plane of the crystal, laterally embedded in epoxy. We monitored the process with a profilometer, until the exposed edge of the crystal was at the same level as the glass surfaces. The counterelectrode sandwich was then evaporated using a metallic shadow mask shaped as in Fig. 1, forming thin film strips 0.1 mm in width. The deposition was controlled using a calibrated quartz thickness-monitor. Above a 30Å silver film, five 30Å iron films were deposited at a rate of 0.1Å/s for uniformity [16]. The residual resistivity ratio of the Fe film RRR = R(300K)/R(40K) ≈ 8.3 indicates a good deposition quality. The tunneling barrier is formed naturally on the exposed edge of BSCCO. It had a resistance R_B (300K) ≈ 450Ω, for the typical junction presented here, showing a high transparency. We evaluated the elastic mean free path l of conduction electrons in one of our Fe films using an expression derived from Pippard relations [16]: v_F l = (πk_B /e)^2 (σ/γ). With the iron film conductance σ ≈4×10^3 S/m^2, electronic specific heat γ= 5×10^{−3} J/K^2, and Fermi velocity v_F = 1.98×10^6m/s, we obtained l ≈100Å. Since the quasiclassical description of conductance assumes l < d [5], we see that such a model is applicable to our first three Fe layers. We performed conventional 4-point measurements, with a constant current driving bias.

The tunneling spectra at the interface with the BSCCO crystal were obtained successively for the six layers, starting with the Ag counterelectrode, then probing an increasing thickness in the FM region from 0 to 150Å, by 30Åincrement for each electrode. Each layer was measured at different temperatures, from 150 to 4.2 K. Fig.2 represents the temperature dependence for the first three layers, each curve being normalized by the spectrum at 150K. All layers manifested a sudden change in the background conductance at T_c. This phenomenon can be attributed to the competition between a screening spinaccumulation close to the interface, responsible for a drop in the barrier conductance, and the onset of Andreev reflections, with an adverse effect [17]. In an Andreev reflection, the electron incident on the barrier with energy lower than the superconductive gap is reflected as a

FIG. 2: Temperature dependence of the conductance spectra. The arrows indicate the background conductance variation at Tc as the temperature is decreased. a) Normal layer b) 30Å iron layer, and c) 60Å iron layer.

hole, while a Cooper pair is transmitted into the SC. In the case of d-wave superconductors the Andreev reflections are phase sensitive. This leads to the formation of bound states at the junction interface with amplitudes dependent on the angle of incidence. In a quasiclassical picture [5], the particles move along trajectories reflected between the boundaries of the counterelectrode, the density of states per trajectory being correlated to the length of the trajectory or number of reflections which in turn depends on the energy and exchange potential. The tunneling conductance spectrum is a measure of the energy resolved total density of states and is regarded as a sum of local bound states averaged over all trajectories distributed by length. Therefore, the thickness of the counterelectrode influences the amplitude of the bound states and thus the spectral features, like the ZBCP. For our Ag terminal, since the amplitude of the Andreev states is low (Fig. 2 and 3), and it is in direct contact with the next iron layer, the background conductance at T_c decreases with decreasing temperature, due to the predominance

FIG. 3: Tunneling spectra normalized by the background conductance G0, represented for increasing counterelectrode thickness d, at three temperatures T . a) T = 5 K. The arrow on the Ag/BSCCO spectrum points to the minigap edge. The asymmetric spectrum at d = 60Å permits an evaluation of the Fe film polarization from the peak ratio, PF e ≈ 43%. b) T = 40 K spectra (continuous lines) compared to the theoretical fits (dash lines) with h = 170 meV (20 meV for the first Fe layer), Δ = 44 meV, and Z = 0.51. The fitted d values (Fig. 2b) match close enough the actual values. c) T = 60 K. The ZBCP for d = 150Å is not split at this higher temperature approaching Tc, due to the suppression of the BTRS and the bigger effect from the spin-splitting field on the superconductivity since Δ decreases while the h remains constant.

of a spin accumulation at the junction barrier. The temperature dependence of the Ag/BSCCO tunneling spectrum shows no ZBCP (Fig. 2a). This may indicate a predominant injection normal on the [100] plane [13, 14] combined with a rarefied distribution of long trajectories due to the very low thickness of the film, leading to the suppression of low energy states. The energy resolved DOS shows signs of a minigap (Fig. 3) at zero energy bias, which points out to some degree of disorder in the counterelectrode favorable to short trajectories or higher energy subgap bound states. A pseudogap opens at T^∗ ≈ 160 K and the superconducting transition takes place at T_c ≈ 85 K, clearly visible on the T-V plane contour. We measured a peak to peak SC energy gap Δ ≈ 44 meV at 40 K.

Next we probed the FM region of the junction. With each Fe layer, 30Å are added to the total distance accessible to the pairs injected into the counterelectrode. The pairs survive along a distance of several coherence lengths ξ ≈ 38Å as the SC order parameter decays oscillatory around zero. We performed theoretical fits for the DOS spectra at the intermediate temperature 40 K. The model we employed [5] calculates the DOS taking into account the thickness d of the FM film when the interface with the SC is highly transparent and d is smaller than the electron mean free path l. With l calculated above, the model is applicable mostly for the first few layers, which are anyway the most suggestive. Since we expect our boundaries to be rough, leading to an admixture of trajectories and a smearing of the spectral features, the DOS was averaged over a Gaussian distribution of thicknesses around each d. The best fits imposed a value h

= 20 meV for the first iron layer and h = 170 meV for the second one (consistent with the accepted value [16]). The fits for all other Fe layers were obtained by keeping constant the exchange energy h = 170 meV, the gap Δ = 44 meV, and the barrier transparency Z = 0.51. The only adjusted variable was the thickness scaled by the coherence length, d/πξ_F . The procedure resulted into five values for the layer thickness remarkably close to the actual values (see Fig. 4b), confirming the validity of the model and also the regularity of the thin films. We also take advantage from the BTK type models to underline the effect of the d-wave (possibly mixed with s-wave) pairing symmetry of BSCCO.

The temperature dependent spectra measured on the first FM layer (d = 30Å) (Fig. 2b) also has a pseudogap. The T_c is slightly smaller and the background conductance after the transition increases, indicating the growing influence of the Andreev reflections. The most remarkable features (Fig. 3), are the dips replacing the ±Δ coherence peaks. Due to the direct contact with the Ag layer, the spectrum rather shapes up the effect of a distribution of spin-polarized quasiparticles in the Ag film, so that the theoretical fit on this curve imposed an exchange energy h=20 meV, lower than that for the other Fe layers. For 0< h < Δ, the ±Δ peaks move to subgap energies, being replaced by minima in the DOS [5]. The resulted subgap peaks are expected to merge into a ZBCP with increasing d, and to exhibit local oscillatory variations. Indeed, the next FM layers show the oscillations, but the peaks do not merge with increasing d. This may be due to properties of the junction unaffected by the thickness of the FM environment, like the presence of a mixed su-

FIG. 4: The reduced DOS develops coherent oscillations dependent on d. a) The experimental results approach better the predicted behavior for increasing temperature, due to the decreased s-wave component. b) There is a remarkable match between the theoretical thicknesses and the actual d values.

perconductive phase with broken time-reversal symmetry (BTRS) at the junction interface (e.g., (d+is)-wave)[11]. This splits the ZBCP, forming a gaplike feature with the size given by the magnitude of the sub-component s, and influenced by temperature. In this case, the s-wave gap remains unchanged with increasing d, while the subgap DOS oscillates up and down as the decaying order parameter alternatively takes negative and positive values respectively.

As seen in Fig. 2c, the next Fe layer (d = 60Å) measures a flatter pseudogap at high temperatures. The conductance enhancement at the superconductive transition is larger, consistent with the high amplitude of the Andreev peaks. The electronlike and holelike quasiparticle branches of the spectrum are asymmetric at lower temperatures. The split ZBCP is high and it becomes broader and less asymmetric with increasing temperature (Fig. 3a,c). This asymmetry may be attributed [13] to the presence of a spin dependent contribution to the ZBCP split at lower temperatures. If a spin imbalance is present in the barrier, the ZBCP corresponding to up (down) spin currents are shifted at higher (lower) energies. The polarization in the FM layer decreases the spinup peak and increases the spin-down peak. The ratio of the peaks can be used to evaluate the spin polarization P in iron. In our case, P_{F e} ≈ 43%, which is consistent with the values reported in literature [16]. The broader ZBCP at temperatures closer to T_c may be the effect of a thermal smearing and the suppression of superconductivity due to the diminishing Δ.

The next three layers (d = 90-150Å) complete an oscillatory cycle. The curves are too noisy to discern the more delicate features but the general behavior is sufficiently clear: the superconductivity is highly suppresed and the LOFF states develop d-dependent coherent oscillations, with smaller and smaller amplitude. The sign of these oscillations depend on the energy. In Fig. 4, the reduced DOS, G(E)/G_0 − 1, oscillates in antiphase at energy E = 0 with respect to the E = ±Δ values. At lower temperatures the zero energy conductance is lower than the theoretically predicted curve (Fig. 4a), due to the significant presence of the BTRS induced ZBCP split. The BTRS states disappear at a temperature lower than BSCCO T_c, so that the 150Å spectrum presents a 60K ZBCP without the split. Consequently, the points taken at temperatures nearer to T_c approach better the theoretical expectation.

In summary, we constructed planar Fe/Ag/BSCCO junctions, with the Fe region imparted in layers of equal thickness. Temperature dependent tunneling spectra were collected on each layer, probing a reproducible spatial dependent instance of the LOFF state. The spectral features are affected by the pair-braking exchange field in the FM region, the thickness of this area and the unconventional pairing symmetry in the BSCCO. As the Fe thickness is increased, the conductance spectra show decaying oscillations with energy dependent amplitude and sign. The ZBCP is split regardless the thickness, but dependent on the temperature, due to the presence of a subcomponent added to the dominant d-wave component at the junction interface to form a BTRS state. The spectrum is asymmetric at low temperature due to the spin-polarization.

This work is supported by NSF Grant No. DMR9972071.

[1] T.P. Orlando et al., Physica C 368, 294 (2002) [2] P. Fulde and R.A. Ferrell, Phys. Rev. 135, A550 (1964);

A. I. Larkin and Yu. N. Ovchinnikov, Sov. Phys. JETP. 20, 762 (1965) [3] A.I. Buzdin, Phys. Rev. B 62, 11 377 (2000) [4] T. Kontos et al., Phys. Rev. Lett 86, 304 (2001) [5] M. Zareyan et al., Phys. Rev. Lett. 86, 308 (2001) and Phys. Rev. B 65, 184 505 (2002) [6] G. Sun et al., Phys. Rev. B, 65, 174 508 (2002) [7] O. Bourgeouis and R. C. Dynes, Phys. Rev. B 65, 144 503 (2002) [8] V.V. Ryazanov et al., Phys. Rev. Lett. 86, 2427 (2001) [9] A. Sawa et al., Physica B 284-288, 493 (2000) [10] C.C. Tsuei and J.R. Kirtley, Rev. Mod. Phys. 72, 969 (2000) [11] M. Covington et al., Phys. Rev. Lett. 79, 277 (1997) [12] D. Pines, Physica C 282-287, 273 (1993) [13] S. Kashiwaya et al., Phys. Rev. B 60, 3572 (1999) [14] N. Stefanakis, Phys. Rev. B 64, 224 502 (2001) [15] M. Rubistein et al., Phys. Rev. B 47, 15350 (1993) [16] L. Lazar et al., Phys. Rev. B 61, 3711, (2000) [17] W. Belzig et al., Phys. Rev. B 62, 9726, (2000)