arXiv:hep-ph/0611178v3 12 Mar 2007

Probing Active to Sterile Neutrino Oscillations in the LENS Detector

C. Grieb, J. M. Link, and R. S. Raghavan Institute of Particle, Nuclear and Astronomical Sciences Virginia Polytechnic Institute and State University, Blacksburg, VA 24061 (Dated: March 31, 2018)

Abstract

Sterile neutrino (ν_s) conversion in meter scale baselines can be sensitively probed using monoenergetic, sub-MeV, flavor pure ν_e’s from an artificial MCi source and the unique technology of the LENS low energy solar ν_e detector. Active-sterile oscillations can be directly observed in the granular LENS detector itself to critically test and extend results of short baseline accelerator and reactor experiments.

PACS numbers: 14.60.Pq, 12.15.Ff, 14.60.St

Sterile neutrinos occur naturally in models of ν mass generation and figure in a variety of contemporary problems of particle physics, astrophysics and cosmology [1]. Evidence for sterile ν’s is thus of high interest, fueled by the LSND experiment [2] that has claimed appearance of ν̄_e from a ν̄_μ beam at a baseline of 30 m. The large Δm^2 (∼1 eV^2) implied by LSND cannot be accommodated by the usual 3 active ν’s with small mass splittings 10^{−5} to 10^{−3} eV^2. An extended model of 3+1 mass eigenstates can explain the LSND effect as P_{μe} = sin^2 2θ_{μe} = 4U^2_{e4}U^2_{μ4} where U_{α4} are the mixing matrix elements with the fourth (mostly sterile) mass state in the 3+1 model. If so, a complementary probe is ν̄_e disappearance in reactor experiments such as BUGEY [3] that has set limits on Δm^2 and sin^2 2θ_{ee} = 4U^2_{e4}(1−U^2_{e4}). These limits however, exclude most of the parameter space implied by LSND [4]. The two results do seem more compatible in a model of 3 active +2 sterile states [4].

The MiniBooNE-ν_μ experiment [5] (ν_μ → ν_e) will directly test the LSND result (assuming CPT invariance). In the next step it is vital to explicitly observe active to sterile ν oscillations and measure the sterile ν mixing probabilities directly. In addition, light sterile ν’s, even with potentially smaller mixing angles than LSND, can fix problems with r-process nucleosynthesis in supernovae [6], so it is important to push beyond LSND regardless of what MiniBooNE finds. New tools are needed for these tasks. In this Letter we show that these objectives can be achieved by the unique technology of LENS (Low Energy Neutrino Spectroscopy detector) [7] and a MCi, sub-MeV, mono-energetic, flavor-pure, ν_e source. The MCi source technology is well established for the^{51}Cr source considered here and the LENS technology is ready for testing in a prototype (MINILENS).

The LENS ν_e detector is based on the charged current (CC) driven ν_e capture in^{115}In [8]:

ν_e +^{115} In(95.6%) →^{115}Sn^∗ + e^− (1) |→ 115Sn + 2γ

The ν_e capture leads to an isomeric state in^{115}Sn at 614 keV which emits a delayed (τ = 4.76 μs) cascade 2γ (= 116+498 keV) that de-excites to the ground state of^{115}Sn. The reaction threshold is low, Q = 114(4) keV. The ν_e signal energy, E_e = E_ν − Q leads to the incident ν_e energy. The spectroscopic power of LENS is illustrated in Fig. 1 by its expected result on the low energy solar ν_e spectrum.

The delayed 2γ signal is a powerful tag for the ν_e capture. The only valid events in LENS are coincidence events, the time distribution of which is shown in Fig. 1 (top panel). An exponential decay fit (with the signature lifetime of^{115}Sn^∗) to the time spectrum leads to the true signal events that occur at early delays ∼10 μs and the background from random coincidences at long delays. This background arises dominantly via random coincidences with β’s from the natural decay of the target^{115}In with the end point at 498(4) keV. It presents a severe (but soluble) problem for solar pp ν_e (E_e <300 keV, see Fig. 1) but it is far less problematic for E_e >500 keV (e.g. for^7Be solar neutrinos in Fig. 1). The background is, in any case, measured at long delays separately and concurrently. The ν_e event analysis tests the validity of a candidate tag by the time and space coincidence as well as the detailed template of the 2γ tag shower. This determines the coincidence efficiency, modeled to be >85% for signals >500 keV (^{51}Cr provides a ∼640 keV signal).

The LENS technology thus extends the power of tagged ν detection from the case of broadband ν̄_e beam with E_ν > 1.8 MeV in reactor experiments to monoenergetic sub-MeV ν_e that lead to explicit, meter scale oscillations directly detectable in modest sized granular detectors. Most issues in shape analyses of P_{ee} and systematic normalization errors endemic to reactor ν experiments are thus avoided in LENS. A ν_e test allows direct comparison to MiniBooNE (ν_μ) without invoking CPT invariance and with LSND and MiniBooNE (ν̄_μ) to test CPT invariance.

The detection medium in LENS is a liquid scintillator chemically loaded with indium (InLS). This technology uses a robust, well tested (Bell Labs [9], BNL, LNGS, Virginia Tech) procedure that produces high quality InLS (In loading 8-10 wt.%, scintillation output ∼8000 hν/MeV and signal light attenuation length L(1/e) of 8 m that is stable for >1 year) [7]. InLS with up to 15% In has been produced with promising properties and is currently in development. Anticipating positive results, we consider both 8% and 15% In loading.

The granular LENS detector is based on a novel “scintillation lattice chamber” design [7]. In this design the detector volume is optically segmented into cubic cells (7.5×7.5×7.5 cm) by a 3-dimensional cage of thin (∼0.1 mm), double layered, transparent foils which provide an air gap between the foils (even in contact under pressure of ∼2 bars). The scintillation light is then channeled only along 3 coordinate axes centered on the vertex cell of the event. Coincident hits on phototubes at the end of the channels digitally determine the 3-D location of the event to a precision set by the cell size. Each cell is always viewed by the

FIG. 1: Simulated 5 year-solar ν_e signal spectra in LENS. Top panel: delayed coincidence time spectrum fitted to the isomeric lifetime τ=4.76 μs. Middle panel: energy spectrum (with ∼2000 pp events) at delays <10 μs, and random coincidences (from the pure β-decay of In target) at long delays. Bottom panel: Spectrum from 4×100 day exposure to a 10 MCi source of^{51}Cr with the scaled solar spectrum included. The Cr signal has 1.3 × 10^4 events with ∼0.1% background (from the^7Be line).

same combination of 6 or less phototubes. Thus LENS is, in effect, a 3-D array of 10^5 nuclear counters with bench top sensitivity. The spherical ν_e oscillation wave can then be observed by the radial variation P_{ee}(R) of ν_e from a source placed at the center of the detector. The LENS experiment thus uses 10^5 detectors to trace the ν_e oscillation profile in detail. The result is thus far more transparent than that from usual methods with 2 to 3 static or movable detectors. As in the reactor experiment theoretical uncertainties due to ν cross section are common to all “detectors” and thus cancel. In addition the uncertainty from indium concentration cancels, or at least should average out because the scintillator volume is fully connected, and detection efficiency can be made flat across the detector because the mono-energetic signal allows triggering thresholds to be set to tune out any instability.

Several MCi sources of^{51}Cr have been produced and used to calibrate the Ga radiochemical solar ν_e detectors (1.7 MCi in GALLEX [10, 11] and 0.52 MCi in SAGE [12, 13]). (Recently, small inconsistencies in the SAGE ν_e calibration results has been attributed to sterile ν conversion [14]). Studies show that the production of ∼10 MCi^{51}Cr sources is feasible. The electron-capture decay (τ = 40 d) of^{51}Cr emits a mono-energetic ν_e of energy 0.753 MeV (90%) which produces a ν_e signal at 0.639 MeV in LENS. We note that a MCi source experiment for precision calibration of the^{115}In ν_e capture cross-section is already part of the LENS program as LENS-CAL [15].

The source experiment requires a ∼ 4π source-detector geometry for maximum sensitivity. The primary design criterion is then the background arising from hard γ’s of impurity activities in the source (the only γ from^{51}Cr itself is of energy 0.32 MeV, easily shielded and far below the ν_e signal energy). The source will be encased in a heavy-metal shielding container to cut down radiation outside the container below permissible safety limits. The SAGE data [12] show that the dominant γ-rays outside the container are from the impurity activity^46Sc (3 Ci/MCi^{51}Cr) of 2 hard γ’s (1.12 and 0.889 MeV). In a ∼25 cm radius tungsten container this releases ∼ 10^3 γ/s into the detector, ≪ 10^6/s, the benchmark rate of^{115}In β’s that underlies all random coincidence background considerations in LENS [7]. Thus, a 10 MCi^{51}Cr source in a ∼50 cm diameter heavy-metal sphere at the center of the LENS detector is a viable concept with state-of-the art technology.

The ν_e spectroscopy of^{51}Cr (4 × 100 day exposure to a 10 MCi source) in a full scale LENS detector is shown in the bottom panel of Fig. 1 (notice the log scale). The Cr signal (∼13,300 events) is ∼1000 times the solar “background”. An internal MCi source in a real-time rare event counting detector is, by itself, a major first (SAGE/GALLEX are radio-chemical activation experiments).

In 3+2 models, with mixing angles and oscillation frequencies in flavor states α = e, μ, τ, s_{1,2}, mass states n=1-5 where states 4 and 5 are mostly sterile and U_{αn} are the elements of the ν mixing matrix, the e-flavor survival, P_{ee}, is:

P_{ee} ≃ 1−4U^2_{e4}(1−U^2_{e4}) sin^2 x_{41} −4U^2_{e5}(1−U^2_{e5}) sin^2 x_{51} (2)

where cross terms such as U^2_{e4}U^2_{e5} are neglected, and x_{ij} = 1.27Δm^2_{ij} (eV^2)L(m)/E_ν (MeV). The values of U_{ei} and Δm^2 (shown in Table I) are from Ref [4]. With Δm^2 = 1 eV and E_ν ∼ 0.753 MeV (from^{51}Cr), full flavor recovery occurs in ∼2 m, directly observable in a

Model Δm^2_{ij} (eV^2) U^2 sin^2 2θ_{ee} =4U^2(1−U^2) 3+1 0.92_{14} 0.0185 0.073 3+2a 0.92_{14} 0.0146 0.057 22.1_{15} 0.0013 0.005 3+2b 0.46_{14} 0.0081 0.032 0.89_{15} 0.0156 0.062 TABLE I: Active-Sterile splittings and mixing parameters campatible with LSND and the null short baseline data [4], as used in the analyses shown in Fig. 2.

FIG. 2: Analysis of 3+1 and 3+2 models of sterile neutrinos in LENS. In 10t=8% In LENS-Sol (A); In 5t=15% In LENS-Sterile (B); Cr=4 MCi×100 days exposure to^{51}Cr; and Fe=10 MCi×2 years exposure to^{55}Fe.

lab-scale detector.

We consider two detector configurations, A and B (Table II), based on the lattice array design with 7.5×7.5×7.5 cm cells. Design A is the full scale solar detector (LENS-Sol 8% In). The smaller detector B, anticipates further development of a higher density (15% In) InLS to exploit the linear dependence of the event rate with In density. It is thus specific for sterile ν search and costs ∼50% less than A. With comparable (density × In mass), the event rate is comparable for a source assembly at the center of A or B in a 50 cm spherical volume.

The sensitivity of radial distributions of events in designs A and B to sterile ν oscillation parameters was analyzed by a Monte Carlo technique. The number of ν_e detected, N_{0i} is calculated for each cubic cell element i of the detector assuming no oscillations. Then, assuming an oscillation model of (3+1) or (3+2) with parameters (Δm^2, sin^2 2θ) or (Δm^2_1, sin^2 2θ_1; Δm^2, sin^2 2θ_2) the number of ν_e detected in each cell, N_i, is calculated. The cells are then grouped into k bins according to their distance, d_i, from the source. A random sample data set for one experiment is created under the oscillation assumption. Then the theoretical event ratio as a function of d, N_i/N_{0i} = f(sin^2 2θ, Δm^2, d), is fitted to the sample data set with the oscillation parameters as free parameters. The process is repeated 10^6 times with random data sets and each resulting set of fitted parameters (sin^2 2θ, Δm^2)_i is stored. The distribution of these values (see Fig. 2) is a direct measure of the statistical uncertainty of (sin^2 2θ, Δm^2) in a single measurement.

The models in Table I predict 2 main effects: 1) the minimum oscillation amplitude of ∼5% occurs with a single frequency for 3+1 and (practically also in 3+2a); 2) two frequencies occur in 3+2b. In the analysis, we test designs A and B for 1) a single frequency and 2) double frequency as in 3+2b. Figs. 2a,b for design A (full scale solar detector) show that a 5% single frequency oscillation (3+1, 3+2a) as well as the double frequency oscillation for 3+2b can be clearly observed with 4 × 100 day exposure to a 10 MCi^{51}Cr source. The mixing parameter sin^2 2θ can be determined with 1σ precision of 25% in both cases. In the smaller detector B the lower of the double frequency is not picked up with Cr because the radial dimension of B is insufficient to catch the P_{ee} recovery. In this case, another source, 55Fe with E_ν = 236 keV, can be used. A 2-year exposure to a 10 MCi Fe source (τ = 3.8 y) (Fig. 2d), shows excellent resolution of the double frequency effect. A MCi Fe source has not been produced so far, thus, this technology awaits ab initio development. Configuration ρ_{In} d_{detector} m_{In} m_{total} (wt. %) (meters) (tons) (tons) A – LENS-Sol 8 5.1 9.9 125 B – LENS-Sterile 15 3.3 5.1 34 TABLE II: Design options for LENS sterile ν search.

FIG. 3: Exclusion plots of sensitivity to active-sterile oscillations in LENS (with 4×100 day exposure to 10 MCi Cr source) compared to those for LSND, BUGEY, and the projected sensitivity of MiniBooNE [16]. LSND and MiniBooNE are plotted assuming the best fit U_{e4} and U_{μ4} from Ref [4].

Fig. 3 shows the exclusion plots of Δm^2 vs. sin^2 2θ_{ee} for 90% confidence level sensitivity to oscillations in the designs A and B compared to those from BUGEY, LSND and MiniBooNE. Fig. 4 shows that, indeed, a relatively modest 3 MCi source of^{51}Cr is sufficient to reach the projected oscillation sensitivity of MiniBoonNE.

These analyses show that the LENS approach in A or B can exclude parameter regions of active-sterile oscillations significantly beyond those of BUGEY, LSND and MiniBooNE. Further, the LENS approach is complementary to the proposed NC-based ν_μ disappearance test which is sensitive to sin^2 2θ_{μμ} [17].

In summary, the LENS technology offers a novel attack for discovery of active-sterile oscillations with sensitivities well beyond those in LSND, MiniBooNE and BUGEY. Design B offers the opportunity to accomplish these goals in a relatively modest detector that can map the full oscillation as a function of radius. However, R&D on the high density InLS needs to be completed and the technology of the Fe source developed ab initio. The straightforward approach would use the full scale LENS detector, design A, for which the Cr source and detector technologies are already well developed. The next step in the latter

FIG. 4: Sensitivity to sterile oscillations vs^{51}Cr source strength. The projected MiniBooNE sensitivity can be achieved with a source of less than 2 MCi.

is the construction and operational tests of the prototype detector MINILENS which is now being initiated.

We thank Bruce Vogelaar, Mark Pitt, and the other members of the Virginia Tech particle and nuclear group for helpful discussions.

[1] A. Kusenko (2006), hep-ph/0609158.

[2] C. Athanassopoulos et al. (LSND), Phys. Rev. Lett. 75, 2650 (1995), nucl-ex/9504002. [3] Y. Declais et al. (Bugey), Nucl. Phys. B434, 503 (1995).

[4] M. Sorel, J. M. Conrad, and M. Shaevitz, Phys. Rev. D70, 073004 (2004), hep-ph/0305255. [5] A. O. Bazarko (BooNE) (1999), hep-ex/9906003.

[6] G. C. McLaughlin, J. M. Fetter, A. B. Balantekin, and G. M. Fuller, Phys. Rev. C59, 2873 (1999), astro-ph/9902106.

[7] Detailed information on LENS technology can be found in several presentations made in the recent workshop LONU-LENS (Virginia Tech) and posted at http://www.phys.vt.edu/∼dusel/low-energy-workshop/.

[8] R. S. Raghavan, Phys. Rev. Lett. 37, 259 (1976).

[9] E. C. Chandross and R. S. Raghavan (2004), U.S. Patent #6809210. [10] M. Cribier et al., Nucl. Instrum. Meth. A378, 233 (1996). [11] W. Hampel et al. (GALLEX), Phys. Lett. B420, 114 (1998). [12] D. N. Abdurashitov et al., Phys. Rev. Lett. 77, 4708 (1996).

[13] J. N. Abdurashitov et al. (SAGE), Phys. Rev. Lett. 83, 4686 (1999), astro-ph/9907131.

[14] C. Giunti and M. Laveder (2006), hep-ph/0610352.

[15] See talk on LENS-CAL in Ref. [7]. The B(GT) matrix element needed to evaluate the crosssection has been measured by (p,n), based on strong interactions, to be 0.17±10%. Lens-Cal will measure B(GT) directly using a ν_e source with a precisionon of a few percent.

[16] A. A. Aguilar-Arevalo et al. (MiniBooNE) (2003), http://wwwboone.fnal.gov/publicpages/runplan.ps.gz.

[17] G. T. Garvey et al., Phys. Rev. D72, 092001 (2005), hep-ph/0501013.