arXiv:1506.09212v1 [physics.flu-dyn] 30 Jun 2015

A note on the breathing mode of an elastic sphere in Newtonian and complex fluids Vahe Galstyan,^1 On Shun Pak,^{2, 3} and Howard A. Stone^3 1)Department of Physics, Columbia University, New York, NY 10027 2)Department of Mechanical Engineering, Santa Clara University, Santa Clara, CA 95053 3)Department of Mechanical and Aerospace Engineering, Princeton University, Princeton, NJ 08544

Experiments on the acoustic vibrations of elastic nanostructures in fluid media have been used to study the mechanical properties of materials, as well as for mechanical and biological sensing. The medium surrounding the nanostructure is typically modeled as a Newtonian fluid. A recent experiment however suggested that highfrequency longitudinal vibration of bipyramidal nanoparticles could trigger a viscoelastic response in water-glycerol mixtures [M. Pelton et al., “Viscoelastic flows in simple liquids generated by vibrating nanostructures,” Phys. Rev. Lett. 111, 244502 (2013)]. Motivated by these experimental studies, we first revisit a classical continuum mechanics problem of the purely radial vibration of an elastic sphere, also called the breathing mode, in a compressible viscous fluid, and then extend our analysis to a viscoelastic medium using the Maxwell fluid model. The effects of fluid compressibility and viscoelasticity are discussed. Although in the case of longitudinal vibration of bipyramidal nanoparticles, the effects of fluid compressibility were shown to be negligible, we demonstrate that it plays a significant role in the breathing mode of an elastic sphere. On the other hand, despite the different vibration modes, the breathing mode of a sphere triggers a viscoelastic response in water-glycerol mixtures similar to that triggered by the longitudinal vibration of bipyramidal nanoparticles. We also comment on the effect of fluid viscoelasticity on the idea of destroying virus particles by acoustic resonance.

I. INTRODUCTION

Studies on the vibration of elastic nanoparticles embedded in fluid media have attracted considerable attention recently, due to potential applications, for example, as an alternative nondestructive tool for characterizing material properties^1 and designing mechanical and biological sensors.^{2–4} Low damping, i.e., a high quality factor, is desirable in these applications for high detection sensitivity. It is therefore of interest to investigate the damping mechanisms due to energy dissipation or energy transfer to the surrounding media. In addition, biological nanoparticles such as viruses have also been modeled as elastic spheres in the studies of their vibration characteristics in different media, motivated by the idea of destroying viruses in a living host with ultrasound waves via resonance.^{5–9} The resonant frequencies and damping characteristics of mechanical nanostructures with various shapes have been measured by a variety of experimental techniques.^{10–12} From the modeling perspective, acoustic vibrations of elastic bodies are classical problems in continuum mechanics. For example, Lamb^{13} studied theoretically the vibrations of an elastic sphere in vacuum. Subsequent works considered the vibration modes of elastic structures with different geometries, which are summarized briefly in Table I. In addition, the effect of different surrounding environments, including an elastic solid matrix,^{14} and inviscid^{15} and viscous^{16,17} fluid media, were also considered in later studies (Table I). As a remark, for a nanoparticle with a typical size of tens of nanometers, the atomic spacing is usually sufficiently small that a continuum description is valid.^{16,17} Such a continuum approach was also shown to be successful in predicting the resonant frequency (on the order of tens of GHz) of a gold nanoparticle vibrating in water.^{17}

Recently, an experiment on the vibration of a bipyramidal gold nanoparticle (in the shape of a pair of truncated cones) in water-glycerol mixtures suggested that the highfrequency (20 GHz) vibration could trigger viscoelastic responses in the mixture, even in small molecule liquids.^{18} The bipyramidal nanoparticle was excited to vibrate longitudinally along its major axis in a water-glycerol mixture. When increasing the glycerol mass fraction, the quality factor of the vibration displayed non-monotonic variations not explained by a Newtonian fluid model; a viscoelastic fluid model (linear Maxwell model) however captured the behavior. In contrast to the longitudinal vibrations of bipyramidal nanoparticles, the breathing mode, which refers to purely radial vibrations, is mainly excited for spherical

Elastic Structure

Surrounding Medium Vibration Modes Viscosity Compressibility Rheology Lamb^{13} (1882) Sphere Vacuum Torsional & spheroidal Kheisin^{15} (1967) Sphere Inviscid Compressible Newtonian fluid Breathing Dubrovskiy & Morochnik^{14} (1981)

Sphere Elastic solid matrix Torsional & spheroidal

Saviot et al.^{16}

(2007)

Sphere Viscous Compressible Newtonian fluid Torsional & spheroidal

Chakraborty et al.^{17} (2013)

Circular cylinder Conical cylinder Bipyramid

Viscous Incompressible Newtonian fluid

Longitudinal vibrations along the major axis

Pelton et al.^{18}

(2013)

Bipyramid Viscous

Compressible & incompressible

Viscoelastic fluid (Maxwell model)

Longitudinal vibrations along the major axis

This work Sphere Viscous

Compressible & incompressible

Viscoelastic fluid (Maxwell model)

Breathing

TABLE I: Some theoretical studies of the vibrations of elastic structures in different media.

nanoparticles,^{11} whose behavior in a viscoelastic fluid medium remains unexplored. In this paper, we first revisit the classical problem of the breathing mode of a vibrating elastic sphere in a Newtonian fluid, and then extend our studies to complex fluid media.

We organize the paper by first presenting a continuum mechanics formulation in Sec. II for the elasticity problem of a radially vibrating sphere (Sec. II A) and the propagation of acoustic waves in the fluid medium (Sec. II B). The two problems are then coupled by matching the velocities and stresses at the interface of the solid (Sec. II C). An analytical eigenvalue equation determining the vibration frequencies of an elastic sphere in a compressible, viscous, Newtonian fluid medium is obtained in Sec. III. The results are validated against previous theoretical and experimental studies of a vibrating gold nanosphere in water (Sec. III A), followed by parametric studies of the quality factor (Sec. III B). The calculations are then extended to the viscoelastic case in Sec. III C, with results and remarks discussed in Sec. IV.

II. FORMULATION

We consider the purely radial vibration of an elastic sphere of radius R in a compressible viscous fluid. This spherically symmetric motion is also called the breathing mode (see Fig. 1 for a schematic representation of the problem). The displacement field of the elastic

FIG. 1: Schematic representation of the breathing mode (purely radial vibration) of an elastic sphere (density ρ_s, longitudinal wave speed c_ℓ, and transverse wave speed c_t) in a fluid medium (density ρ_f , wave speed c, shear viscosity η, and bulk viscosity κ).

sphere, u, is governed by the Navier equation in elasticity ρ_s ∂^2u ∂t^2 = μ∇^2u + (μ + λ)∇(∇ · u), (1)

where ρ_s is the density of the solid, and μ and λ are the Lamé elastic parameters. We consider small-amplitude acoustic waves in the fluid, and hence the velocity field, v, is governed by the linearized Navier-Stokes equation for compressible flows ρ_f ∂v ∂t = −∇p + η∇^2v + ( κ + η 3 ) ∇(∇ · v), (2)

where ρ_f is the density of the fluid, η is the shear viscosity, κ is the bulk viscosity, and p is the thermodynamic pressure.

Since the vibration is purely radial, we utilize a spherical coordinate system located at the center of the sphere. The displacement field of the elastic sphere, u(r, t) = u(r, t)e_r, and the velocity field of the fluid, v(r, t) = v(r, t)e_r, have only radial components that are functions of the distance from the origin r and time t. With this geometrical symmetry, the identity ∇^2a ≡ ∇(∇ · a) holds for a vector field a, which simplifies (1) and (2), respectively, to ρ_s ∂^2u ∂t^2 = (2μ + λ)∇^2u, (3a) ρ_f ∂v ∂t = −∇p + β∇^2v, (3b)

where β = κ + 4η/3.

A. Elasticity: radial vibration of an elastic sphere

We take the divergence of (3a) and define the scalar function ϕ = ∇ · u to obtain ∂^2ϕ ∂t^2 = c^2_ℓ ∇^2ϕ, (4)

where c_ℓ = √ (2μ + λ)/ρ_s, which physically represents the velocity of longitudinal waves in an elastic material. We find time-periodic solutions of the form ϕ(r, t) = Φ(r)e^{−iωt} for the breathing mode. By separation of variables we obtain ϕ(r, t) = ∞∑ n=1 A_n sin(k_{s,n}r) r e^{−iωnt}, (5) where A_n are arbitrary constants, and k_{s,n} = ω_n/c_ℓ are the unknown eigenvalues. The displacement field of the elastic sphere can then be determined by direct integration using the definition ϕ = ∇ · u = (1/r^2)∂(r^2u)/∂r, which results in u(r, t) = ∞∑ n=1 A_n [ sin(k_{s,n}r) k^2_{s,n}r^2 − cos(k_{s,n}r) k_{s,n}r ] e^{−iωnt}. (6)

B. Fluid dynamics: propagation of acoustic waves

We now turn to the propagation of small-amplitude acoustic waves in the fluid surrounding the vibrating sphere. The linearized continuity equation for a compressible fluid is given by ∂ρ^′ ∂t + ρ_f ∇ · v = 0, (7)

where ρ^′(r, t) represents the density fluctuation; | ρ^′ |≪ ρ_f . Together with the equation of state, p = c^2ρ^′, where c is the speed of sound in the fluid, (7) can be combined with (3b) to arrive at an equation for the density fluctuations ∂^2ρ^′ ∂t^2 = c^2∇^2ρ^′ + β ρ_f ∇^2 ∂ρ^′ ∂t · (8)

We again seek time-periodic solutions with the same vibration frequencies of the elastic sphere. Then, (8) can be solved by separation of variables to yield ρ^′(r, t) = ρ_f ∞∑ n=1 Ã_n e^{i(kf,n r−ωnt)} r , (9) where Ã_n are arbitrary constants and k_{f,n} =^{ωn}_c√_{1−iωnβ/ρf c2} . The corresponding velocity field can then be obtained from the continuity equation (7) as v(r, t) = ∞∑ n=1 Ã_niω_n (1 − ik^{f,n}r) k^2_{f,n}r^2 e^{i(kf,nr−ωnt)}. (10)

C. Elastohydrodynamics: coupling the radial vibration of an elastic sphere to the surrounding fluid

We couple the vibration of the elastic sphere to the fluid by matching the velocities and normal stresses at the boundary between the fluid and the vibrating sphere. Since small amplitude vibrations are considered, we use domain perturbation and expand the velocities and stresses at the boundary about the equilibrium radius of the sphere, R, a constant, keeping only the leading-order terms. For continuity of velocity, we compute the time derivative of the displacement field of the elastic sphere (6) and equate it to the velocity field in the fluid (10) evaluated at r = R, which results in −A_n [ sin(k_{s,n}R) k^2_{s,n}R^2 − cos(k_{s,n}R) k_{s,n}R ] = Ã_n (1 − ik_{f,n}R) k^2_{f,n}R^2 e^{ikf,nR}. (11) The stress tensor in the solid is given by

σ^s = λ(∇ · u)I + 2μγ, (12)

where γ =^1_2 (∇u+(∇u)^T ) is the strain tensor. For the spherically symmetric case considered here, the only non-zero component of the stress tensor is σ^s_{rr}(r, t) = ∞∑ n=1 A_n { λ + 2μ r sin(k_{s,n}r) − 4μ r ( sin(k_{s,n}r) k^2_{s,n}r^2 − cos(k_{s,n}r) k_{s,n}r )} e^{−iωnt}. (13) The stress tensor in the fluid is given by

σ^f = (−p + κ tr(γ̇)) I + 2η ( γ̇ − tr(γ̇) 3 I ) , (14)

where tr(γ̇) = ∇ · v, and γ̇ =^1_2 (∇v + (∇v)^T ) represents the rate-of-strain tensor. The only non-zero component of the stress tensor is σ^f_{rr}(r, t) = ∞∑ n=1 Ã_n e^{i(kf,n r−ωnt)} r ( −ρ_f c^2 + iβω_n − 4ηiω_n (1 − ik_{f,n}r) k^2_{f,n}r^2 ) , (15) where the equation of state and the continuity equation have been used.

Evaluating and matching the stresses in the solid (13) and fluid (15) at r = R leads to A_n ( (λ + 2μ) sin(k_{s,n}R) − 4μ [ sin(k_{s,n}R) k^2_{s,n}R^2 − cos(k_{s,n}R) k_{s,n}R ])

= Ã_n ( −ρ_f c^2 + iβω_n − 4ηiω_n (1 − ik_{f,n}R) k^2_{f,n}R^2 ) e^{ikf,nR}. (16)

III. RESULTS

For non-trivial solutions to the system of equations formed by equations (11) and (16), we require the determinant of the matrix representing this system to vanish, which leads to the eigenvalue equation for the natural frequencies ω_n k^2_{s,n}R^2 [ ρ_f ρ_s(1 − ik_{f,n}R) + ( k_{s,n}R tan(k_{s,n}R) − 1 )_{−1}] + 4iηk_{s,n} ρ_sc_ℓ + 4 ( c_t c_ℓ )_2 = 0. (17)

We note that (17) is a transcendental equation to be solved numerically. Here c_t = √ μ/ρ_s represents the velocity of transverse elastic waves. We calculate only the results for the fundamental mode (n = 1) here, since it is mainly the mode detected in experimental measurements;^{11} higher order modes can be obtained by finding other roots of the same equation. Hereafter, for simplicity we denote ω = ω_1, k_s = k_{s,1} = ω/c_ℓ, and k_f = k_{f,1} = ω c √_{1−iωβ/ρf c2} . For an inviscid flow (κ = η = 0), the eigenvalue condition (17) for ω reduces to ρ_f ρ_s = [ 4 k^2_s R^2 ( c_t c_ℓ )_2 + ( k_sR tan(k_sR) − 1 )_{−1}] (iωR/c − 1), (18) which was previously obtained by Kheisin.^{15} The case ρ_f = 0 corresponds to an elastic sphere vibrating in a vacuum,^{13} where the eigenvalue condition further simplifies to k_sR tan(k_sR)

= 1 − k^2_s R^2 4 ( c_ℓ c_t )_2 . (19)

Dubrovsky and Morochnik^{14} considered the breathing mode of an elastic sphere surrounded by another elastic medium. The eigenvalue conditions (17)–(19) can be alternatively obtained from the inviscid results of Dubrovsky and Morochnik by modifying the constitutive relation to include the viscous contribution from the fluid.^{16}

For the case of vacuum surrounding the vibrating sphere, the frequencies determined from (19) are real because there is no damping outside the sphere. When the vacuum is replaced by an inviscid fluid medium, the frequencies determined from the roots of (18) become complex, which implies that the free oscillation of the elastic sphere in a fluid takes the form of a sinusoid attenuating exponentially.^{15}

A. Breathing mode of a gold nanosphere in a Newtonian fluid

Here we first consider the experimental setup of Ruijgrok et al.,^{11} where the breathing mode of a single gold nanosphere of 40 nm radius in water was measured. We denote the complex frequency ω = ω_r + iω_i, where ω_r and ω_i are, respectively, the real and imaginary parts of the frequency. In this paper we define the quality factor as Q = − √ ω^2_r + ω^2_i /(2ω_i), which is the same as the definition adopted in Pelton et al.^{18} Note that Ruijgrok et al.^{11} defined the quality factor differently as Q^′ = −ω_r/(2ω_i), which gives only small quantitative differences for the vibrations with low damping (ω_i/ω_r ≪ 1) considered in this section. With the material constants of water given in Table II,^{19} in the inviscid limit a quality factor Q = 53.7 is obtained using (18).^{11} Note that the attenuation in oscillation is not due to viscous dissipation in the fluid since an inviscid medium is considered. Instead, the attenuation comes from the propagation of energy into the surrounding medium away from the vibrating sphere. Compressibility in the fluid provides a mechanism for energy to propagate away from the vibrating sphere through acoustic waves. When the shear and bulk viscosities of water are taken into account, (17) gives a slightly reduced quality factor of Q = 52.6, as reported by Ruijgrok et al.^{11}

Although the modification of the quality factor by the viscous effects is relatively minor in this case, a more significant reduction in the quality factor can occur when water is replaced by a water-glycerol mixture, which is the fluid medium considered by Pelton et al.^{18} The quality factor drops from Q = 40.6 (inviscid) to Q = 33.4 (viscous) for the vibration of the same gold nanosphere in a water-glycerol mixture with the glycerol mass fraction χ = 0.56, where the mixture is modeled as a Newtonian fluid. The parameter values and quality factors of these theoretical predictions are summarized in Table II. The viscous effects are discussed in terms of dimensionless variables in Sec. III B.

The natural frequency of an elastic sphere oscillating in an incompressible flow can be obtained by using the corresponding continuity equation, ∇ · v = 0 (see Appendix A), or by simply taking the wave speed in the fluid to infinity (c → ∞) in (17), which leads to

Gold nanoparticle Surrounding medium

Predicted quality factor, Q Inviscid Viscous Viscoelastic Water:

ρ_f = 1000 kg/m^3, c = 1510 m/s 53.7 52.6 52.2 ρ_s = 19700 kg/m^3 η = 0.000894 Pa·s, κ = 0.00286 Pa·s (f = 37.9 GHz) (f = 37.8 GHz) (f = 37.8 GHz) c_ℓ = 3240 m/s λ = 0.647 ps (for viscoelastic case) c_t = 1200 m/s Water-glycerol mixture (χ = 0.56):

ρ_f = 1140 kg/m^3, c = 1760 m/s 40.6 33.4 34.5 η = 0.00527 Pa·s, κ = 0.0116 Pa·s (f = 37.9 GHz) (f = 37.6 GHz) (f = 37.7 GHz) λ = 3.51 ps (for viscoelastic case)

TABLE II: Theoretical predictions of the quality factor Q and vibration frequency f = ω_r/(2π) of the breathing mode of a single gold nanosphere with 40 nm radius vibrating in inviscid, viscous, and viscoelastic fluid media. Refer to Appendix B for the details of the material constants.

k^2_s R^2 [ ρ_f ρ_s + ( k_sR tan(k_sR) − 1 )_{−1}] + 4iηk_s ρ_sc_ℓ + 4 ( c_t c_ℓ )_2

= 0. (20)

Using the material constants of water from Table II, we obtain a quality factor Q = 841 for the incompressible viscous case, which is significantly larger than the quality factor when compressibility is taken into account (Q = 52.6). Although Pelton et al.^{18} showed numerically that the effect of compressibility is insignificant for the longitudinal oscillations of a bipyramidal gold nanoparticle (with 25 nm base diameter and 90 nm total height), we demonstrate here an example of the breathing mode of nanospheres where fluid compressibility should be considered to obtain a reasonable prediction of the quality factor.

B. Parametric studies

We study the effects of different physical parameters on the quality factor by nondimensionalizing (17) to identify the dimensionless groups in our problem: s = ωR c_ℓ , ρ̃ = ρ_f ρ_s , c̃_t = c_t c_ℓ , c̃ = c c_ℓ , R̃ = ρ_f cR η , α = κ η . (21)

The dimensionless form of the eigenvalue equation (17) is

s^2 [ ρ̃ 1 − ik̃_f + ( s tan s − 1 )_{−1} ] + 4isc̃ρ̃ R̃ + 4c̃^{2t} = 0, (22) where k̃_f (s) = s/c̃ √ 1 − i ( α +^4_3 ) s/(R̃c̃) · (23)

We first examine the relative importance of the viscous dissipation mechanism compared with the damping caused by the propagation of acoustic waves away from the elastic nanosphere at different values of R̃ = ρ_f cR/η. The relative importance is characterized by comparing the quality factor when viscous effects are considered Q_{visc}, to the quality factor when the fluid medium is assumed to be inviscid Q_{inv} (hence, all damping is due to the propagation of acoustic waves away from the source). The ratio Q_{visc}/Q_{inv} should approach unity when viscous effects are negligible and decrease as the viscous effects become significant.

FIG. 2: Parametric study of the ratio Q_{visc}/Q_{inv} for different values of R̃ using the Newtonian fluid model. The symbols represent the vibrations of a gold nanosphere with 40 nm radius in pure water (blue dot) and water-glycerol mixture (glycerol mass fraction χ = 0.56, red square). The blue solid (red dotted) line is obtained by varying R̃ with all other dimensionless parameters (ρ̃, c̃_t, c̃ and α) kept the same as those represented by the blue dot (red square). The dimensionless parameters (see equation (21)) are obtained from the material constants presented in Table II.

For the case of a gold nanosphere with 40 nm radius vibrating in water, we obtain the corresponding values of R̃ = 67.6 and the ratio Q_{visc}/Q_{inv} ≈ 0.98 (blue dot, Fig. 2). Viscous dissipation is therefore negligible as reported by Ruijgrok et al.^{11} However, the viscous effects become more significant for the same vibration in a water-glycerol mixture with glycerol mass fraction χ = 0.56. (see Table II for the properties of the mixture^{20}). The corresponding value of R̃ = 15.2, which results in Q_{visc}/Q_{inv} ≈ 0.82 (red square, Fig. 2). The blue solid line (red dotted line) is obtained by varying R̃ while keeping all other dimensionless parameters (ρ̃, c̃_t, c̃ and α) the same as those represented by the blue dot (red square). The dimensionless parameters are obtained from the material constants presented in Table II. In both cases (blue solid and red dotted lines), we see the general trend that the viscous effects become significant when the dimensionless parameter R̃ decreases. As the densities and sound speeds do not change significantly for different fluids, the value of R̃ is mainly determined by the radius R of the vibrating particle and the shear viscosity η. As expected, the viscous effects therefore become significant typically when the vibrating structure decreases in size or when the shear viscosity of the fluid increases.

We also investigate the effect of the viscosity ratio α = κ/η in a compressible flow on the quality factor. Intuitively, the quality factor may decrease with a larger viscosity of the fluid because of the increased viscous dissipation. Such is the case for an incompressible flow. However, for the compressible flow considered here interesting variations are observed. In Fig. 3, we vary the viscosity ratio α at different values of R̃ = 10, 50, 100 (Fig. 3), keeping all other parameters fixed. As α increases, the quality factor can monotonically decrease (Fig. 3a), increase (Fig. 3c) or vary non-monotonically (Fig. 3b), depending on the value of R̃. This indicates that fluid compressibility provides a mechanism through which nonmonotonic behaviors as a function of fluid viscosities are possible.

FIG. 3: Parametric study of the quality factor Q as a function of α for varying values of R̃. Dimensionless parameters ρ̃, c̃_t and c̃ are obtained from material constants in Table II. (a) R̃ = 10. (b) R̃ = 50. (c) R̃ = 100.

C. Breathing mode of a gold nanosphere in a Maxwell fluid

The quality factor of high-frequency longitudinal oscillations of a single bipyramidal gold nanoparticle along its major axis in a water-glycerol mixture was recently measured by Pelton et al.^{18} A non-monotonic dependence of the quality factor on the glycerol mass fraction χ in the mixture was observed: the quality factor first decreased as the glycerol mass fraction increased, reaching a minimum before increasing again. The longitudinal oscillation of the bipyramidal nanoparticle was modeled by dividing the bipyramid into infinitesimal sections along its major axis and approximating each section by a circular cylinder, where the solution for a longitudinally oscillating circular cylinder could be applied.^{17,18} By considering an incompressible flow and increasing glycerol mass fraction (hence, increasing the shear viscosity), a Newtonian fluid model predicted a monotonically decreasing relationship between the quality factor and the glycerol mass fraction, failing to account for the observed experimental dependence. A Maxwell fluid model on the other hand captured the non-monotonic behavior. It was therefore concluded that the non-monotonic variation manifested the intrinsic viscoelastic properties of simple liquids.

For the bipyramidal geometry considered in Pelton et al.,^{18} the laser-induced excitation mechanism mainly excited the longitudinal vibration mode of the bipyramid. For nanospheres, the spherically symmetric fundamental breathing mode described in Sec. II is excited instead.^{11} Motivated by the experiment in Pelton et al.,^{18} we investigate how the quality factor of the breathing mode of an elastic sphere varies with the glycerol mass fraction in water-glycerol mixtures. The spherically symmetric geometry allows exact and analytical eigenvalue equations in both Newtonian (17) and viscoelastic fluid media.

With the same properties of water-glycerol mixtures at different mass fractions used in Pelton et al.^{18,20} (refer to Appendix B for a summary of these material properties), we compute the eigenfrequency predicted by the Newtonian fluid model using (17). A monotonic decrease in the quality factor with the glycerol mass fraction χ is observed in Fig. 4 (blue lines) for nanospheres with radii of 10, 20, and 40 nm.

We employ the Maxwell model to describe the viscoelasticity of the fluid medium and take into account the effect of fluid compressibility in a similar fashion as Khismatullin and

Nadim.^{21} The total stress tensor σ in a compressible viscoelastic fluid can be written as

σ = (−p + κ∇ · v) I + τ , (24)

which represents the sum of the isotropic part and the deviatoric stress tensor τ that has a vanishing trace for the linear viscoelastic case considered here.^{21} In a Maxwell fluid, the viscoelastic behavior is modeled as a purely viscous damper and a purely elastic spring connected in series. Due to the series connection, the total deviatoric stress in the viscoelastic fluid τ is the same as the deviatoric stress in the viscous damper τ_D as well as that in the elastic spring τ_S, i.e.

τ = τ_D = τ_S. (25)

However, the total rate of strain γ is a sum of the contributions from the damper γ_D and elastic spring γ_S

γ = γ_D + γ_S. (26)

The shear stress in the viscous damper is given by a Newtonian constitutive equation

τ_D = 2η_D ( γ̇_D − tr(γ̇_D) 3 I ) , (27)

where η_D is the shear viscosity of the damper. The shear stress in the elastic spring is given by τ_S = 2Eγ_S, (28)

where E is the elastic modulus. We differentiate (26) with respect to time and use (27) and (28) to obtain a constitutive equation for the total shear stress τ and total rate of strain γ̇ τ + λτ̇ = 2η ( γ̇ − tr(γ̇) 3 I ) , (29)

where λ = η/E is the relaxation time. In the derivation we have used that the total deviatoric shear stress is traceless, tr(τ ) = 0, which implies tr(τ_S) = 0 according to (25) and therefore tr(γ_S) = 0 by (28). As a result, we have tr(γ̇_D) = tr(γ̇) in (29). When the relaxation time is zero, λ = 0, (29) reduces to the Newtonian constitutive equation (14). Since harmonic solutions are sought for the velocity field, the total shear stress tensor τ should also have the same temporal dependence, exp(−iωt). We can therefore rewrite (29), with this time dependence assumed, as τ = 2η 1 − iλω ( γ̇ − tr(γ̇) 3 I ) . (30)

Comparing (30) with the Newtonian constitutive relation (14), we observe that the eigenvalue equation for the breathing mode of an elastic sphere in a Maxwell fluid can be obtained simply by making the following transformation in (17),^{18} η → η 1 − iλω · (31)

FIG. 4: Quality factor Q of radial vibrations of a sphere with radius R as a function of glycerol mass-fraction χ. (a) R = 40 nm. (b) R = 20 nm. (c) R = 10 nm. The red dotted lines represent the Maxwell model; the blue solid lines represent the Newtonian model.

Now using the relaxation times of water-glycerol mixtures at different glycerol mass fractions,^{20} with the other parameters the same as in the Newtonian case in Fig. 4 (blue solid lines), we obtain the quality factor as a function of the glycerol mass fraction χ (Fig. 4, red dotted lines) for different values of the nanosphere radius (Fig. 4a, b, c: 40 nm, 20 nm, 10 nm, respectively). The results for the Newtonian and viscoelastic models agree when the glycerol mass fraction χ is smaller than a certain critical value, which depends on the radius of the nanosphere. More significantly, the viscoelastic model predicts a non-monotonic variation as a function of χ, which is similar to the case of longitudinal vibration of bipyramidal gold nanoparticle reported in Pelton et al.,^{18} even though the vibration mechanism is fundamentally different.

In Fig. 4a (R = 40 nm), the Newtonian model predicts similar results as the viscoelastic model when χ ≲ 0.56 because the relaxation time of the mixture for these glycerol mass fractions is not large enough for the elastic effect to be significant. From (31) we can see that the elastic effects become significant if |λω| ≳ 1, i.e. when the relaxation time scale of the fluid λ is comparable with the vibration time scale 1/ω_r. Given a vibration frequency, we can therefore estimate the glycerol mass fraction beyond which the results of the viscoelastic model would deviate significantly from the Newtonian model. For instance, the vibration frequency (f = ω_r/2π) of a gold nanosphere with R = 40 nm in vacuum is given by (19) as f ≈ 38 GHz, and it can be verified that the real part of the vibration frequency depends very weakly on the surrounding medium for low-damping vibrations considered here (see the values for different media in Table II). The critical relaxation time such that |λ_cω| = 1 is given by λ_c ≈ 4 ps, which occurs when χ ≈ 0.56 (refer to Table III for the relaxation times of different water-glycerol mixtures). When the radius of the gold nanosphere decreases to R = 20 nm, the vibration frequency increases to f ≈ 76 GHz by (19), and the corresponding critical relaxation time decreases to λ_c ≈ 2 ps. Hence the results of the viscoelastic model begin to deviate from that of the Newtonian model when χ ≈ 0.36 (Fig. 4b). Similarly, the vibration frequency increases (f ≈ 152 GHz) when the nanosphere radius is reduced to 10 nm, which gives a smaller critical relaxation time (λ_c ≈ 1 ps), and hence a deviation from the Newtonian results at a smaller χ (Fig. 4c).

IV. DISCUSSION AND CONCLUSION

In this paper, we have revisited a classical calculation of the natural frequencies of a radially oscillating elastic sphere in simple and complex fluid media. We first considered the Newtonian fluid model taking into account both shear and bulk viscosities, and demonstrated that the fluid compressibility plays a significant role in the breathing mode of vibrating nanospheres. Should the limit of an incompressible flow be considered (see Appendix A), the quality factor is significantly overestimated (Q = 841), compared with the case of a compressible flow (Q = 52.6). Although Pelton et al.^{18} showed numerically that the effect of compressibility is insignificant for the case of longitudinal vibration of bipyramidal gold nanoparticles, we provide here an example where it is important to consider fluid compressibility in order to reasonably estimate the quality factor of the breathing mode of a nanosphere. Physically, the longitudinal vibration of the bipyramidal nanoparticle propagates through the shearing motion in the fluid, and hence the effect of fluid compressibility is insignificant. In contrast, due to the spherical symmetry in the breathing mode of a nanosphere, fluid compressibility plays a more significant role in propagating the energy through acoustic waves.

A viscoelastic response in a fluid triggered by high-frequency vibrations was demonstrated by Pelton et al.^{18} for a longitudinal vibration of bipyramidal gold nanoparticles, where they observed non-monotonic variations of the quality factor as a function of glycerol mass fraction that were not captured by a Newtonian fluid model. Motivated by these experimental observations, we have extended the classical problem of a radially vibrating elastic sphere in a Newtonian fluid to a viscoelastic fluid, modeled as a Maxwell fluid. Despite the fundamental difference in the vibration mode, the breathing mode of a nanosphere, taking into account the relaxation time, also predicts a non-monotonic variation of the quality factor as a function of the glycerol mass fraction, similar to the response of longitudinal vibration of a gold bipyramidal nanoparticle in a Maxwell fluid. A Newtonian fluid model fails to capture this non-monotonic behavior. Due to the simplicity of the spherical geometry considered in this work, the eigenvalue equation for the breathing mode in the viscoelastic fluid medium is exact and analytical.

The relaxation time λ of water-glycerol mixtures is typically small, on the order of 1– 100 ps (Table III); the viscoelastic response is triggered only when the vibration frequency is sufficiently high such that |λω| ≳ 1. For the cases studied in this paper, the real part of the vibration frequency can be effectively approximated by the vibration frequency of a sphere in vacuum (19), where we solve for s = k_sR for a given ratio of wave speeds in the elastic solid c_l/c_t. One can rewrite the condition |λω| ≳ 1 as |λc_ls/R| ≳ 1, which leads to the condition R ≲ λc_l|s|, a typical radius of the elastic structure smaller than which the viscoelastic response in the fluid would be triggered. For gold, |s| ≈ 3 by (19), and hence the viscoelastic effect has to be taken into account when the radius of the gold nanosphere is smaller than R ≈ 35 nm for a water-glycerol mixture with χ = 0.56, according to the material properties in Tables II and III.

We also comment on the idea of destroying virus particles by acoustic resonance (see Introduction). The lifetime (or damping time, τ_D = −1/ω_i) of the vibration was used in the literature^{6–9} to assess the feasibility of the idea. A major obstacle is the short damping time when the virus particle is embedded in a liquid.^{7,9} Assuming that the density and elastic properties of viruses were close to that of protein crystals (lysozyme),^{22} the inviscid model by Talati and Jha^8 estimated that the damping time for a virus in liquid was of the order of picoseconds.^{23} Specifically, for a virus particle of 50 nm radius, Talati and Jha estimated a damping time of 17.3 ps for a virus-water configuration. A longer damping time (34.4 ps) was estimated for a virus-glycerol configuration,^8 leading to a conclusion that this configuration was more favorable than the virus-water configuration for virus destruction. Here we comment on the effect of fluid viscoelasticity on these estimations. For the viruswater configuration, the relaxation time of water is small compared with the vibration time scale (|λω| ≈ 0.06 in this case), and hence the effect of viscoelasticity is negligible. However, the viscoelastic effect is significant for the virus-glycerol configuration because the relaxation time of glycerol is comparable to the vibration time scale (|λω| ≈ 37). Our calculation shows that the viscoelastic response triggered in glycerol significantly increases the damping time to 111 ps, suggesting a better likelihood of destroying the virus compared with previous estimations.

Finally, we note that experimental measurements of the quality factor of nanoparticles are considerably lower than the theoretical predictions. Previous research attributed the discrepancy to other dissipation mechanisms intrinsic to the particle that were not taken into account in the theoretical model, for example, internal friction within the nanoparticle and the dissipation in the capping layer surrounding the nanoparticle.^{11} Theoretical models taking into account these damping mechanisms and other plausible effects, such as the thermo-acoustic effect, are currently under investigation.

V. ACKNOWLEDGEMENTS

HAS thanks the Thermal Engineering Department of Tsinghua University for hosting a visit, where he first began to think about this problem. OSP thanks the Croucher Foundation for support through a Croucher Fellowship. VG is grateful to the Columbia Undergraduate Scholars Program for the Summer Enhancement Fellowship and to the Department of Mechanical and Aerospace Engineering at Princeton University for financial support and hospitality. We thank the NSF for partial support via grant CBET-1234500.

REFERENCES

1H. Portales, N. Goubet, L. Saviot, S. Adichtchev, D. B. Murray, A. Mermet, E. Duval, and M.-P. Pileni, “Probing atomic ordering and multiple twinning in metal nanocrystals through their vibrations,” Proc. Natl. Acad. Sci. U.S.A. 105, 14784–14789 (2008). 2K. Jensen, K. Kim, and A. Zettl, “An atomic-resolution nanomechanical mass sensor,” Nat. Nanotechnol. 3, 533–537 (2008).

3S. S. Verbridge, L. M. Bellan, J. M. Parpia, and H. G. Craighead, “Optically driven resonance of nanoscale flexural oscillators in liquid,” Nano Lett. 6, 2109–2114 (2006). 4J. L. Arlett, E. B. Myers, and M. L. Roukes, “Comparative advantages of mechanical biosensors,” Nat. Nanotechnol. 6, 203–215 (2011).

5M. Babincová, P. Sourivong, and P. Babinec, “Resonant absorption of ultrasound energy as a method of HIV destruction,” Med. Hypotheses 55, 450–451 (2000). 6L. H. Ford, “Estimate of the vibrational frequencies of spherical virus particles,” Phys. Rev. E 67, 051924 (2003).

7L. Saviot and D. B. Murray, “Comment on ”Estimate of the vibrational frequencies of spherical virus particles”,” Phys. Rev. E 69, 023901 (2004).

8M. Talati and P. K. Jha, “Acoustic phonon quantization and low-frequency Raman spectra of spherical viruses,” Phys. Rev. E 73, 011901 (2006).

9B. Stephanidis, S. Adichtchev, P. Gouet, A. McPherson, and A. Mermet, “Elastic properties of viruses,” Biophys. J. 93, 1354–1359 (2007).

10G. V. Hartland, “Coherent excitation of vibrational modes in metallic nanoparticles,” Annu. Rev. Phys. Chem. 57, 403–430 (2006).

11P. V. Ruijgrok, P. Zijlstra, A. L. Tchebotareva, and M. Orrit, “Damping of acoustic vibrations of single gold nanoparticles optically trapped in water,” Nano Lett. 12, 1063– 1069 (2012).

12M. Fujii, T. Nagareda, S. Hayashi, and K. Yamamoto, “Low-frequency Raman scattering from small silver particles embedded in SiO2 thin films,” Phys. Rev. B 44, 6243–6248 (1991).

13H. Lamb, “On the vibrations of an elastic sphere,” Proc. London Math. Soc. 13, 189–212 (1882).

14V. A. Dubrovskiy and V. S. Morochnik, “Natural vibrations of a spherical inhomogeneity in an elastic medium,” Izv. Earth Phys. 17, 494–504 (1981).

15D. E. Kheisin, “Radial oscillations of an elastic sphere in a compressible fluid,” Fluid Dyn.

2, 53–55 (1967).

16L. Saviot, C. H. Netting, and D. B. Murray, “Damping by bulk and shear viscosity of confined acoustic phonons for nanostructures in aqueous solution,” J. Phys. Chem. B 111, 7457–7461 (2007).

17D. Chakraborty, E. van Leeuwen, M. Pelton, and J. E. Sader, “Vibration of nanoparticles in viscous fluids,” J. Phys. Chem. C 117, 8536–8544 (2013).

18M. Pelton, D. Chakraborty, E. Malachosky, P. Guyot-Sionnest, and J. E. Sader, “Viscoelastic flows in simple liquids generated by vibrating nanostructures,” Phys. Rev. Lett. 111, 244502 (2013).

19The values of material parameters used in Ruijgrok et al.^{11} are slightly different from those in Table II, which result in the slight differences in the calculated quality factors.

20W. M. Slie, A. R. Donfor, and T. A. Litovitz, “Ultrasonic shear and longitudinal measurements in aqueous glycerol,” J. Chem. Phys. 44, 3712–3718 (1966).

21D. Khismatullin and A. Nadim, “Radial oscillations of encapsulated microbubbles in viscoelastic liquids,” Phys. Fluids 14, 3534–3557 (2002).

22M. Tachibana, K. Kojima, R. Ikuyama, Y. Kobayashi, and M. Ataka, “Sound velocity and dynamic elastic constants of lysozyme single crystals,” Chem. Phys. Lett. 332, 259–264 (2000).

23The density of lysozyme is ρ_s = 1210 kg/m^3. The longitudinal and transverse wave speeds are c_ℓ = 1817 m/s and c_t = 915 m/s, respectively. See Refs.^{8,22} for details.

Appendix A: Newtonian Incompressible Fluid

Consider small-amplitude waves in an incompressible viscous fluid described by the linearized Navier-Stokes equation

∇ · v = 0, (A1) ρ_f ∂v ∂t = −∇p + η∇^2v. (A2)

Note that due to the spherical symmetry of the problem the identity ∇^2v = ∇(∇ · v) = 0 holds, and (A2) simplifies to ρ_f ∂v ∂t = −∇p. (A3) Assuming time-periodic oscillations, the velocity field v = v(r, t)e_r can be obtained from the continuity equation (A1) as v(r, t) = ∞∑ n=1 B̃_n r^2 e^{−iωnt}, (A4)

where B̃_n are arbitrary constants, and ω_n are the frequencies of normal modes. The pressure field in the fluid can then be determined from (A3) as p(r, t) = − ∞∑ n=1 B̃_n iρ^f ω^n r e^{−iωnt}. (A5) While the stress in the solid (13) remains unchanged, the stress in the fluid becomes σ^f_{rr} = −p + 2η ∂v ∂r = ∞∑ n=1 B̃_n ( iρ_f ω_n r − 4η r^3 ) e^{−iωnt}. (A6) We again couple the solid and fluid problems by matching the velocity and stress at the boundary, r = R, and requiring the existence of a non-trivial solution, which leads to (20) in the main text.

Appendix B: Material parameters of the water-glycerol mixture

The density, ρ_f , shear viscosity, η, bulk viscosity, κ, and speed of sound, c, of the waterglycerol mixture for different mole fractions of glycerol, χ_ν , were experimentally measured by Slie et al.^{20} We obtain the parameter values for different mass fractions of glycerol, χ, by using the relation χ = χ_ν /(χ_ν + (1 − χ_ν )μ_w/μ_g), where μ_w = 18 g/mol and μ_g = 92 g/mol are the molar masses of pure water and pure glycerol respectively. We use the relation λ = η/G_∞ and the measured values of the high frequency shear modulus, G_∞, to find the relaxation time, λ, of the water-glycerol mixture for different values of χ.^{18,20} Numerical values of the parameters are summarized in Table III.

χ ρ_f (kg/m^3 ) η (Pa · s) κ (Pa · s) c (m/s) λ (ps) 0 1000 0.000894 0.00286 1510 0.647 0.36 1090 0.00270 0.00756 1662 1.87 0.56 1140 0.00527 0.0116 1760 3.51 0.71 1190 0.0200 0.0400 1830 12.7 0.8 1210 0.0447 0.0760 1885 27.1 0.85 1220 0.0923 0.120 1909 54.2 0.95 1250 0.452 0.407 1920 243 1 1260 0.988 0.790 1930 500

TABLE III: Values of fluid density (ρ_f ), shear viscosity (η), bulk viscosity (κ), speed of sound (c) and relaxation time (λ) for different glycerol mass fractions (χ).