arXiv:1909.12466v1 [physics.optics] 27 Sep 2019

Creating locally interacting Hamiltonians in the synthetic frequency dimension for photons

Luqi Yuan^{1,∗}, Avik Dutt^2, Mingpu Qin^3, Shanhui Fan^{2,†}, and Xianfeng Chen^{1,4,‡} 1State Key Laboratory of Advanced Optical Communication Systems and Networks, School of Physics and Astronomy, Shanghai Jiao Tong University, Shanghai 200240, China 2Department of Electrical Engineering, and Ginzton Laboratory, Stanford University, Stanford, CA 94305, USA 3School of Physics and Astronomy, Shanghai Jiao Tong University, Shanghai 200240, China 4Collaborative Innovation Center of Light Manipulations and Applications, Shandong Normal University, Jinan 250358China ∗Corresponding author: yuanluqi@sjtu.edu.cn †Corresponding author: shanhui@stanford.edu ‡Corresponding author: xfchen@sjtu.edu.cn (Dated: September 30, 2019)

Abstract

The recent emerging field of synthetic dimension in photonics offers a variety of opportunities for manipulating different internal degrees of freedom of photons such as the spectrum of light. While nonlinear optical effects can be incorporated into these photonic systems with synthetic dimensions, these nonlinear effects typically result in long-range interactions along the frequency axis. Thus it has been difficult to use of the synthetic dimension concept to study a large class of Hamiltonians that involves local interactions. Here we show that a Hamiltonian that is locally interacting along the synthetic dimension can be achieved in a dynamically-modulated ring resonator incorporating χ^{(3)} nonlinearity, provided that the group velocity dispersion of the waveguide forming the ring is specifically designed. As a demonstration we numerically implement a Bose-Hubbard model, and explore photon blockade effect, in the synthetic frequency space. Our work opens new possiblities for studying fundamental many-body physics in the synthetic space in photonics, with potential applications in optical quantum communication and quantum computation.

The concept of synthetic dimension enables one to explore higher dimensional physics in lower dimensional systems [1–11]. In photonics [12, 13], synthetic dimension can be achieved by exploiting various degrees of freedom of light such as its frequency [14, 15], spatial mode [16], or orbital angular momentum [17], and by specifically controlling the coupling between these degrees of freedom [18–20]. While initially explored mostly theoretically [21–27], very recently there have been a number of important experimental developments, including the first experimental demonstration of topological insulators with synthetic dimensions [16], the measurement of band structure along the frequency axis of light [28], and the control of light spectrum in synthetic space [29, 30].

Most of the existing theoretical and experimental works on synthetic dimension in photonics concerns linear processes without photon-photon interactions. Certainly, it would be of interest to consider nonlinear systems where there is photon-photon interaction. Moreover, since one of the major objectives by going into synthetic dimension is to create a platform to study specific interacting Hamiltonians that are of physical significance, it would be important to develop a strategy to synthesize these interacting Hamiltonians. A very large class of interesting interacting Hamiltonians have local interactions [31–34]. Attempts to achieve such locally interacting Hamiltonians in synthetic space and have been made in photonics in the geometric angular coordinate [35] and also in ultracold atoms with spin being the internal degree of freedom [36]. On the other hand, as is known and we will briefly reiterate below, the standard form of nonlinear optics typically leads to a form of interaction that is nonlocal in the synthetic space [37, 38]. How to achieve a Hamiltonian with local interactions in the synthetic space for photons, thus therefore represents an important open theoretical question.

In this Letter, we consider a synthetic frequency dimension of light, formed in a ring resonator incorporating a modulator. To create photon-photon interaction we consider χ^{(3)} processes in the waveguide forming the ring. We show that a local photon-photon interaction in the frequency dimension can be achieved with a careful design of the group velocity dispersion of the waveguide [Fig. 1(a)]. As a demonstration we show that this system can be used to demonstrate a Bose-Hubbard model, and achieve photon-blockade effects along the synthetic axis. This work here significantly broadens the range of physics phenomena that can be studied in photonic synthetic space, and may lead to new opportunities in quantum simulations and in the manipulation of light.

FIG. 1: (a) A ring resonator, composed by two types of single-mode waveguides A and B, undergoing the dynamic modulation. (b) A ring under the dynamic modulation supports a synthetic lattice along the frequency dimension. (c) The ring is coupled with the through-port and drop-port waveguides.

We start with a brief review of the ring resonator under the dynamic modulation as shown in Fig. 1(b), which naturally leads to a synthetic dimension of light along the frequency axis. We consider a ring composed by a single-mode waveguide with an effective refractive index n_{eff} , and a length l. For simplicity, assuming zero group velocity dispersion in the waveguide, the ring resonator supports resonant modes at the resonant frequencies ω_m = ω_0 + mΩ where Ω ≡ 2πc/n_{eff} l ≪ ω_0 is the free-spectral-range (FSR) for the ring. We place a phase modulator inside the ring and choose the modulation frequency to be equal to the free spectral range. The transmission of light passing through the modulator can be described by a time-dependent transmission coefficient

T = e^{i2α cos(Ωt)}, (1)

where α is the modulation amplitude. We assume that the field experiences small changes for each round-trip. Then after one round-trip, the change of the field amplitude E_m for the m-th resonant mode can be written as 2π Ω ∂E_m ∂T ≡ ΔE_m = iα(E_{m+1} + E_{m−1}), (2)

where T is the slow time variable [39]. The dynamics of Eq. (2) is described by an effective

Hamiltonian: H_0 = −ℏJ ∑ m ( a^†_ma_{m+1} + h.c. ) , (3)

where J = αΩ/2π is the modulation strength and a_m (a^†_m) is the annihilation (creation) operator for the m-th resonant mode. The Hamiltonian (3) describes a one-dimensional tight-binding model along the synthetic frequency axis [see Fig. 1(b)]. With this approach, a wide variety of non-interacting Hamiltonian with different connectivity and topological properties can be created [12]. However, there have been far less works on creating important interacting Hamiltonians.

As an illustration of the general difficulty as well as our approach of creating locally interacting Hamiltonian in the frequency synthetic dimension, we aim to synthesize the effective Bose-Hubbard Hamiltonian in the synthetic frequency dimension H_1 = −ℏJ ∑ m ( a^†_ma_{m+1} + h.c. ) − ℏg 2 ∑ m a^†_ma^†_ma_ma_m, (4)

where g is the local nonlinear strength. Although nonlinear optical phenomena in many photonic materials have been extensively studied, creating the Hamiltonian of Eq. (4) in the frequency synthetic space is in fact non-trivial [37]. The introduction of the nonlinearity typically leads to long-range interactions over all synthetic lattice sites. For example, the dynamically-modulated ring as shown in Fig. 1(b), with a third-order nonlinear susceptibility χ^{(3)} is described by an interacting Hamiltonian [38]: H_2 = −ℏJ ∑ m ( a^†_ma_{m+1} + h.c. ) − ℏg 2 ∑ m,n,p,q a^†_ma^†_na_pa_q − ℏg 3 ∑ m,n ( a^†_ma^3_n + h.c. ) , (5)

as can be derived using the rotating wave approximation. In Eq. (5), the second and third terms describe two four-wave-mixing effects. The second term describes the hyperparametric oscillation process involving four modes with frequencies with ω_m +ω_n = ω_p +ω_q. The third term describes the third harmonic generation (THG) process with ω_m = 3ω_n. Comparing Eq. (4) with Eq. (5), we see that the interacting term in Eq. (4) corresponds to the self-phase modulation (SPM) process. In Eq. (5), however, in addition to the SPM process, other terms which describe the cross phase modulation (XPM) process, other hyper-parametric processes, and the THG process result in long-range interactions between different resonant modes in the ring (see Fig. 2). While here for illustration purposes we consider a specific type of nonlinearity, the observation is in fact rather general: standard nonlinearity does not lead to local interactions in the synthetic frequency dimension.

FIG. 2: Four-wave-mixing processes in a ring with a third-order nonlinear susceptibility including the hyper-parametric processes (SPM, XPM and others) and the THG process.

In order to synthesize the Bose-Hubbard model where the interaction is local along the frequency dimension, we propose a ring consisting of two sections of waveguides. The two sections have the same χ^{(3)} nonlinear susceptibility. However, they have opposite group velocity dispersion (GVD), as illustrated in Fig. 1(a). In the linear regime of light propagation, for each complete round-trip as light goes around the ring, the dispersion effect in the two waveguide sections cancels. Hence this ring also features equally spaced resonances along the frequency axis, same as a ring with zero GVD, and a one-dimensional synthetic frequency dimension can be created in this ring by applying the dynamic modulation. On the other hand, in each waveguide section, due to the the group velocity dispersion, the only phase-matched processes are the SPM and XPM processes. Moreover, as we will show below, in any Hilbert space with a fixed photon number the Hamiltonian for the XPM process in fact reduces to that for the SPM process. We therefore show that our design supports an effective Bose-Hubbard Hamiltonian (4) along the frequency axis.

In the following, we explain our design in details. We first consider light propagating inside a single-mode waveguide. The evolution of the field amplitude A(z, ω) with the frequency ω at the position z in the waveguide can be described as [40]: ∂A(z, ω) ∂z = −iβ(ω)A(z, ω), (6) where β(ω) denotes the propagation wavevector. β(ω) can be expanded around the reference frequency ω_0, i.e.,

β(ω) − β(ω_0) = dβ dω | | |_{ω0} (ω − ω^0) + 1 2 d^2β dω^2 | | |_{ω0} (ω − ω^0)^2 + . . . . (7)

Here we set β_0 = β(ω_0), v_g = (dβ/dω)^{−1} is the group velocity, and β_2 = d^2β/dω^2 is the GVD around ω_0. By neglecting the higher-order terms in Eq. (7), one can write the field amplitude of light after it propagates through a waveguide with the length L A(z = L, ω) = A(z = 0, ω)e^{−iβ0L−i(ω−ω0)L/vg −iβ2(ω−ω0)2L/2}. (8) Note that the GVD induces a frequency-dependent phase delay.

FIG. 3: (a) A general four-wave-mixing process in a waveguide with the third-order susceptibility χ^{(3)}. (b) The plot of ΔI ∝ sinc^2(ΔkL) showing the effect of the phase mismatching .

Next, we explore the light propagates through the waveguide section having the positive GVD (β_2 > 0) and χ^{(3)} as shown in Fig. 1(a). For simplicity, we consider two incident waves with the frequencies ω_1 and ω_2 respectively, in the vicinity of the reference frequency ω_0. We look for the solution for a general four-wave-mixing process where output fields are generated at frequencies ω_3 and ω_4, satisfying the energy conservation relation ω_3 + ω_4 = ω_1 + ω_2 [see Fig. 3(a)]. We also assume the narrowband limit, i.e., |ω_0 − ω_m| ≪ ω_0, m = 1, 2, 3, 4. The resulting coupled-mode equations under the slowly varying amplitude approximation are [37] ∂Ã_3 ∂z = i ω^2_0 2β_0c^2 χ^{(3)}Ã_1Ã_2Ã^∗_4e^{−iΔkz}, (9) ∂Ã_4 ∂z = i ω^2_0 2β_0c^2 χ^{(3)}Ã_1Ã_2Ã^∗_3e^{−iΔkz}, (10) where Ã_m = A_me^{iβ(ωm )z} and the momentum mismatch is

Δk = β_2 2 [ (ω_3 − ω_0)^2 + (ω_4 − ω_0)^2 − (ω_1 − ω_0)^2 − (ω_2 − ω_0)^2 ] . (11)

At frequencies around ω_0, the phase matching condition (Δk = 0) is satisfied if ω_1 = ω_2 = ω_3 = ω_4, which corresponds to the SPM process, or ω_1 = ω_{3(4)} and ω_2 = ω_{4(3)} ≠ ω_1, which corresponds to the XPM process. For other FWM processes with the phase mismatching condition Δk ≠ 0, the efficiency for frequency conversion is proportional to the phase mismatch factor, i.e., sinc^2(ΔkL), as plotted in Fig. 3(b). For |ΔkL| ≥ π, the conversion efficiency is significantly suppressed. In particular, for |ΔkL| = nπ with n being the positive integer, sinc^2(ΔkL) = 0, meaning that FWM processes other than SPM and XPM vanish completely. Similar argument is also valid for the THG process, where the conversion efficiency of THG is also strongly reduced due to the phase mismatching.

Having treated a light propagation effect in a single waveguide section, we now discuss the ring in Fig. 1(a). The waveguide A with the length L = l/2 has a positive GVD (β_{2,A} > 0). The waveguide B with the length L has a negative GVD (β_{2,B} < 0), we assume that β_{2,B} = −β_{2,A}. The quadratic term of the phase delay in Eq. (8) due to the dispersion effect is therefore compensated once the light propagates through the entire ring. Hence this ring supports equally-spaced resonant modes at the resonant frequencies ω_m with the FSR Ω. As light goes through each round trip, its amplitude experiences a small change due to both the nonlinearity and the dynamic modulation. After a round-trip, the change of the field amplitude Ã_m for the m-th mode at frequency ω_m can be written from Eqs. (2), (9), and (10) 2π Ω ∂Ã_m ∂T = iα(Ã_{m+1} + Ã_{m−1}) + i ω^2_0 2β_0c^2 χ^{(3)}|Ã_m|^2Ã_m + i ∑ n≠m 2ω^2_0 β_0c^2 χ^{(3)}|Ã_n|^2Ã_m, (12)

The corresponding effective Hamiltonian from Eq. (12) reads: H_3 = −ℏJ ∑ m ( a^†_ma_{m+1} + h.c. ) − ℏg 2 ∑ m a^†_ma^†_ma_ma_m − ℏg ∑ m,n≠m a^†_na^†_ma_ma_n. (13)

Here g = 3ℏω^2_0χ^{(3)}/V n^4_0ϵ_0 describes the strength of the nonlinearity [41, 42], where V is the effective mode volume, n_0 = n(ω_0), and ϵ_0 is the permittivity of free space.

In a Hilbert space where the total number of photons N is conserved in the the system,

Eq. (13) can be further simplified by noting that ∑ m,n≠m a^†_na^†_ma_ma_n = ∑ m a^†_ma_m ( ∑ n≠m a^†_na_n ) = ∑ m a^†_ma_m ( N − a^†_ma_m ) = N^2−N− ∑ m a^†_ma^†_ma_ma_m. (14) The resulting Hamiltonian reads H_4 = −ℏJ ∑ m ( a^†_ma_{m+1} + h.c. ) + ℏg 2 ∑ m a^†_ma^†_ma_ma_m − ℏg(N^2 − N). (15)

One notices that the third term ℏg(N^2 − N) is just a constant shift in energy. The change of sign in the second term does not affect the physical observables for bosonic systems. Hence, the Hamiltonian (15) [or the Hamiltonian (13)] describes the same physics as our desired Hamiltonian in Eq. (4). We have therefore shown that a Bose-Hubbard model with local interaction in the synthetic frequency dimension can be achieved by the ring shown in Fig. 1(a).

To demonstrate some of the physics effects along the synthetic frequency dimension in the Hamiltonian (13), we perform numerical simulations with photon number N = 2. External waveguides are coupled with the ring, where the photons input into the ring from the through-port and the detection can be made at the drop-port waveguide [see Fig. 1(c)]. Hence, our system becomes open, and the photon transport property is described by the input-output formalism in the Heisenberg picture [43, 44]: da_m(t) dt = i ℏ [H_3, a_m] − γa_m(t) + i √ γc_{in,m}(t), (16)

c_{out,m}(t) = c_{in,m}(t) − i √ γa_m(t), (17) d_{out,m}(t) = −i √ γa_m(t), (18) where γ is the waveguide-cavity coupling strength. c_{in,m} (c_{out,m}) and d_{out,m} are the input (out) annihilation operators for photons at the frequency ω_m in the through-port and dropport waveguides, respectively.

As the input state, we consider a strongly-correlated photon pair [45]: |ϕ(p, q)⟩ = ∫ ∫ dt_1dt_2f ( t_1 + t_2 2 ) h (t_1 − t_2) c^†_{in,q}(t_2)c^†_{in,p}(t_1)|0⟩, (19)

which satisfies the normalization condition ⟨ϕ|ϕ⟩ = 1. We further assume that h(t) has an extremely short temporal width. Hence the input state (19) describes the scenario where two photons at the frequencies ω_p+Δω and ω_q +Δω are simultaneously injected into the throughport waveguide. We choose f(t) = e^{−(t−tD )2/Δt2} e^{−i2Δωt}, where t_D describes the timing of the incident photons, Δt is the pulse temporal width, and Δω is the small frequency detuning. To excite the individual sites in the synthetic lattice along the frequency dimension, the condition 1/Δt ≪ Ω is required.

To measure the quantum statistics of the photons inside the ring, we define the twophoton correlation function G^{(2)}m,n(t, t^′) = ⟨ϕ|d^†_{out,m}(t)d^†_{out,n}(t^′)d_{out,n}(t^′)d_{out,m}(t)|ϕ⟩ [46]. We then compute the two-photon correlation probability that two output photons coincide in time P_{m,n} = ∫ dtG^{(2)}_{m,n}(t, t). (20) The simulation procedure follows the standard formalism [45] but in the synthetic frequency dimension. We consider the synthetic lattice in Fig. 1(b) involving 31 resonant modes (m = −15, . . . , 15), and set γ = 0.2J, t_D = 20J^{−1}, and Δt = 6.4J^{−1}. We also choose Δω = g to compensate for the overall frequency shift in the effective Bose-Hubbard model. A photon pair |ϕ(−4, 4)⟩ is injected into the waveguide. We consider the cases with g = 0, g = 2J, and g = 10J in the simulations. Normalized distributions of the two-photon correlation probability P_{m,n} for each choice of g are plotted in Figs. 4(a)-(c). There is no photon interaction in the g = 0 case. Notice the existence of non-zero probability P_{m,m} where the output photons have the same frequency. As the interaction increases the output photon statistics changes. For a large g = 10J, the correlation probability P_{m,m} = 0 for all m. High nonlinearity thus introduces a large blockade effect at each resonant mode along the synthetic frequency dimension.

We next use the photon pair |ϕ(−15, −15)⟩ as the input and assume that there is a sharp boundary at ω_{−16} in the synthetic frequency dimension. Such an artificial sharp boundary can be created by adding another ring to strongly couple only to the −16th resonant mode but no other modes [27]. In this input state the two photons have the same carrier frequencies. Figs. 4(d)-(f) show the simulated normalized distributions of the twophoton correlation probability P_{m,n} for different g. At g = 0, there is a strong probability for the two photons to have the same frequencies. In contrast, with a large nonlinearity g = 10J, away from the input frequency at ω_{−15}, there is very little probability that the output photons exhibit the same frequencies. Again, we see strong photon-blockade effect in the synthetic frequency dimension.

FIG. 4: Normalized distributions of the two-photon correlation probability P_{m,n}. (a)-(c) The input photon pair is |ϕ(−4, 4)⟩ with g = 0, g = 2J, and g = 10J, respectively. (a)-(c) The input photon pair is |ϕ(−15, −15)⟩ with g = 0, g = 2J, and g = 10J, respectively. Positions inside two dashed lines corresponds to P_{m,m}.

Simulations in Fig. 4 show the photon-photon interaction along the synthetic frequency dimension, which is an analog to the on-site nonlinear interaction in the spatial dimension [47, 48]. Moreover, we note that simulation results in Fig. 4 are the same as results performed by simulating Eqs. (16)-(18) with H_3 replaced by H_1 in Eq. (4), indicating that the Hamiltonian H_3 in Eq. (13) indeed provides an implementation of the Bose-Hubbard model in the synthetic frequency dimension.

Our proposed system requires waveguides with strong nonlinearity and large group velocity dispersion, which is experimentally challenging but may be achievable with the current start-of-the-art technology. For a ring with the length ∼ 1 mm, Ω/2π is ∼ 10 GHz. The modulation strength J/2π can be tuned at the order of 0.1−1 GHz to make the system operate in the weak modulation regime. Photonic crystal fiber filled with a high-density atomic gas has the potential to create a nonlinearity with g/2π up to ∼ 1 GHz in the few-photon level [49]. Strong group velocity dispersion is desired to bring the phase-mismatching condition |ΔkL_A| = nπ, which can be simplified to |β_2L_AΩ^2| ∼ 2π. The necessary high dispersion β_2 ∼ 10^{−19} s^2/m is possible with dispersion engineering in the photonic crystal fiber [50] or by exploiting mode crossing in coupled waveguides [51]. The theoretical proposal here may also be implementable in the microwave frequency range using superconducting quantum circuits [52].

In summary, we show that a ring resonator undergoing dynamic modulation can be used to achieve an interacting Hamiltonian where the interaction is local along the synthetic frequency dimension, provided that the ring incorporates χ^{(3)} nonlinearity, and with a specific design of the group velocity dispersion of the ring. Our work complements other emerging efforts in creating locally interacting Hamiltonian in synthetic space, by showing that such locally interacting Hamiltonian can be achieved in a system that has been widely used in photonics. The possibility of creating locally interacting Hamiltonian in the synthetic frequency dimension is fundamentally important for future studies of photon-photon interactions and many-body physics with synthetic dimensions in photonics, with promising potentials for a variety of quantum optical applications such as quantum information science and quantum communication technology [31, 53].

We notice Ref. [36] when we were in the final stage of preparing this paper.

Acknowledgments

This paper is supported by National Natural Science Foundation of China (11974245), National Key R&D Program of China (2018YFA0306301 and 2017YFA0303701), Natural Science Foundation of Shanghai (19ZR1475700). This work is also partially supported by the U.S. Air Force Office of Scientific Research Grant No. FA9550-18-1-0379, a Vannevar Bush Faculty Fellowship from the U. S. Department of Defense (Grant No. N00014-17-1-3030), as well as the U.S. National Science Foundation Grant No. CBET-1641069.

[1] O. Boada, A. Celi, J. I. Latorre, and M. Lewenstein, “Quantum simulation of an extra dimension,” Phys. Rev. Lett. 108, 133001 (2012).

[2] D. Jukić and H. Buljan, “Four-dimensional photonic lattices and discrete tesseract solitons,” Phys. Rev. A 87, 013814 (2013).

[3] A. Celi, P. Massignan, J. Ruseckas, N. Goldman, I. B. Spielman, G. Juzeliūnas, and M.

Lewenstein, “Synthetic gauge fields in synthetic dimensions,” Phys. Rev. Lett. 112, 043001 (2014).

[4] M. Mancini, G. Pagano, G. Cappellini, L. Livi, M. Rider, J. Catani, C. Sias, P. Zoller, M.

Inguscio, M. Dalmonte, and L. Fallani, “Observation of chiral edge states with neutral fermions in synthetic Hall ribbons,” Science 349, 1510 (2015).

[5] B. K. Stuhl, H.-I. Lu, L. M. Aycock, D. Genkina, and I. B. Spielman, “Visualizing edge states with an atomic Bose gas in the quantum Hall regime,” Science 349, 1514 (2015).

[6] B. Gadway, “Atom-optics approach to studying transport phenomena,” Phys. Rev. A 92, 043606 (2015).

[7] L. F. Livi, G. Cappellini, M. Diem, L. Franchi, C. Clivati, M. Frittelli, F. Levi, D. Calonico, J. Catani, M. Inguscio, and L. Fallani, “Synthetic Dimensions and Spin-Orbit Coupling with an Optical Clock Transition,” Phys. Rev. Lett. 117, 220401 (2016).

[8] S. Kolkowitz, S. L. Bromley, T. Bothwell, M. L. Wall, G. E. Marti, A. P. Koller, X. Zhang, A. M. Rey, and J. Ye, “SpinCorbit-coupled fermions in an optical lattice clock,” Nature 542, 66 (2017).

[9] H. M. Price, T. Ozawa, and N. Goldman, “Synthetic dimensions for cold atoms from shaking a harmonic trap,” Phys. Rev. A 95, 023607 (2017).

[10] I. Martin, G. Refael, and B. Halperin, “Topological Frequency Conversion in Strongly Driven Quantum Systems,” Phys. Rev. X 7, 041008 (2017).

[11] Y. Baum and G. Refael, “Setting Boundaries with Memory: Generation of Topological Boundary States in Floquet-Induced Synthetic Crystals,” Phys. Rev. Lett. 120, 106402 (2018).

[12] L. Yuan, Q. Lin, M. Xiao, and S. Fan, “Synthetic Dimension in Photonics,” Optica 5, 1396 (2018).

[13] T. Ozawa and H. M. Price, “Topological quantum matter in synthetic dimensions,” Nat. Rev.

Phys. 1 349 (2019).

[14] L. Yuan, Y. Shi, and S. Fan, “Photonic gauge potential in a system with a synthetic frequency dimension,” Opt. Lett. 41, 741–744 (2016).

[15] T. Ozawa, H. M. Price, N. Goldman, O. Zilberberg, and I. Carusotto, “Synthetic dimensions in integrated photonics: From optical isolation to four-dimensional quantum Hall physics,” Phys. Rev. A 93, 043827 (2016).

[16] E. Lustig, S. Weimann, Y. Plotnik, Y. Lumer, M. A. Bandres, A. Szameit, and M. Segev, “Photonic topological insulator in synthetic dimensions,” Nature 567, 356 (2019).

[17] X.-W. Luo, X. Zhou, C.-F. Li, J.-S. Xu, G.-C. Guo, and Z.-W. Zhou, “Quantum simulation of 2D topological physics in a 1D array of optical cavities,” Nat. Commun. 6, 7704 (2015).

[18] A. Schwartz and B. Fischer, “Laser mode hyper-combs,” Opt. Express 21, 6196–6204 (2013). [19] L. Yuan, M. Xiao, Q. Lin, and S. Fan, “Synthetic space with arbitrary dimensions in a few rings undergoing dynamic modulation,” Phys. Rev. B 97, 104105 (2018).

[20] E. Lustig, Y. Plotnik, Z. Yang, and M. Segev, “3D Parity Time symmetry in 2D photonic lattices utilizing artificial gauge fields in synthetic dimensions,” Conference on Lasers and Electro-Optics, paper FTu4B.1 (2019).

[21] L. Yuan and S. Fan, “Bloch oscillation and unidirectional translation of frequency in a dynamically modulated ring resonator,” Optica 3, 1014–1018 (2016).

[22] Q. Lin, M. Xiao, L. Yuan, and S. Fan, “Photonic Weyl point in a two-dimensional resonator lattice with a synthetic frequency dimension,” Nat. Commun. 7, 13731 (2016).

[23] Y. Zhang and Y. Zhu, “Generation of Weyl points in coupled optical microdisk-resonator arrays via external modulation,” Phys. Rev. A 96, 013811 (2017).

[24] X.-W. Luo, X. Zhou, J.-S. Xu, C.-F. Li, G.-C. Guo, C. Zhang, and Z.-W. Zhou, “Syntheticlattice enabled all-optical devices based on orbital angular momentum of light,” Nat. Commun. 8, 16097 (2017).

[25] X.-F. Zhou, X.-W. Luo, S. Wang, G.-C. Guo, X. Zhou, H. Pu, and Z.-W. Zhou, “Dynamically manipulating topological physics and edge modes in a single degenerate optical cavity,” Phys. Rev. Lett. 118, 083603 (2017).

[26] X.-W. Luo, C. Zhang, G.-C. Guo, and Z.-W. Zhou, “Topological photonic orbital-angular-momentum switch,” Phys. Rev. A 97, 043841 (2018).

[27] L. Yuan, Q. Lin, A. Zhang, M. Xiao, X. Chen, and S. Fan, “Photonic gauge potential in one cavity with synthetic frequency and orbital angular momentum dimensions,” Phys. Rev. Lett. 122, 083903 (2019).

[28] A. Dutt, M. Monkov, Q. Lin, L. Yuan, D. A. B. Miller, and S. Fan “Experimental band structure spectroscopy along a synthetic dimension,” Nat. Commun. 10, 3122 (2019).

[29] B. A. Bell, K. Wang, A. S. Solntsev, D. N. Neshev, A. A. Sukhorukov, and B. J. Eggleton, “Spectral photonic lattices with complex long-range coupling,” Optica 4, 1433–1436 (2017).

[30] C. Qin, F. Zhou, Y. Peng, D. Sounas, X. Zhu, B. Wang, J. Dong, X. Zhang, A. Alù, and P. Lu, “Spectrum control through discrete frequency diffraction in the presence of photonic gauge potentials,” Phys. Rev. Lett. 120, 133901 (2018).

[31] I. Bloch, J. Dalibard, and W. Zwerger, “Many-body physics with ultracold gases,” Rev. Mod.

Phys. 80, 885 (2008).

[32] D. E. Chang, V. Vuletić, and M. D. Lukin, “Quantum nonlinear optics - photon by photon,” Nat. Photonics 8, 685 (2014).

[33] D. Roy, C. M. Wilson, O. Firstenberg, “Colloquium: Stongly interacting photons in onedimensional continuum,” Rev. Mod. Phys. 89, 021001 (2017).

[34] D. A. Abanin, E. Altman, I. Bloch, and M. Serbyn, “Colloquium: Many-body localization, thermalization, and entanglement,” Rev. Mod. Phys. 91, 021001 (2019).

[35] T. Ozawa and I. Carusotto, “Synthetic dimensions with magnetic fields and local interactions in photonic lattices,” Phys. Rev. Lett. 118, 013601 (2017).

[36] L. Barbiero, L. Chomaz, S. Nascimbene, and N. Goldman, “Bose-Hubbard physics in synthetic dimensions from interaction Trotterization,” arXiv:1907.10555v1 (2019).

[37] R. W. Boyd, Nonlinear Optics, 3rd (Academic Press, Burlington, MA, 2008). [38] D. V. Strekalov, C. Marquardt, A. B. Matsko, H. G. L. Schwefel, and G. Leuchs, “Nonlinear and quantum optics with whispering gallery resonators,” J. Opt. 18, 123002 (2016).

[39] H. A. Haus, “Mode-locking of lasers,” IEEE J. Sel. Top. Quantum Electron. 6, 1173 (2000). [40] H. A. Haus, Waves and Fields in Optoelectronics (Prentice-Hall, 1984). [41] A. B. Matsko, A. A. Savchenkov, D. Strekalov, V. S. Ilchenko, and L. Maleki, “Optical hyperparametric oscillations in a whispering-gallery-mode resonator: Threshold and phase diffusion,” Phys. Rev. A 71, 033804 (2005).

[42] Y. K. Chembo, D. V. Strekalov, and N. Yu, “Spectrum and Dynamics of Optical Frequency Combs Generated with Monolithic Whispering Gallery Mode Resonators,” Phys. Rev. Lett. 104, 103902 (2010).

[43] C. W. Gardiner and M. J. Collett, “Input and output in damped quantum systems: Quantum stochastic differential equations and the master equation,” Phys. Rev. A 31, 3761 (1985).

[44] S. Fan, Ş. E. Kocabaş, and J.-T. Shen, “Input-output formalism for few-photon transport in one-dimensional nanophotonic waveguides coupled to a qubit,” Phys. Rev. A 82, 063821 (2010).

[45] L. Yuan, M. Xiao, S. Xu, and S. Fan, “Creating anyons from photons using a nonlinear resonator lattice subject to dynamic modulation,” Phys. Rev. A 96, 043864 (2017).

[46] M. O. Scully and M. S. Zubairy, Quantum Optics (Cambridge University Press, Cambridge, UK 1997).

[47] K. M. Birnbaum, A. Boca, R. Miller, A. D. Boozer, T. E. Northup, and H. J. Kimble, “Photon blockade in an optical cavity with one trapped atom,” Nature 436, 87 (2005).

[48] A. V. Gorshkov, J. Otterbach, M. Fleischhauer, T. Pohl, and M. D. Lukin, “Photon-Photon Interactions via Rydberg Blockade,” Phys. Rev. Lett. 107, 133602 (2011).

[49] V. Venkataraman, K. Saha, and A. L. Gaeta, “Phase modulation at the few-photon level for weak-nonlinearity-based quantum computing,” Nat. Photonics 7, 138 (2013).

[50] Y. Zhu, J. A. Greenberg, N. Ain Husein, and D. J. Gauthier, “Giant all-optical tunable group velocity dispersion in an optical fiber,” Opt. Express 22, 14382 (2014).

[51] M. B. Mia, N. Jaidye, and S. Kim, “Extremely high dispersions in heterogeneously coupled waveguides,” Opt. Express 27, 10426 (2019).

[52] N. R. A. Lee, M. Pechal, E. Alex Wollack, P. Arrangoiz-Arriola, Z. Wang, and A. H. Safavi- Naeini, “Electric fields for light: Propagation of microwave photons along a synthetic dimension,” arXiv:1908.10329v1 (2019).

[53] T. Ozawa, H. M. Price, A. Amo, N. Goldman, M. Hafei, L. Lu, M. C. Rechtsman, D. Schuster, J. Simon, O. Zilberberg, and I. Carusotto, “Topological Photonics,” Rev. Mod. Phys. 91, 015006 (2019).